From: Kamil Dudka <kdudka@redhat.com>
Date: Mon, 14 Sep 2015 09:37:15 +0200
Subject: [PATCH 3/7] Support major/minor device numbers over 127 (bz#450109)

diff --git a/src/copyin.c b/src/copyin.c
index b29f348..1142d6a 100644
--- a/src/copyin.c
+++ b/src/copyin.c
@@ -1123,15 +1123,15 @@ read_in_binary (struct cpio_file_stat *file_hdr,
       swab_array ((char *) short_hdr, 13);
     }
 
-  file_hdr->c_dev_maj = major (short_hdr->c_dev);
-  file_hdr->c_dev_min = minor (short_hdr->c_dev);
+  file_hdr->c_dev_maj = major ((unsigned short)short_hdr->c_dev);
+  file_hdr->c_dev_min = minor ((unsigned short)short_hdr->c_dev);
   file_hdr->c_ino = short_hdr->c_ino;
   file_hdr->c_mode = short_hdr->c_mode;
   file_hdr->c_uid = short_hdr->c_uid;
   file_hdr->c_gid = short_hdr->c_gid;
   file_hdr->c_nlink = short_hdr->c_nlink;
-  file_hdr->c_rdev_maj = major (short_hdr->c_rdev);
-  file_hdr->c_rdev_min = minor (short_hdr->c_rdev);
+  file_hdr->c_rdev_maj = major ((unsigned short)short_hdr->c_rdev);
+  file_hdr->c_rdev_min = minor ((unsigned short)short_hdr->c_rdev);
   file_hdr->c_mtime = (unsigned long) short_hdr->c_mtimes[0] << 16
                       | short_hdr->c_mtimes[1];
   file_hdr->c_filesize = (unsigned long) short_hdr->c_filesizes[0] << 16
