From a67a0d6060ef0f806f31db80bb7e5627fedaf58c Mon Sep 17 00:00:00 2001
From: Dengdui Huang <huangdengdui@huawei.com>
Date: Wed, 3 Apr 2024 18:16:20 +0800
Subject: [PATCH 38/42] net/hns3: fix read Rx timestamp handle

[ upstream commit 0a96792880b7eb410f3c4ae4843d82df7005a627 ]

The flag RTE_MBUF_F_RX_IEEE1588_PTP depends on the packet
type and does not need to be set when reading Rx timestamp.

Fixes: 38b539d96eb6 ("net/hns3: support IEEE 1588 PTP")
Cc: stable@dpdk.org

Signed-off-by: Dengdui Huang <huangdengdui@huawei.com>
Signed-off-by: Jie Hai <haijie1@huawei.com>
---
 drivers/net/hns3/hns3_rxtx.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

diff --git a/drivers/net/hns3/hns3_rxtx.c b/drivers/net/hns3/hns3_rxtx.c
index dc5246b..bba29a9 100644
--- a/drivers/net/hns3/hns3_rxtx.c
+++ b/drivers/net/hns3/hns3_rxtx.c
@@ -2388,8 +2388,7 @@ hns3_rx_ptp_timestamp_handle(struct hns3_rx_queue *rxq, struct rte_mbuf *mbuf,
 {
 	struct hns3_pf *pf = HNS3_DEV_PRIVATE_TO_PF(rxq->hns);
 
-	mbuf->ol_flags |= RTE_MBUF_F_RX_IEEE1588_PTP |
-			  RTE_MBUF_F_RX_IEEE1588_TMST;
+	mbuf->ol_flags |= RTE_MBUF_F_RX_IEEE1588_TMST;
 	if (hns3_timestamp_rx_dynflag > 0) {
 		*RTE_MBUF_DYNFIELD(mbuf, hns3_timestamp_dynfield_offset,
 			rte_mbuf_timestamp_t *) = timestamp;
-- 
2.33.0

