From 2b679f7b8023298c3942b424545a4eff8aebe683 Mon Sep 17 00:00:00 2001
From: veega2022 <zhuweijia@huawei.com>
Date: Wed, 10 May 2023 18:14:50 +0800
Subject: [PATCH 05/18] fix serdes module dump reg num is not enough problem

The number of new chip registers may increase. Therefore, increase the number of dump registers.

Signed-off-by: wangkang <wangkang124@hisilicon.com>
---
 serdes/hikp_serdes.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/serdes/hikp_serdes.c b/serdes/hikp_serdes.c
index 89e66e1..dd9eee3 100644
--- a/serdes/hikp_serdes.c
+++ b/serdes/hikp_serdes.c
@@ -23,7 +23,7 @@
 
 static struct cmd_serdes_param g_serdes_param = {0xff, 0xff, 0xff, 0xff, 0xff, 0xff, 0xff, 0xff};
 
-#define SERDES_OUTPUT_MAX_SIZE 2048
+#define SERDES_OUTPUT_MAX_SIZE 2560
 static char g_serdes_data_out_buf[SERDES_OUTPUT_MAX_SIZE] = {0};
 
 static int cmd_serdes_maininfo_help(struct major_cmd_ctrl *self, const char *argv)
-- 
2.25.1

