From 9d1e1ac5c1d745bc8108246848152902fd539f26 Mon Sep 17 00:00:00 2001
From: Mingzheng Xing <xingmingzheng@iscas.ac.cn>
Date: Wed, 5 Jun 2024 22:39:47 +0800
Subject: [PATCH] riscv kernel

Signed-off-by: Mingzheng Xing <xingmingzheng@iscas.ac.cn>
---
 .../bindings/gpio/snps,dw-apb-gpio.yaml       |    2 +
 .../bindings/mmc/snps,dwcmshc-sdhci.yaml      |    1 +
 .../devicetree/bindings/net/snps,dwmac.yaml   |    2 +
 .../devicetree/bindings/net/thead,dwmac.yaml  |   77 ++
 .../pinctrl/thead,th1520-pinctrl.yaml         |  372 ++++++
 .../bindings/pwm/thead,th1520-pwm.yaml        |   44 +
 .../bindings/reset/thead,th1520-reset.yaml    |   44 +
 .../bindings/usb/thead,th1520-usb.yaml        |   73 ++
 MAINTAINERS                                   |    2 +
 arch/riscv/Kconfig                            |   14 +-
 arch/riscv/Kconfig.errata                     |    1 +
 arch/riscv/Kconfig.socs                       |   14 +
 arch/riscv/Makefile                           |   19 +-
 arch/riscv/Makefile.isa                       |   18 +
 arch/riscv/boot/dts/Makefile                  |    1 +
 arch/riscv/boot/dts/sophgo/Makefile           |    7 +
 .../riscv/boot/dts/sophgo/mango-2sockets.dtsi |  699 ++++++++++
 .../boot/dts/sophgo/mango-clock-socket0.dtsi  |  124 ++
 .../boot/dts/sophgo/mango-clock-socket1.dtsi  |  124 ++
 .../boot/dts/sophgo/mango-cpus-socket0.dtsi   | 1148 ++++++++++++++++
 .../boot/dts/sophgo/mango-cpus-socket1.dtsi   | 1149 +++++++++++++++++
 .../boot/dts/sophgo/mango-milkv-pioneer.dts   |  170 +++
 .../riscv/boot/dts/sophgo/mango-pcie-2rc.dtsi |   81 ++
 .../dts/sophgo/mango-pcie-3rc-capricorn.dtsi  |  116 ++
 .../boot/dts/sophgo/mango-pcie-3rc-v2.dtsi    |  115 ++
 .../riscv/boot/dts/sophgo/mango-pcie-3rc.dtsi |  112 ++
 .../boot/dts/sophgo/mango-pcie-4rc-v2.dtsi    |  155 +++
 .../riscv/boot/dts/sophgo/mango-pcie-4rc.dtsi |  151 +++
 arch/riscv/boot/dts/sophgo/mango-pinctrl.dtsi |  434 +++++++
 .../dts/sophgo/mango-sophgo-capricorn.dts     |   57 +
 .../boot/dts/sophgo/mango-sophgo-pisces.dts   |   58 +
 .../boot/dts/sophgo/mango-sophgo-x4evb.dts    |  144 +++
 .../boot/dts/sophgo/mango-sophgo-x8evb.dts    |  172 +++
 .../boot/dts/sophgo/mango-top-intc2.dtsi      |   62 +
 .../boot/dts/sophgo/mango-yixin-s2110.dts     |   63 +
 arch/riscv/boot/dts/sophgo/mango.dtsi         |  938 ++++++++++++++
 arch/riscv/boot/dts/thead/Makefile            |    3 +
 .../boot/dts/thead/th1520-beaglev-ahead.dts   |  199 ++-
 .../thead/th1520-lichee-cluster-4a-16g.dts    |   18 +
 .../dts/thead/th1520-lichee-cluster-4a.dts    |   45 +
 .../dts/thead/th1520-lichee-module-4a.dtsi    |  151 ++-
 .../dts/thead/th1520-lichee-pi-4a-16g.dts     |   18 +
 .../boot/dts/thead/th1520-lichee-pi-4a.dts    |  712 ++++++++++
 .../boot/dts/thead/th1520-milkv-meles-4g.dts  |   19 +
 .../boot/dts/thead/th1520-milkv-meles.dts     |  441 +++++++
 arch/riscv/boot/dts/thead/th1520.dtsi         |  573 +++++++-
 arch/riscv/configs/defconfig                  |    3 +
 arch/riscv/configs/openeuler_defconfig        |  265 +++-
 arch/riscv/errata/thead/errata.c              |   69 +-
 arch/riscv/include/asm/barrier.h              |   22 +
 arch/riscv/include/asm/errata_list.h          |   50 +-
 arch/riscv/include/asm/fixmap.h               |   13 +
 arch/riscv/include/asm/highmem.h              |   13 +
 arch/riscv/include/asm/io.h                   |    4 +
 arch/riscv/include/asm/kexec.h                |    1 +
 arch/riscv/include/asm/pgtable-64.h           |   14 +-
 arch/riscv/include/asm/pgtable.h              |   34 +-
 arch/riscv/include/asm/sparsemem.h            |    2 +-
 arch/riscv/include/asm/switch_to.h            |   15 +
 arch/riscv/include/asm/timex.h                |   15 +
 arch/riscv/include/asm/vdso/gettimeofday.h    |   20 +
 arch/riscv/kernel/Makefile                    |    2 +-
 arch/riscv/kernel/elf_kexec.c                 |    6 +
 arch/riscv/kernel/image_kexec.c               |  305 +++++
 arch/riscv/kernel/machine_kexec_file.c        |    1 +
 arch/riscv/kernel/module.c                    |   83 +-
 arch/riscv/kernel/process.c                   |    3 +
 arch/riscv/kvm/vcpu_timer.c                   |    8 +
 arch/riscv/mm/init.c                          |  175 ++-
 arch/riscv/mm/pageattr.c                      |  275 +---
 drivers/base/arch_numa.c                      |    4 +
 drivers/char/ipmi/ipmi_si_hardcode.c          |   26 +-
 drivers/char/ipmi/ipmi_si_intf.c              |    3 +-
 drivers/char/ipmi/ipmi_si_pci.c               |    6 +
 drivers/clk/Kconfig                           |    1 +
 drivers/clk/Makefile                          |    2 +
 drivers/clk/sophgo/Makefile                   |    3 +
 drivers/clk/sophgo/clk-dummy.c                |  600 +++++++++
 drivers/clk/sophgo/clk-mango.c                |  977 ++++++++++++++
 drivers/clk/sophgo/clk.c                      |  883 +++++++++++++
 drivers/clk/sophgo/clk.h                      |  152 +++
 drivers/clk/thead/Kconfig                     |   19 +
 drivers/clk/thead/Makefile                    |    8 +
 drivers/clk/thead/clk-light-fm.c              |  646 +++++++++
 drivers/clk/thead/clk-light-mpw.c             |  492 +++++++
 drivers/clk/thead/clk.c                       |  739 +++++++++++
 drivers/clk/thead/clk.h                       |  117 ++
 drivers/clk/thead/gate/Makefile               |    3 +
 drivers/clk/thead/gate/clk-gate.h             |   35 +
 drivers/clk/thead/gate/dspsys-gate.c          |  109 ++
 drivers/clk/thead/gate/thead-gate.c           |  114 ++
 drivers/clk/thead/gate/visys-gate.c           |  144 +++
 drivers/clk/thead/gate/vosys-gate.c           |  111 ++
 drivers/clk/thead/gate/vpsys-gate.c           |   94 ++
 drivers/clocksource/dw_apb_timer_of.c         |   24 +
 drivers/cpufreq/Kconfig                       |   10 +
 drivers/cpufreq/Makefile                      |    1 +
 drivers/cpufreq/light-mpw-cpufreq.c           |  491 +++++++
 drivers/firmware/Kconfig                      |    1 +
 drivers/firmware/Makefile                     |    1 +
 drivers/firmware/thead/Kconfig                |   18 +
 drivers/firmware/thead/Makefile               |    3 +
 drivers/firmware/thead/light_aon.c            |  261 ++++
 drivers/firmware/thead/light_aon_misc.c       |   74 ++
 drivers/firmware/thead/light_aon_pd.c         |  417 ++++++
 drivers/firmware/thead/light_aon_test.c       |  163 +++
 drivers/gpio/gpio-dwapb.c                     |   15 +-
 drivers/gpu/drm/amd/amdgpu/amdgpu_device.c    |    2 +
 drivers/gpu/drm/amd/display/Kconfig           |    1 +
 .../gpu/drm/amd/display/amdgpu_dm/dc_fpu.c    |    6 +-
 drivers/gpu/drm/amd/display/dc/dml/Makefile   |    6 +
 drivers/gpu/drm/drm_gem_vram_helper.c         |    2 +-
 drivers/gpu/drm/radeon/radeon_drv.c           |    7 +-
 drivers/gpu/drm/radeon/radeon_irq_kms.c       |    2 +
 drivers/gpu/drm/ttm/ttm_bo_util.c             |    5 +-
 drivers/gpu/drm/ttm/ttm_module.c              |    3 +-
 drivers/gpu/drm/ttm/ttm_resource.c            |    7 +-
 drivers/gpu/drm/ttm/ttm_tt.c                  |    2 +-
 drivers/mailbox/Kconfig                       |    8 +
 drivers/mailbox/Makefile                      |    3 +
 drivers/mailbox/light-mailbox-client.c        |  242 ++++
 drivers/mailbox/light-mailbox.c               |  507 ++++++++
 drivers/mmc/host/Kconfig                      |   14 +
 drivers/mmc/host/Makefile                     |    1 +
 drivers/mmc/host/sdhci-of-dwcmshc.c           |  349 +++++
 drivers/mmc/host/sdhci-sophgo.c               |  619 +++++++++
 drivers/mmc/host/sdhci-sophgo.h               |  121 ++
 drivers/mmc/host/sdhci.c                      |   12 +-
 drivers/mmc/host/sdhci.h                      |    4 +
 drivers/mtd/spi-nor/controllers/Kconfig       |   11 +
 drivers/mtd/spi-nor/controllers/Makefile      |    1 +
 .../mtd/spi-nor/controllers/sophgo-spifmc.c   |  445 +++++++
 drivers/mtd/spi-nor/gigadevice.c              |   14 +
 drivers/net/ethernet/intel/i40e/i40e_common.c |    3 +-
 drivers/net/ethernet/intel/ixgbe/ixgbe_type.h |    2 +-
 drivers/net/ethernet/stmicro/stmmac/Kconfig   |   11 +
 drivers/net/ethernet/stmicro/stmmac/Makefile  |    2 +
 .../ethernet/stmicro/stmmac/dwmac-sophgo.c    |  268 ++++
 .../net/ethernet/stmicro/stmmac/dwmac-thead.c |  289 +++++
 drivers/pci/controller/cadence/Kconfig        |   11 +
 drivers/pci/controller/cadence/Makefile       |    1 +
 .../controller/cadence/pcie-cadence-sophgo.c  |  972 ++++++++++++++
 .../controller/cadence/pcie-cadence-sophgo.h  |   17 +
 drivers/pci/msi/msi.c                         |   97 +-
 drivers/pci/pcie/portdrv.c                    |    2 +-
 drivers/pinctrl/Kconfig                       |   11 +-
 drivers/pinctrl/Makefile                      |    2 +
 drivers/pinctrl/pinctrl-th1520.c              |  860 ++++++++++++
 drivers/pinctrl/sophgo/Makefile               |    2 +
 drivers/pinctrl/sophgo/pinctrl-mango.c        |  453 +++++++
 drivers/pinctrl/sophgo/pinctrl-sophgo.c       |  292 +++++
 drivers/pinctrl/sophgo/pinctrl-sophgo.h       |   70 +
 drivers/pwm/Kconfig                           |   11 +
 drivers/pwm/Makefile                          |    2 +
 drivers/pwm/pwm-sophgo.c                      |  276 ++++
 drivers/pwm/pwm-thead.c                       |  269 ++++
 drivers/regulator/Kconfig                     |    9 +
 drivers/regulator/Makefile                    |    1 +
 drivers/regulator/light-regulator-aon.c       |  888 +++++++++++++
 drivers/reset/Kconfig                         |   10 +
 drivers/reset/Makefile                        |    2 +
 drivers/reset/reset-sophgo.c                  |  163 +++
 drivers/reset/reset-th1520.c                  |  109 ++
 drivers/rpmsg/Kconfig                         |    4 +
 drivers/rpmsg/Makefile                        |    1 +
 drivers/rpmsg/light_rpmsg.c                   |  864 +++++++++++++
 drivers/rtc/Kconfig                           |    6 +
 drivers/rtc/Makefile                          |    1 +
 drivers/rtc/rtc-astbmc.c                      |  535 ++++++++
 drivers/soc/Kconfig                           |    1 +
 drivers/soc/Makefile                          |    2 +
 drivers/soc/sophgo/Makefile                   |    3 +
 drivers/soc/sophgo/tach/sophgo-tach.c         |  330 +++++
 drivers/soc/sophgo/top/top_intc.c             |  412 ++++++
 drivers/soc/sophgo/umcu/mcu.c                 | 1144 ++++++++++++++++
 drivers/soc/thead/Kconfig                     |   10 +
 drivers/soc/thead/Makefile                    |    2 +
 drivers/soc/thead/light_event.c               |  279 ++++
 drivers/usb/dwc3/Kconfig                      |   20 +
 drivers/usb/dwc3/Makefile                     |    2 +
 drivers/usb/dwc3/dwc3-thead.c                 |  112 ++
 drivers/watchdog/Kconfig                      |   14 +
 drivers/watchdog/Makefile                     |    1 +
 drivers/watchdog/light_wdt.c                  |  376 ++++++
 include/dt-bindings/clock/light-dspsys.h      |   25 +
 include/dt-bindings/clock/light-fm-ap-clock.h |  513 ++++++++
 include/dt-bindings/clock/light-mpw-clock.h   |  222 ++++
 include/dt-bindings/clock/light-visys.h       |   54 +
 include/dt-bindings/clock/light-vosys.h       |   41 +
 include/dt-bindings/clock/light-vpsys.h       |   24 +
 .../dt-bindings/clock/sophgo-mango-clock.h    |  165 +++
 include/dt-bindings/clock/sophgo.h            |   15 +
 include/dt-bindings/firmware/thead/rsrc.h     |   17 +
 .../dt-bindings/reset/sophgo-mango-resets.h   |   96 ++
 .../dt-bindings/reset/thead,th1520-reset.h    |    9 +
 include/linux/firmware/thead/ipc.h            |   74 ++
 include/linux/firmware/thead/light_event.h    |   35 +
 include/linux/light_rpmsg.h                   |   92 ++
 kernel/kexec_core.c                           |    2 +-
 kernel/panic.c                                |    6 +
 kernel/sched/fair.c                           |    3 +
 kernel/time/tick-oneshot.c                    |    2 +-
 mm/memblock.c                                 |   28 +-
 scripts/package/builddeb                      |    2 +-
 sound/pci/hda/hda_intel.c                     |    5 +-
 tools/lib/perf/cpumap.c                       |   10 +-
 tools/perf/pmu-events/arch/riscv/mapfile.csv  |    1 +
 .../arch/riscv/thead/c900-legacy/cache.json   |   67 +
 .../riscv/thead/c900-legacy/firmware.json     |   68 +
 .../riscv/thead/c900-legacy/instruction.json  |   72 ++
 .../riscv/thead/c900-legacy/microarch.json    |   80 ++
 211 files changed, 29953 insertions(+), 500 deletions(-)
 create mode 100644 Documentation/devicetree/bindings/net/thead,dwmac.yaml
 create mode 100644 Documentation/devicetree/bindings/pinctrl/thead,th1520-pinctrl.yaml
 create mode 100644 Documentation/devicetree/bindings/pwm/thead,th1520-pwm.yaml
 create mode 100644 Documentation/devicetree/bindings/reset/thead,th1520-reset.yaml
 create mode 100644 Documentation/devicetree/bindings/usb/thead,th1520-usb.yaml
 create mode 100644 arch/riscv/Makefile.isa
 create mode 100644 arch/riscv/boot/dts/sophgo/Makefile
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-2sockets.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-clock-socket0.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-clock-socket1.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-cpus-socket0.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-cpus-socket1.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-milkv-pioneer.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-2rc.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-3rc-capricorn.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-3rc-v2.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-3rc.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-4rc-v2.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pcie-4rc.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-pinctrl.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-sophgo-capricorn.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-sophgo-pisces.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-sophgo-x4evb.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-sophgo-x8evb.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-top-intc2.dtsi
 create mode 100644 arch/riscv/boot/dts/sophgo/mango-yixin-s2110.dts
 create mode 100644 arch/riscv/boot/dts/sophgo/mango.dtsi
 create mode 100644 arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a-16g.dts
 create mode 100644 arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a.dts
 create mode 100644 arch/riscv/boot/dts/thead/th1520-lichee-pi-4a-16g.dts
 create mode 100644 arch/riscv/boot/dts/thead/th1520-milkv-meles-4g.dts
 create mode 100644 arch/riscv/boot/dts/thead/th1520-milkv-meles.dts
 create mode 100644 arch/riscv/include/asm/highmem.h
 create mode 100644 arch/riscv/kernel/image_kexec.c
 create mode 100644 drivers/clk/sophgo/Makefile
 create mode 100644 drivers/clk/sophgo/clk-dummy.c
 create mode 100644 drivers/clk/sophgo/clk-mango.c
 create mode 100644 drivers/clk/sophgo/clk.c
 create mode 100644 drivers/clk/sophgo/clk.h
 create mode 100644 drivers/clk/thead/Kconfig
 create mode 100644 drivers/clk/thead/Makefile
 create mode 100644 drivers/clk/thead/clk-light-fm.c
 create mode 100644 drivers/clk/thead/clk-light-mpw.c
 create mode 100644 drivers/clk/thead/clk.c
 create mode 100644 drivers/clk/thead/clk.h
 create mode 100644 drivers/clk/thead/gate/Makefile
 create mode 100644 drivers/clk/thead/gate/clk-gate.h
 create mode 100644 drivers/clk/thead/gate/dspsys-gate.c
 create mode 100644 drivers/clk/thead/gate/thead-gate.c
 create mode 100644 drivers/clk/thead/gate/visys-gate.c
 create mode 100644 drivers/clk/thead/gate/vosys-gate.c
 create mode 100644 drivers/clk/thead/gate/vpsys-gate.c
 create mode 100644 drivers/cpufreq/light-mpw-cpufreq.c
 create mode 100644 drivers/firmware/thead/Kconfig
 create mode 100644 drivers/firmware/thead/Makefile
 create mode 100644 drivers/firmware/thead/light_aon.c
 create mode 100644 drivers/firmware/thead/light_aon_misc.c
 create mode 100644 drivers/firmware/thead/light_aon_pd.c
 create mode 100644 drivers/firmware/thead/light_aon_test.c
 create mode 100644 drivers/mailbox/light-mailbox-client.c
 create mode 100644 drivers/mailbox/light-mailbox.c
 create mode 100644 drivers/mmc/host/sdhci-sophgo.c
 create mode 100644 drivers/mmc/host/sdhci-sophgo.h
 create mode 100644 drivers/mtd/spi-nor/controllers/sophgo-spifmc.c
 create mode 100644 drivers/net/ethernet/stmicro/stmmac/dwmac-sophgo.c
 create mode 100644 drivers/net/ethernet/stmicro/stmmac/dwmac-thead.c
 create mode 100644 drivers/pci/controller/cadence/pcie-cadence-sophgo.c
 create mode 100644 drivers/pci/controller/cadence/pcie-cadence-sophgo.h
 create mode 100644 drivers/pinctrl/pinctrl-th1520.c
 create mode 100644 drivers/pinctrl/sophgo/Makefile
 create mode 100644 drivers/pinctrl/sophgo/pinctrl-mango.c
 create mode 100644 drivers/pinctrl/sophgo/pinctrl-sophgo.c
 create mode 100644 drivers/pinctrl/sophgo/pinctrl-sophgo.h
 create mode 100644 drivers/pwm/pwm-sophgo.c
 create mode 100644 drivers/pwm/pwm-thead.c
 create mode 100644 drivers/regulator/light-regulator-aon.c
 create mode 100644 drivers/reset/reset-sophgo.c
 create mode 100644 drivers/reset/reset-th1520.c
 create mode 100644 drivers/rpmsg/light_rpmsg.c
 create mode 100644 drivers/rtc/rtc-astbmc.c
 create mode 100644 drivers/soc/sophgo/Makefile
 create mode 100644 drivers/soc/sophgo/tach/sophgo-tach.c
 create mode 100644 drivers/soc/sophgo/top/top_intc.c
 create mode 100644 drivers/soc/sophgo/umcu/mcu.c
 create mode 100644 drivers/soc/thead/Kconfig
 create mode 100644 drivers/soc/thead/Makefile
 create mode 100644 drivers/soc/thead/light_event.c
 create mode 100644 drivers/usb/dwc3/dwc3-thead.c
 create mode 100644 drivers/watchdog/light_wdt.c
 create mode 100644 include/dt-bindings/clock/light-dspsys.h
 create mode 100644 include/dt-bindings/clock/light-fm-ap-clock.h
 create mode 100644 include/dt-bindings/clock/light-mpw-clock.h
 create mode 100644 include/dt-bindings/clock/light-visys.h
 create mode 100644 include/dt-bindings/clock/light-vosys.h
 create mode 100644 include/dt-bindings/clock/light-vpsys.h
 create mode 100644 include/dt-bindings/clock/sophgo-mango-clock.h
 create mode 100644 include/dt-bindings/clock/sophgo.h
 create mode 100644 include/dt-bindings/firmware/thead/rsrc.h
 create mode 100644 include/dt-bindings/reset/sophgo-mango-resets.h
 create mode 100644 include/dt-bindings/reset/thead,th1520-reset.h
 create mode 100644 include/linux/firmware/thead/ipc.h
 create mode 100644 include/linux/firmware/thead/light_event.h
 create mode 100644 include/linux/light_rpmsg.h
 create mode 100644 tools/perf/pmu-events/arch/riscv/thead/c900-legacy/cache.json
 create mode 100644 tools/perf/pmu-events/arch/riscv/thead/c900-legacy/firmware.json
 create mode 100644 tools/perf/pmu-events/arch/riscv/thead/c900-legacy/instruction.json
 create mode 100644 tools/perf/pmu-events/arch/riscv/thead/c900-legacy/microarch.json

diff --git a/Documentation/devicetree/bindings/gpio/snps,dw-apb-gpio.yaml b/Documentation/devicetree/bindings/gpio/snps,dw-apb-gpio.yaml
index eefe7b345286..ab2afc0e4153 100644
--- a/Documentation/devicetree/bindings/gpio/snps,dw-apb-gpio.yaml
+++ b/Documentation/devicetree/bindings/gpio/snps,dw-apb-gpio.yaml
@@ -65,6 +65,8 @@ patternProperties:
         minItems: 1
         maxItems: 32
 
+      gpio-ranges: true
+
       ngpios:
         default: 32
         minimum: 1
diff --git a/Documentation/devicetree/bindings/mmc/snps,dwcmshc-sdhci.yaml b/Documentation/devicetree/bindings/mmc/snps,dwcmshc-sdhci.yaml
index a43eb837f8da..42804d955293 100644
--- a/Documentation/devicetree/bindings/mmc/snps,dwcmshc-sdhci.yaml
+++ b/Documentation/devicetree/bindings/mmc/snps,dwcmshc-sdhci.yaml
@@ -19,6 +19,7 @@ properties:
       - rockchip,rk3568-dwcmshc
       - rockchip,rk3588-dwcmshc
       - snps,dwcmshc-sdhci
+      - thead,th1520-dwcmshc
 
   reg:
     maxItems: 1
diff --git a/Documentation/devicetree/bindings/net/snps,dwmac.yaml b/Documentation/devicetree/bindings/net/snps,dwmac.yaml
index 5c2769dc689a..eeed9d2b940e 100644
--- a/Documentation/devicetree/bindings/net/snps,dwmac.yaml
+++ b/Documentation/devicetree/bindings/net/snps,dwmac.yaml
@@ -96,6 +96,7 @@ properties:
         - snps,dwxgmac
         - snps,dwxgmac-2.10
         - starfive,jh7110-dwmac
+        - thead,th1520-dwmac
 
   reg:
     minItems: 1
@@ -591,6 +592,7 @@ allOf:
               - qcom,sa8775p-ethqos
               - qcom,sc8280xp-ethqos
               - snps,dwmac-3.50a
+              - snps,dwmac-3.70a
               - snps,dwmac-4.10a
               - snps,dwmac-4.20a
               - snps,dwmac-5.20
diff --git a/Documentation/devicetree/bindings/net/thead,dwmac.yaml b/Documentation/devicetree/bindings/net/thead,dwmac.yaml
new file mode 100644
index 000000000000..bf8ec8ca2753
--- /dev/null
+++ b/Documentation/devicetree/bindings/net/thead,dwmac.yaml
@@ -0,0 +1,77 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/net/thead,dwmac.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: T-HEAD DWMAC Ethernet controller
+
+maintainers:
+  - Jisheng Zhang <jszhang@kernel.org>
+
+select:
+  properties:
+    compatible:
+      contains:
+        enum:
+          - thead,th1520-dwmac
+  required:
+    - compatible
+
+properties:
+  compatible:
+    items:
+      - enum:
+          - thead,th1520-dwmac
+      - const: snps,dwmac-3.70a
+
+  reg:
+    maxItems: 1
+
+  thead,gmacapb:
+    $ref: /schemas/types.yaml#/definitions/phandle
+    description:
+      The phandle to the syscon node that control ethernet
+      interface and timing delay.
+
+required:
+  - compatible
+  - reg
+  - clocks
+  - clock-names
+  - interrupts
+  - interrupt-names
+  - phy-mode
+  - thead,gmacapb
+
+allOf:
+  - $ref: snps,dwmac.yaml#
+
+unevaluatedProperties: false
+
+examples:
+  - |
+    gmac0: ethernet@e7070000 {
+        compatible = "thead,th1520-dwmac", "snps,dwmac-3.70a";
+        reg = <0xe7070000 0x2000>;
+        clocks = <&clk 1>, <&clk 2>;
+        clock-names = "stmmaceth", "pclk";
+        interrupts = <66>;
+        interrupt-names = "macirq";
+        phy-mode = "rgmii-id";
+        snps,fixed-burst;
+        snps,axi-config = <&stmmac_axi_setup>;
+        snps,pbl = <32>;
+        thead,gmacapb = <&gmacapb_syscon>;
+        phy-handle = <&phy0>;
+
+        mdio {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            compatible = "snps,dwmac-mdio";
+
+            phy0: ethernet-phy@0 {
+                reg = <0>;
+            };
+        };
+    };
diff --git a/Documentation/devicetree/bindings/pinctrl/thead,th1520-pinctrl.yaml b/Documentation/devicetree/bindings/pinctrl/thead,th1520-pinctrl.yaml
new file mode 100644
index 000000000000..b80d0f7b4697
--- /dev/null
+++ b/Documentation/devicetree/bindings/pinctrl/thead,th1520-pinctrl.yaml
@@ -0,0 +1,372 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/pinctrl/thead,th1520-pinctrl.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: T-Head TH1520 SoC pin controller
+
+maintainers:
+  - Emil Renner Berthing <emil.renner.berthing@canonical.com>
+
+description: |
+  Pinmux and pinconf controller in the T-Head TH1520 RISC-V SoC.
+
+  The TH1520 has 3 groups of pads each controlled from different memory ranges.
+  Confusingly the memory ranges are named
+    PADCTRL_AOSYS  -> PAD Group 1
+    PADCTRL1_APSYS -> PAD Group 2
+    PADCTRL0_APSYS -> PAD Group 3
+
+  Each pad can be muxed individually to up to 6 different functions. For most
+  pads only a few of those 6 configurations are valid though, and a few pads in
+  group 1 does not support muxing at all.
+
+  Pinconf is fairly regular except for a few pads in group 1 that either can't
+  be configured or has some special functions. The rest have configurable drive
+  strength, input enable, schmitt trigger, slew rate, pull-up and pull-down in
+  addition to a special strong pull up.
+
+  Certain pads in group 1 can be muxed to AUDIO_PA0 - AUDIO_PA30 functions and
+  are then meant to be used by the audio co-processor. Each such pad can then
+  be further muxed to either audio GPIO or one of 4 functions such as UART, I2C
+  and I2S. If the audio pad is muxed to one of the 4 functions then pinconf is
+  also configured in different registers. All of this is done from a different
+  AUDIO_IOCTRL memory range and is left to the audio co-processor for now.
+
+properties:
+  compatible:
+    enum:
+      - thead,th1520-group1-pinctrl
+      - thead,th1520-group2-pinctrl
+      - thead,th1520-group3-pinctrl
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    maxItems: 1
+
+patternProperties:
+  '-[0-9]+$':
+    type: object
+
+    additionalProperties: false
+
+    patternProperties:
+      '-pins$':
+        type: object
+        $ref: /schemas/pinctrl/pincfg-node.yaml
+
+        additionalProperties: false
+
+        description:
+          A pinctrl node should contain at least one subnode describing one
+          or more pads and their associated pinmux and pinconf settings.
+
+        properties:
+          pins:
+            $ref: /schemas/pinctrl/pinmux-node.yaml#/properties/pins
+            description: List of pads that properties in the node apply to.
+
+          function:
+            $ref: /schemas/pinctrl/pinmux-node.yaml#/properties/function
+            enum: [ gpio, pwm, uart, ir, i2c, spi, qspi, sdio, audio, i2s,
+                    gmac0, gmac1, dpu0, dpu1, isp, hdmi, bootsel, debug,
+                    clock, jtag, iso7816, efuse, reset ]
+            description: The mux function to select for the given pins.
+
+          bias-disable: true
+
+          bias-pull-up:
+            oneOf:
+              - type: boolean
+                description: Enable the regular 48kOhm pull-up
+              - enum: [ 2100, 48000 ]
+                description: Enable the strong 2.1kOhm pull-up or regular 48kOhm pull-up
+
+          bias-pull-down:
+            oneOf:
+              - type: boolean
+              - const: 44000
+            description: Enable the regular 44kOhm pull-down
+
+          drive-strength:
+            description: Drive strength in mA
+            enum: [ 1, 2, 3, 5, 7, 8, 10, 12, 13, 15, 16, 18, 20, 21, 23, 25 ]
+
+          input-enable: true
+
+          input-disable: true
+
+          input-schmitt-enable: true
+
+          input-schmitt-disable: true
+
+          slew-rate:
+            maximum: 1
+
+        required:
+          - pins
+
+required:
+  - compatible
+  - reg
+  - clocks
+
+additionalProperties: false
+
+allOf:
+  - $ref: pinctrl.yaml#
+  - if:
+      properties:
+        compatible:
+          const: thead,th1520-group1-pinctrl
+    then:
+      patternProperties:
+        '-[0-9]+$':
+          patternProperties:
+            '-pins$':
+              properties:
+                pins:
+                  items:
+                    enum:
+                      - OSC_CLK_IN
+                      - OSC_CLK_OUT
+                      - SYS_RST_N
+                      - RTC_CLK_IN
+                      - RTC_CLK_OUT
+                      - TEST_MODE
+                      - DEBUG_MODE
+                      - POR_SEL
+                      - I2C_AON_SCL
+                      - I2C_AON_SDA
+                      - CPU_JTG_TCLK
+                      - CPU_JTG_TMS
+                      - CPU_JTG_TDI
+                      - CPU_JTG_TDO
+                      - CPU_JTG_TRST
+                      - AOGPIO_7
+                      - AOGPIO_8
+                      - AOGPIO_9
+                      - AOGPIO_10
+                      - AOGPIO_11
+                      - AOGPIO_12
+                      - AOGPIO_13
+                      - AOGPIO_14
+                      - AOGPIO_15
+                      - AUDIO_PA0
+                      - AUDIO_PA1
+                      - AUDIO_PA2
+                      - AUDIO_PA3
+                      - AUDIO_PA4
+                      - AUDIO_PA5
+                      - AUDIO_PA6
+                      - AUDIO_PA7
+                      - AUDIO_PA8
+                      - AUDIO_PA9
+                      - AUDIO_PA10
+                      - AUDIO_PA11
+                      - AUDIO_PA12
+                      - AUDIO_PA13
+                      - AUDIO_PA14
+                      - AUDIO_PA15
+                      - AUDIO_PA16
+                      - AUDIO_PA17
+                      - AUDIO_PA27
+                      - AUDIO_PA28
+                      - AUDIO_PA29
+                      - AUDIO_PA30
+  - if:
+      properties:
+        compatible:
+          const: thead,th1520-group2-pinctrl
+    then:
+      patternProperties:
+        '-[0-9]+$':
+          patternProperties:
+            '-pins$':
+              properties:
+                pins:
+                  items:
+                    enum:
+                      - QSPI1_SCLK
+                      - QSPI1_CSN0
+                      - QSPI1_D0_MOSI
+                      - QSPI1_D1_MISO
+                      - QSPI1_D2_WP
+                      - QSPI1_D3_HOLD
+                      - I2C0_SCL
+                      - I2C0_SDA
+                      - I2C1_SCL
+                      - I2C1_SDA
+                      - UART1_TXD
+                      - UART1_RXD
+                      - UART4_TXD
+                      - UART4_RXD
+                      - UART4_CTSN
+                      - UART4_RTSN
+                      - UART3_TXD
+                      - UART3_RXD
+                      - GPIO0_18
+                      - GPIO0_19
+                      - GPIO0_20
+                      - GPIO0_21
+                      - GPIO0_22
+                      - GPIO0_23
+                      - GPIO0_24
+                      - GPIO0_25
+                      - GPIO0_26
+                      - GPIO0_27
+                      - GPIO0_28
+                      - GPIO0_29
+                      - GPIO0_30
+                      - GPIO0_31
+                      - GPIO1_0
+                      - GPIO1_1
+                      - GPIO1_2
+                      - GPIO1_3
+                      - GPIO1_4
+                      - GPIO1_5
+                      - GPIO1_6
+                      - GPIO1_7
+                      - GPIO1_8
+                      - GPIO1_9
+                      - GPIO1_10
+                      - GPIO1_11
+                      - GPIO1_12
+                      - GPIO1_13
+                      - GPIO1_14
+                      - GPIO1_15
+                      - GPIO1_16
+                      - CLK_OUT_0
+                      - CLK_OUT_1
+                      - CLK_OUT_2
+                      - CLK_OUT_3
+                      - GPIO1_21
+                      - GPIO1_22
+                      - GPIO1_23
+                      - GPIO1_24
+                      - GPIO1_25
+                      - GPIO1_26
+                      - GPIO1_27
+                      - GPIO1_28
+                      - GPIO1_29
+                      - GPIO1_30
+  - if:
+      properties:
+        compatible:
+          const: thead,th1520-group3-pinctrl
+    then:
+      patternProperties:
+        '-[0-9]+$':
+          patternProperties:
+            '-pins$':
+              properties:
+                pins:
+                  items:
+                    enum:
+                      - UART0_TXD
+                      - UART0_RXD
+                      - QSPI0_SCLK
+                      - QSPI0_CSN0
+                      - QSPI0_CSN1
+                      - QSPI0_D0_MOSI
+                      - QSPI0_D1_MISO
+                      - QSPI0_D2_WP
+                      - QSPI1_D3_HOLD
+                      - I2C2_SCL
+                      - I2C2_SDA
+                      - I2C3_SCL
+                      - I2C3_SDA
+                      - GPIO2_13
+                      - SPI_SCLK
+                      - SPI_CSN
+                      - SPI_MOSI
+                      - SPI_MISO
+                      - GPIO2_18
+                      - GPIO2_19
+                      - GPIO2_20
+                      - GPIO2_21
+                      - GPIO2_22
+                      - GPIO2_23
+                      - GPIO2_24
+                      - GPIO2_25
+                      - SDIO0_WPRTN
+                      - SDIO0_DETN
+                      - SDIO1_WPRTN
+                      - SDIO1_DETN
+                      - GPIO2_30
+                      - GPIO2_31
+                      - GPIO3_0
+                      - GPIO3_1
+                      - GPIO3_2
+                      - GPIO3_3
+                      - HDMI_SCL
+                      - HDMI_SDA
+                      - HDMI_CEC
+                      - GMAC0_TX_CLK
+                      - GMAC0_RX_CLK
+                      - GMAC0_TXEN
+                      - GMAC0_TXD0
+                      - GMAC0_TXD1
+                      - GMAC0_TXD2
+                      - GMAC0_TXD3
+                      - GMAC0_RXDV
+                      - GMAC0_RXD0
+                      - GMAC0_RXD1
+                      - GMAC0_RXD2
+                      - GMAC0_RXD3
+                      - GMAC0_MDC
+                      - GMAC0_MDIO
+                      - GMAC0_COL
+                      - GMAC0_CRS
+
+examples:
+  - |
+    padctrl0_apsys: pinctrl@ec007000 {
+        compatible = "thead,th1520-group3-pinctrl";
+        reg = <0xec007000 0x1000>;
+        clocks = <&apb_clk>;
+
+        uart0_pins: uart0-0 {
+            tx-pins {
+                pins = "UART0_TXD";
+                function = "uart";
+                bias-disable;
+                drive-strength = <3>;
+                input-disable;
+                input-schmitt-disable;
+                slew-rate = <0>;
+            };
+
+            rx-pins {
+                pins = "UART0_RXD";
+                function = "uart";
+                bias-disable;
+                drive-strength = <1>;
+                input-enable;
+                input-schmitt-enable;
+                slew-rate = <0>;
+            };
+        };
+    };
+
+    padctrl1_apsys: pinctrl@e7f3c000 {
+        compatible = "thead,th1520-group2-pinctrl";
+        reg = <0xe7f3c000 0x1000>;
+        clocks = <&apb_clk>;
+
+        i2c5_pins: i2c5-0 {
+            i2c-pins {
+                pins = "QSPI1_CSN0",    /* I2C5_SCL */
+                       "QSPI1_D0_MOSI"; /* I2C5_SDA */
+                function = "i2c";
+                bias-pull-up = <2100>;
+                drive-strength = <7>;
+                input-enable;
+                input-schmitt-enable;
+                slew-rate = <0>;
+            };
+        };
+    };
diff --git a/Documentation/devicetree/bindings/pwm/thead,th1520-pwm.yaml b/Documentation/devicetree/bindings/pwm/thead,th1520-pwm.yaml
new file mode 100644
index 000000000000..e75d8e9f24c5
--- /dev/null
+++ b/Documentation/devicetree/bindings/pwm/thead,th1520-pwm.yaml
@@ -0,0 +1,44 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/pwm/thead,th1520-pwm.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: T-HEAD TH1520 PWM
+
+maintainers:
+  - Jisheng Zhang <jszhang@kernel.org>
+
+allOf:
+  - $ref: pwm.yaml#
+
+properties:
+  compatible:
+    enum:
+      - thead,th1520-pwm
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    maxItems: 1
+
+  "#pwm-cells":
+    const: 3
+
+required:
+  - compatible
+  - reg
+  - clocks
+
+additionalProperties: false
+
+examples:
+  - |
+
+    pwm@ec01c000 {
+        compatible = "thead,th1520-pwm";
+        reg = <0xec01c000 0x1000>;
+        clocks = <&clk 1>;
+        #pwm-cells = <3>;
+    };
diff --git a/Documentation/devicetree/bindings/reset/thead,th1520-reset.yaml b/Documentation/devicetree/bindings/reset/thead,th1520-reset.yaml
new file mode 100644
index 000000000000..49ea8c6a331f
--- /dev/null
+++ b/Documentation/devicetree/bindings/reset/thead,th1520-reset.yaml
@@ -0,0 +1,44 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/reset/thead,th1520-reset.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: T-HEAD th1520 SoC Reset Controller
+
+maintainers:
+  - Kwanghoon Son <k.son@samsung.com>
+
+properties:
+  compatible:
+    items:
+      - const: thead,th1520-reset
+      - const: syscon
+
+  reg:
+    maxItems: 1
+
+  '#reset-cells':
+    const: 1
+
+required:
+  - compatible
+  - reg
+  - '#reset-cells'
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/reset/thead,th1520-reset.h>
+
+    soc {
+        #address-cells = <2>;
+        #size-cells = <2>;
+
+        reset-controller@ffef014000 {
+            compatible = "thead,th1520-reset", "syscon";
+            reg = <0xff 0xef014000 0x0 0x1000>;
+            #reset-cells = <1>;
+        };
+    };
diff --git a/Documentation/devicetree/bindings/usb/thead,th1520-usb.yaml b/Documentation/devicetree/bindings/usb/thead,th1520-usb.yaml
new file mode 100644
index 000000000000..afb618eb5013
--- /dev/null
+++ b/Documentation/devicetree/bindings/usb/thead,th1520-usb.yaml
@@ -0,0 +1,73 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/usb/thead,th1520-usb.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: T-HEAD TH1520 DWC3 USB Controller Glue
+
+maintainers:
+  - Jisheng Zhang <jszhang@kernel.org>
+
+properties:
+  compatible:
+    const: thead,th1520-usb
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    maxItems: 4
+
+  clock-names:
+    items:
+      - const: ref
+      - const: bus_early
+      - const: phy
+      - const: suspend
+
+  ranges: true
+
+  '#address-cells':
+    enum: [ 1, 2 ]
+
+  '#size-cells':
+    enum: [ 1, 2 ]
+
+# Required child node:
+
+patternProperties:
+  "^usb@[0-9a-f]+$":
+    $ref: snps,dwc3.yaml#
+
+required:
+  - compatible
+  - reg
+  - clocks
+  - clock-names
+  - ranges
+
+additionalProperties: false
+
+examples:
+  - |
+
+    usb {
+          compatible = "thead,th1520-usb";
+          reg = <0xec03f000 0x1000>;
+          clocks = <&clk 1>,
+                   <&clk 2>,
+                   <&clk 3>,
+                   <&clk 4>;
+          clock-names = "ref", "bus_early", "phy", "suspend";
+          ranges;
+          #address-cells = <1>;
+          #size-cells = <1>;
+
+          usb@e7040000 {
+                compatible = "snps,dwc3";
+                reg = <0xe7040000 0x10000>;
+                interrupts = <68>;
+                dr_mode = "host";
+          };
+    };
diff --git a/MAINTAINERS b/MAINTAINERS
index 1c70622103e0..e41153dd877b 100644
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -18529,6 +18529,8 @@ M:	Fu Wei <wefu@redhat.com>
 L:	linux-riscv@lists.infradead.org
 S:	Maintained
 F:	arch/riscv/boot/dts/thead/
+F:	drivers/pinctrl/pinctrl-th1520.c
+F:	drivers/usb/dwc3/dwc3-thead.c
 
 RNBD BLOCK DRIVERS
 M:	Md. Haris Iqbal <haris.iqbal@ionos.com>
diff --git a/arch/riscv/Kconfig b/arch/riscv/Kconfig
index bb40f2eae472..12aba075395c 100644
--- a/arch/riscv/Kconfig
+++ b/arch/riscv/Kconfig
@@ -39,6 +39,7 @@ config RISCV
 	select ARCH_HAS_TICK_BROADCAST if GENERIC_CLOCKEVENTS_BROADCAST
 	select ARCH_HAS_UBSAN_SANITIZE_ALL
 	select ARCH_HAS_VDSO_DATA
+	select ARCH_KEEP_MEMBLOCK
 	select ARCH_OPTIONAL_KERNEL_RWX if ARCH_HAS_STRICT_KERNEL_RWX
 	select ARCH_OPTIONAL_KERNEL_RWX_DEFAULT
 	select ARCH_STACKWALK
@@ -155,7 +156,7 @@ config RISCV
 	select PCI_MSI if PCI
 	select RISCV_ALTERNATIVE if !XIP_KERNEL
 	select RISCV_INTC
-	select RISCV_TIMER if RISCV_SBI
+	select RISCV_TIMER if RISCV_SBI && !SOPHGO_MULTI_CHIP_CLOCK_SYNC
 	select SIFIVE_PLIC
 	select SPARSE_IRQ
 	select SYSCTL_EXCEPTION_TRACE
@@ -402,6 +403,15 @@ config TUNE_GENERIC
 
 endchoice
 
+config HIGHMEM
+	bool "High Memory Support"
+	depends on MMU
+	select KMAP_LOCAL
+	default y
+	help
+	  Enable high memory support on riscv64 which uses supports
+	  max 39-bit virtual address spaces.
+
 # Common NUMA Features
 config NUMA
 	bool "NUMA Memory Allocation and Scheduler Support"
@@ -501,7 +511,7 @@ config RISCV_ISA_V
 	depends on TOOLCHAIN_HAS_V
 	depends on FPU
 	select DYNAMIC_SIGFRAME
-	default y
+	default n
 	help
 	  Say N here if you want to disable all vector related procedure
 	  in the kernel.
diff --git a/arch/riscv/Kconfig.errata b/arch/riscv/Kconfig.errata
index e2c731cfed8c..dedb8b238e73 100644
--- a/arch/riscv/Kconfig.errata
+++ b/arch/riscv/Kconfig.errata
@@ -79,6 +79,7 @@ config ERRATA_THEAD_CMO
 	depends on ERRATA_THEAD && MMU
 	select DMA_DIRECT_REMAP
 	select RISCV_DMA_NONCOHERENT
+	select RISCV_NONSTANDARD_CACHE_OPS
 	default y
 	help
 	  This will apply the cache management errata to handle the
diff --git a/arch/riscv/Kconfig.socs b/arch/riscv/Kconfig.socs
index 30fd6a512828..1adb9086fa42 100644
--- a/arch/riscv/Kconfig.socs
+++ b/arch/riscv/Kconfig.socs
@@ -22,6 +22,20 @@ config SOC_SIFIVE
 	help
 	  This enables support for SiFive SoC platform hardware.
 
+config ARCH_SOPHGO
+	bool "Sophgo SoCs"
+	select DW_APB_TIMER_OF
+	help
+	  This enables support for Sophgo SoC platform hardware.
+
+config SOPHGO_MULTI_CHIP_CLOCK_SYNC
+	bool "Sophgo multi-chip clock synchronous"
+	depends on ARCH_SOPHGO
+	default n
+	help
+	  To solve the problem of asynchronous multi-chip clocks,
+	  the local timer has been replaced with an APB timer.
+
 config ARCH_STARFIVE
 	def_bool SOC_STARFIVE
 
diff --git a/arch/riscv/Makefile b/arch/riscv/Makefile
index b43a6bb7e4dc..c33a055a06f3 100644
--- a/arch/riscv/Makefile
+++ b/arch/riscv/Makefile
@@ -54,22 +54,7 @@ endif
 endif
 endif
 
-# ISA string setting
-riscv-march-$(CONFIG_ARCH_RV32I)	:= rv32ima
-riscv-march-$(CONFIG_ARCH_RV64I)	:= rv64ima
-riscv-march-$(CONFIG_FPU)		:= $(riscv-march-y)fd
-riscv-march-$(CONFIG_RISCV_ISA_C)	:= $(riscv-march-y)c
-riscv-march-$(CONFIG_RISCV_ISA_V)	:= $(riscv-march-y)v
-
-ifdef CONFIG_TOOLCHAIN_NEEDS_OLD_ISA_SPEC
-KBUILD_CFLAGS += -Wa,-misa-spec=2.2
-KBUILD_AFLAGS += -Wa,-misa-spec=2.2
-else
-riscv-march-$(CONFIG_TOOLCHAIN_NEEDS_EXPLICIT_ZICSR_ZIFENCEI) := $(riscv-march-y)_zicsr_zifencei
-endif
-
-# Check if the toolchain supports Zihintpause extension
-riscv-march-$(CONFIG_TOOLCHAIN_HAS_ZIHINTPAUSE) := $(riscv-march-y)_zihintpause
+include $(srctree)/arch/riscv/Makefile.isa
 
 # Remove F,D,V from isa string for all. Keep extensions between "fd" and "v" by
 # matching non-v and non-multi-letter extensions out with the filter ([^v_]*)
@@ -152,7 +137,7 @@ ifeq ($(CONFIG_RISCV_M_MODE)$(CONFIG_ARCH_CANAAN),yy)
 KBUILD_IMAGE := $(boot)/loader.bin
 else
 ifeq ($(CONFIG_EFI_ZBOOT),)
-KBUILD_IMAGE := $(boot)/Image.gz
+KBUILD_IMAGE := $(boot)/Image
 else
 KBUILD_IMAGE := $(boot)/vmlinuz.efi
 endif
diff --git a/arch/riscv/Makefile.isa b/arch/riscv/Makefile.isa
new file mode 100644
index 000000000000..322a83958b96
--- /dev/null
+++ b/arch/riscv/Makefile.isa
@@ -0,0 +1,18 @@
+# SPDX-License-Identifier: GPL-2.0-only
+
+# ISA string setting
+riscv-march-$(CONFIG_ARCH_RV32I)	:= rv32ima
+riscv-march-$(CONFIG_ARCH_RV64I)	:= rv64ima
+riscv-march-$(CONFIG_FPU)		:= $(riscv-march-y)fd
+riscv-march-$(CONFIG_RISCV_ISA_C)	:= $(riscv-march-y)c
+riscv-march-$(CONFIG_RISCV_ISA_V)	:= $(riscv-march-y)v
+
+ifdef CONFIG_TOOLCHAIN_NEEDS_OLD_ISA_SPEC
+KBUILD_CFLAGS += -Wa,-misa-spec=2.2
+KBUILD_AFLAGS += -Wa,-misa-spec=2.2
+else
+riscv-march-$(CONFIG_TOOLCHAIN_NEEDS_EXPLICIT_ZICSR_ZIFENCEI) := $(riscv-march-y)_zicsr_zifencei
+endif
+
+# Check if the toolchain supports Zihintpause extension
+riscv-march-$(CONFIG_TOOLCHAIN_HAS_ZIHINTPAUSE) := $(riscv-march-y)_zihintpause
diff --git a/arch/riscv/boot/dts/Makefile b/arch/riscv/boot/dts/Makefile
index f60a280abb15..72030fd727af 100644
--- a/arch/riscv/boot/dts/Makefile
+++ b/arch/riscv/boot/dts/Makefile
@@ -4,6 +4,7 @@ subdir-y += canaan
 subdir-y += microchip
 subdir-y += renesas
 subdir-y += sifive
+subdir-y += sophgo
 subdir-y += starfive
 subdir-y += thead
 
diff --git a/arch/riscv/boot/dts/sophgo/Makefile b/arch/riscv/boot/dts/sophgo/Makefile
new file mode 100644
index 000000000000..6e7c7763b0a9
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/Makefile
@@ -0,0 +1,7 @@
+# SPDX-License-Identifier: GPL-2.0
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-sophgo-x4evb.dtb
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-sophgo-x8evb.dtb
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-sophgo-pisces.dtb
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-sophgo-capricorn.dtb
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-milkv-pioneer.dtb
+dtb-$(CONFIG_ARCH_SOPHGO) += mango-yixin-s2110.dtb
diff --git a/arch/riscv/boot/dts/sophgo/mango-2sockets.dtsi b/arch/riscv/boot/dts/sophgo/mango-2sockets.dtsi
new file mode 100644
index 000000000000..8c6e22c33cef
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-2sockets.dtsi
@@ -0,0 +1,699 @@
+#define NR_CPUS 128
+
+#include "mango.dtsi"
+#if NR_CPUS > 64
+#include "mango-cpus-socket1.dtsi"
+#endif
+#include "mango-clock-socket1.dtsi"
+
+/ {
+	/delete-node/ distance-map;
+	distance-map {
+		compatible = "numa-distance-map-v1";
+		distance-matrix = <0 0 10>,	//chip0
+				  <0 1 15>,
+				  <0 2 25>,
+				  <0 3 30>,
+				  <0 4 110>,
+				  <0 5 115>,
+				  <0 6 125>,
+				  <0 7 130>,
+				  <1 0 15>,
+				  <1 1 10>,
+				  <1 2 30>,
+				  <1 3 25>,
+				  <1 4 115>,
+				  <1 5 110>,
+				  <1 6 130>,
+				  <1 7 125>,
+				  <2 0 25>,
+				  <2 1 30>,
+				  <2 2 10>,
+				  <2 3 15>,
+				  <2 4 125>,
+				  <2 5 130>,
+				  <2 6 110>,
+				  <2 7 115>,
+				  <3 0 30>,
+				  <3 1 25>,
+				  <3 2 15>,
+				  <3 3 10>,
+				  <3 4 130>,
+				  <3 5 125>,
+				  <3 6 115>,
+				  <3 7 110>,
+				  <4 0 110>,	//chip1
+				  <4 1 115>,
+				  <4 2 125>,
+				  <4 3 130>,
+				  <4 4 10>,
+				  <4 5 15>,
+				  <4 6 25>,
+				  <4 7 30>,
+				  <5 0 115>,
+				  <5 1 110>,
+				  <5 2 130>,
+				  <5 3 125>,
+				  <5 4 15>,
+				  <5 5 10>,
+				  <5 6 30>,
+				  <5 7 25>,
+				  <6 0 125>,
+				  <6 1 130>,
+				  <6 2 110>,
+				  <6 3 115>,
+				  <6 4 25>,
+				  <6 5 30>,
+				  <6 6 10>,
+				  <6 7 15>,
+				  <7 0 130>,
+				  <7 1 125>,
+				  <7 2 115>,
+				  <7 3 110>,
+				  <7 4 30>,
+				  <7 5 25>,
+				  <7 6 15>,
+				  <7 7 10>;
+	};
+
+	soc {
+#if NR_CPUS > 64
+		/delete-node/ clint-mswi@7094000000;
+		clint_mswi: clint-mswi@7094000000 {
+			compatible = "thead,c900-clint-mswi";
+			reg = <0x00000070 0x94000000 0x00000000 0x00004000>;
+			interrupts-extended = <
+				&cpu0_intc 3
+				&cpu1_intc 3
+				&cpu2_intc 3
+				&cpu3_intc 3
+				&cpu4_intc 3
+				&cpu5_intc 3
+				&cpu6_intc 3
+				&cpu7_intc 3
+				&cpu8_intc 3
+				&cpu9_intc 3
+				&cpu10_intc 3
+				&cpu11_intc 3
+				&cpu12_intc 3
+				&cpu13_intc 3
+				&cpu14_intc 3
+				&cpu15_intc 3
+				&cpu16_intc 3
+				&cpu17_intc 3
+				&cpu18_intc 3
+				&cpu19_intc 3
+				&cpu20_intc 3
+				&cpu21_intc 3
+				&cpu22_intc 3
+				&cpu23_intc 3
+				&cpu24_intc 3
+				&cpu25_intc 3
+				&cpu26_intc 3
+				&cpu27_intc 3
+				&cpu28_intc 3
+				&cpu29_intc 3
+				&cpu30_intc 3
+				&cpu31_intc 3
+				&cpu32_intc 3
+				&cpu33_intc 3
+				&cpu34_intc 3
+				&cpu35_intc 3
+				&cpu36_intc 3
+				&cpu37_intc 3
+				&cpu38_intc 3
+				&cpu39_intc 3
+				&cpu40_intc 3
+				&cpu41_intc 3
+				&cpu42_intc 3
+				&cpu43_intc 3
+				&cpu44_intc 3
+				&cpu45_intc 3
+				&cpu46_intc 3
+				&cpu47_intc 3
+				&cpu48_intc 3
+				&cpu49_intc 3
+				&cpu50_intc 3
+				&cpu51_intc 3
+				&cpu52_intc 3
+				&cpu53_intc 3
+				&cpu54_intc 3
+				&cpu55_intc 3
+				&cpu56_intc 3
+				&cpu57_intc 3
+				&cpu58_intc 3
+				&cpu59_intc 3
+				&cpu60_intc 3
+				&cpu61_intc 3
+				&cpu62_intc 3
+				&cpu63_intc 3
+
+				// chip 1
+				&cpu64_intc 3
+				&cpu65_intc 3
+				&cpu66_intc 3
+				&cpu67_intc 3
+				&cpu68_intc 3
+				&cpu69_intc 3
+				&cpu70_intc 3
+				&cpu71_intc 3
+				&cpu72_intc 3
+				&cpu73_intc 3
+				&cpu74_intc 3
+				&cpu75_intc 3
+				&cpu76_intc 3
+				&cpu77_intc 3
+				&cpu78_intc 3
+				&cpu79_intc 3
+				&cpu80_intc 3
+				&cpu81_intc 3
+				&cpu82_intc 3
+				&cpu83_intc 3
+				&cpu84_intc 3
+				&cpu85_intc 3
+				&cpu86_intc 3
+				&cpu87_intc 3
+				&cpu88_intc 3
+				&cpu89_intc 3
+				&cpu90_intc 3
+				&cpu91_intc 3
+				&cpu92_intc 3
+				&cpu93_intc 3
+				&cpu94_intc 3
+				&cpu95_intc 3
+				&cpu96_intc 3
+				&cpu97_intc 3
+				&cpu98_intc 3
+				&cpu99_intc 3
+				&cpu100_intc 3
+				&cpu101_intc 3
+				&cpu102_intc 3
+				&cpu103_intc 3
+				&cpu104_intc 3
+				&cpu105_intc 3
+				&cpu106_intc 3
+				&cpu107_intc 3
+				&cpu108_intc 3
+				&cpu109_intc 3
+				&cpu110_intc 3
+				&cpu111_intc 3
+				&cpu112_intc 3
+				&cpu113_intc 3
+				&cpu114_intc 3
+				&cpu115_intc 3
+				&cpu116_intc 3
+				&cpu117_intc 3
+				&cpu118_intc 3
+				&cpu119_intc 3
+				&cpu120_intc 3
+				&cpu121_intc 3
+				&cpu122_intc 3
+				&cpu123_intc 3
+				&cpu124_intc 3
+				&cpu125_intc 3
+				&cpu126_intc 3
+				&cpu127_intc 3
+				>;
+		};
+
+		clint_mtimer16: clint-mtimer@70ac100000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac100000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu64_intc 7
+				&cpu65_intc 7
+				&cpu66_intc 7
+				&cpu67_intc 7
+				>;
+		};
+
+		clint_mtimer17: clint-mtimer@70ac110000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac110000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu68_intc 7
+				&cpu69_intc 7
+				&cpu70_intc 7
+				&cpu71_intc 7
+				>;
+		};
+
+		clint_mtimer18: clint-mtimer@70ac120000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac120000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu72_intc 7
+				&cpu73_intc 7
+				&cpu74_intc 7
+				&cpu75_intc 7
+				>;
+		};
+
+		clint_mtimer19: clint-mtimer@70ac130000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac130000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu76_intc 7
+				&cpu77_intc 7
+				&cpu78_intc 7
+				&cpu79_intc 7
+				>;
+		};
+
+		clint_mtimer20: clint-mtimer@70ac140000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac140000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu80_intc 7
+				&cpu81_intc 7
+				&cpu82_intc 7
+				&cpu83_intc 7
+				>;
+		};
+
+		clint_mtimer21: clint-mtimer@70ac150000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac150000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu84_intc 7
+				&cpu85_intc 7
+				&cpu86_intc 7
+				&cpu87_intc 7
+				>;
+		};
+
+		clint_mtimer22: clint-mtimer@70ac160000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac160000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu88_intc 7
+				&cpu89_intc 7
+				&cpu90_intc 7
+				&cpu91_intc 7
+				>;
+		};
+
+		clint_mtimer23: clint-mtimer@70ac170000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac170000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu92_intc 7
+				&cpu93_intc 7
+				&cpu94_intc 7
+				&cpu95_intc 7
+				>;
+		};
+
+		clint_mtimer24: clint-mtimer@70ac180000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac180000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu96_intc 7
+				&cpu97_intc 7
+				&cpu98_intc 7
+				&cpu99_intc 7
+				>;
+		};
+
+		clint_mtimer25: clint-mtimer@70ac190000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac190000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu100_intc 7
+				&cpu101_intc 7
+				&cpu102_intc 7
+				&cpu103_intc 7
+				>;
+		};
+
+		clint_mtimer26: clint-mtimer@70ac1a0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1a0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu104_intc 7
+				&cpu105_intc 7
+				&cpu106_intc 7
+				&cpu107_intc 7
+				>;
+		};
+
+		clint_mtimer27: clint-mtimer@70ac1b0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1b0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu108_intc 7
+				&cpu109_intc 7
+				&cpu110_intc 7
+				&cpu111_intc 7
+				>;
+		};
+
+		clint_mtimer28: clint-mtimer@70ac1c0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1c0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu112_intc 7
+				&cpu113_intc 7
+				&cpu114_intc 7
+				&cpu115_intc 7
+				>;
+		};
+
+		clint_mtimer29: clint-mtimer@70ac1d0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1d0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu116_intc 7
+				&cpu117_intc 7
+				&cpu118_intc 7
+				&cpu119_intc 7
+				>;
+		};
+
+		clint_mtimer30: clint-mtimer@70ac1e0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1e0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu120_intc 7
+				&cpu121_intc 7
+				&cpu122_intc 7
+				&cpu123_intc 7
+				>;
+		};
+
+		clint_mtimer31: clint-mtimer@70ac1f0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac1f0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu124_intc 7
+				&cpu125_intc 7
+				&cpu126_intc 7
+				&cpu127_intc 7
+				>;
+		};
+#endif
+
+		/delete-node/ interrupt-controller@7090000000;
+		intc: interrupt-controller@7090000000 {
+			#address-cells = <0>;
+			#interrupt-cells = <2>;
+			compatible = "thead,c900-plic";
+			interrupt-controller;
+			interrupts-extended = <
+				&cpu0_intc  11 &cpu0_intc  9
+				&cpu1_intc  11 &cpu1_intc  9
+				&cpu2_intc  11 &cpu2_intc  9
+				&cpu3_intc  11 &cpu3_intc  9
+				&cpu4_intc  11 &cpu4_intc  9
+				&cpu5_intc  11 &cpu5_intc  9
+				&cpu6_intc  11 &cpu6_intc  9
+				&cpu7_intc  11 &cpu7_intc  9
+				&cpu8_intc  11 &cpu8_intc  9
+				&cpu9_intc  11 &cpu9_intc  9
+				&cpu10_intc  11 &cpu10_intc  9
+				&cpu11_intc  11 &cpu11_intc  9
+				&cpu12_intc  11 &cpu12_intc  9
+				&cpu13_intc  11 &cpu13_intc  9
+				&cpu14_intc  11 &cpu14_intc  9
+				&cpu15_intc  11 &cpu15_intc  9
+				&cpu16_intc  11 &cpu16_intc  9
+				&cpu17_intc  11 &cpu17_intc  9
+				&cpu18_intc  11 &cpu18_intc  9
+				&cpu19_intc  11 &cpu19_intc  9
+				&cpu20_intc  11 &cpu20_intc  9
+				&cpu21_intc  11 &cpu21_intc  9
+				&cpu22_intc  11 &cpu22_intc  9
+				&cpu23_intc  11 &cpu23_intc  9
+				&cpu24_intc  11 &cpu24_intc  9
+				&cpu25_intc  11 &cpu25_intc  9
+				&cpu26_intc  11 &cpu26_intc  9
+				&cpu27_intc  11 &cpu27_intc  9
+				&cpu28_intc  11 &cpu28_intc  9
+				&cpu29_intc  11 &cpu29_intc  9
+				&cpu30_intc  11 &cpu30_intc  9
+				&cpu31_intc  11 &cpu31_intc  9
+				&cpu32_intc  11 &cpu32_intc  9
+				&cpu33_intc  11 &cpu33_intc  9
+				&cpu34_intc  11 &cpu34_intc  9
+				&cpu35_intc  11 &cpu35_intc  9
+				&cpu36_intc  11 &cpu36_intc  9
+				&cpu37_intc  11 &cpu37_intc  9
+				&cpu38_intc  11 &cpu38_intc  9
+				&cpu39_intc  11 &cpu39_intc  9
+				&cpu40_intc  11 &cpu40_intc  9
+				&cpu41_intc  11 &cpu41_intc  9
+				&cpu42_intc  11 &cpu42_intc  9
+				&cpu43_intc  11 &cpu43_intc  9
+				&cpu44_intc  11 &cpu44_intc  9
+				&cpu45_intc  11 &cpu45_intc  9
+				&cpu46_intc  11 &cpu46_intc  9
+				&cpu47_intc  11 &cpu47_intc  9
+				&cpu48_intc  11 &cpu48_intc  9
+				&cpu49_intc  11 &cpu49_intc  9
+				&cpu50_intc  11 &cpu50_intc  9
+				&cpu51_intc  11 &cpu51_intc  9
+				&cpu52_intc  11 &cpu52_intc  9
+				&cpu53_intc  11 &cpu53_intc  9
+				&cpu54_intc  11 &cpu54_intc  9
+				&cpu55_intc  11 &cpu55_intc  9
+				&cpu56_intc  11 &cpu56_intc  9
+				&cpu57_intc  11 &cpu57_intc  9
+				&cpu58_intc  11 &cpu58_intc  9
+				&cpu59_intc  11 &cpu59_intc  9
+				&cpu60_intc  11 &cpu60_intc  9
+				&cpu61_intc  11 &cpu61_intc  9
+				&cpu62_intc  11 &cpu62_intc  9
+				&cpu63_intc  11 &cpu63_intc  9
+
+#if NR_CPUS > 64
+				//chip 1
+				&cpu64_intc  11 &cpu64_intc  9
+				&cpu65_intc  11 &cpu65_intc  9
+				&cpu66_intc  11 &cpu66_intc  9
+				&cpu67_intc  11 &cpu67_intc  9
+				&cpu68_intc  11 &cpu68_intc  9
+				&cpu69_intc  11 &cpu69_intc  9
+				&cpu70_intc  11 &cpu70_intc  9
+				&cpu71_intc  11 &cpu71_intc  9
+				&cpu72_intc  11 &cpu72_intc  9
+				&cpu73_intc  11 &cpu73_intc  9
+				&cpu74_intc  11 &cpu74_intc  9
+				&cpu75_intc  11 &cpu75_intc  9
+				&cpu76_intc  11 &cpu76_intc  9
+				&cpu77_intc  11 &cpu77_intc  9
+				&cpu78_intc  11 &cpu78_intc  9
+				&cpu79_intc  11 &cpu79_intc  9
+				&cpu80_intc  11 &cpu80_intc  9
+				&cpu81_intc  11 &cpu81_intc  9
+				&cpu82_intc  11 &cpu82_intc  9
+				&cpu83_intc  11 &cpu83_intc  9
+				&cpu84_intc  11 &cpu84_intc  9
+				&cpu85_intc  11 &cpu85_intc  9
+				&cpu86_intc  11 &cpu86_intc  9
+				&cpu87_intc  11 &cpu87_intc  9
+				&cpu88_intc  11 &cpu88_intc  9
+				&cpu89_intc  11 &cpu89_intc  9
+				&cpu90_intc  11 &cpu90_intc  9
+				&cpu91_intc  11 &cpu91_intc  9
+				&cpu92_intc  11 &cpu92_intc  9
+				&cpu93_intc  11 &cpu93_intc  9
+				&cpu94_intc  11 &cpu94_intc  9
+				&cpu95_intc  11 &cpu95_intc  9
+				&cpu96_intc  11 &cpu96_intc  9
+				&cpu97_intc  11 &cpu97_intc  9
+				&cpu98_intc  11 &cpu98_intc  9
+				&cpu99_intc  11 &cpu99_intc  9
+				&cpu100_intc  11 &cpu100_intc  9
+				&cpu101_intc  11 &cpu101_intc  9
+				&cpu102_intc  11 &cpu102_intc  9
+				&cpu103_intc  11 &cpu103_intc  9
+				&cpu104_intc  11 &cpu104_intc  9
+				&cpu105_intc  11 &cpu105_intc  9
+				&cpu106_intc  11 &cpu106_intc  9
+				&cpu107_intc  11 &cpu107_intc  9
+				&cpu108_intc  11 &cpu108_intc  9
+				&cpu109_intc  11 &cpu109_intc  9
+				&cpu110_intc  11 &cpu110_intc  9
+				&cpu111_intc  11 &cpu111_intc  9
+				&cpu112_intc  11 &cpu112_intc  9
+				&cpu113_intc  11 &cpu113_intc  9
+				&cpu114_intc  11 &cpu114_intc  9
+				&cpu115_intc  11 &cpu115_intc  9
+				&cpu116_intc  11 &cpu116_intc  9
+				&cpu117_intc  11 &cpu117_intc  9
+				&cpu118_intc  11 &cpu118_intc  9
+				&cpu119_intc  11 &cpu119_intc  9
+				&cpu120_intc  11 &cpu120_intc  9
+				&cpu121_intc  11 &cpu121_intc  9
+				&cpu122_intc  11 &cpu122_intc  9
+				&cpu123_intc  11 &cpu123_intc  9
+				&cpu124_intc  11 &cpu124_intc  9
+				&cpu125_intc  11 &cpu125_intc  9
+				&cpu126_intc  11 &cpu126_intc  9
+				&cpu127_intc  11 &cpu127_intc  9
+#endif
+				>;
+			reg = <0x00000070 0x90000000 0x00000000 0x04000000>;
+			reg-names = "control";
+			riscv,max-priority = <7>;
+			riscv,ndev = <448>;
+		};
+
+		top1_misc: top_misc_ctrl@f030010000 {
+			compatible = "syscon";
+			reg = <0xf0 0x30010000 0x0 0x8000>;
+		};
+
+		rst1: reset1-controller {
+			#reset-cells = <1>;
+			compatible = "bitmain,reset";
+			subctrl-syscon = <&top1_misc>;
+			top_rst_offset = <0x3000>;
+			nr_resets = <RST_MAX_NUM>;
+		};
+
+		gpio3: gpio@f030009000 {
+			compatible = "snps,dw-apb-gpio";
+			reg = <0xf0 0x30009000 0x0 0x400>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			clocks = <&s1_div_clk GATE_CLK_APB_GPIO>,
+				 <&s1_div_clk GATE_CLK_GPIO_DB>;
+			clock-names = "bus", "db";
+
+			port3a: gpio-controller@0 {
+				compatible = "snps,dw-apb-gpio-port";
+				bank-name = "port0a";
+				gpio-controller;
+				#gpio-cells = <2>;
+				snps,nr-gpios = <32>;
+				reg = <0>;
+				interrupt-controller;
+				#interrupt-cells = <2>;
+				interrupt-parent = <&intc>;
+				interrupts = <SOC_PERIPHERAL_IRQ(320) IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		ethernet1: ethernet@f040026000 {
+			compatible = "bitmain,ethernet";
+			reg = <0xf0 0x40026000 0x0 0x4000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(356) IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			clock-names = "clk_tx", "gate_clk_tx", "stmmaceth", "ptp_ref", "gate_clk_ref";
+			clocks = <&s1_div_clk DIV_CLK_FPLL_TX_ETH0>,
+				   <&s1_div_clk GATE_CLK_TX_ETH0>,
+				   <&s1_div_clk GATE_CLK_AXI_ETH0>,
+				   <&s1_div_clk GATE_CLK_PTP_REF_I_ETH0>,
+				   <&s1_div_clk GATE_CLK_REF_ETH0>;
+
+			/* no hash filter and perfect filter support */
+			snps,multicast-filter-bins = <0>;
+			snps,perfect-filter-entries = <1>;
+
+			snps,txpbl = <32>;
+			snps,rxpbl = <32>;
+			snps,aal;
+
+			snps,axi-config = <&stmmac_axi_setup>;
+			snps,mtl-rx-config = <&mtl_rx_setup>;
+			snps,mtl-tx-config = <&mtl_tx_setup>;
+
+			phy-mode = "rgmii-txid";
+			phy-reset-gpios = <&port3a 27 0>;
+			phy-handle = <&phy1>;
+			mdio {
+				#address-cells = <0x1>;
+				#size-cells = <0x0>;
+				compatible = "snps,dwmac-mdio";
+				phy1: phy@0 {
+					compatible = "ethernet-phy-ieee802.3-c22";
+					device_type = "ethernet-phy";
+					reg = <0x0>;
+				};
+			};
+		};
+
+		emmc1: bm-emmc@f04002A000 {
+			compatible = "bitmain,bm-emmc";
+			reg = <0xf0 0x4002A000 0x0 0x1000>;
+			reg-names = "core_mem";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(358) IRQ_TYPE_LEVEL_HIGH>;
+			bus-width = <4>;
+			non-removable;
+			no-sdio;
+			no-sd;
+			resets = <&rst1 RST_EMMC>;
+			reset-names = "emmc";
+			clocks =
+				<&s1_div_clk GATE_CLK_EMMC_100M>,
+				<&s1_div_clk GATE_CLK_AXI_EMMC>,
+				<&s1_div_clk GATE_CLK_100K_EMMC>;
+			clock-names =
+				"clk_gate_emmc",
+				"clk_gate_axi_emmc",
+				"clk_gate_100k_emmc";
+		};
+
+		sd1: bm-sd@f04002B000 {
+			compatible = "bitmain,bm-sd";
+			reg = <0xf0 0x4002B000 0x0 0x1000>;
+			reg-names = "core_mem";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(360) IRQ_TYPE_LEVEL_HIGH>;
+			bus-width = <4>;
+			no-sdio;
+			no-mmc;
+			resets = <&rst1 RST_SD>;
+			reset-names = "sdio";
+			clocks =
+				<&s1_div_clk GATE_CLK_SD_100M>,
+				<&s1_div_clk GATE_CLK_AXI_SD>,
+				<&s1_div_clk GATE_CLK_100K_SD>;
+			clock-names =
+				"clk_gate_sd",
+				"clk_gate_axi_sd",
+				"clk_gate_100k_sd";
+		};
+	};
+
+	spifmc2: flash-controller@f000180000 {
+		compatible = "sophgo,spifmc";
+		reg = <0xf0 0x00180000 0x0 0x1000000>;
+		reg-names = "memory";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(332) IRQ_TYPE_LEVEL_HIGH>;
+		clock-frequency = <100000000>;
+		clocks = <&s1_div_clk GATE_CLK_AHB_SF>;
+		flash@0 {
+			reg = <0>;
+			compatible = "jedec,spi-nor";
+		};
+	};
+
+	spifmc3: flash-controller@f002180000 {
+		compatible = "sophgo,spifmc";
+		reg = <0xf0 0x02180000 0x0 0x1000000>;
+		reg-names = "memory";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(333) IRQ_TYPE_LEVEL_HIGH>;
+		clock-frequency = <100000000>;
+		clocks = <&s1_div_clk GATE_CLK_AHB_SF>;
+		flash@0 {
+			reg = <0>;
+			compatible = "jedec,spi-nor";
+		};
+	};
+
+	aliases {
+	        serial0 = &uart0;
+	        ethernet0 = &ethernet0;
+	        ethernet1 = &ethernet1;
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-clock-socket0.dtsi b/arch/riscv/boot/dts/sophgo/mango-clock-socket0.dtsi
new file mode 100644
index 000000000000..af3380412f1d
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-clock-socket0.dtsi
@@ -0,0 +1,124 @@
+/ {
+	socket0-clocks {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		cgi: ctrystal {
+			compatible = "fixed-clock";
+			clock-frequency = <25000000>;
+			clock-output-names = "cgi";
+			#clock-cells = <0>;
+		};
+
+		/* pll clock */
+		mpll: mpll {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <MPLL_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top_misc>;
+			clocks = <&cgi>;
+			clock-output-names = "mpll_clock";
+		};
+
+		fpll: fpll {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <FPLL_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top_misc>;
+			clocks = <&cgi>;
+			clock-output-names = "fpll_clock";
+		};
+
+		dpll0: dpll0 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <DPLL0_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top_misc>;
+			clocks = <&cgi>;
+			clock-output-names = "dpll0_clock";
+		};
+
+		dpll1: dpll1 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top_misc>;
+			clocks = <&cgi>;
+			id = <DPLL1_CLK>;
+			clock-output-names = "dpll1_clock";
+		};
+
+		div_clk: div_clk {
+			compatible = "mango, pll-child-clock";
+			#clock-cells = <1>;
+			id = <S0_DIV_CLK_TABLE>;
+			subctrl-syscon = <&top_misc>;
+		};
+
+		mux_clk: mux_clk {
+			compatible = "mango, pll-mux-clock";
+			#clock-cells = <1>;
+			id = <S0_MUX_CLK_TABLE>;
+			subctrl-syscon = <&top_misc>;
+		};
+
+		socket0_default_rates {
+			compatible = "mango, clk-default-rates";
+			#clock-cells = <1>;
+			subctrl-syscon = <&top_misc>;
+			clocks = \
+				<&mpll>, <&fpll>,
+
+				<&div_clk DIV_CLK_FPLL_RP_CPU_NORMAL_1>,
+				<&div_clk DIV_CLK_FPLL_50M_A53>,
+				<&div_clk DIV_CLK_FPLL_TOP_RP_CMN_DIV2>,
+				<&div_clk DIV_CLK_FPLL_UART_500M>,
+				<&div_clk DIV_CLK_FPLL_AHB_LPC>,
+				<&div_clk DIV_CLK_FPLL_EFUSE>,
+				<&div_clk DIV_CLK_FPLL_TX_ETH0>,
+				<&div_clk DIV_CLK_FPLL_PTP_REF_I_ETH0>,
+				<&div_clk DIV_CLK_FPLL_REF_ETH0>,
+				<&div_clk DIV_CLK_FPLL_EMMC>,
+				<&div_clk DIV_CLK_FPLL_SD>,
+				<&div_clk DIV_CLK_FPLL_TOP_AXI0>,
+				<&div_clk DIV_CLK_FPLL_TOP_AXI_HSPERI>,
+				<&div_clk DIV_CLK_FPLL_AXI_DDR_1>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER1>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER2>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER3>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER4>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER5>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER6>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER7>,
+				<&div_clk DIV_CLK_FPLL_DIV_TIMER8>,
+				<&div_clk DIV_CLK_FPLL_100K_EMMC>,
+				<&div_clk DIV_CLK_FPLL_100K_SD>,
+				<&div_clk DIV_CLK_FPLL_GPIO_DB>,
+
+				<&div_clk DIV_CLK_MPLL_RP_CPU_NORMAL_0>,
+				<&div_clk DIV_CLK_MPLL_AXI_DDR_0>;
+
+			clock-rates = \
+				<2000000000>, <1000000000>,
+
+				<2000000000>, <50000000>,
+				<1000000000>, <500000000>,
+				<200000000>, <25000000>,
+				<125000000>, <50000000>,
+				<25000000>, <100000000>,
+				<100000000>, <100000000>,
+				<250000000>, <1000000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<100000>, <100000>, <100000>,
+
+				<2000000001>, <1000000001>;
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-clock-socket1.dtsi b/arch/riscv/boot/dts/sophgo/mango-clock-socket1.dtsi
new file mode 100644
index 000000000000..cfe34495e4fd
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-clock-socket1.dtsi
@@ -0,0 +1,124 @@
+/ {
+	socket1-clocks {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		cgi1: ctrystal1 {
+			compatible = "fixed-clock";
+			clock-frequency = <25000000>;
+			clock-output-names = "s1_cgi";
+			#clock-cells = <0>;
+		};
+
+		/* pll clock */
+		mpll1: mpll1 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <MPLL_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top1_misc>;
+			clocks = <&cgi1>;
+			clock-output-names = "s1_mpll_clock";
+		};
+
+		fpll1: fpll1 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <FPLL_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top1_misc>;
+			clocks = <&cgi1>;
+			clock-output-names = "s1_fpll_clock";
+		};
+
+		dpll01: dpll01 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			id = <DPLL0_CLK>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top1_misc>;
+			clocks = <&cgi1>;
+			clock-output-names = "s1_dpll0_clock";
+		};
+
+		dpll11: dpll11 {
+			compatible = "mango, pll-clock";
+			#clock-cells = <0>;
+			mode = <NORMAL_MODE>;
+			subctrl-syscon = <&top1_misc>;
+			clocks = <&cgi1>;
+			id = <DPLL1_CLK>;
+			clock-output-names = "s1_dpll1_clock";
+		};
+
+		s1_div_clk: s1_div_clk {
+			compatible = "mango, pll-child-clock";
+			#clock-cells = <1>;
+			id = <S1_DIV_CLK_TABLE>;
+			subctrl-syscon = <&top1_misc>;
+		};
+
+		s1_mux_clk: s1_mux_clk {
+			compatible = "mango, pll-mux-clock";
+			#clock-cells = <1>;
+			id = <S1_MUX_CLK_TABLE>;
+			subctrl-syscon = <&top1_misc>;
+		};
+
+		socket1_default_rates {
+			compatible = "mango, clk-default-rates";
+			#clock-cells = <1>;
+			subctrl-syscon = <&top1_misc>;
+			clocks = \
+				<&mpll1>, <&fpll1>,
+
+				<&s1_div_clk DIV_CLK_FPLL_RP_CPU_NORMAL_1>,
+				<&s1_div_clk DIV_CLK_FPLL_50M_A53>,
+				<&s1_div_clk DIV_CLK_FPLL_TOP_RP_CMN_DIV2>,
+				<&s1_div_clk DIV_CLK_FPLL_UART_500M>,
+				<&s1_div_clk DIV_CLK_FPLL_AHB_LPC>,
+				<&s1_div_clk DIV_CLK_FPLL_EFUSE>,
+				<&s1_div_clk DIV_CLK_FPLL_TX_ETH0>,
+				<&s1_div_clk DIV_CLK_FPLL_PTP_REF_I_ETH0>,
+				<&s1_div_clk DIV_CLK_FPLL_REF_ETH0>,
+				<&s1_div_clk DIV_CLK_FPLL_EMMC>,
+				<&s1_div_clk DIV_CLK_FPLL_SD>,
+				<&s1_div_clk DIV_CLK_FPLL_TOP_AXI0>,
+				<&s1_div_clk DIV_CLK_FPLL_TOP_AXI_HSPERI>,
+				<&s1_div_clk DIV_CLK_FPLL_AXI_DDR_1>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER1>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER2>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER3>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER4>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER5>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER6>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER7>,
+				<&s1_div_clk DIV_CLK_FPLL_DIV_TIMER8>,
+				<&s1_div_clk DIV_CLK_FPLL_100K_EMMC>,
+				<&s1_div_clk DIV_CLK_FPLL_100K_SD>,
+				<&s1_div_clk DIV_CLK_FPLL_GPIO_DB>,
+
+				<&s1_div_clk DIV_CLK_MPLL_RP_CPU_NORMAL_0>,
+				<&s1_div_clk DIV_CLK_MPLL_AXI_DDR_0>;
+
+			clock-rates = \
+				<2000000000>, <1000000000>,
+
+				<2000000000>, <50000000>,
+				<1000000000>, <500000000>,
+				<200000000>, <25000000>,
+				<125000000>, <50000000>,
+				<25000000>, <100000000>,
+				<100000000>, <100000000>,
+				<250000000>, <1000000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<50000000>, <50000000>,
+				<100000>, <100000>, <100000>,
+
+				<2000000001>, <1000000001>;
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-cpus-socket0.dtsi b/arch/riscv/boot/dts/sophgo/mango-cpus-socket0.dtsi
new file mode 100644
index 000000000000..7efc9741f3e7
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-cpus-socket0.dtsi
@@ -0,0 +1,1148 @@
+/ {
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		timebase-frequency = <50000000>;
+
+		cpu-map {
+			socket0 {
+				cluster0 {
+					 core0 {
+						cpu = <&cpu0>;
+					 };
+					 core1 {
+						cpu = <&cpu1>;
+					 };
+					 core2 {
+						cpu = <&cpu2>;
+					 };
+					 core3 {
+						cpu = <&cpu3>;
+					 };
+				};
+
+				cluster1 {
+					 core0 {
+						cpu = <&cpu4>;
+					 };
+					 core1 {
+						cpu = <&cpu5>;
+					 };
+					 core2 {
+						cpu = <&cpu6>;
+					 };
+					 core3 {
+						cpu = <&cpu7>;
+					 };
+				};
+
+				cluster2 {
+					 core0 {
+						cpu = <&cpu16>;
+					 };
+					 core1 {
+						cpu = <&cpu17>;
+					 };
+					 core2 {
+						cpu = <&cpu18>;
+					 };
+					 core3 {
+						cpu = <&cpu19>;
+					 };
+				};
+
+				cluster3 {
+					 core0 {
+						cpu = <&cpu20>;
+					 };
+					 core1 {
+						cpu = <&cpu21>;
+					 };
+					 core2 {
+						cpu = <&cpu22>;
+					 };
+					 core3 {
+						cpu = <&cpu23>;
+					 };
+				};
+
+				cluster4 {
+					 core0 {
+						cpu = <&cpu8>;
+					 };
+					 core1 {
+						cpu = <&cpu9>;
+					 };
+					 core2 {
+						cpu = <&cpu10>;
+					 };
+					 core3 {
+						cpu = <&cpu11>;
+					 };
+				};
+
+				cluster5 {
+					 core0 {
+						cpu = <&cpu12>;
+					 };
+					 core1 {
+						cpu = <&cpu13>;
+					 };
+					 core2 {
+						cpu = <&cpu14>;
+					 };
+					 core3 {
+						cpu = <&cpu15>;
+					 };
+				};
+
+				cluster6 {
+					 core0 {
+						cpu = <&cpu24>;
+					 };
+					 core1 {
+						cpu = <&cpu25>;
+					 };
+					 core2 {
+						cpu = <&cpu26>;
+					 };
+					 core3 {
+						cpu = <&cpu27>;
+					 };
+				};
+
+				cluster7 {
+					 core0 {
+						cpu = <&cpu28>;
+					 };
+					 core1 {
+						cpu = <&cpu29>;
+					 };
+					 core2 {
+						cpu = <&cpu30>;
+					 };
+					 core3 {
+						cpu = <&cpu31>;
+					 };
+				};
+
+				cluster8 {
+					 core0 {
+						cpu = <&cpu32>;
+					 };
+					 core1 {
+						cpu = <&cpu33>;
+					 };
+					 core2 {
+						cpu = <&cpu34>;
+					 };
+					 core3 {
+						cpu = <&cpu35>;
+					 };
+				};
+
+				cluster9 {
+					 core0 {
+						cpu = <&cpu36>;
+					 };
+					 core1 {
+						cpu = <&cpu37>;
+					 };
+					 core2 {
+						cpu = <&cpu38>;
+					 };
+					 core3 {
+						cpu = <&cpu39>;
+					 };
+				};
+
+				cluster10 {
+					 core0 {
+						cpu = <&cpu48>;
+					 };
+					 core1 {
+						cpu = <&cpu49>;
+					 };
+					 core2 {
+						cpu = <&cpu50>;
+					 };
+					 core3 {
+						cpu = <&cpu51>;
+					 };
+				};
+
+				cluster11 {
+					 core0 {
+						cpu = <&cpu52>;
+					 };
+					 core1 {
+						cpu = <&cpu53>;
+					 };
+					 core2 {
+						cpu = <&cpu54>;
+					 };
+					 core3 {
+						cpu = <&cpu55>;
+					 };
+				};
+
+				cluster12 {
+					 core0 {
+						cpu = <&cpu40>;
+					 };
+					 core1 {
+						cpu = <&cpu41>;
+					 };
+					 core2 {
+						cpu = <&cpu42>;
+					 };
+					 core3 {
+						cpu = <&cpu43>;
+					 };
+				};
+
+				cluster13 {
+					 core0 {
+						cpu = <&cpu44>;
+					 };
+					 core1 {
+						cpu = <&cpu45>;
+					 };
+					 core2 {
+						cpu = <&cpu46>;
+					 };
+					 core3 {
+						cpu = <&cpu47>;
+					 };
+				};
+
+				cluster14 {
+					 core0 {
+						cpu = <&cpu56>;
+					 };
+					 core1 {
+						cpu = <&cpu57>;
+					 };
+					 core2 {
+						cpu = <&cpu58>;
+					 };
+					 core3 {
+						cpu = <&cpu59>;
+					 };
+				};
+
+				cluster15 {
+					 core0 {
+						cpu = <&cpu60>;
+					 };
+					 core1 {
+						cpu = <&cpu61>;
+					 };
+					 core2 {
+						cpu = <&cpu62>;
+					 };
+					 core3 {
+						cpu = <&cpu63>;
+					 };
+				};
+			};
+		};
+
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			reg = <0>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu0_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			reg = <1>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu1_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			reg = <2>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu2_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			reg = <3>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu3_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu4: cpu@4 {
+			device_type = "cpu";
+			reg = <4>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu4_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu5: cpu@5 {
+			device_type = "cpu";
+			reg = <5>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu5_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu6: cpu@6 {
+			device_type = "cpu";
+			reg = <6>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu6_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu7: cpu@7 {
+			device_type = "cpu";
+			reg = <7>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu7_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu8: cpu@8 {
+			device_type = "cpu";
+			reg = <8>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu8_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu9: cpu@9 {
+			device_type = "cpu";
+			reg = <9>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu9_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu10: cpu@10 {
+			device_type = "cpu";
+			reg = <10>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu10_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu11: cpu@11 {
+			device_type = "cpu";
+			reg = <11>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu11_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu12: cpu@12 {
+			device_type = "cpu";
+			reg = <12>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu12_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu13: cpu@13 {
+			device_type = "cpu";
+			reg = <13>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu13_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu14: cpu@14 {
+			device_type = "cpu";
+			reg = <14>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu14_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu15: cpu@15 {
+			device_type = "cpu";
+			reg = <15>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu15_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu16: cpu@16 {
+			device_type = "cpu";
+			reg = <16>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu16_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu17: cpu@17 {
+			device_type = "cpu";
+			reg = <17>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu17_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu18: cpu@18 {
+			device_type = "cpu";
+			reg = <18>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu18_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu19: cpu@19 {
+			device_type = "cpu";
+			reg = <19>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu19_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu20: cpu@20 {
+			device_type = "cpu";
+			reg = <20>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu20_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu21: cpu@21 {
+			device_type = "cpu";
+			reg = <21>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu21_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu22: cpu@22 {
+			device_type = "cpu";
+			reg = <22>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu22_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu23: cpu@23 {
+			device_type = "cpu";
+			reg = <23>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <0>;
+			cpu23_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu24: cpu@24 {
+			device_type = "cpu";
+			reg = <24>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu24_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu25: cpu@25 {
+			device_type = "cpu";
+			reg = <25>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu25_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu26: cpu@26 {
+			device_type = "cpu";
+			reg = <26>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu26_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu27: cpu@27 {
+			device_type = "cpu";
+			reg = <27>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu27_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu28: cpu@28 {
+			device_type = "cpu";
+			reg = <28>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu28_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu29: cpu@29 {
+			device_type = "cpu";
+			reg = <29>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu29_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu30: cpu@30 {
+			device_type = "cpu";
+			reg = <30>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu30_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu31: cpu@31 {
+			device_type = "cpu";
+			reg = <31>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <1>;
+			cpu31_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu32: cpu@32 {
+			device_type = "cpu";
+			reg = <32>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu32_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu33: cpu@33 {
+			device_type = "cpu";
+			reg = <33>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu33_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu34: cpu@34 {
+			device_type = "cpu";
+			reg = <34>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu34_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu35: cpu@35 {
+			device_type = "cpu";
+			reg = <35>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu35_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu36: cpu@36 {
+			device_type = "cpu";
+			reg = <36>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu36_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu37: cpu@37 {
+			device_type = "cpu";
+			reg = <37>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu37_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu38: cpu@38 {
+			device_type = "cpu";
+			reg = <38>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu38_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu39: cpu@39 {
+			device_type = "cpu";
+			reg = <39>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu39_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu40: cpu@40 {
+			device_type = "cpu";
+			reg = <40>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu40_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu41: cpu@41 {
+			device_type = "cpu";
+			reg = <41>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu41_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu42: cpu@42 {
+			device_type = "cpu";
+			reg = <42>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu42_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu43: cpu@43 {
+			device_type = "cpu";
+			reg = <43>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu43_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu44: cpu@44 {
+			device_type = "cpu";
+			reg = <44>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu44_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu45: cpu@45 {
+			device_type = "cpu";
+			reg = <45>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu45_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu46: cpu@46 {
+			device_type = "cpu";
+			reg = <46>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu46_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu47: cpu@47 {
+			device_type = "cpu";
+			reg = <47>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu47_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu48: cpu@48 {
+			device_type = "cpu";
+			reg = <48>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu48_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu49: cpu@49 {
+			device_type = "cpu";
+			reg = <49>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu49_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu50: cpu@50 {
+			device_type = "cpu";
+			reg = <50>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu50_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu51: cpu@51 {
+			device_type = "cpu";
+			reg = <51>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu51_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu52: cpu@52 {
+			device_type = "cpu";
+			reg = <52>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu52_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu53: cpu@53 {
+			device_type = "cpu";
+			reg = <53>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu53_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu54: cpu@54 {
+			device_type = "cpu";
+			reg = <54>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu54_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu55: cpu@55 {
+			device_type = "cpu";
+			reg = <55>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <2>;
+			cpu55_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu56: cpu@56 {
+			device_type = "cpu";
+			reg = <56>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu56_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu57: cpu@57 {
+			device_type = "cpu";
+			reg = <57>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu57_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu58: cpu@58 {
+			device_type = "cpu";
+			reg = <58>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu58_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu59: cpu@59 {
+			device_type = "cpu";
+			reg = <59>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu59_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu60: cpu@60 {
+			device_type = "cpu";
+			reg = <60>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu60_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu61: cpu@61 {
+			device_type = "cpu";
+			reg = <61>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu61_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu62: cpu@62 {
+			device_type = "cpu";
+			reg = <62>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu62_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu63: cpu@63 {
+			device_type = "cpu";
+			reg = <63>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <3>;
+			cpu63_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-cpus-socket1.dtsi b/arch/riscv/boot/dts/sophgo/mango-cpus-socket1.dtsi
new file mode 100644
index 000000000000..255306410f40
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-cpus-socket1.dtsi
@@ -0,0 +1,1149 @@
+/ {
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		timebase-frequency = <50000000>;
+
+		cpu-map {
+			socket1 {
+				cluster0 {
+					 core0 {
+						cpu = <&cpu64>;
+					 };
+					 core1 {
+						cpu = <&cpu65>;
+					 };
+					 core2 {
+						cpu = <&cpu66>;
+					 };
+					 core3 {
+						cpu = <&cpu67>;
+					 };
+				};
+
+				cluster1 {
+					 core0 {
+						cpu = <&cpu68>;
+					 };
+					 core1 {
+						cpu = <&cpu69>;
+					 };
+					 core2 {
+						cpu = <&cpu70>;
+					 };
+					 core3 {
+						cpu = <&cpu71>;
+					 };
+				};
+
+				cluster2 {
+					 core0 {
+						cpu = <&cpu80>;
+					 };
+					 core1 {
+						cpu = <&cpu81>;
+					 };
+					 core2 {
+						cpu = <&cpu82>;
+					 };
+					 core3 {
+						cpu = <&cpu83>;
+					 };
+				};
+
+				cluster3 {
+					 core0 {
+						cpu = <&cpu84>;
+					 };
+					 core1 {
+						cpu = <&cpu85>;
+					 };
+					 core2 {
+						cpu = <&cpu86>;
+					 };
+					 core3 {
+						cpu = <&cpu87>;
+					 };
+				};
+
+				cluster4 {
+					 core0 {
+						cpu = <&cpu72>;
+					 };
+					 core1 {
+						cpu = <&cpu73>;
+					 };
+					 core2 {
+						cpu = <&cpu74>;
+					 };
+					 core3 {
+						cpu = <&cpu75>;
+					 };
+				};
+
+				cluster5 {
+					 core0 {
+						cpu = <&cpu76>;
+					 };
+					 core1 {
+						cpu = <&cpu77>;
+					 };
+					 core2 {
+						cpu = <&cpu78>;
+					 };
+					 core3 {
+						cpu = <&cpu79>;
+					 };
+				};
+
+				cluster6 {
+					 core0 {
+						cpu = <&cpu88>;
+					 };
+					 core1 {
+						cpu = <&cpu89>;
+					 };
+					 core2 {
+						cpu = <&cpu90>;
+					 };
+					 core3 {
+						cpu = <&cpu91>;
+					 };
+				};
+
+				cluster7 {
+					 core0 {
+						cpu = <&cpu92>;
+					 };
+					 core1 {
+						cpu = <&cpu93>;
+					 };
+					 core2 {
+						cpu = <&cpu94>;
+					 };
+					 core3 {
+						cpu = <&cpu95>;
+					 };
+				};
+
+				cluster8 {
+					 core0 {
+						cpu = <&cpu96>;
+					 };
+					 core1 {
+						cpu = <&cpu97>;
+					 };
+					 core2 {
+						cpu = <&cpu98>;
+					 };
+					 core3 {
+						cpu = <&cpu99>;
+					 };
+				};
+
+				cluster9 {
+					 core0 {
+						cpu = <&cpu100>;
+					 };
+					 core1 {
+						cpu = <&cpu101>;
+					 };
+					 core2 {
+						cpu = <&cpu102>;
+					 };
+					 core3 {
+						cpu = <&cpu103>;
+					 };
+				};
+
+				cluster10 {
+					 core0 {
+						cpu = <&cpu112>;
+					 };
+					 core1 {
+						cpu = <&cpu113>;
+					 };
+					 core2 {
+						cpu = <&cpu114>;
+					 };
+					 core3 {
+						cpu = <&cpu115>;
+					 };
+				};
+
+				cluster11 {
+					 core0 {
+						cpu = <&cpu116>;
+					 };
+					 core1 {
+						cpu = <&cpu117>;
+					 };
+					 core2 {
+						cpu = <&cpu118>;
+					 };
+					 core3 {
+						cpu = <&cpu119>;
+					 };
+				};
+
+				cluster12 {
+					 core0 {
+						cpu = <&cpu104>;
+					 };
+					 core1 {
+						cpu = <&cpu105>;
+					 };
+					 core2 {
+						cpu = <&cpu106>;
+					 };
+					 core3 {
+						cpu = <&cpu107>;
+					 };
+				};
+
+				cluster13 {
+					 core0 {
+						cpu = <&cpu108>;
+					 };
+					 core1 {
+						cpu = <&cpu109>;
+					 };
+					 core2 {
+						cpu = <&cpu110>;
+					 };
+					 core3 {
+						cpu = <&cpu111>;
+					 };
+				};
+
+				cluster14 {
+					 core0 {
+						cpu = <&cpu120>;
+					 };
+					 core1 {
+						cpu = <&cpu121>;
+					 };
+					 core2 {
+						cpu = <&cpu122>;
+					 };
+					 core3 {
+						cpu = <&cpu123>;
+					 };
+				};
+
+				cluster15 {
+					 core0 {
+						cpu = <&cpu124>;
+					 };
+					 core1 {
+						cpu = <&cpu125>;
+					 };
+					 core2 {
+						cpu = <&cpu126>;
+					 };
+					 core3 {
+						cpu = <&cpu127>;
+					 };
+				};
+			};
+		};
+
+
+		cpu64: cpu@64 {
+			device_type = "cpu";
+			reg = <64>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu64_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu65: cpu@65 {
+			device_type = "cpu";
+			reg = <65>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu65_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu66: cpu@66 {
+			device_type = "cpu";
+			reg = <66>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu66_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu67: cpu@67 {
+			device_type = "cpu";
+			reg = <67>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu67_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu68: cpu@68 {
+			device_type = "cpu";
+			reg = <68>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu68_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu69: cpu@69 {
+			device_type = "cpu";
+			reg = <69>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu69_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu70: cpu@70 {
+			device_type = "cpu";
+			reg = <70>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu70_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu71: cpu@71 {
+			device_type = "cpu";
+			reg = <71>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu71_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu72: cpu@72 {
+			device_type = "cpu";
+			reg = <72>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu72_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu73: cpu@73 {
+			device_type = "cpu";
+			reg = <73>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu73_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu74: cpu@74 {
+			device_type = "cpu";
+			reg = <74>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu74_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu75: cpu@75 {
+			device_type = "cpu";
+			reg = <75>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu75_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu76: cpu@76 {
+			device_type = "cpu";
+			reg = <76>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu76_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu77: cpu@77 {
+			device_type = "cpu";
+			reg = <77>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu77_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu78: cpu@78 {
+			device_type = "cpu";
+			reg = <78>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu78_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu79: cpu@79 {
+			device_type = "cpu";
+			reg = <79>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu79_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu80: cpu@80 {
+			device_type = "cpu";
+			reg = <80>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu80_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu81: cpu@81 {
+			device_type = "cpu";
+			reg = <81>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu81_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu82: cpu@82 {
+			device_type = "cpu";
+			reg = <82>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu82_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu83: cpu@83 {
+			device_type = "cpu";
+			reg = <83>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu83_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu84: cpu@84 {
+			device_type = "cpu";
+			reg = <84>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu84_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu85: cpu@85 {
+			device_type = "cpu";
+			reg = <85>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu85_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu86: cpu@86 {
+			device_type = "cpu";
+			reg = <86>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu86_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu87: cpu@87 {
+			device_type = "cpu";
+			reg = <87>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <4>;
+			cpu87_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu88: cpu@88 {
+			device_type = "cpu";
+			reg = <88>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu88_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu89: cpu@89 {
+			device_type = "cpu";
+			reg = <89>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu89_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu90: cpu@90 {
+			device_type = "cpu";
+			reg = <90>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu90_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu91: cpu@91 {
+			device_type = "cpu";
+			reg = <91>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu91_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu92: cpu@92 {
+			device_type = "cpu";
+			reg = <92>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu92_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu93: cpu@93 {
+			device_type = "cpu";
+			reg = <93>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu93_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu94: cpu@94 {
+			device_type = "cpu";
+			reg = <94>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu94_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu95: cpu@95 {
+			device_type = "cpu";
+			reg = <95>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <5>;
+			cpu95_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu96: cpu@96 {
+			device_type = "cpu";
+			reg = <96>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu96_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu97: cpu@97 {
+			device_type = "cpu";
+			reg = <97>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu97_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu98: cpu@98 {
+			device_type = "cpu";
+			reg = <98>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu98_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu99: cpu@99 {
+			device_type = "cpu";
+			reg = <99>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu99_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu100: cpu@100 {
+			device_type = "cpu";
+			reg = <100>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu100_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu101: cpu@101 {
+			device_type = "cpu";
+			reg = <101>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu101_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu102: cpu@102 {
+			device_type = "cpu";
+			reg = <102>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu102_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu103: cpu@103 {
+			device_type = "cpu";
+			reg = <103>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu103_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu104: cpu@104 {
+			device_type = "cpu";
+			reg = <104>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu104_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu105: cpu@105 {
+			device_type = "cpu";
+			reg = <105>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu105_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu106: cpu@106 {
+			device_type = "cpu";
+			reg = <106>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu106_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu107: cpu@107 {
+			device_type = "cpu";
+			reg = <107>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu107_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu108: cpu@108 {
+			device_type = "cpu";
+			reg = <108>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu108_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu109: cpu@109 {
+			device_type = "cpu";
+			reg = <109>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu109_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu110: cpu@110 {
+			device_type = "cpu";
+			reg = <110>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu110_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu111: cpu@111 {
+			device_type = "cpu";
+			reg = <111>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu111_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu112: cpu@112 {
+			device_type = "cpu";
+			reg = <112>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu112_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu113: cpu@113 {
+			device_type = "cpu";
+			reg = <113>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu113_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu114: cpu@114 {
+			device_type = "cpu";
+			reg = <114>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu114_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu115: cpu@115 {
+			device_type = "cpu";
+			reg = <115>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu115_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu116: cpu@116 {
+			device_type = "cpu";
+			reg = <116>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu116_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu117: cpu@117 {
+			device_type = "cpu";
+			reg = <117>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu117_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu118: cpu@118 {
+			device_type = "cpu";
+			reg = <118>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu118_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu119: cpu@119 {
+			device_type = "cpu";
+			reg = <119>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <6>;
+			cpu119_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu120: cpu@120 {
+			device_type = "cpu";
+			reg = <120>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu120_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu121: cpu@121 {
+			device_type = "cpu";
+			reg = <121>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu121_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu122: cpu@122 {
+			device_type = "cpu";
+			reg = <122>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu122_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu123: cpu@123 {
+			device_type = "cpu";
+			reg = <123>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu123_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu124: cpu@124 {
+			device_type = "cpu";
+			reg = <124>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu124_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu125: cpu@125 {
+			device_type = "cpu";
+			reg = <125>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu125_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu126: cpu@126 {
+			device_type = "cpu";
+			reg = <126>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu126_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+		cpu127: cpu@127 {
+			device_type = "cpu";
+			reg = <127>;
+			status = "okay";
+			compatible = "riscv";
+			riscv,isa = "rv64imafdc";
+			mmu-type = "riscv,sv39";
+			numa-node-id = <7>;
+			cpu127_intc: interrupt-controller {
+				#interrupt-cells = <1>;
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+			};
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-milkv-pioneer.dts b/arch/riscv/boot/dts/sophgo/mango-milkv-pioneer.dts
new file mode 100644
index 000000000000..3e9bd7ca6793
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-milkv-pioneer.dts
@@ -0,0 +1,170 @@
+#include "mango.dtsi"
+#include "mango-pcie-4rc.dtsi"
+
+/ {
+	info {
+		file-name = "mango-milkv-pioneer.dts";
+	};
+};
+
+&i2c0 {
+	rtc: rtc@68 {
+		compatible = "dallas,ds1307";
+		reg = <0x68>;
+	};
+};
+
+&i2c1 {
+	mcu: sg2042mcu@17 {
+		compatible = "sophgo,sg20xx-mcu";
+		reg = <0x17>;
+		#thermal-sensor-cells = <1>;
+	};
+
+	mango_srst: mango-reset@17 {
+		compatible = "mango,reset";
+		reg = <0x17>;
+	};
+};
+
+&i2c2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c2_acquire>;
+};
+
+&soc {
+	/delete-node/ ethernet@7040026000;
+	gpio-poweroff {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pwr_key>;
+
+		power {
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&port0a 22 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+
+	gpio-restart {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&restart_key>;
+
+		restart {
+			label = "GPIO Key Restart";
+			linux,code = <KEY_RESTART>;
+			gpios = <&port0a 23 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+};
+
+&tach0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan0_acquire>;
+};
+
+&tach1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan1_acquire>;
+};
+
+/ {
+	pwmfan: pwm-fan {
+		compatible = "pwm-fan";
+		pwms = <&pwm 0 40000>, <&pwm 1 40000>; // period_ns
+		pwm-names = "pwm0","pwm1";
+		pwm_inuse = "pwm0";
+		#cooling-cells = <2>;
+		cooling-levels = <1 1 1 1 1>;  //total 255
+	};
+
+	thermal_zones: thermal-zones {
+		soc {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 0>;
+
+			trips {
+				soc_pwmfan_trip1: soc_pwmfan_trip@1 {
+					temperature = <30000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip2: soc_pwmfan_trip@2 {
+					temperature = <40000>; /* millicelsius */
+					hysteresis = <12000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip3: soc_pwmfan_trip@3 {
+					temperature = <50000>; /* millicelsius */
+					hysteresis = <10000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip4: soc_pwmfan_trip@4 {
+					temperature = <60000>; /* millicelsius */
+					hysteresis = <5000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map0 {
+					trip = <&soc_pwmfan_trip1>;
+					cooling-device = <&pwmfan 0 1>;
+				};
+
+				map1 {
+					trip = <&soc_pwmfan_trip2>;
+					cooling-device = <&pwmfan 1 2>;
+				};
+
+				map2 {
+					trip = <&soc_pwmfan_trip3>;
+					cooling-device = <&pwmfan 2 3>;
+				};
+
+				map3 {
+					trip = <&soc_pwmfan_trip4>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+
+		};
+
+		board {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 1>;
+
+			trips {
+				board_pwmfan_trip1: board_pwmfan_trip@1 {
+					temperature = <75000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map4 {
+					trip = <&board_pwmfan_trip1>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+		};
+	};
+
+};
+
+&chosen {
+	bootargs = "console=ttyS0,115200 console=tty1 earlycon maxcpus=1";
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-2rc.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-2rc.dtsi
new file mode 100644
index 000000000000..e39b3a80bf06
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-2rc.dtsi
@@ -0,0 +1,81 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x00 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <1>;
+		interrupt-parent = <&intc1>;
+		//interrupts = <SOC_PERIPHERAL_IRQ(123) IRQ_TYPE_LEVEL_HIGH>;
+		//interrupt-names = "msi";
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0000000  0x48 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@f060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xff>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <1>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc2>;
+		//interrupts = <SOC_PERIPHERAL_IRQ(346) IRQ_TYPE_LEVEL_HIGH>;
+		//interrupt-names = "msi";
+		reg = <0xf0 0x60000000  0x0 0x02000000>,
+		      <0xc0 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0800000  0xc0 0xc0800000  0x0 0x00800000>,
+			 <0x42000000 0x0  0xd0000000  0xc0 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0xc0 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0xc2 0x00000000  0xc2 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0xc1 0x00000000  0xc1 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-capricorn.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-capricorn.dtsi
new file mode 100644
index 000000000000..776889585272
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-capricorn.dtsi
@@ -0,0 +1,116 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x0 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x70 0x60000000  0x0 0x02000000>,
+		      <0x40 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0000000  0x40 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x40 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x40 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x42 0x00000000  0x42 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x41 0x00000000  0x41 0x00000000  0x1 0x00000000>;
+		//dma-ranges = <0x03000000 0x0 0x0 0x0 0x0 0x1f 0x0>;
+
+		status = "okay";
+	};
+
+	pcie@7060800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x40 0x7f>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <0>;
+		top-intc-id = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(122) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x44 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0400000  0x44 0xc0400000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xe0000000  0x44 0xe0000000  0x0 0x20000000>,
+			 <0x02000000 0x0  0xd0000000  0x44 0xd0000000  0x0 0x10000000>,
+			 <0x43000000 0x46 0x00000000  0x46 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x45 0x00000000  0x45 0x00000000  0x1 0x00000000>;
+		//dma-ranges = <0x03000000 0x0 0x0 0x0 0x0 0x1f 0x0>;
+
+		status = "okay";
+	};
+
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xff>;
+		linux,pci-domain = <2>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(123) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0800000  0x48 0xc0800000  0x0 0x00800000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>;
+		//dma-ranges = <0x03000000 0x0 0x0 0x0 0x0 0x1f 0x0>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-v2.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-v2.dtsi
new file mode 100644
index 000000000000..9c4c9641e1c0
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc-v2.dtsi
@@ -0,0 +1,115 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x0 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		top-intc-id = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(122) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x60000000  0x0 0x02000000>,
+		      <0x40 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0000000  0x40 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x40 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x40 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x42 0x00000000  0x42 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x41 0x00000000  0x41 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7060800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x40 0x7f>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		//interrupts = <SOC_PERIPHERAL_IRQ(122) IRQ_TYPE_LEVEL_HIGH>;
+		//interrupt-names = "msi";
+		reg = <0x44 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0400000  0x44 0xc0400000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xe0000000  0x44 0xe0000000  0x0 0x20000000>,
+			 <0x02000000 0x0  0xd0000000  0x44 0xd0000000  0x0 0x10000000>,
+			 <0x43000000 0x46 0x00000000  0x46 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x45 0x00000000  0x45 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xff>;
+		linux,pci-domain = <2>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(123) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0800000  0x48 0xc0800000  0x0 0x00800000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-3rc.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc.dtsi
new file mode 100644
index 000000000000..63fb41b43809
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-3rc.dtsi
@@ -0,0 +1,112 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x0 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(122) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x60000000  0x0 0x02000000>,
+		      <0x40 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0000000  0x40 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x40 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x40 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x42 0x00000000  0x42 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x41 0x00000000  0x41 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7060800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x40 0x7f>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x44 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0400000  0x44 0xc0400000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x44 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x44 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x46 0x00000000  0x46 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x45 0x00000000  0x45 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xff>;
+		linux,pci-domain = <2>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(123) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0800000  0x48 0xc0800000  0x0 0x00800000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>,
+			 <0x03000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-4rc-v2.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-4rc-v2.dtsi
new file mode 100644
index 000000000000..efbcc5c04740
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-4rc-v2.dtsi
@@ -0,0 +1,155 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x00 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		/*
+		 * IO, check IO_SPACE_LIMIT
+		 * 32bit prefetchable memory
+		 * 32bit non-prefetchable memory
+		 * 64bit prefetchable memory
+		 * 64bit non-prefetchable memory
+		 */
+		ranges = <0x01000000 0x0  0xc0000000  0x48 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7062800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x40 0x7f>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x4c 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		/*
+		 * IO, check IO_SPACE_LIMIT
+		 * 32bit prefetchable memory
+		 * 32bit non-prefetchable memory
+		 * 64bit prefetchable memory
+		 * 64bit non-prefetchable memory
+		 */
+		ranges = <0x01000000 0x0  0xc0000000  0x4c 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x4c 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x4c 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x4e 0x00000000  0x4e 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x4d 0x00000000  0x4d 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@f060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xbf>;
+		linux,pci-domain = <2>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <1>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc2>;
+		reg = <0xf0 0x60000000  0x0 0x02000000>,
+		      <0xc0 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		/*
+		 * IO, check IO_SPACE_LIMIT
+		 * 32bit prefetchable memory
+		 * 32bit non-prefetchable memory
+		 * 64bit prefetchable memory
+		 * 64bit non-prefetchable memory
+		 */
+		ranges = <0x01000000 0x0  0xc0000000  0xc0 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0xc0 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0xc0 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0xc2 0x00000000  0xc2 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0xc1 0x00000000  0xc1 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+	
+	pcie@f068000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0xc0 0xff>;
+		linux,pci-domain = <3>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <1>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc2>;
+		reg = <0xc4 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		/*
+		 * IO, check IO_SPACE_LIMIT
+		 * 32bit prefetchable memory
+		 * 32bit non-prefetchable memory
+		 * 64bit prefetchable memory
+		 * 64bit non-prefetchable memory
+		 */
+		ranges = <0x01000000 0x0  0xc0000000  0xc4 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0xc4 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0xc4 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0xc6 0x00000000  0xc6 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0xc5 0x00000000  0xc5 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pcie-4rc.dtsi b/arch/riscv/boot/dts/sophgo/mango-pcie-4rc.dtsi
new file mode 100644
index 000000000000..22bc466757bf
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pcie-4rc.dtsi
@@ -0,0 +1,151 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	pcie@7060000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x0 0x3f>;
+		linux,pci-domain = <0>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <1>;
+		interrupt-parent = <&intc1>;
+		//top-intc-used = <0>;
+		//interrupt-parent = <&intc>;
+		//interrupts = <SOC_PERIPHERAL_IRQ(122) IRQ_TYPE_LEVEL_HIGH>;
+		//interrupt-names = "msi";
+		reg = <0x70 0x60000000  0x0 0x02000000>,
+		      <0x40 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0000000  0x40 0xc0000000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x40 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x40 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x42 0x00000000  0x42 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x41 0x00000000  0x41 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+#if 0
+	pcie@7060800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x40 0x7f>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x0>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x44 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0400000  0x44 0xc0400000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x44 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x44 0xe0000000  0x0 0x20000000>,
+			 <0x43000000 0x46 0x00000000  0x46 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x45 0x00000000  0x45 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+#endif
+	pcie@7062000000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0x80 0xbf>;
+		linux,pci-domain = <1>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x0>;
+		top-intc-used = <0>;
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(123) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi";
+		reg = <0x70 0x62000000  0x0 0x02000000>,
+		      <0x48 0x00000000  0x0 0x00001000>;
+		reg-names = "reg", "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0800000  0x48 0xc0800000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xd0000000  0x48 0xd0000000  0x0 0x10000000>,
+			 <0x02000000 0x0  0xe0000000  0x48 0xe0000000  0x0 0x20000000>,
+			 <0x03000000 0x49 0x00000000  0x49 0x00000000  0x1 0x00000000>,
+			 <0x43000000 0x4a 0x00000000  0x4a 0x00000000  0x2 0x00000000>;
+
+		status = "okay";
+	};
+
+	pcie@7062800000 {
+		compatible = "sophgo,cdns-pcie-host";
+		device_type = "pci";
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		bus-range = <0xc0 0xff>;
+		linux,pci-domain = <2>;
+		cdns,max-outbound-regions = <16>;
+		cdns,no-bar-match-nbits = <48>;
+		vendor-id = /bits/ 16 <0x1E30>;
+		device-id = /bits/ 16 <0x2042>;
+		pcie-id = /bits/ 16 <0x1>;
+		link-id = /bits/ 16 <0x1>;
+		top-intc-used = <1>;
+		top-intc-id = <0>;
+		msix-supported = <0>;
+		interrupt-parent = <&intc1>;
+		reg = <0x4c 0x00000000  0x0 0x00001000>;
+		reg-names = "cfg";
+
+		// IO, check IO_SPACE_LIMIT
+		// 32bit prefetchable memory
+		// 32bit non-prefetchable memory
+		// 64bit prefetchable memory
+		// 64bit non-prefetchable memory
+		ranges = <0x01000000 0x0  0xc0c00000  0x4c 0xc0c00000  0x0 0x00400000>,
+			 <0x42000000 0x0  0xf8000000  0x4c 0xf8000000  0x0 0x04000000>,
+			 <0x02000000 0x0  0xfc000000  0x4c 0xfc000000  0x0 0x04000000>,
+			 <0x43000000 0x4e 0x00000000  0x4e 0x00000000  0x2 0x00000000>,
+			 <0x03000000 0x4d 0x00000000  0x4d 0x00000000  0x1 0x00000000>;
+
+		status = "okay";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-pinctrl.dtsi b/arch/riscv/boot/dts/sophgo/mango-pinctrl.dtsi
new file mode 100644
index 000000000000..f3fb2e39af26
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-pinctrl.dtsi
@@ -0,0 +1,434 @@
+/ {
+	bmpctrl: pinctrl@50010400 {
+		compatible = "sophgo, pinctrl-mango";
+		subctrl-syscon = <&top_misc>;
+		top_pinctl_offset = <0x1000>;
+
+		lpc_acquire: lpc_acquire {
+			mux {
+				groups = "lpc_grp";
+				function = "lpc_a";
+			};
+		};
+
+		lpc_release: lpc_release{
+			mux {
+				groups = "lpc_grp";
+				function = "lpc_r";
+			};
+		};
+
+		pcie_acquire: pcie_acquire {
+			mux {
+				groups = "pcie_grp";
+				function = "pcie_a";
+			};
+		};
+
+		pcie_release: pcie_release{
+			mux {
+				groups = "pcie_grp";
+				function = "pcie_r";
+			};
+		};
+
+		spif_acquire: spif_acquire {
+			mux {
+				groups = "spif_grp";
+				function = "spif_a";
+			};
+		};
+
+		spif_release: spif_release{
+			mux {
+				groups = "spif_grp";
+				function = "spif_r";
+			};
+		};
+
+		emmc_acquire: emmc_acquire {
+			mux {
+				groups = "emmc_grp";
+				function = "emmc_a";
+			};
+		};
+
+		emmc_release: emmc_release{
+			mux {
+				groups = "emmc_grp";
+				function = "emmc_r";
+			};
+		};
+
+		sdio_acquire: sdio_acquire {
+			mux {
+				groups = "sdio_grp";
+				function = "sdio_a";
+			};
+		};
+
+		sdio_release: sdio_release{
+			mux {
+				groups = "sdio_grp";
+				function = "sdio_r";
+			};
+		};
+
+		eth0_acquire: eth0_acquire {
+			mux {
+				groups = "eth0_grp";
+				function = "eth0_a";
+			};
+		};
+
+		eth0_release: eth0_release{
+			mux {
+				groups = "eth0_grp";
+				function = "eth0_r";
+			};
+		};
+
+		pwm0_acquire: pwm0_acquire {
+			mux {
+				groups = "pwm0_grp";
+				function = "pwm0_a";
+			};
+		};
+
+		pwm0_release: pwm0_release{
+			mux {
+				groups = "pwm0_grp";
+				function = "pwm0_r";
+			};
+		};
+
+		pwm1_acquire: pwm1_acquire {
+			mux {
+				groups = "pwm1_grp";
+				function = "pwm1_a";
+			};
+		};
+
+		pwm1_release: pwm1_release{
+			mux {
+				groups = "pwm1_grp";
+				function = "pwm1_r";
+			};
+		};
+
+		pwm2_acquire: pwm2_acquire {
+			mux {
+				groups = "pwm2_grp";
+				function = "pwm2_a";
+			};
+		};
+
+		pwm2_release: pwm2_release{
+			mux {
+				groups = "pwm2_grp";
+				function = "pwm2_r";
+			};
+		};
+
+		pwm3_acquire: pwm3_acquire {
+			mux {
+				groups = "pwm3_grp";
+				function = "pwm3_a";
+			};
+		};
+
+		pwm3_release: pwm3_release{
+			mux {
+				groups = "pwm3_grp";
+				function = "pwm3_r";
+			};
+		};
+
+		fan0_acquire: fan0_acquire {
+			mux {
+				groups = "fan0_grp";
+				function = "fan0_a";
+			};
+		};
+
+		fan0_release: fan0_release{
+			mux {
+				groups = "fan0_grp";
+				function = "fan0_r";
+			};
+		};
+
+		fan1_acquire: fan1_acquire {
+			mux {
+				groups = "fan1_grp";
+				function = "fan1_a";
+			};
+		};
+
+		fan1_release: fan1_release{
+			mux {
+				groups = "fan1_grp";
+				function = "fan1_r";
+			};
+		};
+
+		fan2_acquire: fan2_acquire {
+			mux {
+				groups = "fan2_grp";
+				function = "fan2_a";
+			};
+		};
+
+		fan2_release: fan2_release{
+			mux {
+				roups = "fan2_grp";
+				function = "fan2_r";
+			};
+		};
+
+		fan3_acquire: fan3_acquire {
+			mux {
+				groups = "fan3_grp";
+				function = "fan3_a";
+			};
+		};
+
+		fan3_release: fan3_release{
+			mux {
+				groups = "fan3_grp";
+				function = "fan3_r";
+			};
+		};
+
+		i2c0_acquire: i2c0_acquire {
+			mux {
+				groups = "i2c0_grp";
+				function = "i2c0_a";
+			};
+		};
+
+		i2c0_release: i2c0_release{
+			mux {
+				groups = "i2c0_grp";
+				function = "i2c0_r";
+			};
+		};
+
+		i2c1_acquire: i2c1_acquire {
+			mux {
+				groups = "i2c1_grp";
+				function = "i2c1_a";
+			};
+		};
+
+		i2c1_release: i2c1_release{
+			mux {
+				groups = "i2c1_grp";
+				function = "i2c1_r";
+			};
+		};
+
+		i2c2_acquire: i2c2_acquire {
+			mux {
+				groups = "i2c2_grp";
+				function = "i2c2_a";
+			};
+		};
+
+		i2c2_release: i2c2_release{
+			mux {
+				groups = "i2c2_grp";
+				function = "i2c2_r";
+			};
+		};
+
+		i2c3_acquire: i2c3_acquire {
+			mux {
+				groups = "i2c3_grp";
+				function = "i2c3_a";
+			};
+		};
+
+		i2c3_release: i2c3_release{
+			mux {
+				groups = "i2c3_grp";
+				function = "i2c3_r";
+			};
+		};
+
+		uart0_acquire: uart0_acquire {
+			mux {
+				groups = "uart0_grp";
+				function = "uart0_a";
+			};
+		};
+
+		uart0_release: uart0_release{
+			mux {
+				groups = "uart0_grp";
+				function = "uart0_r";
+			};
+		};
+
+		uart1_acquire: uart1_acquire {
+			mux {
+				groups = "uart1_grp";
+				function = "uart1_a";
+			};
+		};
+
+		uart1_release: uart1_release{
+			mux {
+				groups = "uart1_grp";
+				function = "uart1_r";
+			};
+		};
+
+		uart2_acquire: uart2_acquire {
+			mux {
+				groups = "uart2_grp";
+				function = "uart2_a";
+			};
+		};
+
+		uart2_release: uart2_release{
+			mux {
+				groups = "uart2_grp";
+				function = "uart2_r";
+			};
+		};
+
+		uart3_acquire: uart3_acquire {
+			mux {
+				groups = "uart3_grp";
+				function = "uart3_a";
+			};
+		};
+
+		uart3_release: uart3_release{
+			mux {
+				groups = "uart3_grp";
+				function = "uart3_r";
+			};
+		};
+
+		spi0_acquire: spi0_acquire {
+			mux {
+				groups = "spi0_grp";
+				function = "spi0_a";
+			};
+		};
+
+		spi0_release: spi0_release{
+			mux {
+				groups = "spi0_grp";
+				function = "spi0_r";
+			};
+		};
+
+		spi1_acquire: spi1_acquire {
+			mux {
+				groups = "spi1_grp";
+				function = "spi1_a";
+			};
+		};
+
+		spi1_release: spi1_release{
+			mux {
+				groups = "spi1_grp";
+				function = "spi1_r";
+			};
+		};
+
+		jtag0_acquire: jtag0_acquire {
+			mux {
+				groups = "jtag0_grp";
+				function = "jtag0_a";
+			};
+		};
+
+		jtag0_release: jtag0_release{
+			mux {
+				groups = "jtag0_grp";
+				function = "jtag0_r";
+			};
+		};
+
+		jtag1_acquire: jtag1_acquire {
+			mux {
+				groups = "jtag1_grp";
+				function = "jtag1_a";
+			};
+		};
+
+		jtag1_release: jtag1_release{
+			mux {
+				groups = "jtag1_grp";
+				function = "jtag1_r";
+			};
+		};
+
+		jtag2_acquire: jtag2_acquire {
+			mux {
+				groups = "jtag2_grp";
+				function = "jtag2_a";
+			};
+		};
+
+		jtag2_release: jtag2_release{
+			mux {
+				groups = "jtag2_grp";
+				function = "jtag2_r";
+			};
+		};
+
+		gpio2_acquire: gpio2_acquire {
+			mux {
+				pins = <127>;
+				function = "gpio0_a";
+			};
+		};
+
+		gpio3_release: gpio3_release {
+			mux {
+				pins = <128>;
+				function = "gpio0_r";
+			};
+		};
+
+		gpio5_release: gpio5_release {
+			mux {
+				pins = <130>;
+				function = "gpio0_r";
+			};
+		};
+
+		pwr_key: pwr-key {
+			mux {
+				pins = <147>;
+				function = "gpio0_a";
+			};
+		};
+
+		restart_key: restart-key {
+			mux {
+				pins = <148>;
+				function = "gpio0_a";
+			};
+		};
+
+		dbgi2c_acquire: dbgi2c_acquire {
+			mux {
+				groups = "dbgi2c_grp";
+				function = "dbgi2c_a";
+			};
+		};
+
+		dbgi2c_release: dbgi2c_release{
+			mux {
+				groups = "dbgi2c_grp";
+				function = "dbgi2c_r";
+			};
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-sophgo-capricorn.dts b/arch/riscv/boot/dts/sophgo/mango-sophgo-capricorn.dts
new file mode 100644
index 000000000000..94892b74467f
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-sophgo-capricorn.dts
@@ -0,0 +1,57 @@
+#include "mango.dtsi"
+#include "mango-pcie-3rc-capricorn.dtsi"
+
+/ {
+	info {
+		file-name = "mango-sophgo-capricorn.dts";
+	};
+};
+
+&ethernet0 {
+	max-speed = <1000>;
+	eth-sophgo-config {
+		autoneg = "enable";
+	};
+};
+
+&soc {
+	gpio-poweroff {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gpio2_acquire>;
+
+		power {
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&port0a 2 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+};
+
+&port0a {
+	compatible = "snps,dw-apb-gpio-port", "sophgo,gpio0";
+
+	cpld_poweroff: cpld-poweroff {
+		compatible = "mango,cpld-poweroff";
+		gpios = <&port0a 3 GPIO_ACTIVE_HIGH>;
+	};
+
+	cpld_reboot: cpld-reboot {
+		compatible = "mango,cpld-reboot";
+		gpios = <&port0a 5 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+/ {
+	 board-info {
+		/* compatible MUST be sophgo,board-info */
+		compatible = "sophgo,board-info";
+		/* valid values are: full-function, xmr */
+		chip-package = "full-function";
+		/* valid values are: x4, x8 */
+		ddr-pcb-type = "x4";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-sophgo-pisces.dts b/arch/riscv/boot/dts/sophgo/mango-sophgo-pisces.dts
new file mode 100644
index 000000000000..98761cbf42e8
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-sophgo-pisces.dts
@@ -0,0 +1,58 @@
+#include "mango-2sockets.dtsi"
+#include "mango-top-intc2.dtsi"
+#include "mango-pcie-2rc.dtsi"
+
+/ {
+	info {
+		file-name = "mango-sophgo-pisces.dts";
+	};
+};
+
+&ethernet0 {
+	max-speed = <1000>;
+	eth-sophgo-config {
+		autoneg = "enable";
+	};
+};
+
+&soc {
+	gpio-poweroff {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gpio2_acquire>;
+
+		power {
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&port0a 2 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+};
+
+&port0a {
+	compatible = "snps,dw-apb-gpio-port", "sophgo,gpio0";
+
+	cpld_poweroff: cpld-poweroff {
+		compatible = "mango,cpld-poweroff";
+		gpios = <&port0a 3 GPIO_ACTIVE_HIGH>;
+	};
+
+	cpld_reboot: cpld-reboot {
+		compatible = "mango,cpld-reboot";
+		gpios = <&port0a 5 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+/ {
+	 board-info {
+		/* compatible MUST be sophgo,board-info */
+		compatible = "sophgo,board-info";
+		/* valid values are: full-function, xmr */
+		chip-package = "full-function";
+		/* valid values are: x4, x8 */
+		ddr-pcb-type = "x4";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-sophgo-x4evb.dts b/arch/riscv/boot/dts/sophgo/mango-sophgo-x4evb.dts
new file mode 100644
index 000000000000..3fe655eaf69a
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-sophgo-x4evb.dts
@@ -0,0 +1,144 @@
+#include "mango.dtsi"
+#include "mango-pcie-3rc-v2.dtsi"
+
+/ {
+	info {
+		file-name = "mango-sophgo-x4evb.dts";
+	};
+};
+
+&i2c0 {
+	rtc: rtc@68 {
+		compatible = "dallas,ds1307";
+		reg = <0x68>;
+	};
+};
+
+&i2c1 {
+	mcu: sg2042mcu@17 {
+		compatible = "sophgo,sg20xx-mcu";
+		reg = <0x17>;
+		#thermal-sensor-cells = <1>;
+	};
+
+	mango_srst: mango-reset@17 {
+		compatible = "mango,reset";
+		reg = <0x17>;
+	};
+};
+
+&i2c2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c2_acquire>;
+};
+
+&tach0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan0_acquire>;
+};
+
+&tach1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan1_acquire>;
+};
+
+&ethernet0 {
+	max-speed = <1000>;
+	eth-sophgo-config {
+		autoneg = "enable";
+	};
+};
+
+&soc {
+	/delete-node/ flash-controller@7000180000;
+};
+
+/ {
+	pwmfan: pwm-fan {
+		compatible = "pwm-fan";
+		pwms = <&pwm 0 40000>, <&pwm 1 40000>; // period_ns
+		pwm-names = "pwm0","pwm1";
+		pwm_inuse = "pwm0";
+		#cooling-cells = <2>;
+		cooling-levels = <102 127 178 229 254>;  //total 255
+	};
+
+	thermal_zones: thermal-zones {
+		soc {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 0>;
+
+			trips {
+				soc_pwmfan_trip1: soc_pwmfan_trip@1 {
+					temperature = <40000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip2: soc_pwmfan_trip@2 {
+					temperature = <58000>; /* millicelsius */
+					hysteresis = <12000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip3: soc_pwmfan_trip@3 {
+					temperature = <70000>; /* millicelsius */
+					hysteresis = <10000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip4: soc_pwmfan_trip@4 {
+					temperature = <85000>; /* millicelsius */
+					hysteresis = <5000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map0 {
+					trip = <&soc_pwmfan_trip1>;
+					cooling-device = <&pwmfan 0 1>;
+				};
+
+				map1 {
+					trip = <&soc_pwmfan_trip2>;
+					cooling-device = <&pwmfan 1 2>;
+				};
+
+				map2 {
+					trip = <&soc_pwmfan_trip3>;
+					cooling-device = <&pwmfan 2 3>;
+				};
+
+				map3 {
+					trip = <&soc_pwmfan_trip4>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+
+		};
+
+		board {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 1>;
+
+			trips {
+				board_pwmfan_trip1: board_pwmfan_trip@1 {
+					temperature = <75000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map4 {
+					trip = <&board_pwmfan_trip1>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+		};
+	};
+
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-sophgo-x8evb.dts b/arch/riscv/boot/dts/sophgo/mango-sophgo-x8evb.dts
new file mode 100644
index 000000000000..9e0cf5348051
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-sophgo-x8evb.dts
@@ -0,0 +1,172 @@
+#include "mango.dtsi"
+#include "mango-pcie-3rc.dtsi"
+
+/ {
+	info {
+		file-name = "mango-sophgo-x8evb.dts";
+	};
+};
+
+&i2c0 {
+	rtc: rtc@68 {
+		compatible = "dallas,ds1307";
+		reg = <0x68>;
+	};
+};
+
+&i2c1 {
+	mcu: sg2042mcu@17 {
+		compatible = "sophgo,sg20xx-mcu";
+		reg = <0x17>;
+		#thermal-sensor-cells = <1>;
+	};
+
+	mango_srst: mango-reset@17 {
+		compatible = "mango,reset";
+		reg = <0x17>;
+	};
+};
+
+&i2c2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c2_acquire>;
+};
+
+&soc {
+	gpio-poweroff {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pwr_key>;
+
+		power {
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&port0a 22 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+
+	gpio-restart {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&restart_key>;
+
+		restart {
+			label = "GPIO Key Restart";
+			linux,code = <KEY_RESTART>;
+			gpios = <&port0a 23 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+};
+
+&tach0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan0_acquire>;
+};
+
+&tach1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&fan1_acquire>;
+};
+
+&ethernet0 {
+	max-speed = <1000>;
+	eth-sophgo-config {
+		autoneg = "enable";
+	};
+};
+
+/ {
+	pwmfan: pwm-fan {
+		compatible = "pwm-fan";
+		pwms = <&pwm 0 40000>, <&pwm 1 40000>; // period_ns
+		pwm-names = "pwm0","pwm1";
+		pwm_inuse = "pwm0";
+		#cooling-cells = <2>;
+		cooling-levels = <153 128 77 26 1>;  //total 255
+	};
+
+	thermal_zones: thermal-zones {
+		soc {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 0>;
+
+			trips {
+				soc_pwmfan_trip1: soc_pwmfan_trip@1 {
+					temperature = <40000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip2: soc_pwmfan_trip@2 {
+					temperature = <58000>; /* millicelsius */
+					hysteresis = <12000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip3: soc_pwmfan_trip@3 {
+					temperature = <70000>; /* millicelsius */
+					hysteresis = <10000>; /* millicelsius */
+					type = "active";
+				};
+
+				soc_pwmfan_trip4: soc_pwmfan_trip@4 {
+					temperature = <85000>; /* millicelsius */
+					hysteresis = <5000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map0 {
+					trip = <&soc_pwmfan_trip1>;
+					cooling-device = <&pwmfan 0 1>;
+				};
+
+				map1 {
+					trip = <&soc_pwmfan_trip2>;
+					cooling-device = <&pwmfan 1 2>;
+				};
+
+				map2 {
+					trip = <&soc_pwmfan_trip3>;
+					cooling-device = <&pwmfan 2 3>;
+				};
+
+				map3 {
+					trip = <&soc_pwmfan_trip4>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+
+		};
+
+		board {
+			polling-delay-passive = <1000>; /* milliseconds */
+			polling-delay = <1000>; /* milliseconds */
+			thermal-sensors = <&mcu 1>;
+
+			trips {
+				board_pwmfan_trip1: board_pwmfan_trip@1 {
+					temperature = <75000>; /* millicelsius */
+					hysteresis = <8000>; /* millicelsius */
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map4 {
+					trip = <&board_pwmfan_trip1>;
+					cooling-device = <&pwmfan 3 4>;
+				};
+			};
+		};
+	};
+
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-top-intc2.dtsi b/arch/riscv/boot/dts/sophgo/mango-top-intc2.dtsi
new file mode 100644
index 000000000000..6d364cf6b3c5
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-top-intc2.dtsi
@@ -0,0 +1,62 @@
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	intc2: top_intc@f030010300 {
+		compatible = "sophgo,top-intc";
+		reg = <0xf0 0x300102E0 0x0 0x4>,
+		      <0xf0 0x30010300 0x0 0x4>,
+		      <0xf0 0x30010304 0x0 0x4>;
+		reg-names = "sta", "set", "clr";
+		reg-bitwidth = <32>;
+		top-intc-id = <1>;
+		interrupt-controller;
+		#interrupt-cells = <0x1>; // only applies to child node
+		for-msi;
+
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(288) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(289) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(290) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(291) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(292) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(293) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(294) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(295) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(296) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(297) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(298) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(299) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(300) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(301) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(302) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(303) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(304) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(305) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(306) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(307) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(308) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(309) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(310) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(311) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(312) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(313) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(314) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(315) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(316) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(317) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(318) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(319) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi0",  "msi1",  "msi2",  "msi3",
+				  "msi4",  "msi5",  "msi6",  "msi7",
+				  "msi8",  "msi9",  "msi10", "msi11",
+				  "msi12", "msi13", "msi14", "msi15",
+				  "msi16", "msi17", "msi18", "msi19",
+				  "msi20", "msi21", "msi22", "msi23",
+				  "msi24", "msi25", "msi26", "msi27",
+				  "msi28", "msi29", "msi30", "msi31";
+
+	};
+
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango-yixin-s2110.dts b/arch/riscv/boot/dts/sophgo/mango-yixin-s2110.dts
new file mode 100644
index 000000000000..172421ffc196
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango-yixin-s2110.dts
@@ -0,0 +1,63 @@
+#include "mango-2sockets.dtsi"
+#include "mango-top-intc2.dtsi"
+#include "mango-pcie-4rc-v2.dtsi"
+
+/ {
+	info {
+		file-name = "mango-yixin-s2110.dts";
+	};
+};
+
+&ethernet0 {
+	max-speed = <1000>;
+	eth-sophgo-config {
+		autoneg = "enable";
+	};
+};
+
+&soc {
+	gpio-poweroff {
+		compatible = "gpio-keys";
+		input-name = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gpio2_acquire>;
+
+		power {
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&port0a 2 GPIO_ACTIVE_HIGH>;
+			linux,input-type = <1>;
+			debounce-interval = <100>;
+		};
+	};
+};
+
+&gpio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&dbgi2c_release>;
+};
+
+&port0a {
+	compatible = "snps,dw-apb-gpio-port", "sophgo,gpio0";
+
+	cpld_poweroff: cpld-poweroff {
+		compatible = "mango,cpld-poweroff";
+		gpios = <&port0a 3 GPIO_ACTIVE_HIGH>;
+	};
+
+	cpld_reboot: cpld-reboot {
+		compatible = "mango,cpld-reboot";
+		gpios = <&port0a 29 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+/ {
+	 board-info {
+		/* compatible MUST be sophgo,board-info */
+		compatible = "sophgo,board-info";
+		/* valid values are: full-function, xmr */
+		chip-package = "full-function";
+		/* valid values are: x4, x8 */
+		ddr-pcb-type = "x8";
+	};
+};
diff --git a/arch/riscv/boot/dts/sophgo/mango.dtsi b/arch/riscv/boot/dts/sophgo/mango.dtsi
new file mode 100644
index 000000000000..57f304fc778f
--- /dev/null
+++ b/arch/riscv/boot/dts/sophgo/mango.dtsi
@@ -0,0 +1,938 @@
+/dts-v1/;
+#include <dt-bindings/clock/sophgo.h>
+#include <dt-bindings/clock/sophgo-mango-clock.h>
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/reset/sophgo-mango-resets.h>
+#include <dt-bindings/interrupt-controller/irq.h>
+
+#include "mango-cpus-socket0.dtsi"
+#include "mango-clock-socket0.dtsi"
+#include "mango-pinctrl.dtsi"
+
+#define SOC_PERIPHERAL_IRQ(nr)	(nr)
+
+/ {
+	model = "Sophgo Mango";
+	compatible = "sophgo,mango";
+	#address-cells = <2>;
+	#size-cells = <2>;
+	dma-noncoherent;
+
+	distance-map {
+		compatible = "numa-distance-map-v1";
+		distance-matrix = <0 0 10>,
+				  <0 1 15>,
+				  <0 2 25>,
+				  <0 3 30>,
+				  <1 0 15>,
+				  <1 1 10>,
+				  <1 2 30>,
+				  <1 3 25>,
+				  <2 0 25>,
+				  <2 1 30>,
+				  <2 2 10>,
+				  <2 3 15>,
+				  <3 0 30>,
+				  <3 1 25>,
+				  <3 2 15>,
+				  <3 3 10>;
+	};
+
+	pmu {
+		compatible = "riscv,pmu";
+		riscv,event-to-mhpmevent =
+			<0x00003 0x00000000 0x00000010>,
+			<0x00004 0x00000000 0x00000011>,
+			<0x00005 0x00000000 0x00000007>,
+			<0x00006 0x00000000 0x00000006>,
+			<0x00008 0x00000000 0x00000027>,
+			<0x00009 0x00000000 0x00000028>,
+			<0x10000 0x00000000 0x0000000c>,
+			<0x10001 0x00000000 0x0000000d>,
+			<0x10002 0x00000000 0x0000000e>,
+			<0x10003 0x00000000 0x0000000f>,
+			<0x10008 0x00000000 0x00000001>,
+			<0x10009 0x00000000 0x00000002>,
+			<0x10010 0x00000000 0x00000010>,
+			<0x10011 0x00000000 0x00000011>,
+			<0x10012 0x00000000 0x00000012>,
+			<0x10013 0x00000000 0x00000013>,
+			<0x10019 0x00000000 0x00000004>,
+			<0x10021 0x00000000 0x00000003>,
+			<0x10030 0x00000000 0x0000001c>,
+			<0x10031 0x00000000 0x0000001b>;
+		riscv,event-to-mhpmcounters =
+			<0x00003 0x00003 0xfffffff8>,
+			<0x00004 0x00004 0xfffffff8>,
+			<0x00005 0x00005 0xfffffff8>,
+			<0x00006 0x00006 0xfffffff8>,
+			<0x00007 0x00007 0xfffffff8>,
+			<0x00008 0x00008 0xfffffff8>,
+			<0x00009 0x00009 0xfffffff8>,
+			<0x0000a 0x0000a 0xfffffff8>,
+			<0x10000 0x10000 0xfffffff8>,
+			<0x10001 0x10001 0xfffffff8>,
+			<0x10002 0x10002 0xfffffff8>,
+			<0x10003 0x10003 0xfffffff8>,
+			<0x10008 0x10008 0xfffffff8>,
+			<0x10009 0x10009 0xfffffff8>,
+			<0x10010 0x10010 0xfffffff8>,
+			<0x10011 0x10011 0xfffffff8>,
+			<0x10012 0x10012 0xfffffff8>,
+			<0x10013 0x10013 0xfffffff8>,
+			<0x10019 0x10019 0xfffffff8>,
+			<0x10021 0x10021 0xfffffff8>,
+			<0x10030 0x10030 0xfffffff8>,
+			<0x10031 0x10031 0xfffffff8>;
+		riscv,raw-event-to-mhpmcounters =
+			<0x00000000 0x00000001 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000002 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000003 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000004 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000005 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000006 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000007 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000008 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000009 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000a 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000b 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000c 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000d 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000e 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000000f 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000010 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000011 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000012 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000013 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000014 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000015 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000016 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000017 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000018 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000019 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001a 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001b 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001c 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001d 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001e 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000001f 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000020 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000021 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000022 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000023 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000024 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000025 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000026 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000027 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000028 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x00000029 0xffffffff 0xffffffff 0xfffffff8>,
+			<0x00000000 0x0000002a 0xffffffff 0xffffffff 0xfffffff8>;
+	};
+
+	soc: soc {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		compatible = "simple-bus";
+		ranges;
+		dma-ranges = <0x0 0x0 0x0 0x0 0x1f 0x0>;
+
+		clint_mswi: clint-mswi@7094000000 {
+			compatible = "thead,c900-clint-mswi";
+			reg = <0x00000070 0x94000000 0x00000000 0x00004000>;
+			interrupts-extended = <
+				&cpu0_intc 3
+				&cpu1_intc 3
+				&cpu2_intc 3
+				&cpu3_intc 3
+				&cpu4_intc 3
+				&cpu5_intc 3
+				&cpu6_intc 3
+				&cpu7_intc 3
+				&cpu8_intc 3
+				&cpu9_intc 3
+				&cpu10_intc 3
+				&cpu11_intc 3
+				&cpu12_intc 3
+				&cpu13_intc 3
+				&cpu14_intc 3
+				&cpu15_intc 3
+				&cpu16_intc 3
+				&cpu17_intc 3
+				&cpu18_intc 3
+				&cpu19_intc 3
+				&cpu20_intc 3
+				&cpu21_intc 3
+				&cpu22_intc 3
+				&cpu23_intc 3
+				&cpu24_intc 3
+				&cpu25_intc 3
+				&cpu26_intc 3
+				&cpu27_intc 3
+				&cpu28_intc 3
+				&cpu29_intc 3
+				&cpu30_intc 3
+				&cpu31_intc 3
+				&cpu32_intc 3
+				&cpu33_intc 3
+				&cpu34_intc 3
+				&cpu35_intc 3
+				&cpu36_intc 3
+				&cpu37_intc 3
+				&cpu38_intc 3
+				&cpu39_intc 3
+				&cpu40_intc 3
+				&cpu41_intc 3
+				&cpu42_intc 3
+				&cpu43_intc 3
+				&cpu44_intc 3
+				&cpu45_intc 3
+				&cpu46_intc 3
+				&cpu47_intc 3
+				&cpu48_intc 3
+				&cpu49_intc 3
+				&cpu50_intc 3
+				&cpu51_intc 3
+				&cpu52_intc 3
+				&cpu53_intc 3
+				&cpu54_intc 3
+				&cpu55_intc 3
+				&cpu56_intc 3
+				&cpu57_intc 3
+				&cpu58_intc 3
+				&cpu59_intc 3
+				&cpu60_intc 3
+				&cpu61_intc 3
+				&cpu62_intc 3
+				&cpu63_intc 3
+				>;
+		};
+
+		clint_mtimer0: clint-mtimer@70ac000000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac000000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu0_intc 7
+				&cpu1_intc 7
+				&cpu2_intc 7
+				&cpu3_intc 7
+				>;
+		};
+
+		clint_mtimer1: clint-mtimer@70ac010000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac010000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu4_intc 7
+				&cpu5_intc 7
+				&cpu6_intc 7
+				&cpu7_intc 7
+				>;
+		};
+
+		clint_mtimer2: clint-mtimer@70ac020000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac020000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu8_intc 7
+				&cpu9_intc 7
+				&cpu10_intc 7
+				&cpu11_intc 7
+				>;
+		};
+
+		clint_mtimer3: clint-mtimer@70ac030000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac030000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu12_intc 7
+				&cpu13_intc 7
+				&cpu14_intc 7
+				&cpu15_intc 7
+				>;
+		};
+
+		clint_mtimer4: clint-mtimer@70ac040000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac040000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu16_intc 7
+				&cpu17_intc 7
+				&cpu18_intc 7
+				&cpu19_intc 7
+				>;
+		};
+
+		clint_mtimer5: clint-mtimer@70ac050000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac050000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu20_intc 7
+				&cpu21_intc 7
+				&cpu22_intc 7
+				&cpu23_intc 7
+				>;
+		};
+
+		clint_mtimer6: clint-mtimer@70ac060000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac060000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu24_intc 7
+				&cpu25_intc 7
+				&cpu26_intc 7
+				&cpu27_intc 7
+				>;
+		};
+
+		clint_mtimer7: clint-mtimer@70ac070000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac070000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu28_intc 7
+				&cpu29_intc 7
+				&cpu30_intc 7
+				&cpu31_intc 7
+				>;
+		};
+
+		clint_mtimer8: clint-mtimer@70ac080000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac080000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu32_intc 7
+				&cpu33_intc 7
+				&cpu34_intc 7
+				&cpu35_intc 7
+				>;
+		};
+
+		clint_mtimer9: clint-mtimer@70ac090000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac090000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu36_intc 7
+				&cpu37_intc 7
+				&cpu38_intc 7
+				&cpu39_intc 7
+				>;
+		};
+
+		clint_mtimer10: clint-mtimer@70ac0a0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0a0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu40_intc 7
+				&cpu41_intc 7
+				&cpu42_intc 7
+				&cpu43_intc 7
+				>;
+		};
+
+		clint_mtimer11: clint-mtimer@70ac0b0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0b0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu44_intc 7
+				&cpu45_intc 7
+				&cpu46_intc 7
+				&cpu47_intc 7
+				>;
+		};
+
+		clint_mtimer12: clint-mtimer@70ac0c0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0c0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu48_intc 7
+				&cpu49_intc 7
+				&cpu50_intc 7
+				&cpu51_intc 7
+				>;
+		};
+
+		clint_mtimer13: clint-mtimer@70ac0d0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0d0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu52_intc 7
+				&cpu53_intc 7
+				&cpu54_intc 7
+				&cpu55_intc 7
+				>;
+		};
+
+		clint_mtimer14: clint-mtimer@70ac0e0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0e0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu56_intc 7
+				&cpu57_intc 7
+				&cpu58_intc 7
+				&cpu59_intc 7
+				>;
+		};
+
+		clint_mtimer15: clint-mtimer@70ac0f0000 {
+			compatible = "thead,c900-clint-mtimer";
+			reg = <0x00000070 0xac0f0000 0x00000000 0x00007ff8>;
+			interrupts-extended = <
+				&cpu60_intc 7
+				&cpu61_intc 7
+				&cpu62_intc 7
+				&cpu63_intc 7
+				>;
+		};
+
+		intc: interrupt-controller@7090000000 {
+			#address-cells = <0>;
+			#interrupt-cells = <2>;
+			compatible = "thead,c900-plic";
+			interrupt-controller;
+			interrupts-extended = <
+				&cpu0_intc  11 &cpu0_intc  9
+				&cpu1_intc  11 &cpu1_intc  9
+				&cpu2_intc  11 &cpu2_intc  9
+				&cpu3_intc  11 &cpu3_intc  9
+				&cpu4_intc  11 &cpu4_intc  9
+				&cpu5_intc  11 &cpu5_intc  9
+				&cpu6_intc  11 &cpu6_intc  9
+				&cpu7_intc  11 &cpu7_intc  9
+				&cpu8_intc  11 &cpu8_intc  9
+				&cpu9_intc  11 &cpu9_intc  9
+				&cpu10_intc  11 &cpu10_intc  9
+				&cpu11_intc  11 &cpu11_intc  9
+				&cpu12_intc  11 &cpu12_intc  9
+				&cpu13_intc  11 &cpu13_intc  9
+				&cpu14_intc  11 &cpu14_intc  9
+				&cpu15_intc  11 &cpu15_intc  9
+				&cpu16_intc  11 &cpu16_intc  9
+				&cpu17_intc  11 &cpu17_intc  9
+				&cpu18_intc  11 &cpu18_intc  9
+				&cpu19_intc  11 &cpu19_intc  9
+				&cpu20_intc  11 &cpu20_intc  9
+				&cpu21_intc  11 &cpu21_intc  9
+				&cpu22_intc  11 &cpu22_intc  9
+				&cpu23_intc  11 &cpu23_intc  9
+				&cpu24_intc  11 &cpu24_intc  9
+				&cpu25_intc  11 &cpu25_intc  9
+				&cpu26_intc  11 &cpu26_intc  9
+				&cpu27_intc  11 &cpu27_intc  9
+				&cpu28_intc  11 &cpu28_intc  9
+				&cpu29_intc  11 &cpu29_intc  9
+				&cpu30_intc  11 &cpu30_intc  9
+				&cpu31_intc  11 &cpu31_intc  9
+				&cpu32_intc  11 &cpu32_intc  9
+				&cpu33_intc  11 &cpu33_intc  9
+				&cpu34_intc  11 &cpu34_intc  9
+				&cpu35_intc  11 &cpu35_intc  9
+				&cpu36_intc  11 &cpu36_intc  9
+				&cpu37_intc  11 &cpu37_intc  9
+				&cpu38_intc  11 &cpu38_intc  9
+				&cpu39_intc  11 &cpu39_intc  9
+				&cpu40_intc  11 &cpu40_intc  9
+				&cpu41_intc  11 &cpu41_intc  9
+				&cpu42_intc  11 &cpu42_intc  9
+				&cpu43_intc  11 &cpu43_intc  9
+				&cpu44_intc  11 &cpu44_intc  9
+				&cpu45_intc  11 &cpu45_intc  9
+				&cpu46_intc  11 &cpu46_intc  9
+				&cpu47_intc  11 &cpu47_intc  9
+				&cpu48_intc  11 &cpu48_intc  9
+				&cpu49_intc  11 &cpu49_intc  9
+				&cpu50_intc  11 &cpu50_intc  9
+				&cpu51_intc  11 &cpu51_intc  9
+				&cpu52_intc  11 &cpu52_intc  9
+				&cpu53_intc  11 &cpu53_intc  9
+				&cpu54_intc  11 &cpu54_intc  9
+				&cpu55_intc  11 &cpu55_intc  9
+				&cpu56_intc  11 &cpu56_intc  9
+				&cpu57_intc  11 &cpu57_intc  9
+				&cpu58_intc  11 &cpu58_intc  9
+				&cpu59_intc  11 &cpu59_intc  9
+				&cpu60_intc  11 &cpu60_intc  9
+				&cpu61_intc  11 &cpu61_intc  9
+				&cpu62_intc  11 &cpu62_intc  9
+				&cpu63_intc  11 &cpu63_intc  9
+				>;
+			reg = <0x00000070 0x90000000 0x00000000 0x04000000>;
+			reg-names = "control";
+			riscv,max-priority = <7>;
+			riscv,ndev = <224>;
+		};
+
+		timer0: dw-apb-timer0@7030003000 {
+			compatible = "snps,dw-apb-timer";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(100) IRQ_TYPE_LEVEL_HIGH>;
+			reg = <0x70 0x30003000 0x0 0x14>;
+			clocks = <&div_clk GATE_CLK_TIMER1>,
+				 <&div_clk GATE_CLK_APB_TIMER>;
+			clock-names = "timer", "pclk";
+			clk-drv-rating = <300>;
+		};
+
+		timer1: dw-apb-timer1@7030003014 {
+			compatible = "snps,dw-apb-timer";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(100) IRQ_TYPE_LEVEL_HIGH>;
+			reg = <0x70 0x30003014 0x0 0x10>;
+			clocks = <&div_clk GATE_CLK_TIMER2>,
+				 <&div_clk GATE_CLK_APB_TIMER>;
+			clock-names = "timer", "pclk";
+			clk-drv-rating = <300>;
+		};
+
+		top_misc: top_misc_ctrl@7030010000 {
+			compatible = "syscon";
+			reg = <0x70 0x30010000 0x0 0x8000>;
+		};
+
+		rst: reset-controller {
+			#reset-cells = <1>;
+			compatible = "bitmain,reset";
+			subctrl-syscon = <&top_misc>;
+			top_rst_offset = <0x3000>;
+			nr_resets = <RST_MAX_NUM>;
+		};
+
+		i2c0: i2c@7030005000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "snps,designware-i2c";
+			clocks = <&div_clk GATE_CLK_APB_I2C>;
+			clock-names = "clk_gate_apb_i2c";
+			reg = <0x70 0x30005000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(101) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000>;
+			resets = <&rst RST_I2C0>;
+			reset-names = "i2c0";
+		};
+
+		i2c1: i2c@7030006000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "snps,designware-i2c";
+			clocks = <&div_clk GATE_CLK_APB_I2C>;
+			clock-names = "clk_gate_apb_i2c";
+			reg = <0x70 0x30006000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(102) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000>;
+			resets = <&rst RST_I2C1>;
+			reset-names = "i2c1";
+		};
+
+		i2c2: i2c@7030007000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "snps,designware-i2c";
+			clocks = <&div_clk GATE_CLK_APB_I2C>;
+			clock-names = "clk_gate_apb_i2c";
+			reg = <0x70 0x30007000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(103) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000>;
+			resets = <&rst RST_I2C2>;
+			reset-names = "i2c2";
+		};
+
+		i2c3: i2c@7030008000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "snps,designware-i2c";
+			clocks = <&div_clk GATE_CLK_APB_I2C>;
+			clock-names = "clk_gate_apb_i2c";
+			reg = <0x70 0x30008000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(104) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000>;
+			resets = <&rst RST_I2C3>;
+			reset-names = "i2c3";
+		};
+
+		gpio0: gpio@7030009000 {
+			compatible = "snps,dw-apb-gpio";
+			reg = <0x70 0x30009000 0x0 0x400>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			clocks = <&div_clk GATE_CLK_APB_GPIO>,
+				 <&div_clk GATE_CLK_GPIO_DB>;
+			clock-names = "bus", "db";
+
+			port0a: gpio-controller@0 {
+				compatible = "snps,dw-apb-gpio-port";
+				bank-name = "port0a";
+				gpio-controller;
+				#gpio-cells = <2>;
+				snps,nr-gpios = <32>;
+				reg = <0>;
+				interrupt-controller;
+				#interrupt-cells = <2>;
+				interrupt-parent = <&intc>;
+				interrupts = <SOC_PERIPHERAL_IRQ(96) IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		gpio1: gpio@703000a000 {
+			compatible = "snps,dw-apb-gpio";
+			reg = <0x70 0x3000a000 0x0 0x400>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			clocks = <&div_clk GATE_CLK_APB_GPIO>,
+				 <&div_clk GATE_CLK_GPIO_DB>;
+			clock-names = "bus", "db";
+
+			port1a: gpio-controller@0 {
+				compatible = "snps,dw-apb-gpio-port";
+				bank-name = "port0a";
+				gpio-controller;
+				#gpio-cells = <2>;
+				snps,nr-gpios = <32>;
+				reg = <0>;
+				interrupt-controller;
+				#interrupt-cells = <2>;
+				interrupt-parent = <&intc>;
+				interrupts = <SOC_PERIPHERAL_IRQ(97) IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		gpio2: gpio@703000b000 {
+			compatible = "snps,dw-apb-gpio";
+			reg = <0x70 0x3000b000 0x0 0x400>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			clocks = <&div_clk GATE_CLK_APB_GPIO>,
+				 <&div_clk GATE_CLK_GPIO_DB>;
+			clock-names = "bus", "db";
+
+			port2a: gpio-controller@0 {
+				compatible = "snps,dw-apb-gpio-port";
+				bank-name = "port0a";
+				gpio-controller;
+				#gpio-cells = <2>;
+				snps,nr-gpios = <32>;
+				reg = <0>;
+				interrupt-controller;
+				#interrupt-cells = <2>;
+				interrupt-parent = <&intc>;
+				interrupts = <SOC_PERIPHERAL_IRQ(98) IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		pwm: pwm@703000C000 {
+			compatible = "sophgo,sophgo-pwm";
+			reg = <0x70 0x3000C000 0x0 0x20>;
+			clocks = <&div_clk GATE_CLK_APB_PWM>;
+			clock-names = "clk_gate_apb_pwm";
+			#pwm-cells = <2>;
+			pwm-num = <2>;
+			no-polarity;
+		};
+
+		tach0: tach@703000C020 {
+			compatible = "sophgo,sophgo-tach";
+			reg = <0x70 0x3000C020 0x0 0x8>;
+		};
+
+		tach1: tach@703000C028 {
+			compatible = "sophgo,sophgo-tach";
+			reg = <0x70 0x3000C028 0x0 0x8>;
+		};
+
+		uart0: serial@7040000000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x00000070 0x40000000 0x00000000 0x00001000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(112) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <500000000>;
+			clocks = <&div_clk GATE_CLK_UART_500M>,
+				 <&div_clk GATE_CLK_APB_UART>;
+			clock-names = "baudclk", "apb_pclk";
+			reg-shift = <2>;
+			reg-io-width = <4>;
+		};
+
+		uart1: serial@7040001000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x00000070 0x40001000 0x00000000 0x00001000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(113) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <500000000>;
+			clocks = <&div_clk GATE_CLK_UART_500M>,
+				 <&div_clk GATE_CLK_APB_UART>;
+			clock-names = "baudclk", "apb_pclk";
+			reg-shift = <2>;
+			reg-io-width = <4>;
+		};
+
+		uart2: serial@7040002000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x00000070 0x40002000 0x00000000 0x00001000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(114) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <500000000>;
+			clocks = <&div_clk GATE_CLK_UART_500M>,
+				 <&div_clk GATE_CLK_APB_UART>;
+			clock-names = "baudclk", "apb_pclk";
+			reg-shift = <2>;
+			reg-io-width = <4>;
+		};
+
+		uart3: serial@7040003000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x00000070 0x40003000 0x00000000 0x00001000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(115) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <500000000>;
+			clocks = <&div_clk GATE_CLK_UART_500M>,
+				 <&div_clk GATE_CLK_APB_UART>;
+			clock-names = "baudclk", "apb_pclk";
+			reg-shift = <2>;
+			reg-io-width = <4>;
+		};
+
+		emmc: bm-emmc@704002A000 {
+			compatible = "bitmain,bm-emmc";
+			reg = <0x70 0x4002A000 0x0 0x1000>;
+			reg-names = "core_mem";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(134) IRQ_TYPE_LEVEL_HIGH>;
+			bus-width = <4>;
+			non-removable;
+			no-sdio;
+			no-sd;
+			resets = <&rst RST_EMMC>;
+			reset-names = "emmc";
+			clocks =
+				<&div_clk GATE_CLK_EMMC_100M>,
+				<&div_clk GATE_CLK_AXI_EMMC>,
+				<&div_clk GATE_CLK_100K_EMMC>;
+			clock-names =
+				"clk_gate_emmc",
+				"clk_gate_axi_emmc",
+				"clk_gate_100k_emmc";
+		};
+
+		sd: bm-sd@704002B000 {
+			compatible = "bitmain,bm-sd";
+			reg = <0x70 0x4002B000 0x0 0x1000>;
+			reg-names = "core_mem";
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(136) IRQ_TYPE_LEVEL_HIGH>;
+			bus-width = <4>;
+			no-sdio;
+			no-mmc;
+			resets = <&rst RST_SD>;
+			reset-names = "sdio";
+			clocks =
+				<&div_clk GATE_CLK_SD_100M>,
+				<&div_clk GATE_CLK_AXI_SD>,
+				<&div_clk GATE_CLK_100K_SD>;
+			clock-names =
+				"clk_gate_sd",
+				"clk_gate_axi_sd",
+				"clk_gate_100k_sd";
+		};
+
+		spifmc0: flash-controller@7000180000 {
+			compatible = "sophgo,spifmc";
+			reg = <0x70 0x00180000 0x0 0x1000000>;
+			reg-names = "memory";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(108) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000000>;
+			clocks = <&div_clk GATE_CLK_AHB_SF>;
+			flash@0 {
+				reg = <0>;
+				compatible = "jedec,spi-nor";
+			};
+		};
+
+		spifmc1: flash-controller@7002180000 {
+			compatible = "sophgo,spifmc";
+			reg = <0x70 0x02180000 0x0 0x1000000>;
+			reg-names = "memory";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(109) IRQ_TYPE_LEVEL_HIGH>;
+			clock-frequency = <100000000>;
+			clocks = <&div_clk GATE_CLK_AHB_SF>;
+			flash@0 {
+				reg = <0>;
+				compatible = "jedec,spi-nor";
+			};
+		};
+
+                spi0: spi@7040004000 {
+			compatible = "snps,dw-apb-ssi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x70 0x40004000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(110) IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&div_clk GATE_CLK_APB_SPI>,
+			          <&div_clk GATE_CLK_SYSDMA_AXI>;
+			clock-frequency = <250000000>;
+			resets = <&rst RST_SPI0>;
+			reset-names = "spi0";
+			num-cs = <2>;
+			status = "okay";
+                };
+
+                spi1: spi@7040005000 {
+			compatible = "snps,dw-apb-ssi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x70 0x40005000 0x0 0x1000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(111) IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&div_clk GATE_CLK_APB_SPI>,
+			           <&div_clk GATE_CLK_SYSDMA_AXI>;
+			clock-frequency = <250000000>;
+			resets = <&rst RST_SPI1>;
+			reset-names = "spi1";
+			num-cs = <2>;
+			status = "okay";
+                };
+
+		stmmac_axi_setup: stmmac-axi-config {
+			snps,wr_osr_lmt = <1>;
+			snps,rd_osr_lmt = <2>;
+			snps,blen = <4 8 16 0 0 0 0>;
+		};
+
+		mtl_rx_setup: rx-queues-config {
+			snps,rx-queues-to-use = <8>;
+			queue0 {};
+			queue1 {};
+			queue2 {};
+			queue3 {};
+			queue4 {};
+			queue5 {};
+			queue6 {};
+			queue7 {};
+		};
+
+		mtl_tx_setup: tx-queues-config {
+			snps,tx-queues-to-use = <8>;
+			queue0 {};
+			queue1 {};
+			queue2 {};
+			queue3 {};
+			queue4 {};
+			queue5 {};
+			queue6 {};
+			queue7 {};
+		};
+
+		ethernet0: ethernet@7040026000 {
+			compatible = "bitmain,ethernet";
+			reg = <0x70 0x40026000 0x0 0x4000>;
+			interrupt-parent = <&intc>;
+			interrupts = <SOC_PERIPHERAL_IRQ(132) IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			clock-names = "clk_tx", "gate_clk_tx", "stmmaceth", "ptp_ref", "gate_clk_ref";
+			clocks = <&div_clk DIV_CLK_FPLL_TX_ETH0>,
+				   <&div_clk GATE_CLK_TX_ETH0>,
+				   <&div_clk GATE_CLK_AXI_ETH0>,
+				   <&div_clk GATE_CLK_PTP_REF_I_ETH0>,
+				   <&div_clk GATE_CLK_REF_ETH0>;
+
+			/* no hash filter and perfect filter support */
+			snps,multicast-filter-bins = <0>;
+			snps,perfect-filter-entries = <1>;
+
+			snps,txpbl = <32>;
+			snps,rxpbl = <32>;
+			snps,aal;
+
+			snps,axi-config = <&stmmac_axi_setup>;
+			snps,mtl-rx-config = <&mtl_rx_setup>;
+			snps,mtl-tx-config = <&mtl_tx_setup>;
+
+			phy-mode = "rgmii-txid";
+			phy-reset-gpios = <&port0a 27 0>;
+			phy-handle = <&phy0>;
+			mdio {
+				#address-cells = <0x1>;
+				#size-cells = <0x0>;
+				compatible = "snps,dwmac-mdio";
+				phy0: phy@0 {
+					compatible = "ethernet-phy-ieee802.3-c22";
+					device_type = "ethernet-phy";
+					reg = <0x0>;
+				};
+			};
+		};
+	};
+
+	intc1: top_intc@7030010300 {
+		compatible = "sophgo,top-intc";
+		reg = <0x70 0x300102E0 0x0 0x4>,
+		      <0x70 0x30010300 0x0 0x4>,
+		      <0x70 0x30010304 0x0 0x4>;
+		reg-names = "sta", "set", "clr";
+		reg-bitwidth = <32>;
+		top_intc_id = <0>;
+		interrupt-controller;
+		#interrupt-cells = <0x1>; // only applies to child node
+		for-msi;
+
+		interrupt-parent = <&intc>;
+		interrupts = <SOC_PERIPHERAL_IRQ(64) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(65) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(66) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(67) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(68) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(69) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(70) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(71) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(72) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(73) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(74) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(75) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(76) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(77) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(78) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(79) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(80) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(81) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(82) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(83) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(84) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(85) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(86) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(87) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(88) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(89) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(90) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(91) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(92) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(93) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(94) IRQ_TYPE_LEVEL_HIGH>,
+			     <SOC_PERIPHERAL_IRQ(95) IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "msi0",  "msi1",  "msi2",  "msi3",
+				  "msi4",  "msi5",  "msi6",  "msi7",
+				  "msi8",  "msi9",  "msi10", "msi11",
+				  "msi12", "msi13", "msi14", "msi15",
+				  "msi16", "msi17", "msi18", "msi19",
+				  "msi20", "msi21", "msi22", "msi23",
+				  "msi24", "msi25", "msi26", "msi27",
+				  "msi28", "msi29", "msi30", "msi31";
+
+	};
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen: chosen {
+		bootargs = "console=ttyS0,115200 earlycon maxcpus=1";
+		stdout-path = "serial0";
+	};
+};
diff --git a/arch/riscv/boot/dts/thead/Makefile b/arch/riscv/boot/dts/thead/Makefile
index b55a17127c2b..1f14fdaf6add 100644
--- a/arch/riscv/boot/dts/thead/Makefile
+++ b/arch/riscv/boot/dts/thead/Makefile
@@ -1,2 +1,5 @@
 # SPDX-License-Identifier: GPL-2.0
 dtb-$(CONFIG_ARCH_THEAD) += th1520-lichee-pi-4a.dtb th1520-beaglev-ahead.dtb
+dtb-$(CONFIG_ARCH_THEAD) += th1520-lichee-pi-4a-16g.dtb
+dtb-$(CONFIG_ARCH_THEAD) += th1520-lichee-cluster-4a.dtb th1520-lichee-cluster-4a-16g.dtb
+dtb-$(CONFIG_ARCH_THEAD) += th1520-milkv-meles.dtb th1520-milkv-meles-4g.dtb
diff --git a/arch/riscv/boot/dts/thead/th1520-beaglev-ahead.dts b/arch/riscv/boot/dts/thead/th1520-beaglev-ahead.dts
index 70e8042c8304..2c2d43433586 100644
--- a/arch/riscv/boot/dts/thead/th1520-beaglev-ahead.dts
+++ b/arch/riscv/boot/dts/thead/th1520-beaglev-ahead.dts
@@ -7,22 +7,29 @@
 /dts-v1/;
 
 #include "th1520.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/leds/common.h>
 
 / {
 	model = "BeagleV Ahead";
 	compatible = "beagle,beaglev-ahead", "thead,th1520";
 
 	aliases {
+		ethernet0 = &gmac0;
 		gpio0 = &gpio0;
 		gpio1 = &gpio1;
 		gpio2 = &gpio2;
 		gpio3 = &gpio3;
+		gpio4 = &gpio4;
+		gpio5 = &aogpio;
 		serial0 = &uart0;
 		serial1 = &uart1;
 		serial2 = &uart2;
 		serial3 = &uart3;
 		serial4 = &uart4;
 		serial5 = &uart5;
+                mmc0 = &emmc;
+                mmc1 = &sdio0;
 	};
 
 	chosen {
@@ -32,11 +39,46 @@ chosen {
 	memory@0 {
 		device_type = "memory";
 		reg = <0x0  0x00000000  0x1 0x00000000>;
+	};
+
+	leds {
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins>;
+		compatible = "gpio-leds";
+
+		led-1 {
+			gpios = <&gpio4 8 GPIO_ACTIVE_LOW>;
+			color = <LED_COLOR_ID_BLUE>;
+			label = "led1";
+		};
+
+		led-2 {
+			gpios = <&gpio4 9 GPIO_ACTIVE_LOW>;
+			color = <LED_COLOR_ID_BLUE>;
+			label = "led2";
+		};
+
+		led-3 {
+			gpios = <&gpio4 10 GPIO_ACTIVE_LOW>;
+			color = <LED_COLOR_ID_BLUE>;
+			label = "led3";
+		};
 
+		led-4 {
+			gpios = <&gpio4 11 GPIO_ACTIVE_LOW>;
+			color = <LED_COLOR_ID_BLUE>;
+			label = "led4";
+		};
+
+		led-5 {
+			gpios = <&gpio4 12 GPIO_ACTIVE_LOW>;
+			color = <LED_COLOR_ID_BLUE>;
+			label = "led5";
+		};
 	};
 };
 
-&osc {
+&osc_24m {
 	clock-frequency = <24000000>;
 };
 
@@ -44,10 +86,18 @@ &osc_32k {
 	clock-frequency = <32768>;
 };
 
+&aonsys_clk {
+	clock-frequency = <73728000>;
+};
+
 &apb_clk {
 	clock-frequency = <62500000>;
 };
 
+&sdhci_clk {
+	clock-frequency = <198000000>;
+};
+
 &uart_sclk {
 	clock-frequency = <100000000>;
 };
@@ -56,6 +106,153 @@ &dmac0 {
 	status = "okay";
 };
 
+&gmac_clk {
+        clock-frequency = <500000000>;
+};
+
+&gmac_axi_clk {
+        clock-frequency = <100000000>;
+};
+
+&emmc {
+	bus-width = <8>;
+	max-frequency = <198000000>;
+	mmc-hs400-1_8v;
+	non-removable;
+	no-sdio;
+	no-sd;
+	status = "okay";
+};
+
+&gmac0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&gmac0_pins>;
+	phy-mode = "rgmii-id";
+	status = "okay";
+};
+
+&mdio0 {
+        phy0: ethernet-phy@1 {
+                reg = <1>;
+        };
+};
+
+&padctrl_aosys {
+	led_pins: led-0 {
+		led-pins {
+			pins = "AUDIO_PA8",  /* GPIO4_8 */
+			       "AUDIO_PA9",  /* GPIO4_9 */
+			       "AUDIO_PA10", /* GPIO4_10 */
+			       "AUDIO_PA11", /* GPIO4_11 */
+			       "AUDIO_PA12"; /* GPIO4_12 */
+			function = "gpio";
+			bias-disable;
+			drive-strength = <3>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+	};
+};
+
+&padctrl0_apsys {
+	gmac0_pins: gmac0-0 {
+		tx-pins {
+			pins = "GMAC0_TX_CLK",
+			       "GMAC0_TXEN",
+			       "GMAC0_TXD0",
+			       "GMAC0_TXD1",
+			       "GMAC0_TXD2",
+			       "GMAC0_TXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <25>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "GMAC0_RX_CLK",
+			       "GMAC0_RXDV",
+			       "GMAC0_RXD0",
+			       "GMAC0_RXD1",
+			       "GMAC0_RXD2",
+			       "GMAC0_RXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		mdc-pins {
+			pins = "GMAC0_MDC";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		mdio-pins {
+			pins = "GMAC0_MDIO";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	sdio0_pins: sdio0-0 {
+		detn-pins {
+			pins = "SDIO0_DETN";
+			function = "sdio";
+			bias-disable; /* external pull-up */
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	uart0_pins: uart0-0 {
+		tx-pins {
+			pins = "UART0_TXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <3>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "UART0_RXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+};
+
+&sdio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio0_pins>;
+	bus-width = <4>;
+	max-frequency = <198000000>;
+	status = "okay";
+};
+
 &uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins>;
 	status = "okay";
 };
diff --git a/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a-16g.dts b/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a-16g.dts
new file mode 100644
index 000000000000..c65cd1c83101
--- /dev/null
+++ b/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a-16g.dts
@@ -0,0 +1,18 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright (C) 2024 NekoRouter <nekorouter@outlook.com>
+ */
+
+/dts-v1/;
+
+#include "th1520-lichee-cluster-4a.dts"
+
+/ {
+        model = "Sipeed Lichee Cluster 4A 16G";
+        compatible = "sipeed,lichee-cluster-4a", "sipeed,lichee-module-4a", "thead,th1520";
+
+        memory@0 {
+                device_type = "memory";
+                reg = <0x0 0x00000000 0x4 0x00000000>;
+        };
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a.dts b/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a.dts
new file mode 100644
index 000000000000..f1116426233f
--- /dev/null
+++ b/arch/riscv/boot/dts/thead/th1520-lichee-cluster-4a.dts
@@ -0,0 +1,45 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright (C) 2024 NekoRouter <nekorouter@outlook.com>
+ */
+
+/dts-v1/;
+
+#include "th1520-lichee-pi-4a.dts"
+
+/ {
+	model = "Sipeed Lichee Cluster 4A";
+	compatible = "sipeed,lichee-cluster-4a", "sipeed,lichee-module-4a", "thead,th1520";
+
+	/delete-node/ regulator-hub_5v;
+
+	/delete-node/ regulator-vcc5v_usb;
+
+	/delete-node/ regulator-hub_5v;
+
+	/delete-node/ regulator-vcc5v_usb;
+
+	/delete-node/ wireless-wlan;
+
+	/delete-node/ wireless-bluetooth;
+	
+	/delete-node/ soc_wcn33_en;
+};
+
+&i2c0 {
+	status = "okay";
+
+	/delete-node/ gpio@18;
+};
+
+&i2c3 {
+	status = "okay";
+
+	/delete-node/ gpio@18;
+};
+
+&usb_dwc3 {
+	/delete-node/ hub@1;
+
+	/delete-node/ hub@2;
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-lichee-module-4a.dtsi b/arch/riscv/boot/dts/thead/th1520-lichee-module-4a.dtsi
index a802ab110429..8e2d281c7dee 100644
--- a/arch/riscv/boot/dts/thead/th1520-lichee-module-4a.dtsi
+++ b/arch/riscv/boot/dts/thead/th1520-lichee-module-4a.dtsi
@@ -15,9 +15,33 @@ memory@0 {
 		device_type = "memory";
 		reg = <0x0 0x00000000 0x2 0x00000000>;
 	};
+
+	resmem: reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		//Note: with "no-map" reserv mem not saved in hibernation
+		rpmsgmem: memory@1E000000 {
+			reg = <0x0 0x1E000000 0x0 0x10000>;
+		};
+	};
+
+	light_rpmsg: light_rpmsg {
+		compatible = "light,rpmsg-bus", "simple-bus";
+		memory-region = <&rpmsgmem>;
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		rpmsg: rpmsg {
+			vdev-nums = <1>;
+			reg = <0x0 0x1E000000 0 0x10000>;
+			compatible = "light,light-rpmsg";
+			status = "okay";
+		};
+	};
 };
 
-&osc {
+&osc_24m {
 	clock-frequency = <24000000>;
 };
 
@@ -25,14 +49,139 @@ &osc_32k {
 	clock-frequency = <32768>;
 };
 
+&aonsys_clk {
+	clock-frequency = <73728000>;
+};
+
 &apb_clk {
 	clock-frequency = <62500000>;
 };
 
+&sdhci_clk {
+	clock-frequency = <198000000>;
+};
+
 &uart_sclk {
 	clock-frequency = <100000000>;
 };
 
+&gmac_clk {
+	clock-frequency = <500000000>;
+};
+
+&gmac_axi_clk {
+	clock-frequency = <100000000>;
+};
+
 &dmac0 {
 	status = "okay";
 };
+
+&emmc {
+	bus-width = <8>;
+	max-frequency = <198000000>;
+	mmc-hs400-1_8v;
+	non-removable;
+	no-sdio;
+	no-sd;
+	status = "okay";
+};
+
+&padctrl0_apsys {
+	sdio0_pins: sdio0-0 {
+		detn-pins {
+			pins = "SDIO0_DETN";
+			function = "sdio";
+			bias-disable; /* external pull-up */
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+};
+
+&sdio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio0_pins>;
+	bus-width = <4>;
+	max-frequency = <198000000>;
+	status = "okay";
+};
+
+&cpus {
+	c910_0: cpu@0 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+	c910_1: cpu@1 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+	c910_2: cpu@2 {
+
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+	c910_3: cpu@3 {
+
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a-16g.dts b/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a-16g.dts
new file mode 100644
index 000000000000..a3a991baf716
--- /dev/null
+++ b/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a-16g.dts
@@ -0,0 +1,18 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright (C) 2023 Han Gao <gaohan@iscas.ac.cn>
+ */
+
+/dts-v1/;
+
+#include "th1520-lichee-pi-4a.dts"
+
+/ {
+        model = "Sipeed Lichee Pi 4A 16G";
+        compatible = "sipeed,lichee-pi-4a", "sipeed,lichee-module-4a", "thead,th1520";
+
+        memory@0 {
+                device_type = "memory";
+                reg = <0x0 0x00000000 0x4 0x00000000>;
+        };
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a.dts b/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a.dts
index 9a3884a73e13..6c0709e5193f 100644
--- a/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a.dts
+++ b/arch/riscv/boot/dts/thead/th1520-lichee-pi-4a.dts
@@ -4,29 +4,741 @@
  */
 
 #include "th1520-lichee-module-4a.dtsi"
+#include <dt-bindings/gpio/gpio.h>
 
 / {
 	model = "Sipeed Lichee Pi 4A";
 	compatible = "sipeed,lichee-pi-4a", "sipeed,lichee-module-4a", "thead,th1520";
 
 	aliases {
+		ethernet0 = &gmac0;
+		ethernet1 = &gmac1;
 		gpio0 = &gpio0;
 		gpio1 = &gpio1;
 		gpio2 = &gpio2;
 		gpio3 = &gpio3;
+		gpio4 = &gpio4;
+		gpio5 = &aogpio;
 		serial0 = &uart0;
 		serial1 = &uart1;
 		serial2 = &uart2;
 		serial3 = &uart3;
 		serial4 = &uart4;
 		serial5 = &uart5;
+		i2c0 = &i2c0;
+		i2c1 = &i2c1;
+		i2c2 = &i2c2;
+		i2c3 = &i2c3;
+		i2c4 = &i2c4;
+		i2c5 = &audio_i2c0;
+		i2c6 = &audio_i2c1;
+		mmc0 = &emmc;
+		mmc1 = &sdio0;
 	};
 
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	fan: pwm-fan {
+		pinctrl-names = "default";
+		pinctrl-0 = <&fan_pins>;
+		compatible = "pwm-fan";
+		#cooling-cells = <2>;
+		pwms = <&pwm 1 10000000 0>;
+		cooling-levels = <0 66 196 255>;
+	};
+
+	hub_5v: regulator-hub_5v {
+		compatible = "regulator-fixed";
+		regulator-name = "HUB_5V";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&ioexp3 3 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		regulator-always-on;
+	};
+
+	vcc5v_usb: regulator-vcc5v_usb {
+		compatible = "regulator-fixed";
+		regulator-name = "VCC5V_USB";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&gpio1 22 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		regulator-always-on;
+	};
+
+	thermal-zones {
+		cpu-thermal {
+			polling-delay = <1000>;
+			polling-delay-passive = <1000>;
+			thermal-sensors = <&pvt 0>;
+
+			trips {
+				trip_active0: active-0 {
+					temperature = <39000>;
+					hysteresis = <5000>;
+					type = "active";
+				};
+
+				trip_active1: active-1 {
+					temperature = <50000>;
+					hysteresis = <5000>;
+					type = "active";
+				};
+
+				trip_active2: active-2 {
+					temperature = <60000>;
+					hysteresis = <5000>;
+					type = "active";
+				};
+			};
+
+			cooling-maps {
+				map-active-0 {
+					cooling-device = <&fan 1 1>;
+					trip = <&trip_active0>;
+				};
+
+				map-active-1 {
+					cooling-device = <&fan 2 2>;
+					trip = <&trip_active1>;
+				};
+
+				map-active-2 {
+					cooling-device = <&fan 3 3>;
+					trip = <&trip_active2>;
+				};
+			};
+		};
+	};
+
+	hub_5v: regulator-hub_5v {
+		compatible = "regulator-fixed";
+		regulator-name = "HUB_5V";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&ioexp3 3 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		regulator-always-on;
+	};
+
+	vcc5v_usb: regulator-vcc5v_usb {
+		compatible = "regulator-fixed";
+		regulator-name = "VCC5V_USB";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&gpio1 22 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		regulator-always-on;
+	};
+
+	wcn_wifi: wireless-wlan {
+		compatible = "wlan-platdata";
+		clock-names = "clk_wifi";
+		ref-clock-frequency = <24000000>;
+		keep_wifi_power_on;
+		pinctrl-names = "default";
+		wifi_chip_type = "rtl8723ds";
+		WIFI,poweren_gpio = <&ioexp2 5 0>;
+		status = "okay";
+	};
+
+	wcn_bt: wireless-bluetooth {
+		compatible = "bluetooth-platdata";
+		pinctrl-names = "default", "rts_gpio";
+		BT,power_gpio    = <&ioexp2 6 0>;
+		status = "okay";
+	};
+
+	aon: aon {
+		compatible = "thead,light-aon";
+		mbox-names = "aon";
+		mboxes = <&mbox_910t 1 0>;
+		status = "okay";
+
+		pd: light-aon-pd {
+			compatible = "thead,light-aon-pd";
+			#power-domain-cells = <1>;
+		};
+
+		soc_aud_3v3_en_reg: soc_aud_3v3_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_aud_3v3_en";
+			regulator-min-microvolt = <3300000>;
+			regulator-max-microvolt = <3300000>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+		soc_aud_1v8_en_reg: soc_aud_1v8_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_aud_1v8_en";
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+		soc_vdd_3v3_en_reg: soc_vdd_3v3_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_vdd_3v3_en";
+			regulator-min-microvolt = <3300000>;
+			regulator-max-microvolt = <3300000>;
+			gpio = <&gpio0 30 1>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+		soc_vdd33_lcd0_en_reg: soc_lcd0_vdd33_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_lcd0_vdd33_en";
+			regulator-min-microvolt = <3300000>;
+			regulator-max-microvolt = <3300000>;
+			gpio = <&ioexp2 5 1>;
+			enable-active-high;
+		};
+
+		soc_vdd18_lcd0_en_reg: soc_lcd0_vdd18_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_lcd0_vdd18_en";
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			gpio = <&ioexp2 6 1>;
+			enable-active-high;
+		};
+
+		soc_vdd5v_se_en_reg: soc_vdd5v_se_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_vdd5v_se_en";
+			regulator-min-microvolt = <5000000>;
+			regulator-max-microvolt = <5000000>;
+			gpio = <&gpio2 14 1>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+		soc_wcn33_en_reg: soc_wcn33_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_wcn33_en";
+			regulator-min-microvolt = <3300000>;
+			regulator-max-microvolt = <3300000>;
+			gpio = <&gpio2 29 1>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+		soc_vbus_en_reg: soc_vbus_en {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_vbus_en";
+			regulator-min-microvolt = <3300000>;
+			regulator-max-microvolt = <3300000>;
+			gpio = <&gpio1 22 1>;
+			enable-active-high;
+			regulator-always-on;
+		};
+
+
+		soc_avdd28_rgb_reg: soc_avdd28_rgb {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_avdd28_rgb";
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+			gpio = <&ioexp2 1 1>;
+			enable-active-high;
+		};
+
+		soc_dovdd18_rgb_reg: soc_dovdd18_rgb {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_dovdd18_rgb";
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+			gpio = <&ioexp2 2 1>;
+			enable-active-high;
+		};
+
+		soc_dvdd12_rgb_reg: soc_dvdd12_rgb {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_dvdd12_rgb";
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+			gpio = <&ioexp2 0 1>;
+			enable-active-high;
+		};
+
+		soc_avdd25_ir_reg: soc_avdd25_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_avdd25_ir";
+			regulator-min-microvolt = <2500000>;
+			regulator-max-microvolt = <2500000>;
+			gpio = <&ioexp2 5 1>;
+			enable-active-high;
+		};
+
+		soc_dovdd18_ir_reg: soc_dovdd18_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_dovdd18_ir";
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			gpio = <&ioexp2 3 1>;
+			enable-active-high;
+		};
+
+		soc_dvdd12_ir_reg: soc_dvdd12_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_dvdd12_ir";
+			regulator-min-microvolt = <1200000>;
+			regulator-max-microvolt = <1200000>;
+			gpio = <&ioexp2 4 1>;
+			enable-active-high;
+		};
+
+		soc_cam2_avdd25_ir_reg: soc_cam2_avdd25_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_cam2_avdd25_ir";
+			regulator-min-microvolt = <2500000>;
+			regulator-max-microvolt = <2500000>;
+			gpio = <&ioexp2 7 1>;
+			enable-active-high;
+		};
+
+		soc_cam2_dovdd18_ir_reg: soc_cam2_dovdd18_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_cam2_dovdd18_ir";
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			gpio = <&ioexp2 6 1>;
+			enable-active-high;
+		};
+
+		soc_cam2_dvdd12_ir_reg: soc_cam2_dvdd12_ir {
+			compatible = "regulator-fixed";
+			regulator-name = "soc_cam2_dvdd12_ir";
+			regulator-min-microvolt = <1200000>;
+			regulator-max-microvolt = <1200000>;
+			gpio = <&ioexp2 0 1>;
+			enable-active-high;
+		};
+
+		aon_reg_dialog: light-dialog-reg {
+			compatible = "thead,light-dialog-pmic-ant";
+			status = "okay";
+
+			dvdd_cpu_reg: appcpu_dvdd {
+				regulator-name = "appcpu_dvdd";
+				regulator-min-microvolt = <300000>;
+				regulator-max-microvolt = <1570000>;
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			dvddm_cpu_reg: appcpu_dvddm {
+				regulator-name = "appcpu_dvddm";
+				regulator-min-microvolt = <300000>;
+				regulator-max-microvolt = <1570000>;
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd18_aon_reg: soc_dvdd18_aon {
+				regulator-name = "soc_dvdd18_aon";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd33_usb3_reg: soc_avdd33_usb3 {
+				regulator-name = "soc_avdd33_usb3";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd08_aon_reg: soc_dvdd08_aon {
+				regulator-name = "soc_dvdd08_aon";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd08_ddr_reg: soc_dvdd08_ddr {
+				regulator-name = "soc_dvdd08_ddr";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_1v8_reg: soc_vdd_ddr_1v8 {
+				regulator-name = "soc_vdd_ddr_1v8";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_1v1_reg: soc_vdd_ddr_1v1 {
+				regulator-name = "soc_vdd_ddr_1v1";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_0v6_reg: soc_vdd_ddr_0v6 {
+				regulator-name = "soc_vdd_ddr_0v6";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd18_ap_reg: soc_dvdd18_ap {
+				regulator-name = "soc_dvdd18_ap";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd08_mipi_hdmi_reg: soc_avdd08_mipi_hdmi {
+				regulator-name = "soc_avdd08_mipi_hdmi";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd18_mipi_hdmi_reg: soc_avdd18_mipi_hdmi {
+				regulator-name = "soc_avdd18_mipi_hdmi";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd33_emmc_reg: soc_vdd33_emmc {
+				regulator-name = "soc_vdd33_emmc";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd18_emmc_reg: soc_vdd18_emmc {
+				regulator-name = "soc_vdd18_emmc";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dovdd18_scan_reg: soc_dovdd18_scan {
+				regulator-name = "soc_dovdd18_scan";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+
+			soc_dvdd12_scan_reg: soc_dvdd12_scan {
+				regulator-name = "soc_dvdd12_scan";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+
+			soc_avdd28_scan_en_reg: soc_avdd28_scan_en {
+				regulator-name = "soc_avdd28_scan_en";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+
+		};
+
+		c910_cpufreq {
+			compatible = "thead,light-mpw-cpufreq";
+			status = "okay";
+		};
+
+		test: light-aon-test {
+			compatible = "thead,light-aon-test";
+		};
+	};
+	
+};
+
+&aogpio {
+	sel-usb-hub-hog {
+		gpio-hog;
+		gpios = <4 GPIO_ACTIVE_HIGH>;
+		output-high;
+	};
+};
+
+&gmac0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&gmac0_pins>;
+	phy-handle = <&phy0>;
+	phy-mode = "rgmii-id";
+	status = "okay";
+};
+
+&gmac1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&gmac1_pins>;
+	phy-handle = <&phy1>;
+	phy-mode = "rgmii-id";
+	status = "okay";
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+	i2c-sda-hold-time-ns = <300>;
+	i2c-sda-falling-time-ns = <510>;
+	i2c-scl-falling-time-ns = <510>;
+	status = "okay";
+
+	ioexp1: gpio@18 {
+		compatible = "nxp,pca9557";
+		reg = <0x18>;
+		gpio-controller;
+		#gpio-cells = <2>;
+		gpio-line-names = "cam0_dvdd12",
+				  "cam0_avdd28",
+				  "cam0_dovdd18";
+	};
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+	i2c-sda-hold-time-ns = <300>;
+	i2c-sda-falling-time-ns = <510>;
+	i2c-scl-falling-time-ns = <510>;
+	status = "okay";
+
+	ioexp2: gpio@18 {
+		compatible = "nxp,pca9557";
+		reg = <0x18>;
+		gpio-controller;
+		#gpio-cells = <2>;
+		gpio-line-names = "",
+				  "cam0_reset",
+				  "cam1_reset",
+				  "cam2_reset",
+				  "wl_host_wake",
+				  "bt_resetn",
+				  "",
+				  "bt_host_wake";
+	};
+};
+
+&i2c3 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c3_pins>;
+	clock-frequency = <100000>;
+	i2c-sda-hold-time-ns = <300>;
+	i2c-sda-falling-time-ns = <510>;
+	i2c-scl-falling-time-ns = <510>;
+	status = "okay";
+
+	ioexp3: gpio@18 {
+		compatible = "nxp,pca9557";
+		reg = <0x18>;
+		gpio-controller;
+		#gpio-cells = <2>;
+		gpio-line-names = "tp0_rst",
+				  "",
+				  "",
+				  "vcc5v_usb",
+				  "vdd28_tp0",
+				  "vdd33_lcd0",
+				  "vdd18_lcd0",
+				  "lcd0_reset";
+	};
+};
+
+&mdio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mdio0_pins>;
+
+	phy0: ethernet-phy@1 {
+		reg = <1>;
+	};
+
+	phy1: ethernet-phy@2 {
+		reg = <2>;
+	};
+};
+
+&padctrl0_apsys {
+	fan_pins: fan-0 {
+		pwm1-pins {
+			pins = "GPIO3_3"; /* PWM1 */
+			function = "pwm";
+			bias-disable;
+			drive-strength = <25>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+	};
+
+	gmac0_pins: gmac0-0 {
+		tx-pins {
+			pins = "GMAC0_TX_CLK",
+			       "GMAC0_TXEN",
+			       "GMAC0_TXD0",
+			       "GMAC0_TXD1",
+			       "GMAC0_TXD2",
+			       "GMAC0_TXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <25>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "GMAC0_RX_CLK",
+			       "GMAC0_RXDV",
+			       "GMAC0_RXD0",
+			       "GMAC0_RXD1",
+			       "GMAC0_RXD2",
+			       "GMAC0_RXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+	};
+
+	gmac1_pins: gmac1-0 {
+		tx-pins {
+			pins = "GPIO2_18", /* GMAC1_TX_CLK */
+			       "GPIO2_20", /* GMAC1_TXEN */
+			       "GPIO2_21", /* GMAC1_TXD0 */
+			       "GPIO2_22", /* GMAC1_TXD1 */
+			       "GPIO2_23", /* GMAC1_TXD2 */
+			       "GPIO2_24"; /* GMAC1_TXD3 */
+			function = "gmac1";
+			bias-disable;
+			drive-strength = <25>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "GPIO2_19", /* GMAC1_RX_CLK */
+			       "GPIO2_25", /* GMAC1_RXDV */
+			       "GPIO2_30", /* GMAC1_RXD0 */
+			       "GPIO2_31", /* GMAC1_RXD1 */
+			       "GPIO3_0",  /* GMAC1_RXD2 */
+			       "GPIO3_1";  /* GMAC1_RXD3 */
+			function = "gmac1";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+	};
+
+	i2c3_pins: i2c3-0 {
+		i2c-pins {
+			pins = "I2C3_SCL", "I2C3_SDA";
+			function = "i2c";
+			bias-disable;
+			drive-strength = <7>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	mdio0_pins: mdio0-0 {
+		mdc-pins {
+			pins = "GMAC0_MDC";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		mdio-pins {
+			pins = "GMAC0_MDIO";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	uart0_pins: uart0-0 {
+		tx-pins {
+			pins = "UART0_TXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <3>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "UART0_RXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+};
+
+&padctrl1_apsys {
+	i2c0_pins: i2c0-0 {
+		i2c-pins {
+			pins = "I2C0_SCL", "I2C0_SDA";
+			function = "i2c";
+			bias-disable;
+			drive-strength = <7>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	i2c1_pins: i2c1-0 {
+		i2c-pins {
+			pins = "I2C1_SCL", "I2C1_SDA";
+			function = "i2c";
+			bias-disable;
+			drive-strength = <7>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
 };
 
 &uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins>;
+	status = "okay";
+};
+
+&usb {
 	status = "okay";
 };
+
+&usb_dwc3 {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	hub_2_0: hub@1 {
+		compatible = "usb2109,2817";
+		reg = <1>;
+		peer-hub = <&hub_3_0>;
+		vdd-supply = <&hub_5v>;
+		vbus-supply = <&vcc5v_usb>;
+	};
+
+	hub_3_0: hub@2 {
+		compatible = "usb2109,817";
+		reg = <2>;
+		peer-hub = <&hub_2_0>;
+		vbus-supply = <&vcc5v_usb>;
+	};
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-milkv-meles-4g.dts b/arch/riscv/boot/dts/thead/th1520-milkv-meles-4g.dts
new file mode 100644
index 000000000000..5a6baccd1684
--- /dev/null
+++ b/arch/riscv/boot/dts/thead/th1520-milkv-meles-4g.dts
@@ -0,0 +1,19 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ * Copyright (C) 2024 Milk-V Limited.
+ */
+
+/dts-v1/;
+
+#include "th1520-milkv-meles.dts"
+
+/ {
+	model = "Milk-V Meles 4G";
+	compatible = "milkv,meles", "thead,light";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x0 0x00000000 0x1 0x00000000>;
+	};
+};
diff --git a/arch/riscv/boot/dts/thead/th1520-milkv-meles.dts b/arch/riscv/boot/dts/thead/th1520-milkv-meles.dts
new file mode 100644
index 000000000000..394385afd53d
--- /dev/null
+++ b/arch/riscv/boot/dts/thead/th1520-milkv-meles.dts
@@ -0,0 +1,441 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ * Copyright (C) 2024 Milk-V Limited.
+ */
+
+/dts-v1/;
+
+#include "th1520.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "Milk-V Meles";
+	compatible = "milkv,meles", "thead,th1520";
+
+	aliases {
+		ethernet0 = &gmac0;
+		gpio0 = &gpio0;
+		gpio1 = &gpio1;
+		gpio2 = &gpio2;
+		gpio3 = &gpio3;
+		gpio4 = &gpio4;
+		gpio5 = &aogpio;
+		serial0 = &uart0;
+		serial1 = &uart1;
+		serial2 = &uart2;
+		serial3 = &uart3;
+		serial4 = &uart4;
+		serial5 = &uart5;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x0 0x00000000 0x2 0x00000000>;
+	};
+
+	resmem: reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		//Note: with "no-map" reserv mem not saved in hibernation
+		rpmsgmem: memory@1E000000 {
+			reg = <0x0 0x1E000000 0x0 0x10000>;
+		};
+	};
+
+	light_rpmsg: light_rpmsg {
+		compatible = "light,rpmsg-bus", "simple-bus";
+		memory-region = <&rpmsgmem>;
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		rpmsg: rpmsg {
+			vdev-nums = <1>;
+			reg = <0x0 0x1E000000 0 0x10000>;
+			compatible = "light,light-rpmsg";
+			status = "okay";
+		};
+	};
+
+	aon: aon {
+		compatible = "thead,light-aon";
+		mbox-names = "aon";
+		mboxes = <&mbox_910t 1 0>;
+		status = "okay";
+
+		pd: light-aon-pd {
+			compatible = "thead,light-aon-pd";
+			#power-domain-cells = <1>;
+		};
+
+		aon_reg_dialog: light-dialog-reg {
+			compatible = "thead,light-dialog-pmic-ant";
+			status = "okay";
+
+			dvdd_cpu_reg: appcpu_dvdd {
+				regulator-name = "appcpu_dvdd";
+				regulator-min-microvolt = <300000>;
+				regulator-max-microvolt = <1570000>;
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			dvddm_cpu_reg: appcpu_dvddm {
+				regulator-name = "appcpu_dvddm";
+				regulator-min-microvolt = <300000>;
+				regulator-max-microvolt = <1570000>;
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd18_aon_reg: soc_dvdd18_aon {
+				regulator-name = "soc_dvdd18_aon";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd33_usb3_reg: soc_avdd33_usb3 {
+				regulator-name = "soc_avdd33_usb3";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd08_aon_reg: soc_dvdd08_aon {
+				regulator-name = "soc_dvdd08_aon";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd08_ddr_reg: soc_dvdd08_ddr {
+				regulator-name = "soc_dvdd08_ddr";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_1v8_reg: soc_vdd_ddr_1v8 {
+				regulator-name = "soc_vdd_ddr_1v8";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_1v1_reg: soc_vdd_ddr_1v1 {
+				regulator-name = "soc_vdd_ddr_1v1";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd_ddr_0v6_reg: soc_vdd_ddr_0v6 {
+				regulator-name = "soc_vdd_ddr_0v6";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dvdd18_ap_reg: soc_dvdd18_ap {
+				regulator-name = "soc_dvdd18_ap";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd08_mipi_hdmi_reg: soc_avdd08_mipi_hdmi {
+				regulator-name = "soc_avdd08_mipi_hdmi";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_avdd18_mipi_hdmi_reg: soc_avdd18_mipi_hdmi {
+				regulator-name = "soc_avdd18_mipi_hdmi";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd33_emmc_reg: soc_vdd33_emmc {
+				regulator-name = "soc_vdd33_emmc";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_vdd18_emmc_reg: soc_vdd18_emmc {
+				regulator-name = "soc_vdd18_emmc";
+				regulator-boot-on;
+				regulator-always-on;
+			};
+
+			soc_dovdd18_scan_reg: soc_dovdd18_scan {
+				regulator-name = "soc_dovdd18_scan";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+
+			soc_dvdd12_scan_reg: soc_dvdd12_scan {
+				regulator-name = "soc_dvdd12_scan";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+
+			soc_avdd28_scan_en_reg: soc_avdd28_scan_en {
+				regulator-name = "soc_avdd28_scan_en";
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <3600000>;
+			};
+		};
+
+		c910_cpufreq {
+			compatible = "thead,light-mpw-cpufreq";
+			status = "okay";
+		};
+
+		test: light-aon-test {
+			compatible = "thead,light-aon-test";
+		};
+	};
+};
+
+&osc_24m {
+	clock-frequency = <24000000>;
+};
+
+&osc_32k {
+	clock-frequency = <32768>;
+};
+
+&aonsys_clk {
+	clock-frequency = <73728000>;
+};
+
+&apb_clk {
+	clock-frequency = <62500000>;
+};
+
+&sdhci_clk {
+	clock-frequency = <198000000>;
+};
+
+&uart_sclk {
+	clock-frequency = <100000000>;
+};
+
+&gmac_clk {
+	clock-frequency = <500000000>;
+};
+
+&gmac_axi_clk {
+	clock-frequency = <100000000>;
+};
+
+&dmac0 {
+	status = "okay";
+};
+
+&emmc {
+	bus-width = <8>;
+	max-frequency = <198000000>;
+	mmc-hs400-1_8v;
+	non-removable;
+	no-sdio;
+	no-sd;
+	status = "okay";
+};
+
+&gmac0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&gmac0_pins>;
+	phy-handle = <&phy0>;
+	phy-mode = "rgmii-id";
+	status = "okay";
+};
+
+&mdio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mdio0_pins>;
+
+	phy0: ethernet-phy@1 {
+		reg = <1>;
+	};
+};
+
+&sdio0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio0_pins>;
+	bus-width = <4>;
+	max-frequency = <198000000>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins>;
+	status = "okay";
+};
+
+&cpus {
+	c910_0: cpu@0 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+
+	c910_1: cpu@1 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+
+	c910_2: cpu@2 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+
+	c910_3: cpu@3 {
+		operating-points = <
+			/* kHz    uV */
+			300000	650000
+			800000	700000
+			1500000	800000
+			1848000 1000000
+		>;
+		light,dvddm-operating-points = <
+			/* kHz   uV */
+			300000	800000
+			800000	800000
+			1500000	800000
+			1848000 1000000
+		>;
+		dvdd-supply = <&dvdd_cpu_reg>;
+		dvddm-supply = <&dvddm_cpu_reg>;
+	};
+};
+
+&padctrl0_apsys {
+	gmac0_pins: gmac0-0 {
+		tx-pins {
+			pins = "GMAC0_TX_CLK",
+			       "GMAC0_TXEN",
+			       "GMAC0_TXD0",
+			       "GMAC0_TXD1",
+			       "GMAC0_TXD2",
+			       "GMAC0_TXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <25>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "GMAC0_RX_CLK",
+			       "GMAC0_RXDV",
+			       "GMAC0_RXD0",
+			       "GMAC0_RXD1",
+			       "GMAC0_RXD2",
+			       "GMAC0_RXD3";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+	};
+
+	mdio0_pins: mdio0-0 {
+		mdc-pins {
+			pins = "GMAC0_MDC";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		mdio-pins {
+			pins = "GMAC0_MDIO";
+			function = "gmac0";
+			bias-disable;
+			drive-strength = <13>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	sdio0_pins: sdio0-0 {
+		detn-pins {
+			pins = "SDIO0_DETN";
+			function = "sdio";
+			bias-disable; /* external pull-up */
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+
+	uart0_pins: uart0-0 {
+		tx-pins {
+			pins = "UART0_TXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <3>;
+			input-disable;
+			input-schmitt-disable;
+			slew-rate = <0>;
+		};
+
+		rx-pins {
+			pins = "UART0_RXD";
+			function = "uart";
+			bias-disable;
+			drive-strength = <1>;
+			input-enable;
+			input-schmitt-enable;
+			slew-rate = <0>;
+		};
+	};
+};
diff --git a/arch/riscv/boot/dts/thead/th1520.dtsi b/arch/riscv/boot/dts/thead/th1520.dtsi
index ff364709a6df..fab3b5f17f22 100644
--- a/arch/riscv/boot/dts/thead/th1520.dtsi
+++ b/arch/riscv/boot/dts/thead/th1520.dtsi
@@ -5,6 +5,9 @@
  */
 
 #include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/clock/light-fm-ap-clock.h>
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/reset/thead,th1520-reset.h>
 
 / {
 	compatible = "thead,th1520";
@@ -29,6 +32,30 @@ c910_0: cpu@0 {
 			d-cache-sets = <512>;
 			next-level-cache = <&l2_cache>;
 			mmu-type = "riscv,sv39";
+			cpu-freq = "1.848Ghz";
+			cpu-cacheline = "64Bytes";
+
+			operating-points = <
+				/* kHz    uV */
+				300000	600000
+				800000	700000
+				1500000	800000
+				1848000	1000000
+			>;
+			light,dvddm-operating-points = <
+				/* kHz   uV */
+				300000	750000
+				800000	800000
+				1500000	800000
+				1848000	1000000
+			>;
+			clock-latency = <61036>;
+			clocks = <&clk C910_CCLK>,
+				 <&clk C910_CCLK_I0>,
+				 <&clk CPU_PLL1_FOUTPOSTDIV>,
+				 <&clk CPU_PLL0_FOUTPOSTDIV>;
+			clock-names = "c910_cclk", "c910_cclk_i0",
+				      "cpu_pll1_foutpostdiv", "cpu_pll0_foutpostdiv";
 
 			cpu0_intc: interrupt-controller {
 				compatible = "riscv,cpu-intc";
@@ -50,6 +77,30 @@ c910_1: cpu@1 {
 			d-cache-sets = <512>;
 			next-level-cache = <&l2_cache>;
 			mmu-type = "riscv,sv39";
+			cpu-freq = "1.848Ghz";
+			cpu-cacheline = "64Bytes";
+
+			operating-points = <
+				/* kHz    uV */
+				300000	600000
+				800000	700000
+				1500000	800000
+				1848000	1000000
+			>;
+			light,dvddm-operating-points = <
+				/* kHz   uV */
+				300000	750000
+				800000	800000
+				1500000	800000
+				1848000	1000000
+			>;
+			clock-latency = <61036>;
+			clocks = <&clk C910_CCLK>,
+				 <&clk C910_CCLK_I0>,
+				 <&clk CPU_PLL1_FOUTPOSTDIV>,
+				 <&clk CPU_PLL0_FOUTPOSTDIV>;
+			clock-names = "c910_cclk", "c910_cclk_i0",
+				      "cpu_pll1_foutpostdiv", "cpu_pll0_foutpostdiv";
 
 			cpu1_intc: interrupt-controller {
 				compatible = "riscv,cpu-intc";
@@ -71,6 +122,30 @@ c910_2: cpu@2 {
 			d-cache-sets = <512>;
 			next-level-cache = <&l2_cache>;
 			mmu-type = "riscv,sv39";
+			cpu-freq = "1.848Ghz";
+			cpu-cacheline = "64Bytes";
+
+			operating-points = <
+				/* kHz    uV */
+				300000	600000
+				800000	700000
+				1500000	800000
+				1848000	1000000
+			>;
+			light,dvddm-operating-points = <
+				/* kHz   uV */
+				300000	750000
+				800000	800000
+				1500000	800000
+				1848000	1000000
+			>;
+			clock-latency = <61036>;
+			clocks = <&clk C910_CCLK>,
+				 <&clk C910_CCLK_I0>,
+				 <&clk CPU_PLL1_FOUTPOSTDIV>,
+				 <&clk CPU_PLL0_FOUTPOSTDIV>;
+			clock-names = "c910_cclk", "c910_cclk_i0",
+				      "cpu_pll1_foutpostdiv", "cpu_pll0_foutpostdiv";
 
 			cpu2_intc: interrupt-controller {
 				compatible = "riscv,cpu-intc";
@@ -92,6 +167,30 @@ c910_3: cpu@3 {
 			d-cache-sets = <512>;
 			next-level-cache = <&l2_cache>;
 			mmu-type = "riscv,sv39";
+			cpu-freq = "1.848Ghz";
+			cpu-cacheline = "64Bytes";
+
+			operating-points = <
+				/* kHz    uV */
+				300000	600000
+				800000	700000
+				1500000	800000
+				1848000	1000000
+			>;
+			light,dvddm-operating-points = <
+				/* kHz   uV */
+				300000	750000
+				800000	800000
+				1500000	800000
+				1848000	1000000
+			>;
+			clock-latency = <61036>;
+			clocks = <&clk C910_CCLK>,
+				 <&clk C910_CCLK_I0>,
+				 <&clk CPU_PLL1_FOUTPOSTDIV>,
+				 <&clk CPU_PLL0_FOUTPOSTDIV>;
+			clock-names = "c910_cclk", "c910_cclk_i0",
+				      "cpu_pll1_foutpostdiv", "cpu_pll0_foutpostdiv";
 
 			cpu3_intc: interrupt-controller {
 				compatible = "riscv,cpu-intc";
@@ -110,15 +209,111 @@ l2_cache: l2-cache {
 		};
 	};
 
-	osc: oscillator {
+	pmu {
+		compatible = "riscv,pmu";
+		riscv,event-to-mhpmcounters =
+			<0x00003 0x00003 0x0007fff8>,
+			<0x00004 0x00004 0x0007fff8>,
+			<0x00005 0x00005 0x0007fff8>,
+			<0x00006 0x00006 0x0007fff8>,
+			<0x00007 0x00007 0x0007fff8>,
+			<0x00008 0x00008 0x0007fff8>,
+			<0x00009 0x00009 0x0007fff8>,
+			<0x0000a 0x0000a 0x0007fff8>,
+			<0x10000 0x10000 0x0007fff8>,
+			<0x10001 0x10001 0x0007fff8>,
+			<0x10002 0x10002 0x0007fff8>,
+			<0x10003 0x10003 0x0007fff8>,
+			<0x10010 0x10010 0x0007fff8>,
+			<0x10011 0x10011 0x0007fff8>,
+			<0x10012 0x10012 0x0007fff8>,
+			<0x10013 0x10013 0x0007fff8>;
+		riscv,event-to-mhpmevent =
+			<0x00003 0x00000000 0x00000001>,
+			<0x00004 0x00000000 0x00000002>,
+			<0x00006 0x00000000 0x00000006>,
+			<0x00005 0x00000000 0x00000007>,
+			<0x00007 0x00000000 0x00000008>,
+			<0x00008 0x00000000 0x00000009>,
+			<0x00009 0x00000000 0x0000000a>,
+			<0x0000a 0x00000000 0x0000000b>,
+			<0x10000 0x00000000 0x0000000c>,
+			<0x10001 0x00000000 0x0000000d>,
+			<0x10002 0x00000000 0x0000000e>,
+			<0x10003 0x00000000 0x0000000f>,
+			<0x10010 0x00000000 0x00000010>,
+			<0x10011 0x00000000 0x00000011>,
+			<0x10012 0x00000000 0x00000012>,
+			<0x10013 0x00000000 0x00000013>;
+		riscv,raw-event-to-mhpmcounters =
+			<0x00000000 0x00000001 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000002 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000003 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000004 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000005 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000006 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000007 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000008 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000009 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000a 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000b 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000c 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000d 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000e 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000000f 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000010 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000011 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000012 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000013 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000014 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000015 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000016 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000017 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000018 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000019 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001a 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001b 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001c 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001d 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001e 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000001f 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000020 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000021 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000022 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000023 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000024 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000025 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000026 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000027 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000028 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x00000029 0xffffffff 0xffffffff 0x0007fff8>,
+			<0x00000000 0x0000002a 0xffffffff 0xffffffff 0x0007fff8>;
+	};
+	
+	osc_32k: clock-osc-32k {
 		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <32768>;
+		clock-output-names = "osc_32k";
+	};
+
+	osc_24m: clock-osc-24m {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <24000000>;
 		clock-output-names = "osc_24m";
+	};
+
+	rc_24m: clock-rc-24m {
+		compatible = "fixed-clock";
 		#clock-cells = <0>;
+		clock-frequency = <24000000>;
+		clock-output-names = "rc_24m";
 	};
 
-	osc_32k: 32k-oscillator {
+	aonsys_clk: aonsys-clk {
 		compatible = "fixed-clock";
-		clock-output-names = "osc_32k";
+		clock-output-names = "aonsys_clk";
 		#clock-cells = <0>;
 	};
 
@@ -134,6 +329,36 @@ uart_sclk: uart-sclk-clock {
 		#clock-cells = <0>;
 	};
 
+	sdhci_clk: sdhci-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <198000000>;
+		clock-output-names = "sdhci_clk";
+		#clock-cells = <0>;
+	};
+
+	gmac_axi_clk: gmac-axi-clock {
+		compatible = "fixed-clock";
+		clock-output-names = "gmac_axi_clk";
+		#clock-cells = <0>;
+	};
+
+	gmac_clk: gmac-clock {
+		compatible = "fixed-clock";
+		clock-output-names = "gmac_clk";
+		#clock-cells = <0>;
+	};
+
+	stmmac_axi_config: stmmac-axi-config {
+		snps,wr_osr_lmt = <15>;
+		snps,rd_osr_lmt = <15>;
+		snps,blen = <0 0 64 32 0 0 0>;
+	};
+
+	aon_iram: aon-iram@ffffef8000 {
+        compatible = "syscon";
+        reg = <0xff 0xffef8000 0x0 0x10000>;
+    };
+
 	soc {
 		compatible = "simple-bus";
 		interrupt-parent = <&plic>;
@@ -142,6 +367,41 @@ soc {
 		dma-noncoherent;
 		ranges;
 
+		cpurst: cpurst {
+			compatible = "thead,reset-sample";
+			entry-reg = <0xff 0xff019050>;
+			entry-cnt = <4>;
+			control-reg = <0xff 0xff015004>;
+			control-val = <0x1c>;
+			csr-copy = <0x7f3 0x7c0 0x7c1 0x7c2 0x7c3 0x7c5 0x7cc>;
+		};
+
+		light_event: light-event {
+            compatible = "thead,light-event";
+            aon-iram-regmap = <&aon_iram>;
+            status = "okay";
+        };
+
+		audio_i2c0: i2c@ffcb01a000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xcb01a000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <182 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		audio_i2c1: i2c@ffcb01b000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xcb01b000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <183 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
 		plic: interrupt-controller@ffd8000000 {
 			compatible = "thead,th1520-plic", "thead,c900-plic";
 			reg = <0xff 0xd8000000 0x0 0x01000000>;
@@ -164,6 +424,50 @@ clint: timer@ffdc000000 {
 					      <&cpu3_intc 3>, <&cpu3_intc 7>;
 		};
 
+		gmac0: ethernet@ffe7070000 {
+			compatible = "thead,th1520-dwmac", "snps,dwmac-3.70a";
+			reg = <0xff 0xe7070000 0x0 0x2000>;
+			interrupts = <66 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			clocks = <&gmac_clk>, <&gmac_axi_clk>;
+			clock-names = "stmmaceth", "pclk";
+			snps,pbl = <32>;
+			snps,fixed-burst;
+			snps,multicast-filter-bins = <64>;
+			snps,perfect-filter-entries = <32>;
+			snps,axi-config = <&stmmac_axi_config>;
+			thead,gmacapb = <&gmac0_apb>;
+			status = "disabled";
+
+			mdio0: mdio {
+				compatible = "snps,dwmac-mdio";
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
+		gmac1: ethernet@ffe7060000 {
+			compatible = "thead,th1520-dwmac", "snps,dwmac-3.70a";
+			reg = <0xff 0xe7060000 0x0 0x2000>;
+			interrupts = <67 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			clocks = <&gmac_clk>, <&gmac_axi_clk>;
+			clock-names = "stmmaceth", "pclk";
+			snps,pbl = <32>;
+			snps,fixed-burst;
+			snps,multicast-filter-bins = <64>;
+			snps,perfect-filter-entries = <32>;
+			snps,axi-config = <&stmmac_axi_config>;
+			thead,gmacapb = <&gmac1_apb>;
+			status = "disabled";
+
+			mdio1: mdio {
+				compatible = "snps,dwmac-mdio";
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
 		uart0: serial@ffe7014000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0xff 0xe7014000 0x0 0x100>;
@@ -194,17 +498,48 @@ uart3: serial@ffe7f04000 {
 			status = "disabled";
 		};
 
-		gpio2: gpio@ffe7f34000 {
+		i2c0: i2c@ffe7f20000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xe7f20000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <44 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c1: i2c@ffe7f24000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xe7f24000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <45 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c4: i2c@ffe7f28000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xe7f28000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <48 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		gpio@ffe7f34000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xe7f34000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			portc: gpio-controller@0 {
+			gpio2: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
 				ngpios = <32>;
+				gpio-ranges = <&padctrl0_apsys 0 0 32>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
@@ -212,17 +547,18 @@ portc: gpio-controller@0 {
 			};
 		};
 
-		gpio3: gpio@ffe7f38000 {
+		gpio@ffe7f38000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xe7f38000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			portd: gpio-controller@0 {
+			gpio3: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
-				ngpios = <32>;
+				ngpios = <23>;
+				gpio-ranges = <&padctrl0_apsys 0 32 23>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
@@ -230,17 +566,34 @@ portd: gpio-controller@0 {
 			};
 		};
 
-		gpio0: gpio@ffec005000 {
+		padctrl1_apsys: pinctrl@ffe7f3c000 {
+			compatible = "thead,th1520-group2-pinctrl";
+			reg = <0xff 0xe7f3c000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+		};
+
+		gmac0_apb: syscon@ffec003000 {
+			compatible = "thead,th1520-gmac-apb", "syscon";
+			reg = <0xff 0xec003000 0x0 0x1000>;
+		};
+
+		gmac1_apb: syscon@ffec004000 {
+			compatible = "thead,th1520-gmac-apb", "syscon";
+			reg = <0xff 0xec004000 0x0 0x1000>;
+		};
+
+		gpio@ffec005000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xec005000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			porta: gpio-controller@0 {
+			gpio0: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
 				ngpios = <32>;
+				gpio-ranges = <&padctrl1_apsys 0 0 32>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
@@ -248,17 +601,18 @@ porta: gpio-controller@0 {
 			};
 		};
 
-		gpio1: gpio@ffec006000 {
+		gpio@ffec006000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xec006000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			portb: gpio-controller@0 {
+			gpio1: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
-				ngpios = <32>;
+				ngpios = <31>;
+				gpio-ranges = <&padctrl1_apsys 0 32 31>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
@@ -266,6 +620,22 @@ portb: gpio-controller@0 {
 			};
 		};
 
+		padctrl0_apsys: pinctrl@ffec007000 {
+			compatible = "thead,th1520-group3-pinctrl";
+			reg = <0xff 0xec007000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+		};
+
+		i2c2: i2c@ffec00c000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xec00c000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <46 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
 		uart2: serial@ffec010000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0xff 0xec010000 0x0 0x4000>;
@@ -276,6 +646,88 @@ uart2: serial@ffec010000 {
 			status = "disabled";
 		};
 
+		i2c3: i2c@ffec014000 {
+			compatible = "snps,designware-i2c";
+			reg = <0xff 0xec014000 0x0 0x1000>;
+			clocks = <&apb_clk>;
+			interrupts = <47 IRQ_TYPE_LEVEL_HIGH>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		pwm: pwm@ffec01c000 {
+			compatible = "thead,th1520-pwm";
+			reg = <0xff 0xec01c000 0x0 0x4000>;
+			#pwm-cells = <3>;
+			clocks = <&osc_24m>;
+		};
+
+		audio_mbox: audio_mbox@0xffefc48000 {
+			compatible = "thead,light-audio-mbox-reg", "syscon";
+			reg = <0xff 0xefc48000 0x0 0x1000>;
+			status = "okay";
+		};
+
+		mbox_910t_client1: mbox_910t_client1 {
+			compatible = "thead,light-mbox-client";
+			mbox-names = "902";
+			mboxes = <&mbox_910t 1 0>;
+			status = "disabled";
+		};
+
+		mbox_910t_client2: mbox_910t_client2 {
+			compatible = "thead,light-mbox-client";
+			mbox-names = "906";
+			mboxes = <&mbox_910t 2 0>;
+			audio-mbox-regmap = <&audio_mbox>;
+			status = "okay";
+		};
+
+		clk: clock-controller@ffef010000 {
+			compatible = "thead,light-fm-ree-clk";
+			reg = <0xff 0xef010000 0x0 0x1000>;
+			#clock-cells = <1>;
+			clocks = <&osc_32k>, <&osc_24m>, <&rc_24m>;
+			clock-names = "osc_32k", "osc_24m", "rc_24m";
+			status = "okay";
+		};
+
+		rst: reset-controller@ffef014000 {
+			compatible = "thead,th1520-reset", "syscon";
+			reg = <0xff 0xef014000 0x0 0x1000>;
+			#reset-cells = <1>;
+		};
+
+		sys_reg: sys_reg@ffef010100 {
+			compatible = "thead,light_sys_reg";
+			reg = <0xff 0xef010100 0x0 0x100>;
+			status = "okay";
+		};
+
+		misc_sysreg: misc_sysreg@ffec02c000 {
+			compatible = "thead,th1520-misc-sysreg", "syscon";
+			reg = <0xff 0xec02c000 0x0 0x1000>;
+		};
+
+		usb: usb@ffec03f000 {
+			compatible = "thead,th1520-usb";
+			reg = <0xff 0xec03f000 0x0 0x1000>;
+			thead,misc-sysreg = <&misc_sysreg>;
+			#address-cells = <2>;
+			#size-cells = <2>;
+			ranges;
+
+			usb_dwc3: usb@ffe7040000 {
+				compatible = "snps,dwc3";
+				reg = <0xff 0xe7040000 0x0 0x10000>;
+				interrupts = <68 IRQ_TYPE_LEVEL_HIGH>;
+				dr_mode = "host";
+				snps,usb3_lpm_capable;
+				status = "disabled";
+			};
+		};
+
 		dmac0: dma-controller@ffefc00000 {
 			compatible = "snps,axi-dma-1.01a";
 			reg = <0xff 0xefc00000 0x0 0x1000>;
@@ -292,6 +744,33 @@ dmac0: dma-controller@ffefc00000 {
 			status = "disabled";
 		};
 
+		emmc: mmc@ffe7080000 {
+			compatible = "thead,th1520-dwcmshc";
+			reg = <0xff 0xe7080000 0x0 0x10000>;
+			interrupts = <62 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&sdhci_clk>;
+			clock-names = "core";
+			status = "disabled";
+		};
+
+		sdio0: mmc@ffe7090000 {
+			compatible = "thead,th1520-dwcmshc";
+			reg = <0xff 0xe7090000 0x0 0x10000>;
+			interrupts = <64 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&sdhci_clk>;
+			clock-names = "core";
+			status = "disabled";
+		};
+
+		sdio1: mmc@ffe70a0000 {
+			compatible = "thead,th1520-dwcmshc";
+			reg = <0xff 0xe70a0000 0x0 0x10000>;
+			interrupts = <71 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&sdhci_clk>;
+			clock-names = "core";
+			status = "disabled";
+		};
+
 		timer0: timer@ffefc32000 {
 			compatible = "snps,dw-apb-timer";
 			reg = <0xff 0xefc32000 0x0 0x14>;
@@ -384,17 +863,18 @@ timer7: timer@ffffc3303c {
 			status = "disabled";
 		};
 
-		ao_gpio0: gpio@fffff41000 {
+		gpio@fffff41000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xfff41000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			porte: gpio-controller@0 {
+			aogpio: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
-				ngpios = <32>;
+				ngpios = <16>;
+				gpio-ranges = <&padctrl_aosys 0 9 16>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
@@ -402,22 +882,77 @@ porte: gpio-controller@0 {
 			};
 		};
 
-		ao_gpio1: gpio@fffff52000 {
+		padctrl_aosys: pinctrl@fffff4a000 {
+			compatible = "thead,th1520-group1-pinctrl";
+			reg = <0xff 0xfff4a000 0x0 0x2000>;
+			clocks = <&aonsys_clk>;
+		};
+
+		pvt: pvt@fffff4e000 {
+			compatible = "moortec,mr75203";
+			reg = <0xff 0xfff4e000 0x0 0x80>,
+			      <0xff 0xfff4e080 0x0 0x100>,
+			      <0xff 0xfff4e180 0x0 0x680>,
+			      <0xff 0xfff4e800 0x0 0x600>;
+			reg-names = "common", "ts", "pd", "vm";
+			clocks = <&aonsys_clk>;
+			#thermal-sensor-cells = <1>;
+		};
+
+		gpio@fffff52000 {
 			compatible = "snps,dw-apb-gpio";
 			reg = <0xff 0xfff52000 0x0 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			portf: gpio-controller@0 {
+			gpio4: gpio-controller@0 {
 				compatible = "snps,dw-apb-gpio-port";
 				gpio-controller;
 				#gpio-cells = <2>;
-				ngpios = <32>;
+				ngpios = <23>;
+				gpio-ranges = <&padctrl_aosys 0 25 22>, <&padctrl_aosys 22 7 1>;
 				reg = <0>;
 				interrupt-controller;
 				#interrupt-cells = <2>;
 				interrupts = <55 IRQ_TYPE_LEVEL_HIGH>;
 			};
 		};
+		
+		mbox_910t: mbox@ffffc38000 {
+			compatible = "thead,light-mbox";
+			reg = <0xff 0xffc38000 0x0 0x4000>,
+				<0xff 0xffc44000 0x0 0x1000>,
+				<0xff 0xffc4c000 0x0 0x1000>,
+				<0xff 0xffc54000 0x0 0x1000>;
+			reg-names = "local_base", "remote_icu0", "remote_icu1", "remote_icu2";
+			#interrupt-cells = <2>;
+			interrupts = <28 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&apb_clk>;
+			clock-names = "ipg";
+			icu_cpu_id = <0>;
+			#mbox-cells = <2>;
+		};
+
+		watchdog0: watchdog@ffefc30000 {
+			compatible = "snps,dw-wdt";
+			reg = <0xff 0xefc30000 0x0 0x1000>;
+			interrupt-parent = <&plic>;
+			interrupts = <24>;
+			clocks = <&clk CLKGEN_WDT0_PCLK>;
+			clock-names = "tclk";
+			resets = <&rst TH1520_RESET_WDT0>; 
+			status = "okay";
+		};
+
+		watchdog1: watchdog@ffefc31000 {
+			compatible = "snps,dw-wdt";
+			reg = <0xff 0xefc31000 0x0 0x1000>;
+			interrupt-parent = <&plic>;
+			interrupts = <25>;
+			clocks = <&clk CLKGEN_WDT1_PCLK>;
+			clock-names = "tclk";
+			resets = <&rst TH1520_RESET_WDT1>; 
+			status = "okay";
+		};
 	};
 };
diff --git a/arch/riscv/configs/defconfig b/arch/riscv/configs/defconfig
index ab86ec3b9eab..b715550e3ed1 100644
--- a/arch/riscv/configs/defconfig
+++ b/arch/riscv/configs/defconfig
@@ -168,12 +168,15 @@ CONFIG_MMC=y
 CONFIG_MMC_SDHCI=y
 CONFIG_MMC_SDHCI_PLTFM=y
 CONFIG_MMC_SDHCI_CADENCE=y
+CONFIG_MMC_SDHCI_OF_DWCMSHC=y
 CONFIG_MMC_SPI=y
 CONFIG_MMC_SUNXI=y
 CONFIG_RTC_CLASS=y
 CONFIG_RTC_DRV_SUN6I=y
 CONFIG_DMADEVICES=y
 CONFIG_DMA_SUN6I=m
+CONFIG_DW_AXI_DMAC=y
+CONFIG_RZ_DMAC=y
 CONFIG_VIRTIO_PCI=y
 CONFIG_VIRTIO_BALLOON=y
 CONFIG_VIRTIO_INPUT=y
diff --git a/arch/riscv/configs/openeuler_defconfig b/arch/riscv/configs/openeuler_defconfig
index 026582613f2c..a948aadd1d6f 100644
--- a/arch/riscv/configs/openeuler_defconfig
+++ b/arch/riscv/configs/openeuler_defconfig
@@ -2,6 +2,7 @@
 # Automatically generated file; DO NOT EDIT.
 # Linux/riscv 6.6.0 Kernel Configuration
 #
+CONFIG_GCC_ASM_GOTO_OUTPUT_WORKAROUND=y
 CONFIG_IRQ_WORK=y
 CONFIG_BUILDTIME_TABLE_SORT=y
 CONFIG_THREAD_INFO_IN_TASK=y
@@ -148,7 +149,7 @@ CONFIG_GENERIC_SCHED_CLOCK=y
 
 CONFIG_ARCH_SUPPORTS_NUMA_BALANCING=y
 CONFIG_CC_IMPLICIT_FALLTHROUGH="-Wimplicit-fallthrough=5"
-CONFIG_GCC11_NO_ARRAY_BOUNDS=y
+CONFIG_GCC10_NO_ARRAY_BOUNDS=y
 CONFIG_CC_NO_ARRAY_BOUNDS=y
 CONFIG_ARCH_SUPPORTS_INT128=y
 CONFIG_NUMA_BALANCING=y
@@ -301,6 +302,7 @@ CONFIG_FIX_EARLYCON_MEM=y
 CONFIG_PGTABLE_LEVELS=5
 CONFIG_LOCKDEP_SUPPORT=y
 CONFIG_RISCV_DMA_NONCOHERENT=y
+CONFIG_RISCV_NONSTANDARD_CACHE_OPS=y
 
 #
 # SoC selection
@@ -309,6 +311,8 @@ CONFIG_RISCV_DMA_NONCOHERENT=y
 # CONFIG_ARCH_RENESAS is not set
 CONFIG_ARCH_SIFIVE=y
 CONFIG_SOC_SIFIVE=y
+CONFIG_ARCH_SOPHGO=y
+# CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC is not set
 CONFIG_ARCH_STARFIVE=y
 CONFIG_SOC_STARFIVE=y
 # CONFIG_ARCH_SUNXI is not set
@@ -343,17 +347,19 @@ CONFIG_SMP=y
 CONFIG_NR_CPUS=512
 CONFIG_HOTPLUG_CPU=y
 CONFIG_TUNE_GENERIC=y
+CONFIG_HIGHMEM=y
 CONFIG_NUMA=y
 CONFIG_NODES_SHIFT=7
 CONFIG_RISCV_ALTERNATIVE=y
 CONFIG_RISCV_ALTERNATIVE_EARLY=y
 CONFIG_RISCV_ISA_C=y
-CONFIG_RISCV_ISA_SVNAPOT=y
+# CONFIG_RISCV_ISA_SVNAPOT is not set
 CONFIG_RISCV_ISA_SVPBMT=y
 CONFIG_TOOLCHAIN_HAS_V=y
-CONFIG_RISCV_ISA_V=y
-CONFIG_RISCV_ISA_V_DEFAULT_ENABLE=y
-CONFIG_RISCV_ISA_ZICBOM=y
+# CONFIG_RISCV_ISA_V is not set
+CONFIG_TOOLCHAIN_HAS_ZBB=y
+CONFIG_RISCV_ISA_ZBB=y
+# CONFIG_RISCV_ISA_ZICBOM is not set
 CONFIG_RISCV_ISA_ZICBOZ=y
 CONFIG_TOOLCHAIN_HAS_ZIHINTPAUSE=y
 CONFIG_TOOLCHAIN_NEEDS_EXPLICIT_ZICSR_ZIFENCEI=y
@@ -471,6 +477,7 @@ CONFIG_CPU_FREQ_GOV_SCHEDUTIL=y
 #
 CONFIG_CPUFREQ_DT=y
 CONFIG_CPUFREQ_DT_PLATDEV=y
+CONFIG_RISCV_THEAD_LIGHT_CPUFREQ=y
 # end of CPU Frequency scaling
 # end of CPU Power Management
 
@@ -488,6 +495,19 @@ CONFIG_VIRTUALIZATION=y
 CONFIG_KVM=m
 CONFIG_ARCH_SUPPORTS_ACPI=y
 # CONFIG_ACPI is not set
+CONFIG_HAVE_LIVEPATCH_WO_FTRACE=y
+
+#
+# Enable Livepatch
+#
+CONFIG_LIVEPATCH=y
+CONFIG_LIVEPATCH_WO_FTRACE=y
+CONFIG_LIVEPATCH_STOP_MACHINE_CONSISTENCY=y
+CONFIG_LIVEPATCH_STACK=y
+CONFIG_LIVEPATCH_RESTRICT_KPROBE=y
+# end of Enable Livepatch
+
+CONFIG_CPU_MITIGATIONS=y
 
 #
 # General architecture-dependent options
@@ -576,7 +596,6 @@ CONFIG_HAVE_PREEMPT_DYNAMIC_KEY=y
 CONFIG_ARCH_WANT_LD_ORPHAN_WARN=y
 CONFIG_ARCH_SUPPORTS_DEBUG_PAGEALLOC=y
 CONFIG_ARCH_SUPPORTS_PAGE_TABLE_CHECK=y
-CONFIG_DYNAMIC_SIGFRAME=y
 
 #
 # GCOV-based kernel profiling
@@ -753,9 +772,9 @@ CONFIG_ZSMALLOC_CHAIN_SIZE=8
 # CONFIG_SLAB_DEPRECATED is not set
 CONFIG_SLUB=y
 # CONFIG_SLUB_TINY is not set
-CONFIG_SLAB_MERGE_DEFAULT=y
+# CONFIG_SLAB_MERGE_DEFAULT is not set
 CONFIG_SLAB_FREELIST_RANDOM=y
-# CONFIG_SLAB_FREELIST_HARDENED is not set
+CONFIG_SLAB_FREELIST_HARDENED=y
 # CONFIG_SLUB_STATS is not set
 CONFIG_SLUB_CPU_PARTIAL=y
 # CONFIG_RANDOM_KMALLOC_CACHES is not set
@@ -768,8 +787,9 @@ CONFIG_SPARSEMEM_MANUAL=y
 CONFIG_SPARSEMEM=y
 CONFIG_SPARSEMEM_EXTREME=y
 CONFIG_SPARSEMEM_VMEMMAP_ENABLE=y
-CONFIG_SPARSEMEM_VMEMMAP=y
+# CONFIG_SPARSEMEM_VMEMMAP is not set
 CONFIG_ARCH_WANT_OPTIMIZE_HUGETLB_VMEMMAP=y
+CONFIG_ARCH_KEEP_MEMBLOCK=y
 CONFIG_MEMORY_ISOLATION=y
 CONFIG_EXCLUSIVE_SYSTEM_RAM=y
 CONFIG_SPLIT_PTLOCK_CPUS=4
@@ -785,13 +805,15 @@ CONFIG_ARCH_ENABLE_THP_MIGRATION=y
 CONFIG_CONTIG_ALLOC=y
 CONFIG_PCP_BATCH_SCALE_MAX=5
 CONFIG_PHYS_ADDR_T_64BIT=y
+CONFIG_BOUNCE=y
 CONFIG_MMU_NOTIFIER=y
 CONFIG_KSM=y
 CONFIG_DEFAULT_MMAP_MIN_ADDR=4096
+CONFIG_ARCH_WANT_GENERAL_HUGETLB=y
 CONFIG_ARCH_WANTS_THP_SWAP=y
 CONFIG_TRANSPARENT_HUGEPAGE=y
-CONFIG_TRANSPARENT_HUGEPAGE_ALWAYS=y
-# CONFIG_TRANSPARENT_HUGEPAGE_MADVISE is not set
+# CONFIG_TRANSPARENT_HUGEPAGE_ALWAYS is not set
+CONFIG_TRANSPARENT_HUGEPAGE_MADVISE=y
 CONFIG_THP_SWAP=y
 # CONFIG_READ_ONLY_THP_FOR_FS is not set
 CONFIG_NEED_PER_CPU_EMBED_FIRST_CHUNK=y
@@ -808,19 +830,19 @@ CONFIG_IDLE_PAGE_TRACKING=y
 CONFIG_ARCH_HAS_CURRENT_STACK_POINTER=y
 CONFIG_ZONE_DMA32=y
 CONFIG_HMM_MIRROR=y
+CONFIG_GET_FREE_REGION=y
 CONFIG_VM_EVENT_COUNTERS=y
 # CONFIG_PERCPU_STATS is not set
 # CONFIG_GUP_TEST is not set
 # CONFIG_DMAPOOL_TEST is not set
 CONFIG_ARCH_HAS_PTE_SPECIAL=y
+CONFIG_KMAP_LOCAL=y
 CONFIG_MEMFD_CREATE=y
 CONFIG_SECRETMEM=y
 # CONFIG_ANON_VMA_NAME is not set
 CONFIG_USERFAULTFD=y
 CONFIG_HAVE_ARCH_USERFAULTFD_MINOR=y
-CONFIG_LRU_GEN=y
-CONFIG_LRU_GEN_ENABLED=y
-# CONFIG_LRU_GEN_STATS is not set
+# CONFIG_LRU_GEN is not set
 CONFIG_ARCH_SUPPORTS_PER_VMA_LOCK=y
 CONFIG_PER_VMA_LOCK=y
 CONFIG_LOCK_MM_AND_FIND_VMA=y
@@ -1585,6 +1607,7 @@ CONFIG_PCIEPORTBUS=y
 CONFIG_HOTPLUG_PCI_PCIE=y
 CONFIG_PCIEAER=y
 CONFIG_PCIEAER_INJECT=m
+CONFIG_PCIEAER_CXL=y
 CONFIG_PCIE_ECRC=y
 CONFIG_PCIEASPM=y
 CONFIG_PCIEASPM_DEFAULT=y
@@ -1601,6 +1624,7 @@ CONFIG_PCI_QUIRKS=y
 CONFIG_PCI_STUB=y
 # CONFIG_PCI_PF_STUB is not set
 CONFIG_PCI_ATS=y
+CONFIG_PCI_DOE=y
 CONFIG_PCI_ECAM=y
 CONFIG_PCI_IOV=y
 CONFIG_PCI_PRI=y
@@ -1635,6 +1659,7 @@ CONFIG_PCIE_CADENCE_EP=y
 CONFIG_PCIE_CADENCE_PLAT=y
 CONFIG_PCIE_CADENCE_PLAT_HOST=y
 CONFIG_PCIE_CADENCE_PLAT_EP=y
+CONFIG_PCIE_CADENCE_SOPHGO=y
 CONFIG_PCI_J721E=y
 CONFIG_PCI_J721E_HOST=y
 # CONFIG_PCI_J721E_EP is not set
@@ -1674,7 +1699,16 @@ CONFIG_PCI_ENDPOINT_CONFIGFS=y
 # CONFIG_PCI_SW_SWITCHTEC is not set
 # end of PCI switch controller drivers
 
-# CONFIG_CXL_BUS is not set
+CONFIG_CXL_BUS=y
+CONFIG_CXL_PCI=y
+# CONFIG_CXL_MEM_RAW_COMMANDS is not set
+CONFIG_CXL_PMEM=m
+CONFIG_CXL_MEM=y
+CONFIG_CXL_PORT=y
+CONFIG_CXL_SUSPEND=y
+CONFIG_CXL_REGION=y
+# CONFIG_CXL_REGION_INVALIDATION_TEST is not set
+CONFIG_CXL_PMU=y
 # CONFIG_PCCARD is not set
 # CONFIG_RAPIDIO is not set
 
@@ -1694,11 +1728,13 @@ CONFIG_PREVENT_FIRMWARE_BUILD=y
 #
 CONFIG_FW_LOADER=y
 CONFIG_FW_LOADER_DEBUG=y
+CONFIG_FW_LOADER_PAGED_BUF=y
+CONFIG_FW_LOADER_SYSFS=y
 CONFIG_EXTRA_FIRMWARE=""
 # CONFIG_FW_LOADER_USER_HELPER is not set
 # CONFIG_FW_LOADER_COMPRESS is not set
 CONFIG_FW_CACHE=y
-# CONFIG_FW_UPLOAD is not set
+CONFIG_FW_UPLOAD=y
 # end of Firmware loader
 
 CONFIG_WANT_DEV_COREDUMP=y
@@ -1709,7 +1745,7 @@ CONFIG_WANT_DEV_COREDUMP=y
 # CONFIG_TEST_ASYNC_DRIVER_PROBE is not set
 CONFIG_GENERIC_CPU_DEVICES=y
 CONFIG_REGMAP=y
-CONFIG_REGMAP_I2C=m
+CONFIG_REGMAP_I2C=y
 CONFIG_REGMAP_SPI=m
 CONFIG_REGMAP_MMIO=y
 CONFIG_DMA_SHARED_BUFFER=y
@@ -1774,6 +1810,9 @@ CONFIG_EFI_EARLYCON=y
 # Tegra firmware driver
 #
 # end of Tegra firmware driver
+
+CONFIG_LIGHT_AON=y
+CONFIG_LIGHT_AON_PD=y
 # end of Firmware Drivers
 
 # CONFIG_GNSS is not set
@@ -1899,6 +1938,7 @@ CONFIG_MTD_SPI_NOR_USE_4K_SECTORS=y
 # CONFIG_MTD_SPI_NOR_SWP_DISABLE is not set
 CONFIG_MTD_SPI_NOR_SWP_DISABLE_ON_VOLATILE=y
 # CONFIG_MTD_SPI_NOR_SWP_KEEP is not set
+CONFIG_SPI_SOPHGO_SPIFMC=m
 CONFIG_MTD_UBI=m
 CONFIG_MTD_UBI_WL_THRESHOLD=4096
 CONFIG_MTD_UBI_BEB_LIMIT=20
@@ -2277,7 +2317,6 @@ CONFIG_DM_THIN_PROVISIONING=m
 CONFIG_DM_CACHE=m
 CONFIG_DM_CACHE_SMQ=m
 # CONFIG_DM_WRITECACHE is not set
-# CONFIG_DM_EBS is not set
 CONFIG_DM_ERA=m
 # CONFIG_DM_CLONE is not set
 CONFIG_DM_MIRROR=m
@@ -2365,6 +2404,7 @@ CONFIG_VSOCKMON=m
 CONFIG_ETHERNET=y
 CONFIG_MDIO=m
 # CONFIG_NET_VENDOR_3COM is not set
+# CONFIG_NET_VENDOR_3SNIC is not set
 # CONFIG_NET_VENDOR_ADAPTEC is not set
 # CONFIG_NET_VENDOR_AGERE is not set
 CONFIG_NET_VENDOR_ALACRITECH=y
@@ -2441,6 +2481,7 @@ CONFIG_NET_VENDOR_FUNGIBLE=y
 # CONFIG_FUN_ETH is not set
 CONFIG_NET_VENDOR_GOOGLE=y
 CONFIG_NET_VENDOR_HUAWEI=y
+# CONFIG_BMA is not set
 # CONFIG_NET_VENDOR_I825XX is not set
 CONFIG_NET_VENDOR_INTEL=y
 # CONFIG_E100 is not set
@@ -2465,6 +2506,10 @@ CONFIG_FM10K=m
 # CONFIG_IGC is not set
 CONFIG_NET_VENDOR_MUCSE=y
 # CONFIG_MXGBE is not set
+# CONFIG_MXGBEVF is not set
+# CONFIG_MXGBEM is not set
+# CONFIG_MGBE is not set
+# CONFIG_MGBEVF is not set
 # CONFIG_JME is not set
 CONFIG_NET_VENDOR_ADI=y
 # CONFIG_ADIN1110 is not set
@@ -2569,7 +2614,16 @@ CONFIG_EPIC100=m
 CONFIG_SMSC911X=m
 CONFIG_SMSC9420=m
 # CONFIG_NET_VENDOR_SOCIONEXT is not set
-# CONFIG_NET_VENDOR_STMICRO is not set
+CONFIG_NET_VENDOR_STMICRO=y
+CONFIG_STMMAC_ETH=m
+# CONFIG_STMMAC_SELFTESTS is not set
+CONFIG_STMMAC_PLATFORM=m
+# CONFIG_DWMAC_DWC_QOS_ETH is not set
+CONFIG_DWMAC_GENERIC=m
+CONFIG_DWMAC_STARFIVE=m
+CONFIG_DWMAC_THEAD=m
+# CONFIG_DWMAC_INTEL_PLAT is not set
+# CONFIG_STMMAC_PCI is not set
 # CONFIG_NET_VENDOR_SUN is not set
 # CONFIG_NET_VENDOR_SYNOPSYS is not set
 # CONFIG_NET_VENDOR_TEHUTI is not set
@@ -2583,6 +2637,8 @@ CONFIG_NGBE=m
 CONFIG_TXGBE=m
 # CONFIG_NET_VENDOR_WIZNET is not set
 # CONFIG_NET_VENDOR_XILINX is not set
+CONFIG_NET_VENDOR_BZWX=y
+# CONFIG_NCE is not set
 # CONFIG_FDDI is not set
 # CONFIG_HIPPI is not set
 CONFIG_PHYLINK=y
@@ -3366,6 +3422,7 @@ CONFIG_GENERIC_PINCONF=y
 # CONFIG_PINCTRL_SINGLE is not set
 # CONFIG_PINCTRL_STMFX is not set
 # CONFIG_PINCTRL_SX150X is not set
+CONFIG_PINCTRL_TH1520=y
 
 #
 # Renesas pinctrl drivers
@@ -3416,7 +3473,8 @@ CONFIG_GPIO_SIFIVE=y
 # CONFIG_GPIO_GW_PLD is not set
 # CONFIG_GPIO_MAX7300 is not set
 # CONFIG_GPIO_MAX732X is not set
-# CONFIG_GPIO_PCA953X is not set
+CONFIG_GPIO_PCA953X=y
+CONFIG_GPIO_PCA953X_IRQ=y
 # CONFIG_GPIO_PCA9570 is not set
 # CONFIG_GPIO_PCF857X is not set
 # CONFIG_GPIO_TPIC2810 is not set
@@ -3599,7 +3657,7 @@ CONFIG_SENSORS_MAX31790=m
 CONFIG_SENSORS_MCP3021=m
 # CONFIG_SENSORS_TC654 is not set
 # CONFIG_SENSORS_TPS23861 is not set
-# CONFIG_SENSORS_MR75203 is not set
+CONFIG_SENSORS_MR75203=m
 CONFIG_SENSORS_ADCXX=m
 CONFIG_SENSORS_LM63=m
 CONFIG_SENSORS_LM70=m
@@ -3777,6 +3835,7 @@ CONFIG_ALIM7101_WDT=m
 CONFIG_I6300ESB_WDT=m
 # CONFIG_MEN_A21_WDT is not set
 CONFIG_STARFIVE_WATCHDOG=y
+CONFIG_LIGHT_PMIC_WATCHDOG=y
 
 #
 # PCI-based Watchdog Cards
@@ -3877,7 +3936,6 @@ CONFIG_MFD_CORE=m
 # CONFIG_MFD_SKY81452 is not set
 # CONFIG_MFD_STMPE is not set
 CONFIG_MFD_SYSCON=y
-# CONFIG_MFD_TI_AM335X_TSCADC is not set
 # CONFIG_MFD_LP3943 is not set
 # CONFIG_MFD_LP8788 is not set
 # CONFIG_MFD_TI_LMU is not set
@@ -3998,6 +4056,7 @@ CONFIG_REGULATOR_PWM=y
 # CONFIG_REGULATOR_TPS65132 is not set
 # CONFIG_REGULATOR_TPS6524X is not set
 # CONFIG_REGULATOR_VCTRL is not set
+CONFIG_REGULATOR_LIGHT_AON=y
 # CONFIG_RC_CORE is not set
 
 #
@@ -5357,8 +5416,29 @@ CONFIG_USB_MICROTEK=m
 # USB dual-mode controller drivers
 #
 # CONFIG_USB_CDNS_SUPPORT is not set
-# CONFIG_USB_MUSB_HDRC is not set
-# CONFIG_USB_DWC3 is not set
+CONFIG_USB_MUSB_HDRC=y
+CONFIG_USB_MUSB_HOST=y
+
+#
+# Platform Glue Layer
+#
+
+#
+# MUSB DMA mode
+#
+# CONFIG_MUSB_PIO_ONLY is not set
+CONFIG_USB_DWC3=m
+# CONFIG_USB_DWC3_ULPI is not set
+# CONFIG_USB_DWC3_HOST is not set
+# CONFIG_USB_DWC3_GADGET is not set
+CONFIG_USB_DWC3_DUAL_ROLE=y
+
+#
+# Platform Glue Driver Support
+#
+CONFIG_USB_DWC3_HAPS=m
+CONFIG_USB_DWC3_OF_SIMPLE=m
+CONFIG_USB_DWC3_THEAD=m
 # CONFIG_USB_DWC2 is not set
 # CONFIG_USB_CHIPIDEA is not set
 # CONFIG_USB_ISP1760 is not set
@@ -5450,7 +5530,7 @@ CONFIG_USB_HSIC_USB3503=m
 # CONFIG_USB_HSIC_USB4604 is not set
 # CONFIG_USB_LINK_LAYER_TEST is not set
 CONFIG_USB_CHAOSKEY=m
-# CONFIG_USB_ONBOARD_HUB is not set
+CONFIG_USB_ONBOARD_HUB=m
 CONFIG_USB_ATM=m
 # CONFIG_USB_SPEEDTOUCH is not set
 CONFIG_USB_CXACRU=m
@@ -5465,7 +5545,59 @@ CONFIG_USB_XUSBATM=m
 # CONFIG_USB_ISP1301 is not set
 # end of USB Physical Layer drivers
 
-# CONFIG_USB_GADGET is not set
+CONFIG_USB_GADGET=m
+# CONFIG_USB_GADGET_DEBUG is not set
+# CONFIG_USB_GADGET_DEBUG_FILES is not set
+# CONFIG_USB_GADGET_DEBUG_FS is not set
+CONFIG_USB_GADGET_VBUS_DRAW=2
+CONFIG_USB_GADGET_STORAGE_NUM_BUFFERS=2
+
+#
+# USB Peripheral Controller
+#
+# CONFIG_USB_GR_UDC is not set
+# CONFIG_USB_R8A66597 is not set
+# CONFIG_USB_PXA27X is not set
+# CONFIG_USB_MV_UDC is not set
+# CONFIG_USB_MV_U3D is not set
+# CONFIG_USB_SNP_UDC_PLAT is not set
+# CONFIG_USB_M66592 is not set
+# CONFIG_USB_BDC_UDC is not set
+# CONFIG_USB_AMD5536UDC is not set
+# CONFIG_USB_NET2272 is not set
+# CONFIG_USB_NET2280 is not set
+# CONFIG_USB_GOKU is not set
+# CONFIG_USB_EG20T is not set
+# CONFIG_USB_GADGET_XILINX is not set
+# CONFIG_USB_MAX3420_UDC is not set
+# CONFIG_USB_DUMMY_HCD is not set
+# end of USB Peripheral Controller
+
+# CONFIG_USB_CONFIGFS is not set
+
+#
+# USB Gadget precomposed configurations
+#
+# CONFIG_USB_ZERO is not set
+# CONFIG_USB_AUDIO is not set
+# CONFIG_USB_ETH is not set
+# CONFIG_USB_G_NCM is not set
+# CONFIG_USB_GADGETFS is not set
+# CONFIG_USB_FUNCTIONFS is not set
+# CONFIG_USB_MASS_STORAGE is not set
+# CONFIG_USB_GADGET_TARGET is not set
+# CONFIG_USB_G_SERIAL is not set
+# CONFIG_USB_MIDI_GADGET is not set
+# CONFIG_USB_G_PRINTER is not set
+# CONFIG_USB_CDC_COMPOSITE is not set
+# CONFIG_USB_G_ACM_MS is not set
+# CONFIG_USB_G_MULTI is not set
+# CONFIG_USB_G_HID is not set
+# CONFIG_USB_G_DBGP is not set
+# CONFIG_USB_G_WEBCAM is not set
+# CONFIG_USB_RAW_GADGET is not set
+# end of USB Gadget precomposed configurations
+
 CONFIG_TYPEC=m
 CONFIG_TYPEC_TCPM=m
 CONFIG_TYPEC_TCPCI=m
@@ -5520,12 +5652,13 @@ CONFIG_MMC_RICOH_MMC=y
 CONFIG_MMC_SDHCI_PLTFM=y
 # CONFIG_MMC_SDHCI_OF_ARASAN is not set
 # CONFIG_MMC_SDHCI_OF_AT91 is not set
-# CONFIG_MMC_SDHCI_OF_DWCMSHC is not set
+CONFIG_MMC_SDHCI_OF_DWCMSHC=y
 CONFIG_MMC_SDHCI_CADENCE=y
 # CONFIG_MMC_SDHCI_F_SDH30 is not set
 # CONFIG_MMC_SDHCI_MILBEAUT is not set
 CONFIG_MMC_TIFM_SD=m
 CONFIG_MMC_SPI=y
+CONFIG_MMC_SDHCI_SOPHGO=y
 CONFIG_MMC_CB710=m
 CONFIG_MMC_VIA_SDMMC=m
 CONFIG_MMC_DW=m
@@ -5546,8 +5679,6 @@ CONFIG_MMC_HSQ=m
 CONFIG_MMC_TOSHIBA_PCI=m
 CONFIG_MMC_MTK=m
 CONFIG_MMC_SDHCI_XENON=m
-# CONFIG_MMC_SDHCI_OMAP is not set
-# CONFIG_MMC_SDHCI_AM654 is not set
 # CONFIG_SCSI_UFSHCD is not set
 CONFIG_MEMSTICK=m
 # CONFIG_MEMSTICK_DEBUG is not set
@@ -5670,7 +5801,6 @@ CONFIG_INFINIBAND_USER_MEM=y
 CONFIG_INFINIBAND_ON_DEMAND_PAGING=y
 CONFIG_INFINIBAND_ADDR_TRANS=y
 CONFIG_INFINIBAND_ADDR_TRANS_CONFIGFS=y
-CONFIG_INFINIBAND_VIRT_DMA=y
 CONFIG_INFINIBAND_BNXT_RE=m
 CONFIG_INFINIBAND_CXGB4=m
 # CONFIG_INFINIBAND_EFA is not set
@@ -5681,8 +5811,6 @@ CONFIG_MLX5_INFINIBAND=m
 # CONFIG_INFINIBAND_MTHCA is not set
 # CONFIG_INFINIBAND_OCRDMA is not set
 CONFIG_INFINIBAND_QEDR=m
-CONFIG_RDMA_RXE=m
-# CONFIG_RDMA_SIW is not set
 CONFIG_INFINIBAND_IPOIB=m
 CONFIG_INFINIBAND_IPOIB_CM=y
 # CONFIG_INFINIBAND_IPOIB_DEBUG is not set
@@ -5817,6 +5945,7 @@ CONFIG_RTC_DRV_RP5C01=m
 # HID Sensor RTC drivers
 #
 CONFIG_RTC_DRV_GOLDFISH=y
+# CONFIG_RTC_DRV_ASTBMC is not set
 CONFIG_DMADEVICES=y
 # CONFIG_DMADEVICES_DEBUG is not set
 
@@ -5824,10 +5953,11 @@ CONFIG_DMADEVICES=y
 # DMA Devices
 #
 CONFIG_DMA_ENGINE=y
+CONFIG_DMA_VIRTUAL_CHANNELS=y
 CONFIG_DMA_OF=y
 # CONFIG_ALTERA_MSGDMA is not set
 # CONFIG_AMBA_PL08X is not set
-# CONFIG_DW_AXI_DMAC is not set
+CONFIG_DW_AXI_DMAC=y
 # CONFIG_FSL_EDMA is not set
 # CONFIG_INTEL_IDMA64 is not set
 # CONFIG_PL330_DMA is not set
@@ -5959,6 +6089,9 @@ CONFIG_CLK_STARFIVE_JH7110_ISP=m
 CONFIG_CLK_STARFIVE_JH7110_VOUT=m
 # CONFIG_XILINX_VCU is not set
 # CONFIG_COMMON_CLK_XLNX_CLKWZRD is not set
+CONFIG_THEAD_CLK=y
+# CONFIG_CLK_LIGHT_MPW is not set
+CONFIG_CLK_LIGHT_FM=y
 CONFIG_HWSPINLOCK=y
 
 #
@@ -5966,6 +6099,8 @@ CONFIG_HWSPINLOCK=y
 #
 CONFIG_TIMER_OF=y
 CONFIG_TIMER_PROBE=y
+CONFIG_DW_APB_TIMER=y
+CONFIG_DW_APB_TIMER_OF=y
 CONFIG_RISCV_TIMER=y
 # end of Clock Source drivers
 
@@ -5976,6 +6111,7 @@ CONFIG_MAILBOX=y
 # CONFIG_PL320_MBOX is not set
 # CONFIG_ALTERA_MBOX is not set
 # CONFIG_MAILBOX_TEST is not set
+CONFIG_THEAD_LIGHT_MBOX=y
 CONFIG_IOMMU_API=y
 CONFIG_IOMMU_SUPPORT=y
 
@@ -6005,6 +6141,7 @@ CONFIG_RPMSG_CHAR=y
 CONFIG_RPMSG_CTRL=y
 CONFIG_RPMSG_NS=y
 # CONFIG_RPMSG_QCOM_GLINK_RPM is not set
+CONFIG_RPMSG_THEAD_LIGHT=y
 CONFIG_RPMSG_VIRTIO=y
 # end of Rpmsg drivers
 
@@ -6061,6 +6198,12 @@ CONFIG_JH71XX_PMU=y
 # Xilinx SoC drivers
 #
 # end of Xilinx SoC drivers
+
+#
+# Thead SoC drivers
+#
+CONFIG_LIGHT_REBOOTMODE=y
+# end of Thead SoC drivers
 # end of SOC (System On Chip) specific Drivers
 
 # CONFIG_PM_DEVFREQ is not set
@@ -6089,6 +6232,7 @@ CONFIG_PWM_SYSFS=y
 # CONFIG_PWM_FSL_FTM is not set
 # CONFIG_PWM_PCA9685 is not set
 CONFIG_PWM_SIFIVE=m
+CONFIG_PWM_THEAD=m
 # CONFIG_PWM_XILINX is not set
 
 #
@@ -6104,6 +6248,7 @@ CONFIG_SIFIVE_PLIC=y
 # CONFIG_IPACK_BUS is not set
 CONFIG_RESET_CONTROLLER=y
 CONFIG_RESET_SIMPLE=y
+CONFIG_RESET_TH1520=y
 # CONFIG_RESET_TI_SYSCON is not set
 # CONFIG_RESET_TI_TPS380X is not set
 CONFIG_RESET_STARFIVE_JH71X0=y
@@ -6178,6 +6323,7 @@ CONFIG_NVDIMM_KEYS=y
 # CONFIG_NVDIMM_SECURITY_TEST is not set
 CONFIG_DAX=y
 CONFIG_DEV_DAX=m
+CONFIG_DEV_DAX_CXL=m
 CONFIG_NVMEM=y
 CONFIG_NVMEM_SYSFS=y
 
@@ -6362,8 +6508,6 @@ CONFIG_TMPFS_XATTR=y
 CONFIG_ARCH_SUPPORTS_HUGETLBFS=y
 CONFIG_HUGETLBFS=y
 CONFIG_HUGETLB_PAGE=y
-CONFIG_HUGETLB_PAGE_OPTIMIZE_VMEMMAP=y
-# CONFIG_HUGETLB_PAGE_OPTIMIZE_VMEMMAP_DEFAULT_ON is not set
 # CONFIG_HUGETLB_ALLOC_LIMIT is not set
 CONFIG_ARCH_HAS_GIGANTIC_PAGE=y
 CONFIG_CONFIGFS_FS=y
@@ -6652,6 +6796,8 @@ CONFIG_LSM="lockdown,yama,loadpin,safesetid,integrity,selinux,smack,tomoyo,appar
 # Memory initialization
 #
 CONFIG_INIT_STACK_NONE=y
+# CONFIG_INIT_STACK_ALL_PATTERN is not set
+# CONFIG_INIT_STACK_ALL_ZERO is not set
 # CONFIG_INIT_ON_ALLOC_DEFAULT_ON is not set
 # CONFIG_INIT_ON_FREE_DEFAULT_ON is not set
 # CONFIG_ZERO_CALL_USED_REGS is not set
@@ -6866,6 +7012,7 @@ CONFIG_CRYPTO_HW=y
 # CONFIG_CRYPTO_DEV_QAT_C3XXX is not set
 # CONFIG_CRYPTO_DEV_QAT_C62X is not set
 # CONFIG_CRYPTO_DEV_QAT_4XXX is not set
+# CONFIG_CRYPTO_DEV_QAT_420XX is not set
 # CONFIG_CRYPTO_DEV_QAT_DH895xCCVF is not set
 # CONFIG_CRYPTO_DEV_QAT_C3XXXVF is not set
 # CONFIG_CRYPTO_DEV_QAT_C62XVF is not set
@@ -7108,6 +7255,7 @@ CONFIG_DEBUG_INFO_DWARF_TOOLCHAIN_DEFAULT=y
 # CONFIG_DEBUG_INFO_REDUCED is not set
 CONFIG_DEBUG_INFO_COMPRESSED_NONE=y
 # CONFIG_DEBUG_INFO_COMPRESSED_ZLIB is not set
+# CONFIG_DEBUG_INFO_SPLIT is not set
 CONFIG_DEBUG_INFO_BTF=y
 CONFIG_PAHOLE_HAS_SPLIT_BTF=y
 CONFIG_PAHOLE_HAS_LANG_EXCLUDE=y
@@ -7190,16 +7338,14 @@ CONFIG_DEBUG_KMEMLEAK_AUTO_SCAN=y
 # CONFIG_DEBUG_STACK_USAGE is not set
 # CONFIG_SCHED_STACK_END_CHECK is not set
 CONFIG_ARCH_HAS_DEBUG_VM_PGTABLE=y
-CONFIG_DEBUG_VM_IRQSOFF=y
-CONFIG_DEBUG_VM=y
-# CONFIG_DEBUG_VM_MAPLE_TREE is not set
-# CONFIG_DEBUG_VM_RB is not set
-# CONFIG_DEBUG_VM_PGFLAGS is not set
+# CONFIG_DEBUG_VM is not set
 # CONFIG_DEBUG_VM_PGTABLE is not set
 CONFIG_ARCH_HAS_DEBUG_VIRTUAL=y
 # CONFIG_DEBUG_VIRTUAL is not set
 CONFIG_DEBUG_MEMORY_INIT=y
 CONFIG_DEBUG_PER_CPU_MAPS=y
+# CONFIG_DEBUG_KMAP_LOCAL is not set
+# CONFIG_DEBUG_HIGHMEM is not set
 CONFIG_HAVE_ARCH_KASAN=y
 CONFIG_HAVE_ARCH_KASAN_VMALLOC=y
 # CONFIG_KASAN is not set
@@ -7353,7 +7499,38 @@ CONFIG_RING_BUFFER_BENCHMARK=m
 # CONFIG_SYNTH_EVENT_GEN_TEST is not set
 # CONFIG_KPROBE_EVENT_GEN_TEST is not set
 # CONFIG_RV is not set
-# CONFIG_SAMPLES is not set
+CONFIG_SAMPLES=y
+# CONFIG_SAMPLE_AUXDISPLAY is not set
+# CONFIG_SAMPLE_TRACE_EVENTS is not set
+# CONFIG_SAMPLE_TRACE_CUSTOM_EVENTS is not set
+# CONFIG_SAMPLE_TRACE_PRINTK is not set
+# CONFIG_SAMPLE_FTRACE_OPS is not set
+# CONFIG_SAMPLE_TRACE_ARRAY is not set
+# CONFIG_SAMPLE_KOBJECT is not set
+# CONFIG_SAMPLE_KPROBES is not set
+# CONFIG_SAMPLE_KFIFO is not set
+# CONFIG_SAMPLE_KDB is not set
+# CONFIG_SAMPLE_RPMSG_CLIENT is not set
+CONFIG_SAMPLE_LIVEPATCH=m
+# CONFIG_SAMPLE_CONFIGFS is not set
+# CONFIG_SAMPLE_CONNECTOR is not set
+# CONFIG_SAMPLE_FANOTIFY_ERROR is not set
+# CONFIG_SAMPLE_HIDRAW is not set
+# CONFIG_SAMPLE_LANDLOCK is not set
+# CONFIG_SAMPLE_PIDFD is not set
+# CONFIG_SAMPLE_SECCOMP is not set
+# CONFIG_SAMPLE_TIMER is not set
+# CONFIG_SAMPLE_UHID is not set
+# CONFIG_SAMPLE_VFIO_MDEV_MTTY is not set
+# CONFIG_SAMPLE_VFIO_MDEV_MDPY is not set
+# CONFIG_SAMPLE_VFIO_MDEV_MDPY_FB is not set
+# CONFIG_SAMPLE_VFIO_MDEV_MBOCHS is not set
+# CONFIG_SAMPLE_ANDROID_BINDERFS is not set
+# CONFIG_SAMPLE_VFS is not set
+# CONFIG_SAMPLE_TPS6594_PFSM is not set
+# CONFIG_SAMPLE_WATCHDOG is not set
+# CONFIG_SAMPLE_WATCH_QUEUE is not set
+# CONFIG_SAMPLE_KMEMLEAK is not set
 CONFIG_STRICT_DEVMEM=y
 CONFIG_IO_STRICT_DEVMEM=y
 
@@ -7383,9 +7560,3 @@ CONFIG_ARCH_USE_MEMTEST=y
 # end of Kernel hacking
 
 # CONFIG_KWORKER_NUMA_AFFINITY is not set
-
-# enable openEuler livepatch
-CONFIG_LIVEPATCH=y
-CONFIG_LIVEPATCH_WO_FTRACE=y
-CONFIG_SAMPLES=y
-CONFIG_SAMPLE_LIVEPATCH=m
diff --git a/arch/riscv/errata/thead/errata.c b/arch/riscv/errata/thead/errata.c
index 0554ed4bf087..07c7ab6bcb4a 100644
--- a/arch/riscv/errata/thead/errata.c
+++ b/arch/riscv/errata/thead/errata.c
@@ -12,8 +12,10 @@
 #include <asm/alternative.h>
 #include <asm/cacheflush.h>
 #include <asm/cpufeature.h>
+#include <asm/dma-noncoherent.h>
 #include <asm/errata_list.h>
 #include <asm/hwprobe.h>
+#include <asm/io.h>
 #include <asm/patch.h>
 #include <asm/vendorid_list.h>
 
@@ -33,6 +35,69 @@ static bool errata_probe_pbmt(unsigned int stage,
 	return false;
 }
 
+/*
+ * th.dcache.ipa rs1 (invalidate, physical address)
+ * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
+ *   0000001    01010      rs1       000      00000  0001011
+ * th.dcache.iva rs1 (invalidate, virtual address)
+ *   0000001    00110      rs1       000      00000  0001011
+ *
+ * th.dcache.cpa rs1 (clean, physical address)
+ * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
+ *   0000001    01001      rs1       000      00000  0001011
+ * th.dcache.cva rs1 (clean, virtual address)
+ *   0000001    00101      rs1       000      00000  0001011
+ *
+ * th.dcache.cipa rs1 (clean then invalidate, physical address)
+ * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
+ *   0000001    01011      rs1       000      00000  0001011
+ * th.dcache.civa rs1 (clean then invalidate, virtual address)
+ *   0000001    00111      rs1       000      00000  0001011
+ *
+ * th.sync.s (make sure all cache operations finished)
+ * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
+ *   0000000    11001     00000      000      00000  0001011
+ */
+#define THEAD_INVAL_A0	".long 0x02a5000b"
+#define THEAD_CLEAN_A0	".long 0x0295000b"
+#define THEAD_FLUSH_A0	".long 0x02b5000b"
+#define THEAD_SYNC_S	".long 0x0190000b"
+
+#define THEAD_CMO_OP(_op, _start, _size, _cachesize)			\
+asm volatile("mv a0, %1\n\t"						\
+	     "j 2f\n\t"							\
+	     "3:\n\t"							\
+	     THEAD_##_op##_A0 "\n\t"					\
+	     "add a0, a0, %0\n\t"					\
+	     "2:\n\t"							\
+	     "bltu a0, %2, 3b\n\t"					\
+	     THEAD_SYNC_S						\
+	     : : "r"(_cachesize),					\
+		 "r"((unsigned long)(_start) & ~((_cachesize) - 1UL)),	\
+		 "r"((unsigned long)(_start) + (_size))			\
+	     : "a0")
+
+static void thead_errata_cache_inv(phys_addr_t paddr, size_t size)
+{
+	THEAD_CMO_OP(INVAL, paddr, size, riscv_cbom_block_size);
+}
+
+static void thead_errata_cache_wback(phys_addr_t paddr, size_t size)
+{
+	THEAD_CMO_OP(CLEAN, paddr, size, riscv_cbom_block_size);
+}
+
+static void thead_errata_cache_wback_inv(phys_addr_t paddr, size_t size)
+{
+	THEAD_CMO_OP(FLUSH, paddr, size, riscv_cbom_block_size);
+}
+
+static const struct riscv_nonstd_cache_ops thead_errata_cmo_ops = {
+	.wback = &thead_errata_cache_wback_inv,
+	.inv = &thead_errata_cache_inv,
+	.wback_inv = &thead_errata_cache_wback_inv,
+};
+
 static bool errata_probe_cmo(unsigned int stage,
 			     unsigned long arch_id, unsigned long impid)
 {
@@ -48,6 +113,7 @@ static bool errata_probe_cmo(unsigned int stage,
 	if (stage == RISCV_ALTERNATIVES_BOOT) {
 		riscv_cbom_block_size = L1_CACHE_BYTES;
 		riscv_noncoherent_supported();
+		riscv_noncoherent_register_cache_ops(&thead_errata_cmo_ops);
 	}
 
 	return true;
@@ -77,8 +143,7 @@ static u32 thead_errata_probe(unsigned int stage,
 	if (errata_probe_pbmt(stage, archid, impid))
 		cpu_req_errata |= BIT(ERRATA_THEAD_PBMT);
 
-	if (errata_probe_cmo(stage, archid, impid))
-		cpu_req_errata |= BIT(ERRATA_THEAD_CMO);
+	errata_probe_cmo(stage, archid, impid);
 
 	if (errata_probe_pmu(stage, archid, impid))
 		cpu_req_errata |= BIT(ERRATA_THEAD_PMU);
diff --git a/arch/riscv/include/asm/barrier.h b/arch/riscv/include/asm/barrier.h
index 110752594228..2b1f98b7e9bf 100644
--- a/arch/riscv/include/asm/barrier.h
+++ b/arch/riscv/include/asm/barrier.h
@@ -29,12 +29,22 @@
 #define __smp_rmb()	RISCV_FENCE(r,r)
 #define __smp_wmb()	RISCV_FENCE(w,w)
 
+#ifdef CONFIG_ARCH_SOPHGO
 #define __smp_store_release(p, v)					\
 do {									\
 	compiletime_assert_atomic_type(*p);				\
 	RISCV_FENCE(rw,w);						\
 	WRITE_ONCE(*p, v);						\
+	RISCV_FENCE(w,rw);						\
 } while (0)
+#else
+#define __smp_store_release(p, v)					\
+do {									\
+	compiletime_assert_atomic_type(*p);				\
+	RISCV_FENCE(rw,w);						\
+	WRITE_ONCE(*p, v);						\
+} while (0)
+#endif
 
 #define __smp_load_acquire(p)						\
 ({									\
@@ -44,6 +54,18 @@ do {									\
 	___p1;								\
 })
 
+#define smp_cond_load_acquire(ptr, cond_expr) ({			\
+	typeof(ptr) __PTR = (ptr);					\
+	__unqual_scalar_typeof(*ptr) VAL;				\
+	for (;;) {							\
+		VAL = __smp_load_acquire(__PTR);			\
+		if (cond_expr)						\
+			break;						\
+		cpu_relax();						\
+	}								\
+	(typeof(*ptr))VAL;						\
+})
+
 /*
  * This is a very specific barrier: it's currently only used in two places in
  * the kernel, both in the scheduler.  See include/linux/spinlock.h for the two
diff --git a/arch/riscv/include/asm/errata_list.h b/arch/riscv/include/asm/errata_list.h
index b55b434f0059..ea33288f8a25 100644
--- a/arch/riscv/include/asm/errata_list.h
+++ b/arch/riscv/include/asm/errata_list.h
@@ -24,9 +24,8 @@
 
 #ifdef CONFIG_ERRATA_THEAD
 #define	ERRATA_THEAD_PBMT 0
-#define	ERRATA_THEAD_CMO 1
-#define	ERRATA_THEAD_PMU 2
-#define	ERRATA_THEAD_NUMBER 3
+#define	ERRATA_THEAD_PMU 1
+#define	ERRATA_THEAD_NUMBER 2
 #endif
 
 #ifdef __ASSEMBLY__
@@ -94,54 +93,17 @@ asm volatile(ALTERNATIVE(						\
 #define ALT_THEAD_PMA(_val)
 #endif
 
-/*
- * dcache.ipa rs1 (invalidate, physical address)
- * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
- *   0000001    01010      rs1       000      00000  0001011
- * dache.iva rs1 (invalida, virtual address)
- *   0000001    00110      rs1       000      00000  0001011
- *
- * dcache.cpa rs1 (clean, physical address)
- * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
- *   0000001    01001      rs1       000      00000  0001011
- * dcache.cva rs1 (clean, virtual address)
- *   0000001    00101      rs1       000      00000  0001011
- *
- * dcache.cipa rs1 (clean then invalidate, physical address)
- * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
- *   0000001    01011      rs1       000      00000  0001011
- * dcache.civa rs1 (... virtual address)
- *   0000001    00111      rs1       000      00000  0001011
- *
- * sync.s (make sure all cache operations finished)
- * | 31 - 25 | 24 - 20 | 19 - 15 | 14 - 12 | 11 - 7 | 6 - 0 |
- *   0000000    11001     00000      000      00000  0001011
- */
-#define THEAD_inval_A0	".long 0x0265000b"
-#define THEAD_clean_A0	".long 0x0255000b"
-#define THEAD_flush_A0	".long 0x0275000b"
-#define THEAD_SYNC_S	".long 0x0190000b"
-
 #define ALT_CMO_OP(_op, _start, _size, _cachesize)			\
-asm volatile(ALTERNATIVE_2(						\
-	__nops(6),							\
+asm volatile(ALTERNATIVE(						\
+	__nops(5),							\
 	"mv a0, %1\n\t"							\
 	"j 2f\n\t"							\
 	"3:\n\t"							\
 	CBO_##_op(a0)							\
 	"add a0, a0, %0\n\t"						\
 	"2:\n\t"							\
-	"bltu a0, %2, 3b\n\t"						\
-	"nop", 0, RISCV_ISA_EXT_ZICBOM, CONFIG_RISCV_ISA_ZICBOM,	\
-	"mv a0, %1\n\t"							\
-	"j 2f\n\t"							\
-	"3:\n\t"							\
-	THEAD_##_op##_A0 "\n\t"						\
-	"add a0, a0, %0\n\t"						\
-	"2:\n\t"							\
-	"bltu a0, %2, 3b\n\t"						\
-	THEAD_SYNC_S, THEAD_VENDOR_ID,					\
-			ERRATA_THEAD_CMO, CONFIG_ERRATA_THEAD_CMO)	\
+	"bltu a0, %2, 3b\n\t",						\
+	0, RISCV_ISA_EXT_ZICBOM, CONFIG_RISCV_ISA_ZICBOM)		\
 	: : "r"(_cachesize),						\
 	    "r"((unsigned long)(_start) & ~((_cachesize) - 1UL)),	\
 	    "r"((unsigned long)(_start) + (_size))			\
diff --git a/arch/riscv/include/asm/fixmap.h b/arch/riscv/include/asm/fixmap.h
index 0a55099bb734..672bfe1121fe 100644
--- a/arch/riscv/include/asm/fixmap.h
+++ b/arch/riscv/include/asm/fixmap.h
@@ -10,6 +10,10 @@
 #include <linux/sizes.h>
 #include <linux/pgtable.h>
 #include <asm/page.h>
+#ifdef CONFIG_HIGHMEM
+#include <linux/threads.h>
+#include <asm/kmap_size.h>
+#endif
 
 #ifdef CONFIG_MMU
 /*
@@ -37,6 +41,10 @@ enum fixed_addresses {
 	FIX_TEXT_POKE1,
 	FIX_TEXT_POKE0,
 	FIX_EARLYCON_MEM_BASE,
+#ifdef CONFIG_HIGHMEM
+	FIX_KMAP_BEGIN,
+	FIX_KMAP_END = FIX_KMAP_BEGIN + (KM_MAX_IDX * NR_CPUS) - 1,
+#endif
 
 	__end_of_permanent_fixed_addresses,
 	/*
@@ -47,7 +55,12 @@ enum fixed_addresses {
 #define FIX_BTMAPS_SLOTS	7
 #define TOTAL_FIX_BTMAPS	(NR_FIX_BTMAPS * FIX_BTMAPS_SLOTS)
 
+#ifdef CONFIG_HIGHMEM
+	FIX_BTMAP_END = __ALIGN_MASK(__end_of_permanent_fixed_addresses,
+				     ((PMD_SIZE / PAGE_SIZE) - 1)) + 1,
+#else
 	FIX_BTMAP_END = __end_of_permanent_fixed_addresses,
+#endif
 	FIX_BTMAP_BEGIN = FIX_BTMAP_END + TOTAL_FIX_BTMAPS - 1,
 
 	__end_of_fixed_addresses
diff --git a/arch/riscv/include/asm/highmem.h b/arch/riscv/include/asm/highmem.h
new file mode 100644
index 000000000000..a36fc835b8ab
--- /dev/null
+++ b/arch/riscv/include/asm/highmem.h
@@ -0,0 +1,13 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+
+#ifndef _ASM_HIGHMEM_H
+#define _ASM_HIGHMEM_H
+
+#include <asm/kmap_size.h>
+#include <asm/pgtable.h>
+#include <asm/fixmap.h>
+
+#define flush_cache_kmaps() do {} while (0)
+
+extern pte_t *pkmap_page_table;
+#endif
diff --git a/arch/riscv/include/asm/io.h b/arch/riscv/include/asm/io.h
index 42497d487a17..bbdc3c7ed6ca 100644
--- a/arch/riscv/include/asm/io.h
+++ b/arch/riscv/include/asm/io.h
@@ -140,4 +140,8 @@ __io_writes_outs(outs, u64, q, __io_pbr(), __io_paw())
 	((__force void *)ioremap_prot((addr), (size), _PAGE_KERNEL))
 #endif
 
+#undef ioremap_wc
+#define ioremap_wc(addr, size)		\
+	ioremap_prot((addr), (size), _PAGE_IOREMAP_WC)
+
 #endif /* _ASM_RISCV_IO_H */
diff --git a/arch/riscv/include/asm/kexec.h b/arch/riscv/include/asm/kexec.h
index 2b56769cb530..62f3ddc7c498 100644
--- a/arch/riscv/include/asm/kexec.h
+++ b/arch/riscv/include/asm/kexec.h
@@ -56,6 +56,7 @@ extern riscv_kexec_method riscv_kexec_norelocate;
 
 #ifdef CONFIG_KEXEC_FILE
 extern const struct kexec_file_ops elf_kexec_ops;
+extern const struct kexec_file_ops image_kexec_ops;
 
 struct purgatory_info;
 int arch_kexec_apply_relocations_add(struct purgatory_info *pi,
diff --git a/arch/riscv/include/asm/pgtable-64.h b/arch/riscv/include/asm/pgtable-64.h
index 7a5097202e15..783837bbd878 100644
--- a/arch/riscv/include/asm/pgtable-64.h
+++ b/arch/riscv/include/asm/pgtable-64.h
@@ -126,14 +126,18 @@ enum napot_cont_order {
 
 /*
  * [63:59] T-Head Memory Type definitions:
- *
- * 00000 - NC   Weakly-ordered, Non-cacheable, Non-bufferable, Non-shareable, Non-trustable
+ * bit[63] SO - Strong Order
+ * bit[62] C - Cacheable
+ * bit[61] B - Bufferable
+ * bit[60] SH - Shareable
+ * bit[59] Sec - Trustable
+ * 00110 - NC   Weakly-ordered, Non-cacheable, Bufferable, Shareable, Non-trustable
  * 01110 - PMA  Weakly-ordered, Cacheable, Bufferable, Shareable, Non-trustable
- * 10000 - IO   Strongly-ordered, Non-cacheable, Non-bufferable, Non-shareable, Non-trustable
+ * 10010 - IO   Strongly-ordered, Non-cacheable, Non-bufferable, Shareable, Non-trustable
  */
 #define _PAGE_PMA_THEAD		((1UL << 62) | (1UL << 61) | (1UL << 60))
-#define _PAGE_NOCACHE_THEAD	0UL
-#define _PAGE_IO_THEAD		(1UL << 63)
+#define _PAGE_NOCACHE_THEAD	((1UL << 61) | (1UL << 60))
+#define _PAGE_IO_THEAD		((1UL << 63) | (1UL << 60))
 #define _PAGE_MTMASK_THEAD	(_PAGE_PMA_THEAD | _PAGE_IO_THEAD | (1UL << 59))
 
 static inline u64 riscv_page_mtmask(void)
diff --git a/arch/riscv/include/asm/pgtable.h b/arch/riscv/include/asm/pgtable.h
index a16fcdf91f39..4774cd9e5a83 100644
--- a/arch/riscv/include/asm/pgtable.h
+++ b/arch/riscv/include/asm/pgtable.h
@@ -94,7 +94,12 @@
 #ifdef CONFIG_64BIT
 #define MAX_FDT_SIZE	 PMD_SIZE
 #define FIX_FDT_SIZE	 (MAX_FDT_SIZE + SZ_2M)
+#ifdef CONFIG_HIGHMEM
+#define FIXADDR_PMD_NUM  20
+#define FIXADDR_SIZE     ((PMD_SIZE * FIXADDR_PMD_NUM) + FIX_FDT_SIZE)
+#else
 #define FIXADDR_SIZE     (PMD_SIZE + FIX_FDT_SIZE)
+#endif
 #else
 #define MAX_FDT_SIZE	 PGDIR_SIZE
 #define FIX_FDT_SIZE	 MAX_FDT_SIZE
@@ -104,6 +109,14 @@
 
 #endif
 
+#ifdef CONFIG_HIGHMEM
+#define PKMAP_BASE       ((FIXADDR_START - PMD_SIZE) & (PMD_MASK))
+#define LAST_PKMAP       (PMD_SIZE >> PAGE_SHIFT)
+#define LAST_PKMAP_MASK  (LAST_PKMAP - 1)
+#define PKMAP_NR(virt)   (((virt) - PKMAP_BASE) >> PAGE_SHIFT)
+#define PKMAP_ADDR(nr)   (PKMAP_BASE + ((nr) << PAGE_SHIFT))
+#endif
+
 #ifdef CONFIG_XIP_KERNEL
 #define XIP_OFFSET		SZ_32M
 #define XIP_OFFSET_MASK		(SZ_32M - 1)
@@ -205,7 +218,8 @@ extern struct pt_alloc_ops pt_ops __initdata;
 
 #define PAGE_TABLE		__pgprot(_PAGE_TABLE)
 
-#define _PAGE_IOREMAP	((_PAGE_KERNEL & ~_PAGE_MTMASK) | _PAGE_IO)
+#define _PAGE_IOREMAP		((_PAGE_KERNEL & ~_PAGE_MTMASK) | _PAGE_IO)
+#define _PAGE_IOREMAP_WC	((_PAGE_KERNEL & ~_PAGE_MTMASK) | _PAGE_NOCACHE)
 #define PAGE_KERNEL_IO		__pgprot(_PAGE_IOREMAP)
 
 extern pgd_t swapper_pg_dir[];
@@ -520,12 +534,17 @@ static inline void set_pte(pte_t *ptep, pte_t pteval)
 
 void flush_icache_pte(pte_t pte);
 
-static inline void __set_pte_at(pte_t *ptep, pte_t pteval)
+static inline void __set_pte_at(struct mm_struct *mm, unsigned long addr,
+		pte_t *ptep, pte_t pteval)
 {
 	if (pte_present(pteval) && pte_exec(pteval))
 		flush_icache_pte(pteval);
 
 	set_pte(ptep, pteval);
+
+#ifdef CONFIG_HIGHMEM
+	local_flush_tlb_page(addr);
+#endif
 }
 
 #define PFN_PTE_SHIFT		_PAGE_PFN_SHIFT
@@ -536,9 +555,10 @@ static inline void set_ptes(struct mm_struct *mm, unsigned long addr,
 	page_table_check_ptes_set(mm, ptep, pteval, nr);
 
 	for (;;) {
-		__set_pte_at(ptep, pteval);
+		__set_pte_at(mm, addr, ptep, pteval);
 		if (--nr == 0)
 			break;
+		addr += PAGE_SIZE;
 		ptep++;
 		pte_val(pteval) += 1 << _PAGE_PFN_SHIFT;
 	}
@@ -548,7 +568,7 @@ static inline void set_ptes(struct mm_struct *mm, unsigned long addr,
 static inline void pte_clear(struct mm_struct *mm,
 	unsigned long addr, pte_t *ptep)
 {
-	__set_pte_at(ptep, __pte(0));
+	__set_pte_at(mm, addr, ptep, __pte(0));
 }
 
 #define __HAVE_ARCH_PTEP_SET_ACCESS_FLAGS
@@ -557,7 +577,7 @@ static inline int ptep_set_access_flags(struct vm_area_struct *vma,
 					pte_t entry, int dirty)
 {
 	if (!pte_same(*ptep, entry))
-		__set_pte_at(ptep, entry);
+		__set_pte_at(vma->vm_mm, address, ptep, entry);
 	/*
 	 * update_mmu_cache will unconditionally execute, handling both
 	 * the case that the PTE changed and the spurious fault case.
@@ -730,14 +750,14 @@ static inline void set_pmd_at(struct mm_struct *mm, unsigned long addr,
 				pmd_t *pmdp, pmd_t pmd)
 {
 	page_table_check_pmd_set(mm, pmdp, pmd);
-	return __set_pte_at((pte_t *)pmdp, pmd_pte(pmd));
+	return __set_pte_at(mm, addr, (pte_t *)pmdp, pmd_pte(pmd));
 }
 
 static inline void set_pud_at(struct mm_struct *mm, unsigned long addr,
 				pud_t *pudp, pud_t pud)
 {
 	page_table_check_pud_set(mm, pudp, pud);
-	return __set_pte_at((pte_t *)pudp, pud_pte(pud));
+	return __set_pte_at(mm, addr, (pte_t *)pudp, pud_pte(pud));
 }
 
 #ifdef CONFIG_PAGE_TABLE_CHECK
diff --git a/arch/riscv/include/asm/sparsemem.h b/arch/riscv/include/asm/sparsemem.h
index 63acaecc3374..7ed3519b2d77 100644
--- a/arch/riscv/include/asm/sparsemem.h
+++ b/arch/riscv/include/asm/sparsemem.h
@@ -5,7 +5,7 @@
 
 #ifdef CONFIG_SPARSEMEM
 #ifdef CONFIG_64BIT
-#define MAX_PHYSMEM_BITS	56
+#define MAX_PHYSMEM_BITS	44
 #else
 #define MAX_PHYSMEM_BITS	34
 #endif /* CONFIG_64BIT */
diff --git a/arch/riscv/include/asm/switch_to.h b/arch/riscv/include/asm/switch_to.h
index a727be723c56..1da3f54d52f0 100644
--- a/arch/riscv/include/asm/switch_to.h
+++ b/arch/riscv/include/asm/switch_to.h
@@ -63,6 +63,21 @@ static __always_inline bool has_fpu(void)
 	return riscv_has_extension_likely(RISCV_ISA_EXT_f) ||
 		riscv_has_extension_likely(RISCV_ISA_EXT_d);
 }
+
+
+static inline void kernel_fpu_begin(void)
+{
+		preempt_disable();
+			fstate_save(current, task_pt_regs(current));
+				csr_set(CSR_SSTATUS, SR_FS);
+}
+
+static inline void kernel_fpu_end(void)
+{
+		csr_clear(CSR_SSTATUS, SR_FS);
+			fstate_restore(current, task_pt_regs(current));
+				preempt_enable();
+}
 #else
 static __always_inline bool has_fpu(void) { return false; }
 #define fstate_save(task, regs) do { } while (0)
diff --git a/arch/riscv/include/asm/timex.h b/arch/riscv/include/asm/timex.h
index a06697846e69..a0e24f329381 100644
--- a/arch/riscv/include/asm/timex.h
+++ b/arch/riscv/include/asm/timex.h
@@ -9,6 +9,10 @@
 #include <asm/csr.h>
 
 typedef unsigned long cycles_t;
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+extern u64 dw_timer_read_counter(void);
+extern void __iomem *sched_io_base;
+#endif
 
 #ifdef CONFIG_RISCV_M_MODE
 
@@ -52,7 +56,18 @@ static inline cycles_t get_cycles(void)
 {
 	return csr_read(CSR_TIME);
 }
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+static inline cycles_t dw_get_cycles(void)
+{
+	if (sched_io_base)
+		return dw_timer_read_counter();
+	else
+		return csr_read(CSR_TIME);
+}
+#define get_cycles dw_get_cycles
+#else
 #define get_cycles get_cycles
+#endif
 
 static inline u32 get_cycles_hi(void)
 {
diff --git a/arch/riscv/include/asm/vdso/gettimeofday.h b/arch/riscv/include/asm/vdso/gettimeofday.h
index ba3283cf7acc..ece0654e5767 100644
--- a/arch/riscv/include/asm/vdso/gettimeofday.h
+++ b/arch/riscv/include/asm/vdso/gettimeofday.h
@@ -84,6 +84,26 @@ static __always_inline const struct vdso_data *__arch_get_vdso_data(void)
 	return _vdso_data;
 }
 
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+static inline bool sophgo_vdso_hres_capable(void)
+{
+        return false;
+}
+#define __arch_vdso_hres_capable sophgo_vdso_hres_capable
+
+static inline bool sophgo_vdso_clocksource_ok(const struct vdso_data *vd)
+{
+	return false;
+}
+#define vdso_clocksource_ok sophgo_vdso_clocksource_ok
+
+static inline bool sophgo_vdso_cycles_ok(u64 cycles)
+{
+        return false;
+}
+#define vdso_cycles_ok sophgo_vdso_cycles_ok
+#endif
+
 #ifdef CONFIG_TIME_NS
 static __always_inline
 const struct vdso_data *__arch_get_timens_vdso_data(const struct vdso_data *vd)
diff --git a/arch/riscv/kernel/Makefile b/arch/riscv/kernel/Makefile
index a2499fcc1cf3..668e5e5c8e41 100644
--- a/arch/riscv/kernel/Makefile
+++ b/arch/riscv/kernel/Makefile
@@ -88,7 +88,7 @@ endif
 obj-$(CONFIG_HOTPLUG_CPU)	+= cpu-hotplug.o
 obj-$(CONFIG_KGDB)		+= kgdb.o
 obj-$(CONFIG_KEXEC_CORE)	+= kexec_relocate.o crash_save_regs.o machine_kexec.o
-obj-$(CONFIG_KEXEC_FILE)	+= elf_kexec.o machine_kexec_file.o
+obj-$(CONFIG_KEXEC_FILE)	+= elf_kexec.o image_kexec.o machine_kexec_file.o
 obj-$(CONFIG_CRASH_DUMP)	+= crash_dump.o
 obj-$(CONFIG_CRASH_CORE)	+= crash_core.o
 
diff --git a/arch/riscv/kernel/elf_kexec.c b/arch/riscv/kernel/elf_kexec.c
index e60fbd8660c4..3b80befe0519 100644
--- a/arch/riscv/kernel/elf_kexec.c
+++ b/arch/riscv/kernel/elf_kexec.c
@@ -450,6 +450,12 @@ int arch_kexec_apply_relocations_add(struct purgatory_info *pi,
 		case R_RISCV_SUB32:
 			*(u32 *)loc -= val;
 			break;
+		case R_RISCV_ADD16:
+			*(u16 *)loc += val;
+			break;
+		case R_RISCV_SUB16:
+			*(u16 *)loc -= val;
+			break;
 		/* It has been applied by R_RISCV_PCREL_HI20 sym */
 		case R_RISCV_PCREL_LO12_I:
 		case R_RISCV_ALIGN:
diff --git a/arch/riscv/kernel/image_kexec.c b/arch/riscv/kernel/image_kexec.c
new file mode 100644
index 000000000000..37c5bd813958
--- /dev/null
+++ b/arch/riscv/kernel/image_kexec.c
@@ -0,0 +1,305 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Kexec image loader
+
+ * Adapted from arch/arm64/kernel/kexec_image.c
+ * Copyright (C) 2018 Linaro Limited
+ * Author: AKASHI Takahiro <takahiro.akashi@linaro.org>
+ */
+#define pr_fmt(fmt)	"kexec_file(Image): " fmt
+
+#include <linux/err.h>
+#include <linux/errno.h>
+#include <linux/kernel.h>
+#include <linux/kexec.h>
+#include <linux/pe.h>
+#include <linux/string.h>
+#include <linux/verification.h>
+#include <linux/of.h>
+#include <linux/of_fdt.h>
+#include <linux/libfdt.h>
+#include <linux/slab.h>
+#include <linux/memblock.h>
+#include <linux/types.h>
+#include <asm/byteorder.h>
+#include <asm/image.h>
+
+static int prepare_elf_headers(void **addr, unsigned long *sz)
+{
+	struct crash_mem *cmem;
+	unsigned int nr_ranges;
+	int ret;
+	u64 i;
+	phys_addr_t start, end;
+
+	nr_ranges = 2; /* for exclusion of crashkernel region */
+	for_each_mem_range(i, &start, &end)
+		nr_ranges++;
+
+	cmem = kmalloc(struct_size(cmem, ranges, nr_ranges), GFP_KERNEL);
+	if (!cmem)
+		return -ENOMEM;
+
+	cmem->max_nr_ranges = nr_ranges;
+	cmem->nr_ranges = 0;
+	for_each_mem_range(i, &start, &end) {
+		cmem->ranges[cmem->nr_ranges].start = start;
+		cmem->ranges[cmem->nr_ranges].end = end - 1;
+		cmem->nr_ranges++;
+	}
+
+	/* Exclude crashkernel region */
+	ret = crash_exclude_mem_range(cmem, crashk_res.start, crashk_res.end);
+	if (ret)
+		goto out;
+
+	if (crashk_low_res.end) {
+		ret = crash_exclude_mem_range(cmem, crashk_low_res.start, crashk_low_res.end);
+		if (ret)
+			goto out;
+	}
+
+	ret = crash_prepare_elf64_headers(cmem, true, addr, sz);
+
+out:
+	kfree(cmem);
+	return ret;
+}
+
+/*
+ * Tries to add the initrd and DTB to the image. If it is not possible to find
+ * valid locations, this function will undo changes to the image and return non
+ * zero.
+ */
+static int load_other_segments(struct kimage *image,
+			unsigned long kernel_load_addr,
+			unsigned long kernel_size,
+			char *initrd, unsigned long initrd_len,
+			char *cmdline)
+{
+	struct kexec_buf kbuf;
+	void *headers, *fdt = NULL;
+	unsigned long headers_sz, initrd_load_addr = 0,
+		      orig_segments = image->nr_segments;
+	int ret = 0;
+
+	kbuf.image = image;
+	/* not allocate anything below the kernel */
+	kbuf.buf_min = kernel_load_addr + kernel_size;
+
+	/* load elf core header */
+	if (image->type == KEXEC_TYPE_CRASH) {
+		ret = prepare_elf_headers(&headers, &headers_sz);
+		if (ret) {
+			pr_err("Preparing elf core header failed\n");
+			goto out_err;
+		}
+
+		kbuf.buffer = headers;
+		kbuf.bufsz = headers_sz;
+		kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+		kbuf.memsz = headers_sz;
+		kbuf.buf_align = PAGE_SIZE;
+		kbuf.buf_max = ULONG_MAX;
+		kbuf.top_down = true;
+
+		ret = kexec_add_buffer(&kbuf);
+		if (ret) {
+			vfree(headers);
+			goto out_err;
+		}
+		image->elf_headers = headers;
+		image->elf_load_addr = kbuf.mem;
+		image->elf_headers_sz = headers_sz;
+
+		pr_debug("Loaded elf core header at 0x%lx bufsz=0x%lx memsz=0x%lx\n",
+			 image->elf_load_addr, kbuf.bufsz, kbuf.memsz);
+	}
+
+	/* load initrd */
+	if (initrd) {
+		kbuf.buffer = initrd;
+		kbuf.bufsz = initrd_len;
+		kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+		kbuf.memsz = initrd_len;
+		kbuf.buf_align = PAGE_SIZE;
+		/* avoid to overlap kernel address */
+		kbuf.buf_min = round_up(kernel_load_addr, SZ_1G);
+		kbuf.buf_max = ULONG_MAX;
+		kbuf.top_down = false;
+
+		ret = kexec_add_buffer(&kbuf);
+		if (ret)
+			goto out_err;
+		initrd_load_addr = kbuf.mem;
+
+		pr_debug("Loaded initrd at 0x%lx bufsz=0x%lx memsz=0x%lx\n",
+				initrd_load_addr, kbuf.bufsz, kbuf.memsz);
+	}
+
+	/* load dtb */
+	fdt = of_kexec_alloc_and_setup_fdt(image, initrd_load_addr,
+					   initrd_len, cmdline, 0);
+	if (!fdt) {
+		pr_err("Preparing for new dtb failed\n");
+		ret = -EINVAL;
+		goto out_err;
+	}
+
+	/* trim it */
+	fdt_pack(fdt);
+	kbuf.buffer = fdt;
+	kbuf.bufsz = kbuf.memsz = fdt_totalsize(fdt);
+	kbuf.buf_align = PAGE_SIZE;
+	kbuf.buf_max = ULONG_MAX;
+	kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+	kbuf.top_down = false;
+
+	ret = kexec_add_buffer(&kbuf);
+	if (ret)
+		goto out_err;
+	/* Cache the fdt buffer address for memory cleanup */
+	image->arch.fdt = fdt;
+	image->arch.fdt_addr = kbuf.mem;
+
+	pr_debug("Loaded dtb at 0x%lx bufsz=0x%lx memsz=0x%lx\n",
+			kbuf.mem, kbuf.bufsz, kbuf.memsz);
+
+	return 0;
+
+out_err:
+	image->nr_segments = orig_segments;
+	kvfree(fdt);
+	return ret;
+}
+
+static int image_probe(const char *kernel_buf, unsigned long kernel_len)
+{
+	const struct riscv_image_header *h =
+		(const struct riscv_image_header *)(kernel_buf);
+
+	if (!h || (kernel_len < sizeof(*h)))
+		return -EINVAL;
+
+	if (memcmp(&h->magic2, RISCV_IMAGE_MAGIC2, sizeof(h->magic2)))
+		return -EINVAL;
+
+	return 0;
+}
+
+static void *image_load(struct kimage *image,
+				char *kernel, unsigned long kernel_len,
+				char *initrd, unsigned long initrd_len,
+				char *cmdline, unsigned long cmdline_len)
+{
+	struct riscv_image_header *h;
+	u64 flags;
+	bool be_image, be_kernel;
+	struct kexec_buf kbuf;
+	unsigned long text_offset, kernel_segment_number;
+	unsigned long kernel_start;
+	struct kexec_segment *kernel_segment;
+	int ret;
+
+	h = (struct riscv_image_header *)kernel;
+	if (!h->image_size)
+		return ERR_PTR(-EINVAL);
+
+	/* Check cpu features */
+	flags = le64_to_cpu(h->flags);
+	be_image = __HEAD_FLAG(BE);
+	be_kernel = IS_ENABLED(CONFIG_CPU_BIG_ENDIAN);
+	if (be_image != be_kernel)
+		return ERR_PTR(-EINVAL);
+
+	/* Load the kernel */
+	kbuf.image = image;
+	kbuf.buf_min = 0;
+	kbuf.buf_max = ULONG_MAX;
+	kbuf.top_down = false;
+
+	kbuf.buffer = kernel;
+	kbuf.bufsz = kernel_len;
+	kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+	kbuf.memsz = le64_to_cpu(h->image_size);
+	text_offset = le64_to_cpu(h->text_offset);
+	kbuf.buf_align = PMD_SIZE;
+
+	/* Adjust kernel segment with TEXT_OFFSET */
+	kbuf.memsz += text_offset;
+
+	kernel_segment_number = image->nr_segments;
+
+	/*
+	 * The location of the kernel segment may make it impossible to satisfy
+	 * the other segment requirements, so we try repeatedly to find a
+	 * location that will work.
+	 */
+	while ((ret = kexec_add_buffer(&kbuf)) == 0) {
+		/* Try to load additional data */
+		kernel_segment = &image->segment[kernel_segment_number];
+		ret = load_other_segments(image, kernel_segment->mem,
+					  kernel_segment->memsz, initrd,
+					  initrd_len, cmdline);
+		if (!ret)
+			break;
+
+		/*
+		 * We couldn't find space for the other segments; erase the
+		 * kernel segment and try the next available hole.
+		 */
+		image->nr_segments -= 1;
+		kbuf.buf_min = kernel_segment->mem + kernel_segment->memsz;
+		kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+	}
+
+	if (ret) {
+		pr_err("Could not find any suitable kernel location!");
+		return ERR_PTR(ret);
+	}
+
+	kernel_segment = &image->segment[kernel_segment_number];
+	kernel_segment->mem += text_offset;
+	kernel_segment->memsz -= text_offset;
+	kernel_start = kernel_segment->mem;
+	image->start = kernel_start;
+
+
+	pr_debug("Loaded kernel at 0x%lx bufsz=0x%lx memsz=0x%lx\n",
+				kernel_segment->mem, kbuf.bufsz,
+				kernel_segment->memsz);
+
+#ifdef CONFIG_ARCH_SUPPORTS_KEXEC_PURGATORY
+	/* Add purgatory to the image */
+	kbuf.top_down = true;
+	kbuf.mem = KEXEC_BUF_MEM_UNKNOWN;
+	ret = kexec_load_purgatory(image, &kbuf);
+	if (ret) {
+		pr_err("Error loading purgatory ret=%d\n", ret);
+		return ERR_PTR(ret);
+	}
+	ret = kexec_purgatory_get_set_symbol(image, "riscv_kernel_entry",
+					     &kernel_start,
+					     sizeof(kernel_start), 0);
+	if (ret)
+		pr_err("Error update purgatory ret=%d\n", ret);
+#endif /* CONFIG_ARCH_SUPPORTS_KEXEC_PURGATORY */
+
+	return ret ? ERR_PTR(ret) : NULL;
+}
+
+#ifdef CONFIG_KEXEC_IMAGE_VERIFY_SIG
+static int image_verify_sig(const char *kernel, unsigned long kernel_len)
+{
+	return verify_pefile_signature(kernel, kernel_len, NULL,
+				       VERIFYING_KEXEC_PE_SIGNATURE);
+}
+#endif
+
+const struct kexec_file_ops image_kexec_ops = {
+	.probe = image_probe,
+	.load = image_load,
+#ifdef CONFIG_KEXEC_IMAGE_VERIFY_SIG
+	.verify_sig = image_verify_sig,
+#endif
+};
diff --git a/arch/riscv/kernel/machine_kexec_file.c b/arch/riscv/kernel/machine_kexec_file.c
index b0bf8c1722c0..401edfd1774f 100644
--- a/arch/riscv/kernel/machine_kexec_file.c
+++ b/arch/riscv/kernel/machine_kexec_file.c
@@ -9,6 +9,7 @@
 #include <linux/kexec.h>
 
 const struct kexec_file_ops * const kexec_file_loaders[] = {
+	&image_kexec_ops,
 	&elf_kexec_ops,
 	NULL
 };
diff --git a/arch/riscv/kernel/module.c b/arch/riscv/kernel/module.c
index df4f6fec5d17..ced5a09abaaa 100644
--- a/arch/riscv/kernel/module.c
+++ b/arch/riscv/kernel/module.c
@@ -337,6 +337,45 @@ static int (*reloc_handlers_rela[]) (struct module *me, u32 *location,
 	[R_RISCV_SUB64]			= apply_r_riscv_sub64_rela,
 };
 
+static inline unsigned int apply_calc_pcrel_lo12(Elf_Shdr *sechdrs,
+			Elf_Rela *rel, Elf_Sym *sym, unsigned int idx,
+			unsigned int symindex, unsigned int relsec,
+			struct module *me, Elf_Addr *v)
+{
+	unsigned long hi20_loc =
+		sechdrs[sechdrs[relsec].sh_info].sh_addr
+		+ rel[idx].r_offset;
+	u32 hi20_type = ELF_RISCV_R_TYPE(rel[idx].r_info);
+	unsigned int found = 0;
+
+	/* Find the corresponding HI20 relocation entry */
+	if (hi20_loc == sym->st_value
+	    && (hi20_type == R_RISCV_PCREL_HI20
+		|| hi20_type == R_RISCV_GOT_HI20)) {
+		s32 hi20, lo12;
+		Elf_Sym *hi20_sym =
+			(Elf_Sym *)sechdrs[symindex].sh_addr
+			+ ELF_RISCV_R_SYM(rel[idx].r_info);
+		unsigned long hi20_sym_val =
+			hi20_sym->st_value + rel[idx].r_addend;
+
+		/* Calculate lo12 */
+		size_t offset = hi20_sym_val - hi20_loc;
+		if (IS_ENABLED(CONFIG_MODULE_SECTIONS)
+		    && hi20_type == R_RISCV_GOT_HI20) {
+			offset = module_emit_got_entry(me, hi20_sym_val);
+			offset = offset - hi20_loc;
+		}
+		hi20 = (offset + 0x800) & 0xfffff000;
+		lo12 = offset - hi20;
+		*v = (Elf_Addr)lo12;
+
+		found = 1;
+	}
+
+	return found;
+}
+
 int apply_relocate_add(Elf_Shdr *sechdrs, const char *strtab,
 		       unsigned int symindex, unsigned int relsec,
 		       struct module *me)
@@ -385,40 +424,24 @@ int apply_relocate_add(Elf_Shdr *sechdrs, const char *strtab,
 
 		if (type == R_RISCV_PCREL_LO12_I || type == R_RISCV_PCREL_LO12_S) {
 			unsigned int j;
+			unsigned int found = 0;
 
-			for (j = 0; j < sechdrs[relsec].sh_size / sizeof(*rel); j++) {
-				unsigned long hi20_loc =
-					sechdrs[sechdrs[relsec].sh_info].sh_addr
-					+ rel[j].r_offset;
-				u32 hi20_type = ELF_RISCV_R_TYPE(rel[j].r_info);
-
-				/* Find the corresponding HI20 relocation entry */
-				if (hi20_loc == sym->st_value
-				    && (hi20_type == R_RISCV_PCREL_HI20
-					|| hi20_type == R_RISCV_GOT_HI20)) {
-					s32 hi20, lo12;
-					Elf_Sym *hi20_sym =
-						(Elf_Sym *)sechdrs[symindex].sh_addr
-						+ ELF_RISCV_R_SYM(rel[j].r_info);
-					unsigned long hi20_sym_val =
-						hi20_sym->st_value
-						+ rel[j].r_addend;
-
-					/* Calculate lo12 */
-					size_t offset = hi20_sym_val - hi20_loc;
-					if (IS_ENABLED(CONFIG_MODULE_SECTIONS)
-					    && hi20_type == R_RISCV_GOT_HI20) {
-						offset = module_emit_got_entry(
-							 me, hi20_sym_val);
-						offset = offset - hi20_loc;
-					}
-					hi20 = (offset + 0x800) & 0xfffff000;
-					lo12 = offset - hi20;
-					v = lo12;
+			if (i > 0) {
+				j  = i - 1;
+				found = apply_calc_pcrel_lo12(sechdrs, rel, sym, j,
+							symindex, relsec, me, &v);
+			}
 
-					break;
+			if (found == 0) {
+				for (j = 0; j < sechdrs[relsec].sh_size/sizeof(*rel); j++) {
+					found = apply_calc_pcrel_lo12(sechdrs, rel, sym,
+							j, symindex, relsec, me, &v);
+					if (found) {
+						break;
+					}
 				}
 			}
+
 			if (j == sechdrs[relsec].sh_size / sizeof(*rel)) {
 				pr_err(
 				  "%s: Can not find HI20 relocation information\n",
diff --git a/arch/riscv/kernel/process.c b/arch/riscv/kernel/process.c
index 83e223318822..dd973216e31c 100644
--- a/arch/riscv/kernel/process.c
+++ b/arch/riscv/kernel/process.c
@@ -204,3 +204,6 @@ int copy_thread(struct task_struct *p, const struct kernel_clone_args *args)
 	p->thread.sp = (unsigned long)childregs; /* kernel sp */
 	return 0;
 }
+
+EXPORT_SYMBOL_GPL(__fstate_save);
+EXPORT_SYMBOL_GPL(__fstate_restore);
diff --git a/arch/riscv/kvm/vcpu_timer.c b/arch/riscv/kvm/vcpu_timer.c
index 75486b25ac45..ba803aa15b89 100644
--- a/arch/riscv/kvm/vcpu_timer.c
+++ b/arch/riscv/kvm/vcpu_timer.c
@@ -15,6 +15,10 @@
 #include <asm/delay.h>
 #include <asm/kvm_vcpu_timer.h>
 
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+extern void dw_cs_get_mult_shift(u32 *mult, u32 *shift);
+#endif
+
 static u64 kvm_riscv_current_cycles(struct kvm_guest_timer *gt)
 {
 	return get_cycles64() + gt->time_delta;
@@ -358,6 +362,10 @@ void kvm_riscv_guest_timer_init(struct kvm *kvm)
 {
 	struct kvm_guest_timer *gt = &kvm->arch.timer;
 
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+	dw_cs_get_mult_shift(&gt->nsec_mult, &gt->nsec_shift);
+#else
 	riscv_cs_get_mult_shift(&gt->nsec_mult, &gt->nsec_shift);
+#endif
 	gt->time_delta = -get_cycles64();
 }
diff --git a/arch/riscv/mm/init.c b/arch/riscv/mm/init.c
index ec02ea86aa39..0980d6c683ad 100644
--- a/arch/riscv/mm/init.c
+++ b/arch/riscv/mm/init.c
@@ -36,6 +36,11 @@
 
 #include "../kernel/head.h"
 
+#ifdef CONFIG_HIGHMEM
+#include <asm/highmem.h>
+extern phys_addr_t __init_memblock find_max_low_addr(phys_addr_t limit);
+#endif
+
 struct kernel_mapping kernel_map __ro_after_init;
 EXPORT_SYMBOL(kernel_map);
 #ifdef CONFIG_XIP_KERNEL
@@ -75,6 +80,9 @@ static void __init zone_sizes_init(void)
 	max_zone_pfns[ZONE_DMA32] = PFN_DOWN(dma32_phys_limit);
 #endif
 	max_zone_pfns[ZONE_NORMAL] = max_low_pfn;
+#ifdef CONFIG_HIGHMEM
+	max_zone_pfns[ZONE_HIGHMEM] = max_pfn;
+#endif
 
 	free_area_init(max_zone_pfns);
 }
@@ -131,6 +139,10 @@ static inline void print_ml(char *name, unsigned long b, unsigned long t)
 static void __init print_vm_layout(void)
 {
 	pr_notice("Virtual kernel memory layout:\n");
+#ifdef CONFIG_HIGHMEM
+	print_ml("pkmap", (unsigned long)PKMAP_BASE,
+		(unsigned long)FIXADDR_START);
+#endif
 	print_ml("fixmap", (unsigned long)FIXADDR_START,
 		(unsigned long)FIXADDR_TOP);
 	print_ml("pci io", (unsigned long)PCI_IO_START,
@@ -158,6 +170,106 @@ static void __init print_vm_layout(void)
 static void print_vm_layout(void) { }
 #endif /* CONFIG_DEBUG_VM */
 
+#ifdef CONFIG_HIGHMEM
+
+#ifdef CONFIG_DEBUG_VM
+#error Please unset CONFIG_DEBUG_VM when CONFIG_HIGHMEM is set, \
+because CONFIG_DEBUG_VM will trigger VM_BUG_ON_PAGE in __free_pages()->put_page_testzero().
+#endif
+#if defined(CONFIG_SPARSEMEM_VMEMMAP) && defined(CONFIG_NUMA)
+#error Please unset CONFIG_SPARSEMEM_VMEMMAP when CONFIG_HIGHMEM and CONFIG_NUMA are set, \
+because vmemmap_verify will report warning that [xxx-xxx] potential offnode page_structs.
+#endif
+
+/* free order size pages for optimize system boot time. */
+#define OPTIMIZE_FREE_PAGES
+
+#ifdef OPTIMIZE_FREE_PAGES
+#define ORDER_SIZE(order)              (1UL << order)
+#define ORDER_MASK(order)              (~(ORDER_SIZE(order) - 1))
+#define PFN_ALIGN_ORDER(pfn, order)    \
+	(((u64)(pfn) + (ORDER_SIZE(order) - 1)) & ORDER_MASK(order))
+
+/* Free the reserved page into the buddy system, so it gets managed. */
+static void __init free_highmem_pages(u64 start, u64 order)
+{
+	struct page *page;
+	u64  i, pfn;
+
+	for (i = 0, pfn = start; i < ORDER_SIZE(order); i++, pfn++) {
+		page = pfn_to_page(pfn);
+		ClearPageReserved(page);
+		set_page_count(page, 0);
+	}
+
+	page = pfn_to_page(start);
+	__free_pages(page, order);
+	adjust_managed_page_count(page, ORDER_SIZE(order));
+}
+
+static void __init free_highpages(void)
+{
+	phys_addr_t range_start, range_end;
+	u64 max_low = max_low_pfn;
+	u64 i, order;
+
+	/* set highmem page free */
+	for_each_free_mem_range(i, NUMA_NO_NODE, MEMBLOCK_NONE,
+			&range_start, &range_end, NULL) {
+		u64 start = PFN_UP(range_start), start_align;
+		u64 end = PFN_DOWN(range_end);
+
+		/* Ignore complete lowmem entries */
+		if (end <= max_low)
+			continue;
+
+		/* Truncate partial highmem entries */
+		if (start < max_low)
+			start = max_low;
+
+		order = MAX_ORDER;
+		start_align = PFN_ALIGN_ORDER(start, order);
+
+		for (; start < start_align; start++)
+			free_highmem_page(pfn_to_page(start));
+
+		//step by order size
+		for (; start < end; start += ORDER_SIZE(order))
+			free_highmem_pages(start, order);
+
+		for (; start < end; start++)
+			free_highmem_page(pfn_to_page(start));
+	}
+}
+#else
+static void __init free_highpages(void)
+{
+	unsigned long max_low = max_low_pfn;
+	phys_addr_t range_start, range_end;
+	u64 i;
+
+	/* set highmem page free */
+	for_each_free_mem_range(i, NUMA_NO_NODE, MEMBLOCK_NONE,
+			&range_start, &range_end, NULL) {
+		unsigned long start = PFN_UP(range_start);
+		unsigned long end = PFN_DOWN(range_end);
+
+
+		/* Ignore complete lowmem entries */
+		if (end <= max_low)
+			continue;
+
+		/* Truncate partial highmem entries */
+		if (start < max_low)
+			start = max_low;
+
+		for (; start < end; start++)
+			free_highmem_page(pfn_to_page(start));
+	}
+}
+#endif
+#endif
+
 void __init mem_init(void)
 {
 #ifdef CONFIG_FLATMEM
@@ -166,6 +278,9 @@ void __init mem_init(void)
 
 	swiotlb_init(max_pfn > PFN_DOWN(dma32_phys_limit), SWIOTLB_VERBOSE);
 	memblock_free_all();
+#ifdef CONFIG_HIGHMEM
+	free_highpages();
+#endif
 
 	print_vm_layout();
 }
@@ -197,13 +312,18 @@ static void __init setup_bootmem(void)
 	phys_addr_t vmlinux_end = __pa_symbol(&_end);
 	phys_addr_t max_mapped_addr;
 	phys_addr_t phys_ram_end, vmlinux_start;
+#ifdef CONFIG_HIGHMEM
+	phys_addr_t max_low_addr;
+#endif
 
 	if (IS_ENABLED(CONFIG_XIP_KERNEL))
 		vmlinux_start = __pa_symbol(&_sdata);
 	else
 		vmlinux_start = __pa_symbol(&_start);
 
+#ifndef CONFIG_HIGHMEM
 	memblock_enforce_memory_limit(memory_limit);
+#endif
 
 	/*
 	 * Make sure we align the reservation on PMD_SIZE since we will
@@ -249,12 +369,22 @@ static void __init setup_bootmem(void)
 	}
 
 	min_low_pfn = PFN_UP(phys_ram_base);
+#ifdef CONFIG_HIGHMEM
+	max_low_addr = find_max_low_addr(memory_limit);
+	max_low_pfn = PFN_DOWN(max_low_addr);
+	max_pfn = PFN_DOWN(phys_ram_end);
+	memblock_set_current_limit(max_low_addr);
+#else
 	max_low_pfn = max_pfn = PFN_DOWN(phys_ram_end);
+#endif
 	high_memory = (void *)(__va(PFN_PHYS(max_low_pfn)));
 
 	dma32_phys_limit = min(4UL * SZ_1G, (unsigned long)PFN_PHYS(max_low_pfn));
+#ifdef CONFIG_HIGHMEM
+	set_max_mapnr(max_pfn - ARCH_PFN_OFFSET);
+#else
 	set_max_mapnr(max_low_pfn - ARCH_PFN_OFFSET);
-
+#endif
 	reserve_initrd_mem();
 
 	/*
@@ -283,8 +413,14 @@ struct pt_alloc_ops pt_ops __initdata;
 
 pgd_t swapper_pg_dir[PTRS_PER_PGD] __page_aligned_bss;
 pgd_t trampoline_pg_dir[PTRS_PER_PGD] __page_aligned_bss;
+#ifdef CONFIG_HIGHMEM
+static pte_t fixmap_pte[PTRS_PER_PTE * FIXADDR_PMD_NUM] __page_aligned_bss;
+#else
 static pte_t fixmap_pte[PTRS_PER_PTE] __page_aligned_bss;
-
+#endif
+#ifdef CONFIG_HIGHMEM
+static pte_t pkmap_pte[PTRS_PER_PTE] __page_aligned_bss;
+#endif
 pgd_t early_pg_dir[PTRS_PER_PGD] __initdata __aligned(PAGE_SIZE);
 
 #ifdef CONFIG_XIP_KERNEL
@@ -318,10 +454,17 @@ void __set_fixmap(enum fixed_addresses idx, phys_addr_t phys, pgprot_t prot)
 {
 	unsigned long addr = __fix_to_virt(idx);
 	pte_t *ptep;
+#ifdef CONFIG_HIGHMEM
+	unsigned long pte_idx = (addr - FIXADDR_START) >> PAGE_SHIFT;
+#endif
 
 	BUG_ON(idx <= FIX_HOLE || idx >= __end_of_fixed_addresses);
 
+#ifdef CONFIG_HIGHMEM
+	ptep = &fixmap_pte[pte_idx];
+#else
 	ptep = &fixmap_pte[pte_index(addr)];
+#endif
 
 	if (pgprot_val(prot))
 		set_pte(ptep, pfn_pte(phys >> PAGE_SHIFT, prot));
@@ -1144,8 +1287,26 @@ asmlinkage void __init setup_vm(uintptr_t dtb_pa)
 	if (pgtable_l4_enabled)
 		create_pud_mapping(fixmap_pud, FIXADDR_START,
 				   (uintptr_t)fixmap_pmd, PUD_SIZE, PAGE_TABLE);
+#ifdef CONFIG_HIGHMEM
+	{
+		int i;
+		for (i = 0; i < FIXADDR_PMD_NUM; i++)
+			create_pmd_mapping(fixmap_pmd,
+					   (FIXADDR_START + i * PMD_SIZE),
+					   (uintptr_t)&(fixmap_pte[i * PTRS_PER_PTE]),
+					   PMD_SIZE,
+					   PAGE_TABLE);
+	}
+#else
 	create_pmd_mapping(fixmap_pmd, FIXADDR_START,
 			   (uintptr_t)fixmap_pte, PMD_SIZE, PAGE_TABLE);
+#endif
+#ifdef CONFIG_HIGHMEM
+	/* Setup pkmap PMD */
+	create_pmd_mapping(fixmap_pmd, PKMAP_BASE,
+			   (uintptr_t)pkmap_pte, PMD_SIZE, PAGE_TABLE);
+#endif
+
 	/* Setup trampoline PGD and PMD */
 	create_pgd_mapping(trampoline_pg_dir, kernel_map.virt_addr,
 			   trampoline_pgd_next, PGDIR_SIZE, PAGE_TABLE);
@@ -1488,6 +1649,13 @@ static void __init reserve_crashkernel(void)
 	crashk_res.end = crash_base + crash_size - 1;
 }
 
+#ifdef CONFIG_HIGHMEM
+static void __init pkmap_init(void)
+{
+	pkmap_page_table = &pkmap_pte[pte_index(PKMAP_BASE)];
+}
+#endif
+
 void __init paging_init(void)
 {
 	setup_bootmem();
@@ -1507,6 +1675,9 @@ void __init misc_mem_init(void)
 	local_flush_tlb_kernel_range(VMEMMAP_START, VMEMMAP_END);
 #endif
 	zone_sizes_init();
+#ifdef CONFIG_HIGHMEM
+	pkmap_init();
+#endif
 	reserve_crashkernel();
 	memblock_dump_all();
 }
diff --git a/arch/riscv/mm/pageattr.c b/arch/riscv/mm/pageattr.c
index 01398fee5cf8..161d0b34c2cb 100644
--- a/arch/riscv/mm/pageattr.c
+++ b/arch/riscv/mm/pageattr.c
@@ -5,7 +5,6 @@
 
 #include <linux/pagewalk.h>
 #include <linux/pgtable.h>
-#include <linux/vmalloc.h>
 #include <asm/tlbflush.h>
 #include <asm/bitops.h>
 #include <asm/set_memory.h>
@@ -26,6 +25,19 @@ static unsigned long set_pageattr_masks(unsigned long val, struct mm_walk *walk)
 	return new_val;
 }
 
+static int pageattr_pgd_entry(pgd_t *pgd, unsigned long addr,
+			      unsigned long next, struct mm_walk *walk)
+{
+	pgd_t val = READ_ONCE(*pgd);
+
+	if (pgd_leaf(val)) {
+		val = __pgd(set_pageattr_masks(pgd_val(val), walk));
+		set_pgd(pgd, val);
+	}
+
+	return 0;
+}
+
 static int pageattr_p4d_entry(p4d_t *p4d, unsigned long addr,
 			      unsigned long next, struct mm_walk *walk)
 {
@@ -84,6 +96,7 @@ static int pageattr_pte_hole(unsigned long addr, unsigned long next,
 }
 
 static const struct mm_walk_ops pageattr_ops = {
+	.pgd_entry = pageattr_pgd_entry,
 	.p4d_entry = pageattr_p4d_entry,
 	.pud_entry = pageattr_pud_entry,
 	.pmd_entry = pageattr_pmd_entry,
@@ -92,181 +105,12 @@ static const struct mm_walk_ops pageattr_ops = {
 	.walk_lock = PGWALK_RDLOCK,
 };
 
-#ifdef CONFIG_64BIT
-static int __split_linear_mapping_pmd(pud_t *pudp,
-				      unsigned long vaddr, unsigned long end)
-{
-	pmd_t *pmdp;
-	unsigned long next;
-
-	pmdp = pmd_offset(pudp, vaddr);
-
-	do {
-		next = pmd_addr_end(vaddr, end);
-
-		if (next - vaddr >= PMD_SIZE &&
-		    vaddr <= (vaddr & PMD_MASK) && end >= next)
-			continue;
-
-		if (pmd_leaf(*pmdp)) {
-			struct page *pte_page;
-			unsigned long pfn = _pmd_pfn(*pmdp);
-			pgprot_t prot = __pgprot(pmd_val(*pmdp) & ~_PAGE_PFN_MASK);
-			pte_t *ptep_new;
-			int i;
-
-			pte_page = alloc_page(GFP_KERNEL);
-			if (!pte_page)
-				return -ENOMEM;
-
-			ptep_new = (pte_t *)page_address(pte_page);
-			for (i = 0; i < PTRS_PER_PTE; ++i, ++ptep_new)
-				set_pte(ptep_new, pfn_pte(pfn + i, prot));
-
-			smp_wmb();
-
-			set_pmd(pmdp, pfn_pmd(page_to_pfn(pte_page), PAGE_TABLE));
-		}
-	} while (pmdp++, vaddr = next, vaddr != end);
-
-	return 0;
-}
-
-static int __split_linear_mapping_pud(p4d_t *p4dp,
-				      unsigned long vaddr, unsigned long end)
-{
-	pud_t *pudp;
-	unsigned long next;
-	int ret;
-
-	pudp = pud_offset(p4dp, vaddr);
-
-	do {
-		next = pud_addr_end(vaddr, end);
-
-		if (next - vaddr >= PUD_SIZE &&
-		    vaddr <= (vaddr & PUD_MASK) && end >= next)
-			continue;
-
-		if (pud_leaf(*pudp)) {
-			struct page *pmd_page;
-			unsigned long pfn = _pud_pfn(*pudp);
-			pgprot_t prot = __pgprot(pud_val(*pudp) & ~_PAGE_PFN_MASK);
-			pmd_t *pmdp_new;
-			int i;
-
-			pmd_page = alloc_page(GFP_KERNEL);
-			if (!pmd_page)
-				return -ENOMEM;
-
-			pmdp_new = (pmd_t *)page_address(pmd_page);
-			for (i = 0; i < PTRS_PER_PMD; ++i, ++pmdp_new)
-				set_pmd(pmdp_new,
-					pfn_pmd(pfn + ((i * PMD_SIZE) >> PAGE_SHIFT), prot));
-
-			smp_wmb();
-
-			set_pud(pudp, pfn_pud(page_to_pfn(pmd_page), PAGE_TABLE));
-		}
-
-		ret = __split_linear_mapping_pmd(pudp, vaddr, next);
-		if (ret)
-			return ret;
-	} while (pudp++, vaddr = next, vaddr != end);
-
-	return 0;
-}
-
-static int __split_linear_mapping_p4d(pgd_t *pgdp,
-				      unsigned long vaddr, unsigned long end)
-{
-	p4d_t *p4dp;
-	unsigned long next;
-	int ret;
-
-	p4dp = p4d_offset(pgdp, vaddr);
-
-	do {
-		next = p4d_addr_end(vaddr, end);
-
-		/*
-		 * If [vaddr; end] contains [vaddr & P4D_MASK; next], we don't
-		 * need to split, we'll change the protections on the whole P4D.
-		 */
-		if (next - vaddr >= P4D_SIZE &&
-		    vaddr <= (vaddr & P4D_MASK) && end >= next)
-			continue;
-
-		if (p4d_leaf(*p4dp)) {
-			struct page *pud_page;
-			unsigned long pfn = _p4d_pfn(*p4dp);
-			pgprot_t prot = __pgprot(p4d_val(*p4dp) & ~_PAGE_PFN_MASK);
-			pud_t *pudp_new;
-			int i;
-
-			pud_page = alloc_page(GFP_KERNEL);
-			if (!pud_page)
-				return -ENOMEM;
-
-			/*
-			 * Fill the pud level with leaf puds that have the same
-			 * protections as the leaf p4d.
-			 */
-			pudp_new = (pud_t *)page_address(pud_page);
-			for (i = 0; i < PTRS_PER_PUD; ++i, ++pudp_new)
-				set_pud(pudp_new,
-					pfn_pud(pfn + ((i * PUD_SIZE) >> PAGE_SHIFT), prot));
-
-			/*
-			 * Make sure the pud filling is not reordered with the
-			 * p4d store which could result in seeing a partially
-			 * filled pud level.
-			 */
-			smp_wmb();
-
-			set_p4d(p4dp, pfn_p4d(page_to_pfn(pud_page), PAGE_TABLE));
-		}
-
-		ret = __split_linear_mapping_pud(p4dp, vaddr, next);
-		if (ret)
-			return ret;
-	} while (p4dp++, vaddr = next, vaddr != end);
-
-	return 0;
-}
-
-static int __split_linear_mapping_pgd(pgd_t *pgdp,
-				      unsigned long vaddr,
-				      unsigned long end)
-{
-	unsigned long next;
-	int ret;
-
-	do {
-		next = pgd_addr_end(vaddr, end);
-		/* We never use PGD mappings for the linear mapping */
-		ret = __split_linear_mapping_p4d(pgdp, vaddr, next);
-		if (ret)
-			return ret;
-	} while (pgdp++, vaddr = next, vaddr != end);
-
-	return 0;
-}
-
-static int split_linear_mapping(unsigned long start, unsigned long end)
-{
-	return __split_linear_mapping_pgd(pgd_offset_k(start), start, end);
-}
-#endif	/* CONFIG_64BIT */
-
 static int __set_memory(unsigned long addr, int numpages, pgprot_t set_mask,
 			pgprot_t clear_mask)
 {
 	int ret;
 	unsigned long start = addr;
 	unsigned long end = start + PAGE_SIZE * numpages;
-	unsigned long __maybe_unused lm_start;
-	unsigned long __maybe_unused lm_end;
 	struct pageattr_masks masks = {
 		.set_mask = set_mask,
 		.clear_mask = clear_mask
@@ -276,72 +120,11 @@ static int __set_memory(unsigned long addr, int numpages, pgprot_t set_mask,
 		return 0;
 
 	mmap_write_lock(&init_mm);
-
-#ifdef CONFIG_64BIT
-	/*
-	 * We are about to change the permissions of a kernel mapping, we must
-	 * apply the same changes to its linear mapping alias, which may imply
-	 * splitting a huge mapping.
-	 */
-
-	if (is_vmalloc_or_module_addr((void *)start)) {
-		struct vm_struct *area = NULL;
-		int i, page_start;
-
-		area = find_vm_area((void *)start);
-		page_start = (start - (unsigned long)area->addr) >> PAGE_SHIFT;
-
-		for (i = page_start; i < page_start + numpages; ++i) {
-			lm_start = (unsigned long)page_address(area->pages[i]);
-			lm_end = lm_start + PAGE_SIZE;
-
-			ret = split_linear_mapping(lm_start, lm_end);
-			if (ret)
-				goto unlock;
-
-			ret = walk_page_range_novma(&init_mm, lm_start, lm_end,
-						    &pageattr_ops, NULL, &masks);
-			if (ret)
-				goto unlock;
-		}
-	} else if (is_kernel_mapping(start) || is_linear_mapping(start)) {
-		if (is_kernel_mapping(start)) {
-			lm_start = (unsigned long)lm_alias(start);
-			lm_end = (unsigned long)lm_alias(end);
-		} else {
-			lm_start = start;
-			lm_end = end;
-		}
-
-		ret = split_linear_mapping(lm_start, lm_end);
-		if (ret)
-			goto unlock;
-
-		ret = walk_page_range_novma(&init_mm, lm_start, lm_end,
-					    &pageattr_ops, NULL, &masks);
-		if (ret)
-			goto unlock;
-	}
-
 	ret =  walk_page_range_novma(&init_mm, start, end, &pageattr_ops, NULL,
 				     &masks);
-
-unlock:
-	mmap_write_unlock(&init_mm);
-
-	/*
-	 * We can't use flush_tlb_kernel_range() here as we may have split a
-	 * hugepage that is larger than that, so let's flush everything.
-	 */
-	flush_tlb_all();
-#else
-	ret =  walk_page_range_novma(&init_mm, start, end, &pageattr_ops, NULL,
-				     &masks);
-
 	mmap_write_unlock(&init_mm);
 
 	flush_tlb_kernel_range(start, end);
-#endif
 
 	return ret;
 }
@@ -376,14 +159,36 @@ int set_memory_nx(unsigned long addr, int numpages)
 
 int set_direct_map_invalid_noflush(struct page *page)
 {
-	return __set_memory((unsigned long)page_address(page), 1,
-			    __pgprot(0), __pgprot(_PAGE_PRESENT));
+	int ret;
+	unsigned long start = (unsigned long)page_address(page);
+	unsigned long end = start + PAGE_SIZE;
+	struct pageattr_masks masks = {
+		.set_mask = __pgprot(0),
+		.clear_mask = __pgprot(_PAGE_PRESENT)
+	};
+
+	mmap_read_lock(&init_mm);
+	ret = walk_page_range(&init_mm, start, end, &pageattr_ops, &masks);
+	mmap_read_unlock(&init_mm);
+
+	return ret;
 }
 
 int set_direct_map_default_noflush(struct page *page)
 {
-	return __set_memory((unsigned long)page_address(page), 1,
-			    PAGE_KERNEL, __pgprot(_PAGE_EXEC));
+	int ret;
+	unsigned long start = (unsigned long)page_address(page);
+	unsigned long end = start + PAGE_SIZE;
+	struct pageattr_masks masks = {
+		.set_mask = PAGE_KERNEL,
+		.clear_mask = __pgprot(0)
+	};
+
+	mmap_read_lock(&init_mm);
+	ret = walk_page_range(&init_mm, start, end, &pageattr_ops, &masks);
+	mmap_read_unlock(&init_mm);
+
+	return ret;
 }
 
 #ifdef CONFIG_DEBUG_PAGEALLOC
diff --git a/drivers/base/arch_numa.c b/drivers/base/arch_numa.c
index 96281de7010d..4b0b582bfc1a 100644
--- a/drivers/base/arch_numa.c
+++ b/drivers/base/arch_numa.c
@@ -359,7 +359,11 @@ static int __init numa_alloc_distance(void)
 	int i, j;
 
 	size = nr_node_ids * nr_node_ids * sizeof(numa_distance[0]);
+#ifdef CONFIG_HIGHMEM
+	numa_distance = memblock_alloc_low(size, PAGE_SIZE);
+#else
 	numa_distance = memblock_alloc(size, PAGE_SIZE);
+#endif
 	if (WARN_ON(!numa_distance))
 		return -ENOMEM;
 
diff --git a/drivers/char/ipmi/ipmi_si_hardcode.c b/drivers/char/ipmi/ipmi_si_hardcode.c
index ed5e91b1e040..210644f3d863 100644
--- a/drivers/char/ipmi/ipmi_si_hardcode.c
+++ b/drivers/char/ipmi/ipmi_si_hardcode.c
@@ -6,7 +6,7 @@
 #include <linux/platform_device.h>
 #include "ipmi_si.h"
 #include "ipmi_plat_data.h"
-
+#include <linux/pci.h>
 /*
  * There can be 4 IO ports passed in (with or without IRQs), 4 addresses,
  * a default IO port, and 1 ACPI/SPMI address.  That sets SI_MAX_DRIVERS.
@@ -90,6 +90,24 @@ static void __init ipmi_hardcode_init_one(const char *si_type_str,
 	ipmi_platform_add("hardcode-ipmi-si", i, &p);
 }
 
+#ifdef CONFIG_ARCH_SOPHGO
+static void variable_init(struct pci_dev *pdev)
+{
+	unsigned long addr_data = pci_resource_start(pdev, 1) + 0x0e80;
+	// printk("addr_data=0x%lx\n", addr_data);
+	strcpy(si_type_str, "kcs");
+	addrs[0]        = addr_data;
+	num_addrs       = 1;
+	regspacings[0]  = 4;
+	num_regspacings = 1;
+	regsizes[0]     = 4;
+	num_regsizes    = 1;
+	irqs[0]         = 0;
+	num_irqs        = 1;
+	slave_addrs[0]  = 0;
+	num_slave_addrs = 1;
+}
+#endif
 void __init ipmi_hardcode_init(void)
 {
 	unsigned int i;
@@ -97,7 +115,11 @@ void __init ipmi_hardcode_init(void)
 	char *si_type[SI_MAX_PARMS];
 
 	memset(si_type, 0, sizeof(si_type));
-
+#ifdef CONFIG_ARCH_SOPHGO
+	struct pci_dev *pdev = pci_get_device(0x1A03, 0x2402, NULL);
+	if (pdev != NULL)
+		variable_init(pdev);
+#endif
 	/* Parse out the si_type string into its components. */
 	str = si_type_str;
 	if (*str != '\0') {
diff --git a/drivers/char/ipmi/ipmi_si_intf.c b/drivers/char/ipmi/ipmi_si_intf.c
index 373ee71811e3..8e316d49bce1 100644
--- a/drivers/char/ipmi/ipmi_si_intf.c
+++ b/drivers/char/ipmi/ipmi_si_intf.c
@@ -2158,7 +2158,8 @@ static int __init init_ipmi_si(void)
 		return 0;
 	}
 }
-module_init(init_ipmi_si);
+// module_init(init_ipmi_si);
+late_initcall(init_ipmi_si);
 
 static void wait_msg_processed(struct smi_info *smi_info)
 {
diff --git a/drivers/char/ipmi/ipmi_si_pci.c b/drivers/char/ipmi/ipmi_si_pci.c
index 74fa2055868b..6a935100e1ae 100644
--- a/drivers/char/ipmi/ipmi_si_pci.c
+++ b/drivers/char/ipmi/ipmi_si_pci.c
@@ -111,6 +111,12 @@ static int ipmi_pci_probe(struct pci_dev *pdev,
 	io.regsize = DEFAULT_REGSIZE;
 	io.regshift = 0;
 
+#ifdef CONFIG_ARCH_SOPHGO
+	io.addr_data = pci_resource_start(pdev, 1) + 0x0e80;
+	io.slave_addr = 0x20;
+	io.regspacing = 4;
+	io.regsize = 4;
+#endif
 	io.irq = pdev->irq;
 	if (io.irq)
 		io.irq_setup = ipmi_std_irq_setup;
diff --git a/drivers/clk/Kconfig b/drivers/clk/Kconfig
index c30099866174..1578cc32432d 100644
--- a/drivers/clk/Kconfig
+++ b/drivers/clk/Kconfig
@@ -501,6 +501,7 @@ source "drivers/clk/visconti/Kconfig"
 source "drivers/clk/x86/Kconfig"
 source "drivers/clk/xilinx/Kconfig"
 source "drivers/clk/zynqmp/Kconfig"
+source "drivers/clk/thead/Kconfig"
 
 # Kunit test cases
 config CLK_KUNIT_TEST
diff --git a/drivers/clk/Makefile b/drivers/clk/Makefile
index 18969cbd4bb1..ebecef837e58 100644
--- a/drivers/clk/Makefile
+++ b/drivers/clk/Makefile
@@ -124,6 +124,7 @@ obj-$(CONFIG_ARCH_STM32)		+= stm32/
 obj-y					+= starfive/
 obj-$(CONFIG_ARCH_SUNXI)		+= sunxi/
 obj-y					+= sunxi-ng/
+obj-$(CONFIG_ARCH_SOPHGO)		+= sophgo/
 obj-$(CONFIG_ARCH_TEGRA)		+= tegra/
 obj-y					+= ti/
 obj-$(CONFIG_CLK_UNIPHIER)		+= uniphier/
@@ -136,3 +137,4 @@ endif
 obj-y					+= xilinx/
 obj-$(CONFIG_ARCH_ZYNQ)			+= zynq/
 obj-$(CONFIG_COMMON_CLK_ZYNQMP)         += zynqmp/
+obj-$(CONFIG_ARCH_THEAD)                += thead/
diff --git a/drivers/clk/sophgo/Makefile b/drivers/clk/sophgo/Makefile
new file mode 100644
index 000000000000..55997fc07b5b
--- /dev/null
+++ b/drivers/clk/sophgo/Makefile
@@ -0,0 +1,3 @@
+obj-$(CONFIG_ARCH_SOPHGO)	+= clk-dummy.o
+obj-$(CONFIG_ARCH_SOPHGO)	+= clk.o
+obj-$(CONFIG_ARCH_SOPHGO)	+= clk-mango.o
diff --git a/drivers/clk/sophgo/clk-dummy.c b/drivers/clk/sophgo/clk-dummy.c
new file mode 100644
index 000000000000..99af0e6dae6a
--- /dev/null
+++ b/drivers/clk/sophgo/clk-dummy.c
@@ -0,0 +1,600 @@
+/*
+ * Copyright (c) 2022 SOPHGO
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#include <linux/of_device.h>
+#include <linux/platform_device.h>
+#include <linux/spinlock.h>
+#include <linux/mfd/syscon.h>
+#include <linux/io.h>
+#include <linux/of_address.h>
+#include <linux/string.h>
+#include <linux/log2.h>
+
+#include "clk.h"
+
+/*
+ * @hw:		handle between common and hardware-specific interfaces
+ * @reg:	register containing divider
+ * @shift:	shift to the divider bit field
+ * @width:	width of the divider bit field
+ * @initial_val:initial value of the divider
+ * @table:	the div table that the divider supports
+ * @lock:	register lock
+ */
+struct mango_clk_divider {
+	struct clk_hw	hw;
+	void __iomem	*reg;
+	u8		shift;
+	u8		width;
+	u8		flags;
+	u32		initial_val;
+	const struct clk_div_table *table;
+	spinlock_t	*lock;
+};
+
+static unsigned long mango_clk_divider_recalc_rate(struct clk_hw *hw,
+						unsigned long parent_rate)
+{
+	struct device_node *node;
+	struct of_phandle_args clkspec;
+	int rc, index = 0;
+	u32 rate;
+	struct property *prop;
+	const __be32 *cur;
+	struct clk *clk;
+
+	node = of_find_node_by_name(NULL, "default_rates");
+
+	of_property_for_each_u32 (node, "clock-rates", prop, cur, rate) {
+		if (rate) {
+			rc = of_parse_phandle_with_args(node, "clocks",
+							"#clock-cells", index, &clkspec);
+			if (rc < 0) {
+				/* skip empty (null) phandles */
+				if (rc == -ENOENT)
+					continue;
+				else
+					return rc;
+			}
+
+			clk = of_clk_get_from_provider(&clkspec);
+			if (IS_ERR(clk))
+				return PTR_ERR(clk);
+			if (!strcmp(clk_hw_get_name(hw), __clk_get_name(clk)))
+				return rate;
+		}
+		index++;
+	}
+	return 0;
+}
+
+static long mango_clk_divider_round_rate(struct clk_hw *hw, unsigned long rate,
+				      unsigned long *prate)
+{
+	return rate;
+}
+
+static int mango_clk_divider_set_rate(struct clk_hw *hw, unsigned long rate,
+				   unsigned long parent_rate)
+{
+	return 0;
+}
+
+/*
+ * @hw: ccf use to hook get mango_pll_clock
+ * @parent_rate: parent rate
+ *
+ * The is function will be called through clk_get_rate
+ * and return current rate after decoding reg value
+ */
+static unsigned long mango_clk_pll_recalc_rate(struct clk_hw *hw,
+					    unsigned long parent_rate)
+{
+	struct device_node *node;
+	struct of_phandle_args clkspec;
+	int rc, index = 0;
+	u32 rate;
+	struct property *prop;
+	const __be32 *cur;
+
+	node = of_find_node_by_name(NULL, "default_rates");
+
+	of_property_for_each_u32 (node, "clock-rates", prop, cur, rate) {
+		if (rate) {
+			rc = of_parse_phandle_with_args(node, "clocks",
+							"#clock-cells", index, &clkspec);
+			if (rc < 0) {
+				/* skip empty (null) phandles */
+				if (rc == -ENOENT)
+					continue;
+				else
+					return rc;
+			}
+
+			if (!strncmp(clk_hw_get_name(hw), clkspec.np->name, 4))
+				return rate;
+		}
+		index++;
+	}
+	return 0;
+}
+
+static long mango_clk_pll_round_rate(struct clk_hw *hw,
+				  unsigned long req_rate, unsigned long *prate)
+{
+	return req_rate;
+}
+
+static int mango_clk_pll_determine_rate(struct clk_hw *hw,
+				     struct clk_rate_request *req)
+{
+	req->rate = mango_clk_pll_round_rate(hw, min(req->rate, req->max_rate),
+					  &req->best_parent_rate);
+	return 0;
+}
+
+static int mango_clk_pll_set_rate(struct clk_hw *hw, unsigned long rate,
+			       unsigned long parent_rate)
+{
+	return 0;
+}
+
+const struct clk_ops dm_mango_clk_divider_ops = {
+	.recalc_rate = mango_clk_divider_recalc_rate,
+	.round_rate = mango_clk_divider_round_rate,
+	.set_rate = mango_clk_divider_set_rate,
+};
+
+const struct clk_ops dm_mango_clk_divider_ro_ops = {
+	.recalc_rate = mango_clk_divider_recalc_rate,
+	.round_rate = mango_clk_divider_round_rate,
+};
+
+const struct clk_ops dm_mango_clk_pll_ops = {
+	.recalc_rate = mango_clk_pll_recalc_rate,
+	.round_rate = mango_clk_pll_round_rate,
+	.determine_rate = mango_clk_pll_determine_rate,
+	.set_rate = mango_clk_pll_set_rate,
+};
+
+const struct clk_ops dm_mango_clk_pll_ro_ops = {
+	.recalc_rate = mango_clk_pll_recalc_rate,
+	.round_rate = mango_clk_pll_round_rate,
+};
+
+struct mux_cb_clk_name {
+	const char *name;
+	struct list_head node;
+};
+
+static struct list_head mux_cb_clk_name_list =
+	LIST_HEAD_INIT(mux_cb_clk_name_list);
+static int mux_notifier_cb(struct notifier_block *nb,
+				unsigned long event, void *data)
+{
+	int ret = 0;
+	static unsigned char mux_id = 1;
+	struct clk_notifier_data *ndata = data;
+	struct clk_hw *hw = __clk_get_hw(ndata->clk);
+	const struct clk_ops *ops = &clk_mux_ops;
+	struct mux_cb_clk_name *cb_lsit;
+
+	if (event == PRE_RATE_CHANGE) {
+		struct clk_hw *hw_p = clk_hw_get_parent(hw);
+
+		cb_lsit = kmalloc(sizeof(*cb_lsit), GFP_KERNEL);
+		if (cb_lsit) {
+			INIT_LIST_HEAD(&cb_lsit->node);
+			list_add_tail(&cb_lsit->node, &mux_cb_clk_name_list);
+		} else {
+			pr_err("mux cb kmalloc mem fail\n");
+			goto out;
+		}
+
+		cb_lsit->name = clk_hw_get_name(hw_p);
+		mux_id = ops->get_parent(hw);
+		if (mux_id > 1) {
+			ret = 1;
+			goto out;
+		}
+		ops->set_parent(hw, !mux_id);
+	} else if (event == POST_RATE_CHANGE) {
+		struct clk_hw *hw_p = clk_hw_get_parent(hw);
+
+		cb_lsit = list_first_entry_or_null(&mux_cb_clk_name_list,
+						typeof(*cb_lsit), node);
+		if (cb_lsit) {
+			const char *pre_name = cb_lsit->name;
+
+			list_del_init(&cb_lsit->node);
+			kfree(cb_lsit);
+			if (strcmp(clk_hw_get_name(hw_p), pre_name))
+				goto out;
+		}
+
+		ops->set_parent(hw, mux_id);
+	}
+
+out:
+	return notifier_from_errno(ret);
+}
+
+int dm_set_default_clk_rates(struct device_node *node)
+{
+	struct of_phandle_args clkspec;
+	struct property *prop;
+	const __be32 *cur;
+	int rc, index = 0;
+	struct clk *clk;
+	u32 rate;
+
+	of_property_for_each_u32 (node, "clock-rates", prop, cur, rate) {
+		if (rate) {
+			rc = of_parse_phandle_with_args(node, "clocks",
+							"#clock-cells", index, &clkspec);
+			if (rc < 0) {
+				/* skip empty (null) phandles */
+				if (rc == -ENOENT)
+					continue;
+				else
+					return rc;
+			}
+
+			clk = of_clk_get_from_provider(&clkspec);
+			if (IS_ERR(clk)) {
+				pr_warn("clk: couldn't get clock %d for %s\n",
+					index, node->full_name);
+				return PTR_ERR(clk);
+			}
+
+			rc = clk_set_rate(clk, rate);
+			if (rc < 0)
+				pr_err("clk: couldn't set %s clk rate to %d (%d), current rate: %ld\n",
+				       __clk_get_name(clk), rate, rc,
+				       clk_get_rate(clk));
+			clk_put(clk);
+		}
+		index++;
+	}
+
+	return 0;
+}
+
+static struct clk *__register_divider_clks(struct device *dev, const char *name,
+					   const char *parent_name,
+					   unsigned long flags,
+					   void __iomem *reg, u8 shift,
+					   u8 width, u32 initial_val,
+					   u8 clk_divider_flags,
+					   const struct clk_div_table *table,
+					   spinlock_t *lock)
+{
+	struct mango_clk_divider *div;
+	struct clk_hw *hw;
+	struct clk_init_data init;
+	int ret;
+
+	if (clk_divider_flags & CLK_DIVIDER_HIWORD_MASK) {
+		if (width + shift > 16) {
+			pr_warn("divider value exceeds LOWORD field\n");
+			return ERR_PTR(-EINVAL);
+		}
+	}
+
+	/* allocate the divider */
+	div = kzalloc(sizeof(*div), GFP_KERNEL);
+	if (!div)
+		return ERR_PTR(-ENOMEM);
+
+	init.name = name;
+	if (clk_divider_flags & CLK_DIVIDER_READ_ONLY)
+		init.ops = &dm_mango_clk_divider_ro_ops;
+	else
+		init.ops = &dm_mango_clk_divider_ops;
+	init.flags = flags;
+	init.parent_names = (parent_name ? &parent_name : NULL);
+	init.num_parents = (parent_name ? 1 : 0);
+
+	/* struct mango_clk_divider assignments */
+	div->reg = reg;
+	div->shift = shift;
+	div->width = width;
+	div->flags = clk_divider_flags;
+	div->lock = lock;
+	div->hw.init = &init;
+	div->table = table;
+	div->initial_val = initial_val;
+
+	/* register the clock */
+	hw = &div->hw;
+	ret = clk_hw_register(dev, hw);
+	if (ret) {
+		kfree(div);
+		hw = ERR_PTR(ret);
+		return ERR_PTR(-EBUSY);
+	}
+
+	return hw->clk;
+}
+
+static inline int register_provider_clks
+(struct device_node *node, struct mango_clk_data *clk_data, int clk_num)
+{
+	return of_clk_add_provider(node, of_clk_src_onecell_get,
+				   &clk_data->clk_data);
+}
+
+static int register_gate_clks(struct device *dev, struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_gate_clock *gate_clks = table->gate_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->gate_clks_num;
+	int i;
+
+	for (i = 0; i < clk_num; i++) {
+		clk = clk_register_gate(
+			dev, gate_clks[i].name, gate_clks[i].parent_name,
+			gate_clks[i].flags | CLK_IS_CRITICAL, base + gate_clks[i].offset,
+			gate_clks[i].bit_idx, gate_clks[i].gate_flags,
+			&clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				gate_clks[i].name);
+			goto err;
+		}
+
+		if (gate_clks[i].alias)
+			clk_register_clkdev(clk, gate_clks[i].alias, NULL);
+
+		clk_data->clk_data.clks[gate_clks[i].id] = clk;
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_gate(clk_data->clk_data.clks[gate_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+static int register_divider_clks(struct device *dev,
+				 struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_divider_clock *div_clks = table->div_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->div_clks_num;
+	int i, val;
+
+	for (i = 0; i < clk_num; i++) {
+		clk = __register_divider_clks(
+			NULL, div_clks[i].name, div_clks[i].parent_name,
+			div_clks[i].flags, base + div_clks[i].offset,
+			div_clks[i].shift, div_clks[i].width,
+			div_clks[i].initial_val,
+			(div_clks[i].initial_sel & MANGO_CLK_USE_INIT_VAL) ?
+				div_clks[i].div_flags | CLK_DIVIDER_READ_ONLY :
+				div_clks[i].div_flags,
+			div_clks[i].table, &clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				div_clks[i].name);
+			goto err;
+		}
+
+		clk_data->clk_data.clks[div_clks[i].id] = clk;
+
+		if (div_clks[i].initial_sel == MANGO_CLK_USE_REG_VAL) {
+			regmap_read(clk_data->syscon_top, div_clks[i].offset,
+				    &val);
+
+			/*
+			 * set a default divider factor,
+			 * clk driver should not select divider clock as the
+			 * clock source, before set the divider by right process
+			 * (assert div, set div factor, de assert div).
+			 */
+			if (div_clks[i].initial_val > 0)
+				val |= (div_clks[i].initial_val << 16 | 1 << 3);
+			else {
+				/*
+				 * the div register is config to use divider factor, don't change divider
+				 */
+				if (!(val >> 3 & 0x1))
+					val |= 1 << 16;
+			}
+
+			regmap_write(clk_data->syscon_top, div_clks[i].offset,
+				     val);
+		}
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_divider(clk_data->clk_data.clks[div_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+static int register_mux_clks(struct device *dev, struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_mux_clock *mux_clks = table->mux_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->mux_clks_num;
+	int i;
+
+	for (i = 0; i < clk_num; i++) {
+		u32 mask = BIT(mux_clks[i].width) - 1;
+
+		clk = clk_register_mux_table(
+			dev, mux_clks[i].name, mux_clks[i].parent_names,
+			mux_clks[i].num_parents, mux_clks[i].flags,
+			base + mux_clks[i].offset, mux_clks[i].shift, mask,
+			mux_clks[i].mux_flags, mux_clks[i].table,
+			&clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				mux_clks[i].name);
+			goto err;
+		}
+
+		clk_data->clk_data.clks[mux_clks[i].id] = clk;
+
+		if (!(mux_clks[i].flags & CLK_MUX_READ_ONLY)) {
+			struct clk *parent;
+			struct notifier_block *clk_nb;
+
+			/* set mux clock default parent here, it's parent index
+			 * value is read from the mux clock reg. dts can override
+			 * setting the mux clock parent later.
+			 */
+			parent = clk_get_parent(clk);
+			clk_set_parent(clk, parent);
+
+			/* add a notify callback function */
+			clk_nb = kzalloc(sizeof(*clk_nb), GFP_KERNEL);
+			if (!clk_nb)
+				goto err;
+			clk_nb->notifier_call = mux_notifier_cb;
+			if (clk_notifier_register(clk, clk_nb))
+				pr_err("%s: failed to register clock notifier for %s\n",
+					__func__, mux_clks[i].name);
+		}
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_mux(clk_data->clk_data.clks[mux_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+/* pll clock init */
+int dm_mango_register_pll_clks(struct device_node *node,
+			 struct mango_clk_data *clk_data, const char *clk_name)
+{
+	struct clk *clk = NULL;
+	struct mango_pll_clock *pll_clks;
+	int i, ret = 0;
+	const struct clk_ops *local_ops;
+
+	pll_clks = (struct mango_pll_clock *)clk_data->table->pll_clks;
+	for (i = 0; i < clk_data->table->pll_clks_num; i++) {
+		if (!strcmp(clk_name,  pll_clks[i].name)) {
+			/* have to assigne pll_clks.syscon_top first
+			 * since clk_register_composite will need it
+			 * to calculate current rate.
+			 */
+			pll_clks[i].syscon_top = clk_data->syscon_top;
+			pll_clks[i].lock = &clk_data->lock;
+			if (pll_clks[i].ini_flags & MANGO_CLK_RO)
+				local_ops = &dm_mango_clk_pll_ro_ops;
+			else
+				local_ops = &dm_mango_clk_pll_ops;
+			clk = clk_register_composite(
+				NULL, pll_clks[i].name, &pll_clks[i].parent_name,
+				1, NULL, NULL, &pll_clks[i].hw, local_ops,
+				NULL, NULL, pll_clks[i].flags);
+
+			if (IS_ERR(clk)) {
+				pr_err("%s: failed to register clock %s\n", __func__,
+					pll_clks[i].name);
+				ret = -EINVAL;
+				goto out;
+			}
+			ret = of_clk_add_provider(node, of_clk_src_simple_get, clk);
+			if (ret)
+				clk_unregister(clk);
+		} else {
+			continue;
+		}
+	}
+
+out:
+	return ret;
+}
+
+/* mux clk init */
+int dm_mango_register_mux_clks(struct device_node *node, struct mango_clk_data *clk_data)
+{
+	int ret;
+	int count;
+	struct clk **clk_table;
+
+	count = clk_data->table->mux_clks_num + clk_data->table->gate_clks_num;
+	clk_table = kcalloc(count, sizeof(*clk_table), GFP_KERNEL);
+	if (!clk_table)
+		return -ENOMEM;
+
+	clk_data->clk_data.clks = clk_table;
+	clk_data->clk_data.clk_num = count;
+
+	ret = register_mux_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_gate_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_provider_clks(node, clk_data, count);
+	if (ret)
+		goto err;
+
+	return 0;
+err:
+	kfree(clk_table);
+	return ret;
+}
+
+/* pll divider init */
+int dm_mango_register_div_clks(struct device_node *node, struct mango_clk_data *clk_data)
+{
+	int ret;
+	int count;
+
+	struct clk **clk_table;
+
+	count = clk_data->table->div_clks_num + clk_data->table->gate_clks_num;
+	clk_table = kcalloc(count, sizeof(*clk_table), GFP_KERNEL);
+	if (!clk_table)
+		return -ENOMEM;
+
+	clk_data->clk_data.clks = clk_table;
+	clk_data->clk_data.clk_num = count;
+
+	ret = register_divider_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_gate_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_provider_clks(node, clk_data, count);
+	if (ret)
+		goto err;
+
+
+	return 0;
+err:
+	kfree(clk_table);
+	pr_err("%s error %d\n", __func__, ret);
+	return ret;
+}
diff --git a/drivers/clk/sophgo/clk-mango.c b/drivers/clk/sophgo/clk-mango.c
new file mode 100644
index 000000000000..894f2f177db8
--- /dev/null
+++ b/drivers/clk/sophgo/clk-mango.c
@@ -0,0 +1,977 @@
+/*
+ * Copyright (c) 2022 SOPHGO
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#include <linux/of_address.h>
+#include <linux/mfd/syscon.h>
+#include <dt-bindings/clock/sophgo-mango-clock.h>
+
+#include "clk.h"
+
+/* fixed clocks */
+struct mango_pll_clock mango_root_pll_clks[] = {
+	{
+		.id = FPLL_CLK,
+		.name = "fpll_clock",
+		.parent_name = "cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+	}, {
+		.id = DPLL0_CLK,
+		.name = "dpll0_clock",
+		.parent_name = "cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	}, {
+		.id = DPLL1_CLK,
+		.name = "dpll1_clock",
+		.parent_name = "cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	}, {
+		.id = MPLL_CLK,
+		.name = "mpll_clock",
+		.parent_name = "cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	},{
+		.id = FPLL_CLK,
+		.name = "s1_fpll_clock",
+		.parent_name = "s1_cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+	}, {
+		.id = DPLL0_CLK,
+		.name = "s1_dpll0_clock",
+		.parent_name = "s1_cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	}, {
+		.id = DPLL1_CLK,
+		.name = "s1_dpll1_clock",
+		.parent_name = "s1_cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.ini_flags = MANGO_CLK_RO,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	}, {
+		.id = MPLL_CLK,
+		.name = "s1_mpll_clock",
+		.parent_name = "s1_cgi",
+		.flags = CLK_GET_RATE_NOCACHE | CLK_GET_ACCURACY_NOCACHE,
+		.status_offset = 0xc0,
+		.enable_offset = 0xc4,
+	}
+};
+
+/* divider clocks */
+static const struct mango_divider_clock s0_div_clks[] = {
+	{ DIV_CLK_MPLL_RP_CPU_NORMAL_0, "clk_div_rp_cpu_normal_0", "clk_gate_rp_cpu_normal_div0",
+		0, 0x2044, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_MPLL_AXI_DDR_0, "clk_div_axi_ddr_0", "clk_gate_axi_ddr_div0",
+		0, 0x20a8, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, 5},
+	{ DIV_CLK_FPLL_DDR01_1, "clk_div_ddr01_1", "clk_gate_ddr01_div1",
+		0, 0x20b0, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_FPLL_DDR23_1, "clk_div_ddr23_1", "clk_gate_ddr23_div1",
+		0, 0x20b8, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_FPLL_RP_CPU_NORMAL_1, "clk_div_rp_cpu_normal_1", "clk_gate_rp_cpu_normal_div1",
+		0, 0x2040, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_50M_A53, "clk_div_50m_a53", "fpll_clock",
+		0, 0x2048, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_RP_CMN_DIV2, "clk_div_top_rp_cmn_div2", "clk_mux_rp_cpu_normal",
+		0, 0x204c, 16, 16, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_UART_500M, "clk_div_uart_500m", "fpll_clock",
+		0, 0x2050, 16, 7, CLK_DIVIDER_READ_ONLY, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_AHB_LPC, "clk_div_ahb_lpc", "fpll_clock",
+		0, 0x2054, 16, 16, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_EFUSE, "clk_div_efuse", "fpll_clock",
+		0, 0x2078, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TX_ETH0, "clk_div_tx_eth0", "fpll_clock",
+		0, 0x2080, 16, 11, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_PTP_REF_I_ETH0, "clk_div_ptp_ref_i_eth0", "fpll_clock",
+		0, 0x2084, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_REF_ETH0, "clk_div_ref_eth0", "fpll_clock",
+		0, 0x2088, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_EMMC, "clk_div_emmc", "fpll_clock",
+		0, 0x208c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_SD, "clk_div_sd", "fpll_clock",
+		0, 0x2094, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_AXI0, "clk_div_top_axi0", "fpll_clock",
+		0, 0x209c, 16, 5, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_AXI_HSPERI, "clk_div_top_axi_hsperi", "fpll_clock",
+		0, 0x20a0, 16, 5, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_AXI_DDR_1, "clk_div_axi_ddr_1", "clk_gate_axi_ddr_div1",
+		0, 0x20a4, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, 5},
+	{ DIV_CLK_FPLL_DIV_TIMER1, "clk_div_timer1", "clk_div_50m_a53",
+		0, 0x2058, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER2, "clk_div_timer2", "clk_div_50m_a53",
+		0, 0x205c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER3, "clk_div_timer3", "clk_div_50m_a53",
+		0, 0x2060, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER4, "clk_div_timer4", "clk_div_50m_a53",
+		0, 0x2064, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER5, "clk_div_timer5", "clk_div_50m_a53",
+		0, 0x2068, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER6, "clk_div_timer6", "clk_div_50m_a53",
+		0, 0x206c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER7, "clk_div_timer7", "clk_div_50m_a53",
+		0, 0x2070, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER8, "clk_div_timer8", "clk_div_50m_a53",
+		0, 0x2074, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_100K_EMMC, "clk_div_100k_emmc", "clk_div_top_axi0",
+		0, 0x2090, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_100K_SD, "clk_div_100k_sd", "clk_div_top_axi0",
+		0, 0x2098, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_GPIO_DB, "clk_div_gpio_db", "clk_div_top_axi0",
+		0, 0x207c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_DPLL0_DDR01_0, "clk_div_ddr01_0", "clk_gate_ddr01_div0",
+		0, 0x20ac, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_DPLL1_DDR23_0, "clk_div_ddr23_0", "clk_gate_ddr23_div0",
+		0, 0x20b4, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+};
+
+/* gate clocks */
+static const struct mango_gate_clock s0_gate_clks[] = {
+	{ GATE_CLK_RP_CPU_NORMAL_DIV0, "clk_gate_rp_cpu_normal_div1", "mpll_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR_DIV0, "clk_gate_axi_ddr_div1", "mpll_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_DDR01_DIV0, "clk_gate_ddr01_div0", "fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23_DIV0, "clk_gate_ddr23_div0", "fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 15, 0 },
+	{ GATE_CLK_RP_CPU_NORMAL_DIV1, "clk_gate_rp_cpu_normal_div0", "fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR_DIV1, "clk_gate_axi_ddr_div0", "fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_DDR01_DIV1, "clk_gate_ddr01_div1", "dpll0_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23_DIV1, "clk_gate_ddr23_div1", "dpll1_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 15, 0 },
+	{ GATE_CLK_A53_50M, "clk_gate_a53_50m", "clk_div_50m_a53",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 1, 0 },
+	{ GATE_CLK_TOP_RP_CMN_DIV2, "clk_gate_top_rp_cmn_div2", "clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 2, 0 },
+	{ GATE_CLK_AXI_PCIE0, "clk_gate_axi_pcie0", "clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 8, 0 },
+	{ GATE_CLK_AXI_PCIE1, "clk_gate_axi_pcie1", "clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 9, 0 },
+	{ GATE_CLK_HSDMA, "clk_gate_hsdma", "clk_gate_top_rp_cmn_div2",
+		CLK_SET_RATE_PARENT, 0x2004, 10, 0 },
+	{ GATE_CLK_EMMC_100M, "clk_gate_emmc", "clk_div_emmc",
+		CLK_SET_RATE_PARENT, 0x2004, 3, 0 },
+	{ GATE_CLK_SD_100M, "clk_gate_sd", "clk_div_sd",
+		CLK_SET_RATE_PARENT, 0x2004, 6, 0 },
+	{ GATE_CLK_TX_ETH0, "clk_gate_tx_eth0", "clk_div_tx_eth0",
+		CLK_SET_RATE_PARENT, 0x2000, 30, 0 },
+	{ GATE_CLK_PTP_REF_I_ETH0, "clk_gate_ptp_ref_i_eth0", "clk_div_ptp_ref_i_eth0",
+		CLK_SET_RATE_PARENT, 0x2004, 0, 0 },
+	{ GATE_CLK_REF_ETH0, "clk_gate_ref_eth0", "clk_div_ref_eth0",
+		CLK_SET_RATE_PARENT, 0x2004, 1, 0 },
+	{ GATE_CLK_UART_500M, "clk_gate_uart_500m", "clk_div_uart_500m",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 4, 0 },
+	{ GATE_CLK_AHB_LPC, "clk_gate_ahb_lpc", "clk_div_ahb_lpc",
+		CLK_SET_RATE_PARENT, 0x2000, 7, 0 },
+	{ GATE_CLK_EFUSE, "clk_gate_efuse", "clk_div_efuse",
+		CLK_SET_RATE_PARENT, 0x2000, 20, 0},
+	{ GATE_CLK_TOP_AXI0, "clk_gate_top_axi0", "clk_div_top_axi0",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 11, 0 },
+	{ GATE_CLK_TOP_AXI_HSPERI, "clk_gate_top_axi_hsperi", "clk_div_top_axi_hsperi",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 12, 0 },
+	{ GATE_CLK_AHB_ROM, "clk_gate_ahb_rom", "clk_gate_top_axi0",
+		0, 0x2000, 8, 0 },
+	{ GATE_CLK_AHB_SF, "clk_gate_ahb_sf", "clk_gate_top_axi0",
+		0, 0x2000, 9, 0 },
+	{ GATE_CLK_AXI_SRAM, "clk_gate_axi_sram", "clk_gate_top_axi0",
+		CLK_IGNORE_UNUSED, 0x2000, 10, 0 },
+	{ GATE_CLK_APB_TIMER, "clk_gate_apb_timer", "clk_gate_top_axi0",
+		CLK_IGNORE_UNUSED, 0x2000, 11, 0 },
+	{ GATE_CLK_APB_EFUSE, "clk_gate_apb_efuse", "clk_gate_top_axi0",
+		0, 0x2000, 21, 0 },
+	{ GATE_CLK_APB_GPIO, "clk_gate_apb_gpio", "clk_gate_top_axi0",
+		0, 0x2000, 22, 0 },
+	{ GATE_CLK_APB_GPIO_INTR, "clk_gate_apb_gpio_intr", "clk_gate_top_axi0",
+		CLK_IS_CRITICAL, 0x2000, 23, 0 },
+	{ GATE_CLK_APB_I2C, "clk_gate_apb_i2c", "clk_gate_top_axi0",
+		0, 0x2000, 26, 0 },
+	{ GATE_CLK_APB_WDT, "clk_gate_apb_wdt", "clk_gate_top_axi0",
+		0, 0x2000, 27, 0 },
+	{ GATE_CLK_APB_PWM, "clk_gate_apb_pwm", "clk_gate_top_axi0",
+		0, 0x2000, 28, 0 },
+	{ GATE_CLK_APB_RTC, "clk_gate_apb_rtc", "clk_gate_top_axi0",
+		0, 0x2000, 29, 0 },
+	{ GATE_CLK_SYSDMA_AXI, "clk_gate_sysdma_axi", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 3, 0 },
+	{ GATE_CLK_APB_UART, "clk_gate_apb_uart", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 5, 0 },
+	{ GATE_CLK_AXI_DBG_I2C, "clk_gate_axi_dbg_i2c", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 6, 0 },
+	{ GATE_CLK_APB_SPI, "clk_gate_apb_spi", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 25, 0 },
+	{ GATE_CLK_AXI_ETH0, "clk_gate_axi_eth0", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 31, 0 },
+	{ GATE_CLK_AXI_EMMC, "clk_gate_axi_emmc", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2004, 2, 0 },
+	{ GATE_CLK_AXI_SD, "clk_gate_axi_sd", "clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2004, 5, 0 },
+	{ GATE_CLK_TIMER1, "clk_gate_timer1", "clk_div_timer1",
+		CLK_SET_RATE_PARENT, 0x2000, 12, 0 },
+	{ GATE_CLK_TIMER2, "clk_gate_timer2", "clk_div_timer2",
+		CLK_SET_RATE_PARENT, 0x2000, 13, 0 },
+	{ GATE_CLK_TIMER3, "clk_gate_timer3", "clk_div_timer3",
+		CLK_SET_RATE_PARENT, 0x2000, 14, 0 },
+	{ GATE_CLK_TIMER4, "clk_gate_timer4", "clk_div_timer4",
+		CLK_SET_RATE_PARENT, 0x2000, 15, 0 },
+	{ GATE_CLK_TIMER5, "clk_gate_timer5", "clk_div_timer5",
+		CLK_SET_RATE_PARENT, 0x2000, 16, 0 },
+	{ GATE_CLK_TIMER6, "clk_gate_timer6", "clk_div_timer6",
+		CLK_SET_RATE_PARENT, 0x2000, 17, 0 },
+	{ GATE_CLK_TIMER7, "clk_gate_timer7", "clk_div_timer7",
+		CLK_SET_RATE_PARENT, 0x2000, 18, 0 },
+	{ GATE_CLK_TIMER8, "clk_gate_timer8", "clk_div_timer8",
+		CLK_SET_RATE_PARENT, 0x2000, 19, 0 },
+	{ GATE_CLK_100K_EMMC, "clk_gate_100k_emmc", "clk_div_100k_emmc",
+		CLK_SET_RATE_PARENT, 0x2004, 4, 0 },
+	{ GATE_CLK_100K_SD, "clk_gate_100k_sd", "clk_div_100k_sd",
+		CLK_SET_RATE_PARENT, 0x2004, 7, 0 },
+	{ GATE_CLK_GPIO_DB, "clk_gate_gpio_db", "clk_div_gpio_db",
+		CLK_SET_RATE_PARENT, 0x2000, 24, 0 },
+	{ GATE_CLK_DDR01, "clk_gate_ddr01", "clk_mux_ddr01",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23, "clk_gate_ddr23", "clk_mux_ddr23",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 15, 0 },
+	{ GATE_CLK_RP_CPU_NORMAL, "clk_gate_rp_cpu_normal", "clk_mux_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR, "clk_gate_axi_ddr", "clk_mux_axi_ddr",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_RXU0, "clk_gate_rxu0", "clk_gate_rp_cpu_normal",
+		0, 0x368, 0, 0 },
+	{ GATE_CLK_RXU1, "clk_gate_rxu1", "clk_gate_rp_cpu_normal",
+		0, 0x368, 1, 0 },
+	{ GATE_CLK_RXU2, "clk_gate_rxu2", "clk_gate_rp_cpu_normal",
+		0, 0x368, 2, 0 },
+	{ GATE_CLK_RXU3, "clk_gate_rxu3", "clk_gate_rp_cpu_normal",
+		0, 0x368, 3, 0 },
+	{ GATE_CLK_RXU4, "clk_gate_rxu4", "clk_gate_rp_cpu_normal",
+		0, 0x368, 4, 0 },
+	{ GATE_CLK_RXU5, "clk_gate_rxu5", "clk_gate_rp_cpu_normal",
+		0, 0x368, 5, 0 },
+	{ GATE_CLK_RXU6, "clk_gate_rxu6", "clk_gate_rp_cpu_normal",
+		0, 0x368, 6, 0 },
+	{ GATE_CLK_RXU7, "clk_gate_rxu7", "clk_gate_rp_cpu_normal",
+		0, 0x368, 7, 0 },
+	{ GATE_CLK_RXU8, "clk_gate_rxu8", "clk_gate_rp_cpu_normal",
+		0, 0x368, 8, 0 },
+	{ GATE_CLK_RXU9, "clk_gate_rxu9", "clk_gate_rp_cpu_normal",
+		0, 0x368, 9, 0 },
+	{ GATE_CLK_RXU10, "clk_gate_rxu10", "clk_gate_rp_cpu_normal",
+		0, 0x368, 10, 0 },
+	{ GATE_CLK_RXU11, "clk_gate_rxu11", "clk_gate_rp_cpu_normal",
+		0, 0x368, 11, 0 },
+	{ GATE_CLK_RXU12, "clk_gate_rxu12", "clk_gate_rp_cpu_normal",
+		0, 0x368, 12, 0 },
+	{ GATE_CLK_RXU13, "clk_gate_rxu13", "clk_gate_rp_cpu_normal",
+		0, 0x368, 13, 0 },
+	{ GATE_CLK_RXU14, "clk_gate_rxu14", "clk_gate_rp_cpu_normal",
+		0, 0x368, 14, 0 },
+	{ GATE_CLK_RXU15, "clk_gate_rxu15", "clk_gate_rp_cpu_normal",
+		0, 0x368, 15, 0 },
+	{ GATE_CLK_RXU16, "clk_gate_rxu16", "clk_gate_rp_cpu_normal",
+		0, 0x368, 16, 0 },
+	{ GATE_CLK_RXU17, "clk_gate_rxu17", "clk_gate_rp_cpu_normal",
+		0, 0x368, 17, 0 },
+	{ GATE_CLK_RXU18, "clk_gate_rxu18", "clk_gate_rp_cpu_normal",
+		0, 0x368, 18, 0 },
+	{ GATE_CLK_RXU19, "clk_gate_rxu19", "clk_gate_rp_cpu_normal",
+		0, 0x368, 19, 0 },
+	{ GATE_CLK_RXU20, "clk_gate_rxu20", "clk_gate_rp_cpu_normal",
+		0, 0x368, 20, 0 },
+	{ GATE_CLK_RXU21, "clk_gate_rxu21", "clk_gate_rp_cpu_normal",
+		0, 0x368, 21, 0 },
+	{ GATE_CLK_RXU22, "clk_gate_rxu22", "clk_gate_rp_cpu_normal",
+		0, 0x368, 22, 0 },
+	{ GATE_CLK_RXU23, "clk_gate_rxu23", "clk_gate_rp_cpu_normal",
+		0, 0x368, 23, 0 },
+	{ GATE_CLK_RXU24, "clk_gate_rxu24", "clk_gate_rp_cpu_normal",
+		0, 0x368, 24, 0 },
+	{ GATE_CLK_RXU25, "clk_gate_rxu25", "clk_gate_rp_cpu_normal",
+		0, 0x368, 25, 0 },
+	{ GATE_CLK_RXU26, "clk_gate_rxu26", "clk_gate_rp_cpu_normal",
+		0, 0x368, 26, 0 },
+	{ GATE_CLK_RXU27, "clk_gate_rxu27", "clk_gate_rp_cpu_normal",
+		0, 0x368, 27, 0 },
+	{ GATE_CLK_RXU28, "clk_gate_rxu28", "clk_gate_rp_cpu_normal",
+		0, 0x368, 28, 0 },
+	{ GATE_CLK_RXU29, "clk_gate_rxu29", "clk_gate_rp_cpu_normal",
+		0, 0x368, 29, 0 },
+	{ GATE_CLK_RXU30, "clk_gate_rxu30", "clk_gate_rp_cpu_normal",
+		0, 0x368, 30, 0 },
+	{ GATE_CLK_RXU31, "clk_gate_rxu31", "clk_gate_rp_cpu_normal",
+		0, 0x368, 31, 0 },
+	{ GATE_CLK_MP0, "clk_gate_mp0", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x384, 0, 0 },
+	{ GATE_CLK_MP1, "clk_gate_mp1", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x38c, 0, 0 },
+	{ GATE_CLK_MP2, "clk_gate_mp2", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x394, 0, 0 },
+	{ GATE_CLK_MP3, "clk_gate_mp3", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x39c, 0, 0 },
+	{ GATE_CLK_MP4, "clk_gate_mp4", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3a4, 0, 0 },
+	{ GATE_CLK_MP5, "clk_gate_mp5", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3ac, 0, 0 },
+	{ GATE_CLK_MP6, "clk_gate_mp6", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3b4, 0, 0 },
+	{ GATE_CLK_MP7, "clk_gate_mp7", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3bc, 0, 0 },
+	{ GATE_CLK_MP8, "clk_gate_mp8", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3c4, 0, 0 },
+	{ GATE_CLK_MP9, "clk_gate_mp9", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3cc, 0, 0 },
+	{ GATE_CLK_MP10, "clk_gate_mp10", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3d4, 0, 0 },
+	{ GATE_CLK_MP11, "clk_gate_mp11", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3dc, 0, 0 },
+	{ GATE_CLK_MP12, "clk_gate_mp12", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3e4, 0, 0 },
+	{ GATE_CLK_MP13, "clk_gate_mp13", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3ec, 0, 0 },
+	{ GATE_CLK_MP14, "clk_gate_mp14", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3f4, 0, 0 },
+	{ GATE_CLK_MP15, "clk_gate_mp15", "clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3fc, 0, 0 },
+};
+
+static const struct mango_divider_clock s1_div_clks[] = {
+	{ DIV_CLK_MPLL_RP_CPU_NORMAL_0, "s1_clk_div_rp_cpu_normal_0", "s1_clk_gate_rp_cpu_normal_div0",
+		0, 0x2044, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_MPLL_AXI_DDR_0, "s1_clk_div_axi_ddr_0", "s1_clk_gate_axi_ddr_div0",
+		0, 0x20a8, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, 5},
+	{ DIV_CLK_FPLL_DDR01_1, "s1_clk_div_ddr01_1", "s1_clk_gate_ddr01_div1",
+		0, 0x20b0, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_FPLL_DDR23_1, "s1_clk_div_ddr23_1", "s1_clk_gate_ddr23_div1",
+		0, 0x20b8, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_FPLL_RP_CPU_NORMAL_1, "s1_clk_div_rp_cpu_normal_1", "s1_clk_gate_rp_cpu_normal_div1",
+		0, 0x2040, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_50M_A53, "s1_clk_div_50m_a53", "s1_fpll_clock",
+		0, 0x2048, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_RP_CMN_DIV2, "s1_clk_div_top_rp_cmn_div2", "s1_clk_mux_rp_cpu_normal",
+		0, 0x204c, 16, 16, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_UART_500M, "s1_clk_div_uart_500m", "s1_fpll_clock",
+		0, 0x2050, 16, 7, CLK_DIVIDER_READ_ONLY, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_AHB_LPC, "s1_clk_div_ahb_lpc", "s1_fpll_clock",
+		0, 0x2054, 16, 16, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_EFUSE, "s1_clk_div_efuse", "s1_fpll_clock",
+		0, 0x2078, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TX_ETH0, "s1_clk_div_tx_eth0", "s1_fpll_clock",
+		0, 0x2080, 16, 11, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_PTP_REF_I_ETH0, "s1_clk_div_ptp_ref_i_eth0", "s1_fpll_clock",
+		0, 0x2084, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_REF_ETH0, "s1_clk_div_ref_eth0", "s1_fpll_clock",
+		0, 0x2088, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_EMMC, "s1_clk_div_emmc", "s1_fpll_clock",
+		0, 0x208c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_SD, "s1_clk_div_sd", "s1_fpll_clock",
+		0, 0x2094, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_AXI0, "s1_clk_div_top_axi0", "s1_fpll_clock",
+		0, 0x209c, 16, 5, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_TOP_AXI_HSPERI, "s1_clk_div_top_axi_hsperi", "s1_fpll_clock",
+		0, 0x20a0, 16, 5, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_AXI_DDR_1, "s1_clk_div_axi_ddr_1", "s1_clk_gate_axi_ddr_div1",
+		0, 0x20a4, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, 5},
+	{ DIV_CLK_FPLL_DIV_TIMER1, "s1_clk_div_timer1", "s1_clk_div_50m_a53",
+		0, 0x2058, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER2, "s1_clk_div_timer2", "s1_clk_div_50m_a53",
+		0, 0x205c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER3, "s1_clk_div_timer3", "s1_clk_div_50m_a53",
+		0, 0x2060, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER4, "s1_clk_div_timer4", "s1_clk_div_50m_a53",
+		0, 0x2064, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER5, "s1_clk_div_timer5", "s1_clk_div_50m_a53",
+		0, 0x2068, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER6, "s1_clk_div_timer6", "s1_clk_div_50m_a53",
+		0, 0x206c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER7, "s1_clk_div_timer7", "s1_clk_div_50m_a53",
+		0, 0x2070, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_DIV_TIMER8, "s1_clk_div_timer8", "s1_clk_div_50m_a53",
+		0, 0x2074, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_100K_EMMC, "s1_clk_div_100k_emmc", "s1_clk_div_top_axi0",
+		0, 0x2090, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_100K_SD, "s1_clk_div_100k_sd", "s1_clk_div_top_axi0",
+		0, 0x2098, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_FPLL_GPIO_DB, "s1_clk_div_gpio_db", "s1_clk_div_top_axi0",
+		0, 0x207c, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_REG_VAL, },
+	{ DIV_CLK_DPLL0_DDR01_0, "s1_clk_div_ddr01_0", "s1_clk_gate_ddr01_div0",
+		0, 0x20ac, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+	{ DIV_CLK_DPLL1_DDR23_0, "s1_clk_div_ddr23_0", "s1_clk_gate_ddr23_div0",
+		0, 0x20b4, 16, 8, CLK_DIVIDER_ONE_BASED |
+			CLK_DIVIDER_ALLOW_ZERO, MANGO_CLK_USE_INIT_VAL, },
+};
+
+static const struct mango_gate_clock s1_gate_clks[] = {
+	{ GATE_CLK_RP_CPU_NORMAL_DIV0, "s1_clk_gate_rp_cpu_normal_div1", "s1_mpll_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR_DIV0, "s1_clk_gate_axi_ddr_div1", "s1_mpll_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_DDR01_DIV0, "s1_clk_gate_ddr01_div0", "s1_fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23_DIV0, "s1_clk_gate_ddr23_div0", "s1_fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 15, 0 },
+	{ GATE_CLK_RP_CPU_NORMAL_DIV1, "s1_clk_gate_rp_cpu_normal_div0", "s1_fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR_DIV1, "s1_clk_gate_axi_ddr_div0", "s1_fpll_clock",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_DDR01_DIV1, "s1_clk_gate_ddr01_div1", "s1_dpll0_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23_DIV1, "s1_clk_gate_ddr23_div1", "s1_dpll1_clock",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 15, 0 },
+	{ GATE_CLK_A53_50M, "s1_clk_gate_a53_50m", "s1_clk_div_50m_a53",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 1, 0 },
+	{ GATE_CLK_TOP_RP_CMN_DIV2, "s1_clk_gate_top_rp_cmn_div2", "s1_clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 2, 0 },
+	{ GATE_CLK_AXI_PCIE0, "s1_clk_gate_axi_pcie0", "s1_clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 8, 0 },
+	{ GATE_CLK_AXI_PCIE1, "s1_clk_gate_axi_pcie1", "s1_clk_gate_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2004, 9, 0 },
+	{ GATE_CLK_HSDMA, "s1_clk_gate_hsdma", "s1_clk_gate_top_rp_cmn_div2",
+		CLK_SET_RATE_PARENT, 0x2004, 10, 0 },
+	{ GATE_CLK_EMMC_100M, "s1_clk_gate_emmc", "s1_clk_div_emmc",
+		CLK_SET_RATE_PARENT, 0x2004, 3, 0 },
+	{ GATE_CLK_SD_100M, "s1_clk_gate_sd", "s1_clk_div_sd",
+		CLK_SET_RATE_PARENT, 0x2004, 6, 0 },
+	{ GATE_CLK_TX_ETH0, "s1_clk_gate_tx_eth0", "s1_clk_div_tx_eth0",
+		CLK_SET_RATE_PARENT, 0x2000, 30, 0 },
+	{ GATE_CLK_PTP_REF_I_ETH0, "s1_clk_gate_ptp_ref_i_eth0", "s1_clk_div_ptp_ref_i_eth0",
+		CLK_SET_RATE_PARENT, 0x2004, 0, 0 },
+	{ GATE_CLK_REF_ETH0, "s1_clk_gate_ref_eth0", "s1_clk_div_ref_eth0",
+		CLK_SET_RATE_PARENT, 0x2004, 1, 0 },
+	{ GATE_CLK_UART_500M, "s1_clk_gate_uart_500m", "s1_clk_div_uart_500m",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED, 0x2000, 4, 0 },
+	{ GATE_CLK_AHB_LPC, "s1_clk_gate_ahb_lpc", "s1_clk_div_ahb_lpc",
+		CLK_SET_RATE_PARENT, 0x2000, 7, 0 },
+	{ GATE_CLK_EFUSE, "s1_clk_gate_efuse", "s1_clk_div_efuse",
+		CLK_SET_RATE_PARENT, 0x2000, 20, 0},
+	{ GATE_CLK_TOP_AXI0, "s1_clk_gate_top_axi0", "s1_clk_div_top_axi0",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 11, 0 },
+	{ GATE_CLK_TOP_AXI_HSPERI, "s1_clk_gate_top_axi_hsperi", "s1_clk_div_top_axi_hsperi",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 12, 0 },
+	{ GATE_CLK_AHB_ROM, "s1_clk_gate_ahb_rom", "s1_clk_gate_top_axi0",
+		0, 0x2000, 8, 0 },
+	{ GATE_CLK_AHB_SF, "s1_clk_gate_ahb_sf", "s1_clk_gate_top_axi0",
+		0, 0x2000, 9, 0 },
+	{ GATE_CLK_AXI_SRAM, "s1_clk_gate_axi_sram", "s1_clk_gate_top_axi0",
+		CLK_IGNORE_UNUSED, 0x2000, 10, 0 },
+	{ GATE_CLK_APB_TIMER, "s1_clk_gate_apb_timer", "s1_clk_gate_top_axi0",
+		CLK_IGNORE_UNUSED, 0x2000, 11, 0 },
+	{ GATE_CLK_APB_EFUSE, "s1_clk_gate_apb_efuse", "s1_clk_gate_top_axi0",
+		0, 0x2000, 21, 0 },
+	{ GATE_CLK_APB_GPIO, "s1_clk_gate_apb_gpio", "s1_clk_gate_top_axi0",
+		0, 0x2000, 22, 0 },
+	{ GATE_CLK_APB_GPIO_INTR, "s1_clk_gate_apb_gpio_intr", "s1_clk_gate_top_axi0",
+		CLK_IS_CRITICAL, 0x2000, 23, 0 },
+	{ GATE_CLK_APB_I2C, "s1_clk_gate_apb_i2c", "s1_clk_gate_top_axi0",
+		0, 0x2000, 26, 0 },
+	{ GATE_CLK_APB_WDT, "s1_clk_gate_apb_wdt", "s1_clk_gate_top_axi0",
+		0, 0x2000, 27, 0 },
+	{ GATE_CLK_APB_PWM, "s1_clk_gate_apb_pwm", "s1_clk_gate_top_axi0",
+		0, 0x2000, 28, 0 },
+	{ GATE_CLK_APB_RTC, "s1_clk_gate_apb_rtc", "s1_clk_gate_top_axi0",
+		0, 0x2000, 29, 0 },
+	{ GATE_CLK_SYSDMA_AXI, "s1_clk_gate_sysdma_axi", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 3, 0 },
+	{ GATE_CLK_APB_UART, "s1_clk_gate_apb_uart", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 5, 0 },
+	{ GATE_CLK_AXI_DBG_I2C, "s1_clk_gate_axi_dbg_i2c", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 6, 0 },
+	{ GATE_CLK_APB_SPI, "s1_clk_gate_apb_spi", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 25, 0 },
+	{ GATE_CLK_AXI_ETH0, "s1_clk_gate_axi_eth0", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2000, 31, 0 },
+	{ GATE_CLK_AXI_EMMC, "s1_clk_gate_axi_emmc", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2004, 2, 0 },
+	{ GATE_CLK_AXI_SD, "s1_clk_gate_axi_sd", "s1_clk_gate_top_axi_hsperi",
+		CLK_SET_RATE_PARENT, 0x2004, 5, 0 },
+	{ GATE_CLK_TIMER1, "s1_clk_gate_timer1", "s1_clk_div_timer1",
+		CLK_SET_RATE_PARENT, 0x2000, 12, 0 },
+	{ GATE_CLK_TIMER2, "s1_clk_gate_timer2", "s1_clk_div_timer2",
+		CLK_SET_RATE_PARENT, 0x2000, 13, 0 },
+	{ GATE_CLK_TIMER3, "s1_clk_gate_timer3", "s1_clk_div_timer3",
+		CLK_SET_RATE_PARENT, 0x2000, 14, 0 },
+	{ GATE_CLK_TIMER4, "s1_clk_gate_timer4", "s1_clk_div_timer4",
+		CLK_SET_RATE_PARENT, 0x2000, 15, 0 },
+	{ GATE_CLK_TIMER5, "s1_clk_gate_timer5", "s1_clk_div_timer5",
+		CLK_SET_RATE_PARENT, 0x2000, 16, 0 },
+	{ GATE_CLK_TIMER6, "s1_clk_gate_timer6", "s1_clk_div_timer6",
+		CLK_SET_RATE_PARENT, 0x2000, 17, 0 },
+	{ GATE_CLK_TIMER7, "s1_clk_gate_timer7", "s1_clk_div_timer7",
+		CLK_SET_RATE_PARENT, 0x2000, 18, 0 },
+	{ GATE_CLK_TIMER8, "s1_clk_gate_timer8", "s1_clk_div_timer8",
+		CLK_SET_RATE_PARENT, 0x2000, 19, 0 },
+	{ GATE_CLK_100K_EMMC, "s1_clk_gate_100k_emmc", "s1_clk_div_100k_emmc",
+		CLK_SET_RATE_PARENT, 0x2004, 4, 0 },
+	{ GATE_CLK_100K_SD, "s1_clk_gate_100k_sd", "s1_clk_div_100k_sd",
+		CLK_SET_RATE_PARENT, 0x2004, 7, 0 },
+	{ GATE_CLK_GPIO_DB, "s1_clk_gate_gpio_db", "s1_clk_div_gpio_db",
+		CLK_SET_RATE_PARENT, 0x2000, 24, 0 },
+	{ GATE_CLK_DDR01, "s1_clk_gate_ddr01", "s1_clk_mux_ddr01",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 14, 0 },
+	{ GATE_CLK_DDR23, "s1_clk_gate_ddr23", "s1_clk_mux_ddr23",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 15, 0 },
+	{ GATE_CLK_RP_CPU_NORMAL, "s1_clk_gate_rp_cpu_normal", "s1_clk_mux_rp_cpu_normal",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2000, 0, 0 },
+	{ GATE_CLK_AXI_DDR, "s1_clk_gate_axi_ddr", "s1_clk_mux_axi_ddr",
+		CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x2004, 13, 0 },
+	{ GATE_CLK_RXU0, "s1_clk_gate_rxu0", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 0, 0 },
+	{ GATE_CLK_RXU1, "s1_clk_gate_rxu1", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 1, 0 },
+	{ GATE_CLK_RXU2, "s1_clk_gate_rxu2", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 2, 0 },
+	{ GATE_CLK_RXU3, "s1_clk_gate_rxu3", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 3, 0 },
+	{ GATE_CLK_RXU4, "s1_clk_gate_rxu4", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 4, 0 },
+	{ GATE_CLK_RXU5, "s1_clk_gate_rxu5", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 5, 0 },
+	{ GATE_CLK_RXU6, "s1_clk_gate_rxu6", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 6, 0 },
+	{ GATE_CLK_RXU7, "s1_clk_gate_rxu7", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 7, 0 },
+	{ GATE_CLK_RXU8, "s1_clk_gate_rxu8", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 8, 0 },
+	{ GATE_CLK_RXU9, "s1_clk_gate_rxu9", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 9, 0 },
+	{ GATE_CLK_RXU10, "s1_clk_gate_rxu10", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 10, 0 },
+	{ GATE_CLK_RXU11, "s1_clk_gate_rxu11", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 11, 0 },
+	{ GATE_CLK_RXU12, "s1_clk_gate_rxu12", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 12, 0 },
+	{ GATE_CLK_RXU13, "s1_clk_gate_rxu13", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 13, 0 },
+	{ GATE_CLK_RXU14, "s1_clk_gate_rxu14", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 14, 0 },
+	{ GATE_CLK_RXU15, "s1_clk_gate_rxu15", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 15, 0 },
+	{ GATE_CLK_RXU16, "s1_clk_gate_rxu16", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 16, 0 },
+	{ GATE_CLK_RXU17, "s1_clk_gate_rxu17", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 17, 0 },
+	{ GATE_CLK_RXU18, "s1_clk_gate_rxu18", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 18, 0 },
+	{ GATE_CLK_RXU19, "s1_clk_gate_rxu19", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 19, 0 },
+	{ GATE_CLK_RXU20, "s1_clk_gate_rxu20", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 20, 0 },
+	{ GATE_CLK_RXU21, "s1_clk_gate_rxu21", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 21, 0 },
+	{ GATE_CLK_RXU22, "s1_clk_gate_rxu22", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 22, 0 },
+	{ GATE_CLK_RXU23, "s1_clk_gate_rxu23", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 23, 0 },
+	{ GATE_CLK_RXU24, "s1_clk_gate_rxu24", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 24, 0 },
+	{ GATE_CLK_RXU25, "s1_clk_gate_rxu25", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 25, 0 },
+	{ GATE_CLK_RXU26, "s1_clk_gate_rxu26", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 26, 0 },
+	{ GATE_CLK_RXU27, "s1_clk_gate_rxu27", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 27, 0 },
+	{ GATE_CLK_RXU28, "s1_clk_gate_rxu28", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 28, 0 },
+	{ GATE_CLK_RXU29, "s1_clk_gate_rxu29", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 29, 0 },
+	{ GATE_CLK_RXU30, "s1_clk_gate_rxu30", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 30, 0 },
+	{ GATE_CLK_RXU31, "s1_clk_gate_rxu31", "s1_clk_gate_rp_cpu_normal",
+		0, 0x368, 31, 0 },
+	{ GATE_CLK_MP0, "s1_clk_gate_mp0", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x384, 0, 0 },
+	{ GATE_CLK_MP1, "s1_clk_gate_mp1", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x38c, 0, 0 },
+	{ GATE_CLK_MP2, "s1_clk_gate_mp2", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x394, 0, 0 },
+	{ GATE_CLK_MP3, "s1_clk_gate_mp3", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x39c, 0, 0 },
+	{ GATE_CLK_MP4, "s1_clk_gate_mp4", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3a4, 0, 0 },
+	{ GATE_CLK_MP5, "s1_clk_gate_mp5", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3ac, 0, 0 },
+	{ GATE_CLK_MP6, "s1_clk_gate_mp6", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3b4, 0, 0 },
+	{ GATE_CLK_MP7, "s1_clk_gate_mp7", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3bc, 0, 0 },
+	{ GATE_CLK_MP8, "s1_clk_gate_mp8", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3c4, 0, 0 },
+	{ GATE_CLK_MP9, "s1_clk_gate_mp9", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3cc, 0, 0 },
+	{ GATE_CLK_MP10, "s1_clk_gate_mp10", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3d4, 0, 0 },
+	{ GATE_CLK_MP11, "s1_clk_gate_mp11", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3dc, 0, 0 },
+	{ GATE_CLK_MP12, "s1_clk_gate_mp12", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3e4, 0, 0 },
+	{ GATE_CLK_MP13, "s1_clk_gate_mp13", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3ec, 0, 0 },
+	{ GATE_CLK_MP14, "s1_clk_gate_mp14", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3f4, 0, 0 },
+	{ GATE_CLK_MP15, "s1_clk_gate_mp15", "s1_clk_gate_rp_cpu_normal",
+		CLK_IGNORE_UNUSED | CLK_IS_CRITICAL, 0x3fc, 0, 0 },
+};
+
+/* socket0 mux clocks */
+static const char *const clk_mux_ddr01_p[] = {
+			"clk_div_ddr01_0", "clk_div_ddr01_1"};
+static const char *const clk_mux_ddr23_p[] = {
+			"clk_div_ddr23_0", "clk_div_ddr23_1"};
+static const char *const clk_mux_rp_cpu_normal_p[] = {
+			"clk_div_rp_cpu_normal_0", "clk_div_rp_cpu_normal_1"};
+static const char *const clk_mux_axi_ddr_p[] = {
+			"clk_div_axi_ddr_0", "clk_div_axi_ddr_1"};
+
+struct mango_mux_clock s0_mux_clks[] = {
+	{
+		MUX_CLK_DDR01, "clk_mux_ddr01", clk_mux_ddr01_p,
+		ARRAY_SIZE(clk_mux_ddr01_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT |
+			CLK_MUX_READ_ONLY,
+		0x2020, 2, 1, 0,
+	},
+	{
+		MUX_CLK_DDR23, "clk_mux_ddr23", clk_mux_ddr23_p,
+		ARRAY_SIZE(clk_mux_ddr23_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT |
+			CLK_MUX_READ_ONLY,
+		0x2020, 3, 1, 0,
+	},
+	{
+		MUX_CLK_RP_CPU_NORMAL, "clk_mux_rp_cpu_normal", clk_mux_rp_cpu_normal_p,
+		ARRAY_SIZE(clk_mux_rp_cpu_normal_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT,
+		0x2020, 0, 1, 0,
+	},
+	{
+		MUX_CLK_AXI_DDR, "clk_mux_axi_ddr", clk_mux_axi_ddr_p,
+		ARRAY_SIZE(clk_mux_axi_ddr_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT,
+		0x2020, 1, 1, 0,
+	},
+};
+
+/* socket1 mux clocks */
+static const char *const s1_clk_mux_ddr01_p[] = {
+			"s1_clk_div_ddr01_0", "s1_clk_div_ddr01_1"};
+static const char *const s1_clk_mux_ddr23_p[] = {
+			"s1_clk_div_ddr23_0", "s1_clk_div_ddr23_1"};
+static const char *const s1_clk_mux_rp_cpu_normal_p[] = {
+			"s1_clk_div_rp_cpu_normal_0", "s1_clk_div_rp_cpu_normal_1"};
+static const char *const s1_clk_mux_axi_ddr_p[] = {
+			"s1_clk_div_axi_ddr_0", "s1_clk_div_axi_ddr_1"};
+
+struct mango_mux_clock s1_mux_clks[] = {
+	{
+		MUX_CLK_DDR01, "s1_clk_mux_ddr01", s1_clk_mux_ddr01_p,
+		ARRAY_SIZE(s1_clk_mux_ddr01_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT |
+			CLK_MUX_READ_ONLY,
+		0x2020, 2, 1, 0,
+	},
+	{
+		MUX_CLK_DDR23, "s1_clk_mux_ddr23", s1_clk_mux_ddr23_p,
+		ARRAY_SIZE(s1_clk_mux_ddr23_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT |
+			CLK_MUX_READ_ONLY,
+		0x2020, 3, 1, 0,
+	},
+	{
+		MUX_CLK_RP_CPU_NORMAL, "s1_clk_mux_rp_cpu_normal", s1_clk_mux_rp_cpu_normal_p,
+		ARRAY_SIZE(s1_clk_mux_rp_cpu_normal_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT,
+		0x2020, 0, 1, 0,
+	},
+	{
+		MUX_CLK_AXI_DDR, "s1_clk_mux_axi_ddr", s1_clk_mux_axi_ddr_p,
+		ARRAY_SIZE(s1_clk_mux_axi_ddr_p),
+		CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT,
+		0x2020, 1, 1, 0,
+	},
+};
+
+struct mango_clk_table pll_clk_tables = {
+	.pll_clks_num = ARRAY_SIZE(mango_root_pll_clks),
+	.pll_clks = mango_root_pll_clks,
+};
+
+struct mango_clk_table div_clk_tables[] = {
+	{
+		.id = S0_DIV_CLK_TABLE,
+		.div_clks_num = ARRAY_SIZE(s0_div_clks),
+		.div_clks = s0_div_clks,
+		.gate_clks_num = ARRAY_SIZE(s0_gate_clks),
+		.gate_clks = s0_gate_clks,
+	},{
+		.id = S1_DIV_CLK_TABLE,
+		.div_clks_num = ARRAY_SIZE(s1_div_clks),
+		.div_clks = s1_div_clks,
+		.gate_clks_num = ARRAY_SIZE(s1_gate_clks),
+		.gate_clks = s1_gate_clks,
+	},
+};
+
+struct mango_clk_table mux_clk_tables[] = {
+	{
+		.id = S0_MUX_CLK_TABLE,
+		.mux_clks_num = ARRAY_SIZE(s0_mux_clks),
+		.mux_clks = s0_mux_clks,
+	},{
+		.id = S1_MUX_CLK_TABLE,
+		.mux_clks_num = ARRAY_SIZE(s1_mux_clks),
+		.mux_clks = s1_mux_clks,
+	},
+};
+
+static const struct of_device_id mango_clk_match_ids_tables[] = {
+	{
+		.compatible = "mango, pll-clock",
+		.data = &pll_clk_tables,
+	},
+	{
+		.compatible = "mango, pll-child-clock",
+		.data = div_clk_tables,
+	},
+	{
+		.compatible = "mango, pll-mux-clock",
+		.data = mux_clk_tables,
+	},
+	{
+		.compatible = "mango, clk-default-rates",
+	},
+	{
+		.compatible = "mango, dm-pll-clock",
+		.data = &pll_clk_tables,
+	},
+	{
+		.compatible = "mango, dm-pll-child-clock",
+		.data = div_clk_tables,
+	},
+	{
+		.compatible = "mango, dm-pll-mux-clock",
+		.data = mux_clk_tables,
+	},
+	{
+		.compatible = "mango, dm-clk-default-rates",
+	},
+	{}
+};
+
+static void __init mango_clk_init(struct device_node *node)
+{
+	struct device_node *np_top;
+	struct mango_clk_data *clk_data = NULL;
+	const struct mango_clk_table *dev_data;
+	struct regmap *syscon;
+	void __iomem *base;
+	int i, ret = 0;
+	unsigned int id;
+	const char *clk_name;
+	const struct of_device_id *match = NULL;
+
+	clk_data = kzalloc(sizeof(*clk_data), GFP_KERNEL);
+	if (!clk_data) {
+		ret = -ENOMEM;
+		goto out;
+	}
+	match = of_match_node(mango_clk_match_ids_tables, node);
+	if (match) {
+		dev_data = (struct mango_clk_table *)match->data;
+	} else {
+		pr_err("%s did't match node data\n", __func__);
+		ret = -ENODEV;
+		goto no_match_data;
+	}
+
+	np_top = of_parse_phandle(node, "subctrl-syscon", 0);
+	if (!np_top) {
+		pr_err("%s can't get subctrl-syscon node\n",
+			__func__);
+		ret = -EINVAL;
+		goto no_match_data;
+	}
+
+	syscon = device_node_to_regmap(np_top);
+	if (IS_ERR_OR_NULL(syscon)) {
+		pr_err("%s cannot get regmap %ld\n", __func__, PTR_ERR(syscon));
+		ret = -ENODEV;
+		goto no_match_data;
+	}
+	base = of_iomap(np_top, 0);
+
+	spin_lock_init(&clk_data->lock);
+	if (of_device_is_compatible(node, "mango, pll-clock") ||
+	    of_device_is_compatible(node, "mango, dm-pll-clock")) {
+		if (!dev_data->pll_clks_num) {
+			ret = -EINVAL;
+			goto no_match_data;
+		}
+
+		clk_data->table = dev_data;
+		clk_data->base = base;
+		clk_data->syscon_top = syscon;
+
+		if (of_property_read_string(node, "clock-output-names", &clk_name)) {
+			pr_err("%s cannot get pll name for %s\n",
+				__func__, node->full_name);
+			ret = -ENODEV;
+			goto no_match_data;
+		}
+		if (of_device_is_compatible(node, "mango, pll-clock"))
+			ret = mango_register_pll_clks(node, clk_data, clk_name);
+		else
+			ret = dm_mango_register_pll_clks(node, clk_data, clk_name);
+	}
+
+	if (of_device_is_compatible(node, "mango, pll-child-clock") ||
+	    of_device_is_compatible(node, "mango, dm-pll-child-clock")) {
+		ret = of_property_read_u32(node, "id", &id);
+		if (ret) {
+			pr_err("not assigned id for %s\n", node->full_name);
+			ret = -ENODEV;
+			goto no_match_data;
+		}
+
+		/* Below brute-force to check dts property "id"
+		 * whether match id of array
+		 */
+		for (i = 0; i < ARRAY_SIZE(div_clk_tables); i++) {
+			if (id == dev_data[i].id)
+				break; /* found */
+		}
+		clk_data->table = &dev_data[i];
+		clk_data->base = base;
+		clk_data->syscon_top = syscon;
+		if (of_device_is_compatible(node, "mango, pll-child-clock"))
+			ret = mango_register_div_clks(node, clk_data);
+		else
+			ret = dm_mango_register_div_clks(node, clk_data);
+	}
+
+	if (of_device_is_compatible(node, "mango, pll-mux-clock") ||
+	    of_device_is_compatible(node, "mango, dm-pll-mux-clock")) {
+		ret = of_property_read_u32(node, "id", &id);
+		if (ret) {
+			pr_err("not assigned id for %s\n", node->full_name);
+			ret = -ENODEV;
+			goto no_match_data;
+		}
+
+		/* Below brute-force to check dts property "id"
+		 * whether match id of array
+		 */
+		for (i = 0; i < ARRAY_SIZE(mux_clk_tables); i++) {
+			if (id == dev_data[i].id)
+				break; /* found */
+		}
+		clk_data->table = &dev_data[i];
+		clk_data->base = base;
+		clk_data->syscon_top = syscon;
+		if (of_device_is_compatible(node, "mango, pll-mux-clock"))
+			ret = mango_register_mux_clks(node, clk_data);
+		else
+			ret = dm_mango_register_mux_clks(node, clk_data);
+	}
+
+	if (of_device_is_compatible(node, "mango, clk-default-rates"))
+		ret = set_default_clk_rates(node);
+
+	if (of_device_is_compatible(node, "mango, dm-clk-default-rates"))
+		ret = dm_set_default_clk_rates(node);
+
+	if (!ret)
+		return;
+
+no_match_data:
+	kfree(clk_data);
+
+out:
+	pr_err("%s failed error number %d\n", __func__, ret);
+}
+
+CLK_OF_DECLARE(mango_clk_pll, "mango, pll-clock", mango_clk_init);
+CLK_OF_DECLARE(mango_clk_pll_child, "mango, pll-child-clock", mango_clk_init);
+CLK_OF_DECLARE(mango_clk_pll_mux, "mango, pll-mux-clock", mango_clk_init);
+CLK_OF_DECLARE(mango_clk_default_rate, "mango, clk-default-rates", mango_clk_init);
+CLK_OF_DECLARE(dm_mango_clk_pll, "mango, dm-pll-clock", mango_clk_init);
+CLK_OF_DECLARE(dm_mango_clk_pll_child, "mango, dm-pll-child-clock", mango_clk_init);
+CLK_OF_DECLARE(dm_mango_clk_pll_mux, "mango, dm-pll-mux-clock", mango_clk_init);
+CLK_OF_DECLARE(dm_mango_clk_default_rate, "mango, dm-clk-default-rates", mango_clk_init);
diff --git a/drivers/clk/sophgo/clk.c b/drivers/clk/sophgo/clk.c
new file mode 100644
index 000000000000..4d3893ace2b9
--- /dev/null
+++ b/drivers/clk/sophgo/clk.c
@@ -0,0 +1,883 @@
+/*
+ * Copyright (c) 2022 SOPHGO
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#include <linux/of_device.h>
+#include <linux/platform_device.h>
+#include <linux/spinlock.h>
+#include <linux/mfd/syscon.h>
+#include <linux/io.h>
+#include <linux/of_address.h>
+#include <linux/string.h>
+#include <linux/log2.h>
+
+#include "clk.h"
+
+/*
+ * @hw:		handle between common and hardware-specific interfaces
+ * @reg:	register containing divider
+ * @shift:	shift to the divider bit field
+ * @width:	width of the divider bit field
+ * @initial_val:initial value of the divider
+ * @table:	the div table that the divider supports
+ * @lock:	register lock
+ */
+struct mango_clk_divider {
+	struct clk_hw	hw;
+	void __iomem	*reg;
+	u8		shift;
+	u8		width;
+	u8		flags;
+	u32		initial_val;
+	const struct clk_div_table *table;
+	spinlock_t	*lock;
+};
+
+static inline int mango_pll_enable(struct regmap *map,
+					struct mango_pll_clock *pll, bool en)
+{
+	unsigned int value;
+	unsigned long enter;
+	unsigned int id = pll->id;
+
+	if (en) {
+		/* wait pll lock */
+		enter = jiffies;
+		regmap_read(map, pll->status_offset, &value);
+		while (!((value >> (PLL_STAT_LOCK_OFFSET + id)) & 0x1)) {
+			regmap_read(map, pll->status_offset, &value);
+			if (time_after(jiffies, enter + HZ / 10))
+				pr_warn("%s not locked\n", pll->name);
+		}
+		/* wait pll updating */
+		enter = jiffies;
+		regmap_read(map, pll->status_offset, &value);
+		while (((value >> id) & 0x1)) {
+			regmap_read(map, pll->status_offset, &value);
+			if (time_after(jiffies, enter + HZ / 10))
+				pr_warn("%s still updating\n", pll->name);
+		}
+		/* enable pll */
+		regmap_read(map, pll->enable_offset, &value);
+		regmap_write(map, pll->enable_offset, value | (1 << id));
+	} else {
+		/* disable pll */
+		regmap_read(map, pll->enable_offset, &value);
+		regmap_write(map, pll->enable_offset, value & (~(1 << id)));
+	}
+
+	return 0;
+}
+
+static inline int mango_pll_write(struct regmap *map, int id, int value)
+{
+	return regmap_write(map, PLL_CTRL_OFFSET + (id << 2), value);
+}
+
+static inline int mango_pll_read(struct regmap *map, int id, unsigned int *pvalue)
+{
+	return regmap_read(map, PLL_CTRL_OFFSET + (id << 2), pvalue);
+}
+
+static unsigned int _get_table_div(const struct clk_div_table *table,
+				   unsigned int val)
+{
+	const struct clk_div_table *clkt;
+
+	for (clkt = table; clkt->div; clkt++)
+		if (clkt->val == val)
+			return clkt->div;
+	return 0;
+}
+
+static unsigned int _get_div(const struct clk_div_table *table,
+			     unsigned int val, unsigned long flags, u8 width)
+{
+	if (flags & CLK_DIVIDER_ONE_BASED)
+		return val;
+	if (flags & CLK_DIVIDER_POWER_OF_TWO)
+		return 1 << val;
+	if (flags & CLK_DIVIDER_MAX_AT_ZERO)
+		return val ? val : div_mask(width) + 1;
+	if (table)
+		return _get_table_div(table, val);
+	return val + 1;
+}
+
+static unsigned long mango_clk_divider_recalc_rate(struct clk_hw *hw,
+						unsigned long parent_rate)
+{
+	struct mango_clk_divider *divider = to_mango_clk_divider(hw);
+	unsigned int val;
+
+	val = readl(divider->reg) >> divider->shift;
+	val &= div_mask(divider->width);
+
+#ifdef CONFIG_ARCH_BM1880
+	/* if select divide factor from initial value */
+	if (!(readl(divider->reg) & BIT(3)))
+		val = divider->initial_val;
+#endif
+
+	return divider_recalc_rate(hw, parent_rate, val, divider->table,
+				   divider->flags, divider->width);
+}
+
+static long mango_clk_divider_round_rate(struct clk_hw *hw, unsigned long rate,
+				      unsigned long *prate)
+{
+	int bestdiv;
+	struct mango_clk_divider *divider = to_mango_clk_divider(hw);
+
+	/* if read only, just return current value */
+	if (divider->flags & CLK_DIVIDER_READ_ONLY) {
+		bestdiv = readl(divider->reg) >> divider->shift;
+		bestdiv &= div_mask(divider->width);
+		bestdiv = _get_div(divider->table, bestdiv, divider->flags,
+				   divider->width);
+		return DIV_ROUND_UP_ULL((u64)*prate, bestdiv);
+	}
+
+	return divider_round_rate(hw, rate, prate, divider->table,
+				  divider->width, divider->flags);
+}
+
+static int mango_clk_divider_set_rate(struct clk_hw *hw, unsigned long rate,
+				   unsigned long parent_rate)
+{
+	unsigned int value;
+	unsigned int val;
+	unsigned long flags = 0;
+	struct mango_clk_divider *divider = to_mango_clk_divider(hw);
+
+	value = divider_get_val(rate, parent_rate, divider->table,
+				divider->width, divider->flags);
+
+	if (divider->lock)
+		spin_lock_irqsave(divider->lock, flags);
+	else
+		__acquire(divider->lock);
+
+	/* div assert */
+	val = readl(divider->reg);
+	val &= ~0x1;
+	writel(val, divider->reg);
+
+	if (divider->flags & CLK_DIVIDER_HIWORD_MASK) {
+		val = div_mask(divider->width) << (divider->shift + 16);
+	} else {
+		val = readl(divider->reg);
+		val &= ~(div_mask(divider->width) << divider->shift);
+	}
+
+	val |= value << divider->shift;
+	writel(val, divider->reg);
+
+	if (!(divider->flags & CLK_DIVIDER_READ_ONLY))
+		val |= 1 << 3;
+
+	/* de-assert */
+	val |= 1;
+	writel(val, divider->reg);
+	if (divider->lock)
+		spin_unlock_irqrestore(divider->lock, flags);
+	else
+		__release(divider->lock);
+
+	return 0;
+}
+
+/* Below array is the total combination lists of POSTDIV1 and POSTDIV2
+ * for example:
+ * postdiv1_2[0] = {1, 1, 1}
+ *           ==> div1 = 1, div2 = 1 , div1 * div2 = 1
+ * postdiv1_2[22] = {6, 7, 42}
+ *           ==> div1 = 6, div2 = 7 , div1 * div2 = 42
+ *
+ * And POSTDIV_RESULT_INDEX point to 3rd element in the array
+ */
+#define	POSTDIV_RESULT_INDEX	2
+int postdiv1_2[][3] = {
+	{2, 4,  8}, {3, 3,  9}, {2, 5, 10}, {2, 6, 12},
+	{2, 7, 14}, {3, 5, 15}, {4, 4, 16}, {3, 6, 18},
+	{4, 5, 20}, {3, 7, 21}, {4, 6, 24}, {5, 5, 25},
+	{4, 7, 28}, {5, 6, 30}, {5, 7, 35}, {6, 6, 36},
+	{6, 7, 42}, {7, 7, 49}
+};
+
+/*
+ * @reg_value: current register value
+ * @parent_rate: parent frequency
+ *
+ * This function is used to calculate below "rate" in equation
+ * rate = (parent_rate/REFDIV) x FBDIV/POSTDIV1/POSTDIV2
+ *      = (parent_rate x FBDIV) / (REFDIV x POSTDIV1 x POSTDIV2)
+ */
+static unsigned long __pll_recalc_rate(unsigned int reg_value,
+				       unsigned long parent_rate)
+{
+	unsigned int fbdiv, refdiv;
+	unsigned int postdiv1, postdiv2;
+	u64 rate, numerator, denominator;
+
+	fbdiv = (reg_value >> 16) & 0xfff;
+	refdiv = reg_value & 0x3f;
+	postdiv1 = (reg_value >> 8) & 0x7;
+	postdiv2 = (reg_value >> 12) & 0x7;
+
+	numerator = parent_rate * fbdiv;
+	denominator = refdiv * postdiv1 * postdiv2;
+	do_div(numerator, denominator);
+	rate = numerator;
+
+	return rate;
+}
+
+/*
+ * @reg_value: current register value
+ * @rate: request rate
+ * @prate: parent rate
+ * @pctrl_table: use to save div1/div2/fbdiv/refdiv
+ *
+ * We use below equation to get POSTDIV1 and POSTDIV2
+ * POSTDIV = (parent_rate/REFDIV) x FBDIV/input_rate
+ * above POSTDIV = POSTDIV1*POSTDIV2
+ */
+static int __pll_get_postdiv_1_2(unsigned long rate, unsigned long prate,
+				 unsigned int fbdiv, unsigned int refdiv, unsigned int *postdiv1,
+				 unsigned int *postdiv2)
+{
+	int index = 0;
+	int ret = 0;
+	u64 tmp0;
+
+	/* calculate (parent_rate/refdiv)
+	 * and result save to prate
+	 */
+	tmp0 = prate;
+	do_div(tmp0, refdiv);
+
+	/* calcuate ((parent_rate/REFDIV) x FBDIV)
+	 * and result save to prate
+	 */
+	tmp0 *= fbdiv;
+
+	/* calcuate (((parent_rate/REFDIV) x FBDIV)/input_rate)
+	 * and result save to prate
+	 * here *prate is (POSTDIV1*POSTDIV2)
+	 */
+	do_div(tmp0, rate);
+
+	/* calculate div1 and div2 value */
+	if (tmp0 <= 7) {
+		/* (div1 * div2) <= 7, no need to use array search */
+		*postdiv1 = tmp0;
+		*postdiv2 = 1;
+	} else {
+		/* (div1 * div2) > 7, use array search */
+		for (index = 0; index < ARRAY_SIZE(postdiv1_2); index++) {
+			if (tmp0 > postdiv1_2[index][POSTDIV_RESULT_INDEX]) {
+				continue;
+			} else {
+				/* found it */
+				break;
+			}
+		}
+		if (index < ARRAY_SIZE(postdiv1_2)) {
+			*postdiv1 = postdiv1_2[index][1];
+			*postdiv2 = postdiv1_2[index][0];
+		} else {
+			pr_debug("%s out of postdiv array range!\n", __func__);
+			ret = -ESPIPE;
+		}
+	}
+
+	return ret;
+}
+
+static int __get_pll_ctl_setting(struct mango_pll_ctrl *best,
+			unsigned long req_rate, unsigned long parent_rate)
+{
+	int ret;
+	unsigned int fbdiv, refdiv, fref, postdiv1, postdiv2;
+	unsigned long tmp = 0, foutvco;
+
+	fref = parent_rate;
+
+	for (refdiv = REFDIV_MIN; refdiv < REFDIV_MAX + 1; refdiv++) {
+		for (fbdiv = FBDIV_MIN; fbdiv < FBDIV_MAX + 1; fbdiv++) {
+			foutvco = fref * fbdiv / refdiv;
+			/* check fpostdiv pfd */
+			if (foutvco < PLL_FREQ_MIN || foutvco > PLL_FREQ_MAX
+					|| (fref / refdiv) < 10)
+				continue;
+
+			ret = __pll_get_postdiv_1_2(req_rate, fref, fbdiv,
+					refdiv, &postdiv1, &postdiv2);
+			if (ret)
+				continue;
+
+			tmp = foutvco / (postdiv1 * postdiv2);
+			if (abs_diff(tmp, req_rate) < abs_diff(best->freq, req_rate)) {
+				best->freq = tmp;
+				best->refdiv = refdiv;
+				best->fbdiv = fbdiv;
+				best->postdiv1 = postdiv1;
+				best->postdiv2 = postdiv2;
+				if (tmp == req_rate)
+					return 0;
+			}
+			continue;
+		}
+	}
+
+	return 0;
+}
+
+/*
+ * @hw: ccf use to hook get mango_pll_clock
+ * @parent_rate: parent rate
+ *
+ * The is function will be called through clk_get_rate
+ * and return current rate after decoding reg value
+ */
+static unsigned long mango_clk_pll_recalc_rate(struct clk_hw *hw,
+					    unsigned long parent_rate)
+{
+	unsigned int value;
+	unsigned long rate;
+	struct mango_pll_clock *mango_pll = to_mango_pll_clk(hw);
+
+	mango_pll_read(mango_pll->syscon_top, mango_pll->id, &value);
+	rate = __pll_recalc_rate(value, parent_rate);
+	return rate;
+}
+
+static long mango_clk_pll_round_rate(struct clk_hw *hw,
+				  unsigned long req_rate, unsigned long *prate)
+{
+	unsigned int value;
+	struct mango_pll_ctrl pctrl_table;
+	struct mango_pll_clock *mango_pll = to_mango_pll_clk(hw);
+	long proper_rate;
+
+	memset(&pctrl_table, 0, sizeof(struct mango_pll_ctrl));
+
+	/* use current setting to get fbdiv, refdiv
+	 * then combine with prate, and req_rate to
+	 * get postdiv1 and postdiv2
+	 */
+	mango_pll_read(mango_pll->syscon_top, mango_pll->id, &value);
+	__get_pll_ctl_setting(&pctrl_table, req_rate, *prate);
+	if (!pctrl_table.freq) {
+		proper_rate = 0;
+		goto out;
+	}
+
+	value = TOP_PLL_CTRL(pctrl_table.fbdiv, pctrl_table.postdiv1,
+			     pctrl_table.postdiv2, pctrl_table.refdiv);
+	proper_rate = (long)__pll_recalc_rate(value, *prate);
+
+out:
+	return proper_rate;
+}
+
+static int mango_clk_pll_determine_rate(struct clk_hw *hw,
+				     struct clk_rate_request *req)
+{
+	req->rate = mango_clk_pll_round_rate(hw, min(req->rate, req->max_rate),
+					  &req->best_parent_rate);
+	return 0;
+}
+
+static int mango_clk_pll_set_rate(struct clk_hw *hw, unsigned long rate,
+			       unsigned long parent_rate)
+{
+	unsigned long flags;
+	unsigned int value;
+	int ret = 0;
+	struct mango_pll_ctrl pctrl_table;
+	struct mango_pll_clock *mango_pll = to_mango_pll_clk(hw);
+
+	memset(&pctrl_table, 0, sizeof(struct mango_pll_ctrl));
+	spin_lock_irqsave(mango_pll->lock, flags);
+	if (mango_pll_enable(mango_pll->syscon_top, mango_pll, 0)) {
+		pr_warn("Can't disable pll(%s), status error\n", mango_pll->name);
+		goto out;
+	}
+	mango_pll_read(mango_pll->syscon_top, mango_pll->id, &value);
+	__get_pll_ctl_setting(&pctrl_table, rate, parent_rate);
+	if (!pctrl_table.freq) {
+		pr_warn("%s: Can't find a proper pll setting\n", mango_pll->name);
+		goto out;
+	}
+
+	value = TOP_PLL_CTRL(pctrl_table.fbdiv, pctrl_table.postdiv1,
+			     pctrl_table.postdiv2, pctrl_table.refdiv);
+
+	/* write the value to top register */
+	mango_pll_write(mango_pll->syscon_top, mango_pll->id, value);
+	mango_pll_enable(mango_pll->syscon_top, mango_pll, 1);
+out:
+	spin_unlock_irqrestore(mango_pll->lock, flags);
+	return ret;
+}
+
+const struct clk_ops mango_clk_divider_ops = {
+	.recalc_rate = mango_clk_divider_recalc_rate,
+	.round_rate = mango_clk_divider_round_rate,
+	.set_rate = mango_clk_divider_set_rate,
+};
+
+const struct clk_ops mango_clk_divider_ro_ops = {
+	.recalc_rate = mango_clk_divider_recalc_rate,
+	.round_rate = mango_clk_divider_round_rate,
+};
+
+const struct clk_ops mango_clk_pll_ops = {
+	.recalc_rate = mango_clk_pll_recalc_rate,
+	.round_rate = mango_clk_pll_round_rate,
+	.determine_rate = mango_clk_pll_determine_rate,
+	.set_rate = mango_clk_pll_set_rate,
+};
+
+const struct clk_ops mango_clk_pll_ro_ops = {
+	.recalc_rate = mango_clk_pll_recalc_rate,
+	.round_rate = mango_clk_pll_round_rate,
+};
+
+struct mux_cb_clk_name {
+	const char *name;
+	struct list_head node;
+};
+
+static struct list_head mux_cb_clk_name_list =
+	LIST_HEAD_INIT(mux_cb_clk_name_list);
+static int mux_notifier_cb(struct notifier_block *nb,
+				unsigned long event, void *data)
+{
+	int ret = 0;
+	static unsigned char mux_id = 1;
+	struct clk_notifier_data *ndata = data;
+	struct clk_hw *hw = __clk_get_hw(ndata->clk);
+	const struct clk_ops *ops = &clk_mux_ops;
+	struct mux_cb_clk_name *cb_lsit;
+
+	if (event == PRE_RATE_CHANGE) {
+		struct clk_hw *hw_p = clk_hw_get_parent(hw);
+
+		cb_lsit = kmalloc(sizeof(*cb_lsit), GFP_KERNEL);
+		if (cb_lsit) {
+			INIT_LIST_HEAD(&cb_lsit->node);
+			list_add_tail(&cb_lsit->node, &mux_cb_clk_name_list);
+		} else {
+			pr_err("mux cb kmalloc mem fail\n");
+			goto out;
+		}
+
+		cb_lsit->name = clk_hw_get_name(hw_p);
+		mux_id = ops->get_parent(hw);
+		if (mux_id > 1) {
+			ret = 1;
+			goto out;
+		}
+		ops->set_parent(hw, !mux_id);
+	} else if (event == POST_RATE_CHANGE) {
+		struct clk_hw *hw_p = clk_hw_get_parent(hw);
+
+		cb_lsit = list_first_entry_or_null(&mux_cb_clk_name_list,
+						typeof(*cb_lsit), node);
+		if (cb_lsit) {
+			const char *pre_name = cb_lsit->name;
+
+			list_del_init(&cb_lsit->node);
+			kfree(cb_lsit);
+			if (strcmp(clk_hw_get_name(hw_p), pre_name))
+				goto out;
+		}
+
+		ops->set_parent(hw, mux_id);
+	}
+
+out:
+	return notifier_from_errno(ret);
+}
+
+int set_default_clk_rates(struct device_node *node)
+{
+	struct of_phandle_args clkspec;
+	struct property *prop;
+	const __be32 *cur;
+	int rc, index = 0;
+	struct clk *clk;
+	u32 rate;
+
+	of_property_for_each_u32 (node, "clock-rates", prop, cur, rate) {
+		if (rate) {
+			rc = of_parse_phandle_with_args(node, "clocks",
+							"#clock-cells", index, &clkspec);
+			if (rc < 0) {
+				/* skip empty (null) phandles */
+				if (rc == -ENOENT)
+					continue;
+				else
+					return rc;
+			}
+
+			clk = of_clk_get_from_provider(&clkspec);
+			if (IS_ERR(clk)) {
+				pr_warn("clk: couldn't get clock %d for %s\n",
+					index, node->full_name);
+				return PTR_ERR(clk);
+			}
+
+			rc = clk_set_rate(clk, rate);
+			if (rc < 0)
+				pr_err("clk: couldn't set %s clk rate to %d (%d), current rate: %ld\n",
+				       __clk_get_name(clk), rate, rc,
+				       clk_get_rate(clk));
+			clk_put(clk);
+		}
+		index++;
+	}
+
+	return 0;
+}
+
+static struct clk *__register_divider_clks(struct device *dev, const char *name,
+					   const char *parent_name,
+					   unsigned long flags,
+					   void __iomem *reg, u8 shift,
+					   u8 width, u32 initial_val,
+					   u8 clk_divider_flags,
+					   const struct clk_div_table *table,
+					   spinlock_t *lock)
+{
+	struct mango_clk_divider *div;
+	struct clk_hw *hw;
+	struct clk_init_data init;
+	int ret;
+
+	if (clk_divider_flags & CLK_DIVIDER_HIWORD_MASK) {
+		if (width + shift > 16) {
+			pr_warn("divider value exceeds LOWORD field\n");
+			return ERR_PTR(-EINVAL);
+		}
+	}
+
+	/* allocate the divider */
+	div = kzalloc(sizeof(*div), GFP_KERNEL);
+	if (!div)
+		return ERR_PTR(-ENOMEM);
+
+	init.name = name;
+	if (clk_divider_flags & CLK_DIVIDER_READ_ONLY)
+		init.ops = &mango_clk_divider_ro_ops;
+	else
+		init.ops = &mango_clk_divider_ops;
+	init.flags = flags;
+	init.parent_names = (parent_name ? &parent_name : NULL);
+	init.num_parents = (parent_name ? 1 : 0);
+
+	/* struct mango_clk_divider assignments */
+	div->reg = reg;
+	div->shift = shift;
+	div->width = width;
+	div->flags = clk_divider_flags;
+	div->lock = lock;
+	div->hw.init = &init;
+	div->table = table;
+	div->initial_val = initial_val;
+
+	/* register the clock */
+	hw = &div->hw;
+	ret = clk_hw_register(dev, hw);
+	if (ret) {
+		kfree(div);
+		hw = ERR_PTR(ret);
+		return ERR_PTR(-EBUSY);
+	}
+
+	return hw->clk;
+}
+
+static inline int register_provider_clks
+(struct device_node *node, struct mango_clk_data *clk_data, int clk_num)
+{
+	return of_clk_add_provider(node, of_clk_src_onecell_get,
+				   &clk_data->clk_data);
+}
+
+static int register_gate_clks(struct device *dev, struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_gate_clock *gate_clks = table->gate_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->gate_clks_num;
+	int i;
+
+	for (i = 0; i < clk_num; i++) {
+		clk = clk_register_gate(
+			dev, gate_clks[i].name, gate_clks[i].parent_name,
+			gate_clks[i].flags, base + gate_clks[i].offset,
+			gate_clks[i].bit_idx, gate_clks[i].gate_flags,
+			&clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				gate_clks[i].name);
+			goto err;
+		}
+
+		if (gate_clks[i].alias)
+			clk_register_clkdev(clk, gate_clks[i].alias, NULL);
+
+		clk_data->clk_data.clks[gate_clks[i].id] = clk;
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_gate(clk_data->clk_data.clks[gate_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+static int register_divider_clks(struct device *dev,
+				 struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_divider_clock *div_clks = table->div_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->div_clks_num;
+	int i, val;
+
+	for (i = 0; i < clk_num; i++) {
+		clk = __register_divider_clks(
+			NULL, div_clks[i].name, div_clks[i].parent_name,
+			div_clks[i].flags, base + div_clks[i].offset,
+			div_clks[i].shift, div_clks[i].width,
+			div_clks[i].initial_val,
+			(div_clks[i].initial_sel & MANGO_CLK_USE_INIT_VAL) ?
+				div_clks[i].div_flags | CLK_DIVIDER_READ_ONLY :
+				div_clks[i].div_flags,
+			div_clks[i].table, &clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				div_clks[i].name);
+			goto err;
+		}
+
+		clk_data->clk_data.clks[div_clks[i].id] = clk;
+
+		if (div_clks[i].initial_sel == MANGO_CLK_USE_REG_VAL) {
+			regmap_read(clk_data->syscon_top, div_clks[i].offset,
+				    &val);
+
+			/*
+			 * set a default divider factor,
+			 * clk driver should not select divider clock as the
+			 * clock source, before set the divider by right process
+			 * (assert div, set div factor, de assert div).
+			 */
+			if (div_clks[i].initial_val > 0)
+				val |= (div_clks[i].initial_val << 16 | 1 << 3);
+			else {
+				/*
+				 * the div register is config to use divider factor, don't change divider
+				 */
+				if (!(val >> 3 & 0x1))
+					val |= 1 << 16;
+			}
+
+			regmap_write(clk_data->syscon_top, div_clks[i].offset,
+				     val);
+		}
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_divider(clk_data->clk_data.clks[div_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+static int register_mux_clks(struct device *dev, struct mango_clk_data *clk_data)
+{
+	struct clk *clk;
+	const struct mango_clk_table *table = clk_data->table;
+	const struct mango_mux_clock *mux_clks = table->mux_clks;
+	void __iomem *base = clk_data->base;
+	int clk_num = table->mux_clks_num;
+	int i;
+
+	for (i = 0; i < clk_num; i++) {
+		u32 mask = BIT(mux_clks[i].width) - 1;
+
+		clk = clk_register_mux_table(
+			dev, mux_clks[i].name, mux_clks[i].parent_names,
+			mux_clks[i].num_parents, mux_clks[i].flags,
+			base + mux_clks[i].offset, mux_clks[i].shift, mask,
+			mux_clks[i].mux_flags, mux_clks[i].table,
+			&clk_data->lock);
+		if (IS_ERR(clk)) {
+			pr_err("%s: failed to register clock %s\n", __func__,
+				mux_clks[i].name);
+			goto err;
+		}
+
+		clk_data->clk_data.clks[mux_clks[i].id] = clk;
+
+		if (!(mux_clks[i].flags & CLK_MUX_READ_ONLY)) {
+			struct clk *parent;
+			struct notifier_block *clk_nb;
+
+			/* set mux clock default parent here, it's parent index
+			 * value is read from the mux clock reg. dts can override
+			 * setting the mux clock parent later.
+			 */
+			parent = clk_get_parent(clk);
+			clk_set_parent(clk, parent);
+
+			/* add a notify callback function */
+			clk_nb = kzalloc(sizeof(*clk_nb), GFP_KERNEL);
+			if (!clk_nb)
+				goto err;
+			clk_nb->notifier_call = mux_notifier_cb;
+			if (clk_notifier_register(clk, clk_nb))
+				pr_err("%s: failed to register clock notifier for %s\n",
+					__func__, mux_clks[i].name);
+		}
+	}
+
+	return 0;
+
+err:
+	while (i--)
+		clk_unregister_mux(clk_data->clk_data.clks[mux_clks[i].id]);
+
+	return PTR_ERR(clk);
+}
+
+/* pll clock init */
+int mango_register_pll_clks(struct device_node *node,
+			 struct mango_clk_data *clk_data, const char *clk_name)
+{
+	struct clk *clk = NULL;
+	struct mango_pll_clock *pll_clks;
+	int i, ret = 0;
+	const struct clk_ops *local_ops;
+
+	pll_clks = (struct mango_pll_clock *)clk_data->table->pll_clks;
+	for (i = 0; i < clk_data->table->pll_clks_num; i++) {
+		if (!strcmp(clk_name,  pll_clks[i].name)) {
+			/* have to assigne pll_clks.syscon_top first
+			 * since clk_register_composite will need it
+			 * to calculate current rate.
+			 */
+			pll_clks[i].syscon_top = clk_data->syscon_top;
+			pll_clks[i].lock = &clk_data->lock;
+			if (pll_clks[i].ini_flags & MANGO_CLK_RO)
+				local_ops = &mango_clk_pll_ro_ops;
+			else
+				local_ops = &mango_clk_pll_ops;
+			clk = clk_register_composite(
+				NULL, pll_clks[i].name, &pll_clks[i].parent_name,
+				1, NULL, NULL, &pll_clks[i].hw, local_ops,
+				NULL, NULL, pll_clks[i].flags);
+
+			if (IS_ERR(clk)) {
+				pr_err("%s: failed to register clock %s\n", __func__,
+					pll_clks[i].name);
+				ret = -EINVAL;
+				goto out;
+			}
+			ret = of_clk_add_provider(node, of_clk_src_simple_get, clk);
+			if (ret)
+				clk_unregister(clk);
+		} else {
+			continue;
+		}
+	}
+
+out:
+	return ret;
+}
+
+/* mux clk init */
+int mango_register_mux_clks(struct device_node *node, struct mango_clk_data *clk_data)
+{
+	int ret;
+	int count;
+	struct clk **clk_table;
+
+	count = clk_data->table->mux_clks_num + clk_data->table->gate_clks_num;
+	clk_table = kcalloc(count, sizeof(*clk_table), GFP_KERNEL);
+	if (!clk_table)
+		return -ENOMEM;
+
+	clk_data->clk_data.clks = clk_table;
+	clk_data->clk_data.clk_num = count;
+
+	ret = register_mux_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_gate_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_provider_clks(node, clk_data, count);
+	if (ret)
+		goto err;
+
+	return 0;
+err:
+	kfree(clk_table);
+	return ret;
+}
+
+/* pll divider init */
+int mango_register_div_clks(struct device_node *node, struct mango_clk_data *clk_data)
+{
+	int ret;
+	int count;
+
+	struct clk **clk_table;
+
+	count = clk_data->table->div_clks_num + clk_data->table->gate_clks_num;
+	clk_table = kcalloc(count, sizeof(*clk_table), GFP_KERNEL);
+	if (!clk_table)
+		return -ENOMEM;
+
+	clk_data->clk_data.clks = clk_table;
+	clk_data->clk_data.clk_num = count;
+
+	ret = register_divider_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_gate_clks(NULL, clk_data);
+	if (ret)
+		goto err;
+
+	ret = register_provider_clks(node, clk_data, count);
+	if (ret)
+		goto err;
+
+
+	return 0;
+err:
+	kfree(clk_table);
+	pr_err("%s error %d\n", __func__, ret);
+	return ret;
+}
diff --git a/drivers/clk/sophgo/clk.h b/drivers/clk/sophgo/clk.h
new file mode 100644
index 000000000000..81e9f9eb1b20
--- /dev/null
+++ b/drivers/clk/sophgo/clk.h
@@ -0,0 +1,152 @@
+#ifndef __SOPHGO_CLOCK__
+#define __SOPHGO_CLOCK__
+
+#include <linux/regmap.h>
+#include <linux/slab.h>
+#include <linux/clk.h>
+#include <linux/clk-provider.h>
+#include <linux/device.h>
+#include <linux/clkdev.h>
+
+#include <dt-bindings/clock/sophgo.h>
+
+#define KHZ 1000L
+#define MHZ (KHZ * KHZ)
+
+#define MANGO_CLK_USE_INIT_VAL		BIT(0) /* use default value */
+#define MANGO_CLK_USE_REG_VAL		BIT(1) /* use reg divider value */
+#define MANGO_CLK_RO			BIT(2) /* use reg divider value */
+
+#define CLK_PLL	BIT(0)
+#define CLK_MUX	BIT(1)
+
+#define PLL_CTRL_OFFSET	0xE8
+#define PLL_STAT_LOCK_OFFSET	0x8
+#define CLK_MODE	0x4
+#define CLK_MODE_MASK	0x3
+
+#define REFDIV_MIN 1
+#define REFDIV_MAX 64
+#define FBDIV_MIN 16
+#define FBDIV_MAX 321
+
+#define PLL_FREQ_MIN (16 * MHZ)
+#define PLL_FREQ_MAX (3200 * MHZ)
+
+#define div_mask(width) ((1 << (width)) - 1)
+#define TOP_PLL_CTRL(fbdiv, p1, p2, refdiv) \
+	(((fbdiv & 0xfff) << 16) | ((p2 & 0x7) << 12) | ((p1 & 0x7) << 8) | (refdiv & 0x3f))
+
+struct mango_pll_ctrl {
+	unsigned int mode;
+	unsigned long freq;
+
+	unsigned int fbdiv;
+	unsigned int postdiv1;
+	unsigned int postdiv2;
+	unsigned int refdiv;
+};
+
+struct mango_pll_clock {
+	unsigned int id;
+	char *name;
+	const char *parent_name;
+	unsigned long flags;
+	struct clk_hw	hw;
+	struct regmap *syscon_top;
+
+	/* Below lock used to protect PLL top register during write */
+	spinlock_t *lock;
+	u32 ini_flags;
+
+	u32 status_offset;
+	u32 enable_offset;
+
+	struct mango_pll_ctrl pctrl_table[4];
+};
+
+#define to_mango_pll_clk(_hw) container_of(_hw, struct mango_pll_clock, hw)
+
+#define to_mango_clk_divider(_hw)	\
+	container_of(_hw, struct mango_clk_divider, hw)
+
+#define to_mango_clk_mux(nb) \
+	container_of(nb, struct mango_mux_clock, clk_nb)
+
+struct mango_divider_clock {
+	unsigned int id;
+	const char *name;
+	const char *parent_name;
+	unsigned long flags;
+	unsigned long offset;
+	u8 shift;
+	u8 width;
+	u8 div_flags;
+	u32 initial_sel;
+	u32 initial_val;
+	struct clk_div_table *table;
+};
+
+struct mango_mux_clock {
+	unsigned int id;
+	const char *name;
+	const char *const *parent_names;
+	u8 num_parents;
+	unsigned long flags;
+	unsigned long offset;
+	u8 shift;
+	u8 width;
+	u8 mux_flags;
+	u32 *table;
+
+	struct notifier_block clk_nb;
+};
+
+struct mango_gate_clock {
+	unsigned int id;
+	const char *name;
+	const char *parent_name;
+	unsigned long flags;
+	unsigned long offset;
+	u8 bit_idx;
+	u8 gate_flags;
+	const char *alias;
+};
+
+struct mango_clk_table {
+	u32 id;
+	u32 pll_clks_num;
+	u32 div_clks_num;
+	u32 gate_clks_num;
+	u32 mux_clks_num;
+
+	const struct mango_pll_clock *pll_clks;
+	const struct mango_divider_clock *div_clks;
+	const struct mango_gate_clock *gate_clks;
+	const struct mango_mux_clock *mux_clks;
+};
+
+struct mango_clk_data {
+	void __iomem *base;
+	spinlock_t lock;
+	struct regmap *syscon_top;
+	struct clk_onecell_data	clk_data;
+	const struct mango_clk_table *table;
+};
+
+int mango_register_mux_clks
+(struct device_node *node, struct mango_clk_data *clk_data);
+int mango_register_div_clks
+(struct device_node *node, struct mango_clk_data *clk_data);
+int mango_register_pll_clks
+(struct device_node *node, struct mango_clk_data *clk_data, const char *clk_name);
+int set_default_clk_rates(struct device_node *node);
+
+int dm_mango_register_mux_clks
+(struct device_node *node, struct mango_clk_data *clk_data);
+int dm_mango_register_div_clks
+(struct device_node *node, struct mango_clk_data *clk_data);
+int dm_mango_register_pll_clks
+(struct device_node *node, struct mango_clk_data *clk_data, const char *name);
+int dm_set_default_clk_rates(struct device_node *node);
+#endif
diff --git a/drivers/clk/thead/Kconfig b/drivers/clk/thead/Kconfig
new file mode 100644
index 000000000000..4fa0021a195d
--- /dev/null
+++ b/drivers/clk/thead/Kconfig
@@ -0,0 +1,19 @@
+# SPDX-License-Identifier: GPL-2.0
+
+config THEAD_CLK
+	bool
+	def_bool ARCH_THEAD
+
+config CLK_LIGHT_MPW
+	bool "Thead Light MPW Clock Driver"
+	depends on ARCH_THEAD
+	default n
+	help
+	    Build the driver for light mpw Clock Driver
+
+config CLK_LIGHT_FM
+	bool "Thead Light Fullmask Clock Driver"
+	depends on ARCH_THEAD
+	default n
+	help
+	    Build the driver for light fullmask Clock Driver
diff --git a/drivers/clk/thead/Makefile b/drivers/clk/thead/Makefile
new file mode 100644
index 000000000000..24a349f91989
--- /dev/null
+++ b/drivers/clk/thead/Makefile
@@ -0,0 +1,8 @@
+# SPDX-License-Identifier: GPL-2.0
+
+obj-$(CONFIG_THEAD_CLK) += \
+	clk.o
+
+obj-$(CONFIG_CLK_LIGHT_MPW)  += clk-light-mpw.o
+obj-$(CONFIG_CLK_LIGHT_FM)  += clk-light-fm.o
+obj-$(CONFIG_CLK_LIGHT_FM)  += gate/
diff --git a/drivers/clk/thead/clk-light-fm.c b/drivers/clk/thead/clk-light-fm.c
new file mode 100644
index 000000000000..2fe47c063a53
--- /dev/null
+++ b/drivers/clk/thead/clk-light-fm.c
@@ -0,0 +1,646 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-fm-ap-clock.h>
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+
+#include "clk.h"
+
+static struct clk *clks[CLK_END];
+static struct clk_onecell_data clk_data;
+
+/* Light Fullmask */
+static u32 share_cnt_x2h_cpusys_clk_en;
+static u32 share_cnt_dmac_cpusys_clk_en;
+static u32 share_cnt_timer0_clk_en;
+static u32 share_cnt_timer1_clk_en;
+static u32 share_cnt_axi4_cpusys2_clk_en;
+static u32 share_cnt_bmu_c910_clk_en;
+static u32 share_cnt_aon2cpu_a2x_clk_en;
+static u32 share_cnt_chip_dbg_clk_en;
+static u32 share_cnt_x2x_cpusys_clk_en;
+static u32 share_cnt_cfg2tee_x2h_clk_en;
+static u32 share_cnt_cpu2aon_x2h_clk_en;
+static u32 share_cnt_cpu2vp_x2p_clk_en;
+static u32 share_cnt_npu_core_clk_en;
+static u32 share_cnt_cpu2peri_x2h_clk_en;
+static u32 share_cnt_cpu2vi_x2h_clk_en;
+static u32 share_cnt_vpsys_axi_aclk_en;
+static u32 share_cnt_gmac1_clk_en;
+static u32 share_cnt_gmac0_clk_en;
+static u32 share_cnt_perisys_apb3_hclk_en;
+static u32 share_cnt_qspi0_clk_en;
+static u32 share_cnt_gmac_axi_clk_en;
+static u32 share_cnt_gpio0_clk_en;
+static u32 share_cnt_gpio1_clk_en;
+static u32 share_cnt_pwm_clk_en;
+static u32 share_cnt_spi_clk_en;
+static u32 share_cnt_uart0_clk_en;
+static u32 share_cnt_uart2_clk_en;
+static u32 share_cnt_i2c2_clk_en;
+static u32 share_cnt_peri_i2s_clk_en;
+static u32 share_cnt_qspi1_clk_en;
+static u32 share_cnt_uart1_clk_en;
+static u32 share_cnt_uart3_clk_en;
+static u32 share_cnt_uart4_clk_en;
+static u32 share_cnt_uart5_clk_en;
+static u32 share_cnt_i2c0_clk_en;
+static u32 share_cnt_i2c1_clk_en;
+static u32 share_cnt_i2c4_clk_en;
+static u32 share_cnt_i2c5_clk_en;
+static u32 share_cnt_gpio2_clk_en;
+static u32 share_cnt_gpio3_clk_en;
+static u32 share_cnt_vosys_axi_aclk_en;
+
+/* Light Fullmask PLL Bypass */
+static const char * const cpu_pll0_bypass_sels[] = {"cpu_pll0_foutpostdiv", "osc_24m", };
+static const char * const cpu_pll1_bypass_sels[] = {"cpu_pll1_foutpostdiv", "osc_24m", };
+static const char * const gmac_pll_bypass_sels[] = {"gmac_pll_foutpostdiv", "osc_24m", };
+static const char * const video_pll_bypass_sels[] = {"video_pll_foutpostdiv", "osc_24m", };
+static const char * const tee_pll_bypass_sels[] = {"tee_pll_foutpostdiv", "osc_24m"};
+static const char * const dpu0_pll_bypass_sels[] = {"dpu0_pll_foutpostdiv", "osc_24m"};
+static const char * const dpu1_pll_bypass_sels[] = {"dpu1_pll_foutpostdiv", "osc_24m"};
+
+/* light fullmask mux */
+static const char * const ahb2_cpusys_hclk_sels[] = {"ahb2_cpusys_hclk_out_div", "osc_24m"};
+static const char * const c910_cclk_i0_sels[] = {"cpu_pll0_foutpostdiv", "osc_24m"};
+static const char * const c910_cclk_sels[] = {"c910_cclk_i0", "cpu_pll1_foutpostdiv"};
+static const char * const cfg_axi_aclk_sels[] = {"cfg_axi_aclk_out_div", "osc_24m"};
+static const char * const teesys_hclk_sels[] = {"teesys_i1_hclk", "teesys_i0_hclk"};
+static const char * const perisys_ahb_hclk_sels[] = {"perisys_ahb_hclk_out_div", "osc_24m"};
+static const char * const clk_out_1_sels[] = {"osc_24m", "clk_out_1_out_div"};
+static const char * const clk_out_2_sels[] = {"osc_24m", "clk_out_2_out_div"};
+static const char * const clk_out_3_sels[] = {"osc_24m", "clk_out_3_out_div"};
+static const char * const clk_out_4_sels[] = {"osc_24m", "clk_out_4_out_div"};
+static const char * const peri_i2s_src_clk_sels[] = {"clkgen_peri_i2s_src_clk_0", "clkgen_peri_i2s_src_clk_1"};
+static const char * const npu_cclk_sels[] = {"gmac_pll_foutpostdiv", "npu_cclk_out_div"};
+static const char * const cfg_apb_pclk_sels[] = {"cfg_apb_pclk_out_div", "osc_24m"};
+static const char * const uart_sclk_sels[] = {"clk_100m", "osc_24m"};
+
+static const struct light_pll_rate_table light_cpupll_tbl[] = {
+	LIGHT_PLL_RATE(2616000000U, 2616000000U, 1, 109, 0, 1, 1),
+	LIGHT_PLL_RATE(2592000000U, 2592000000U, 1, 108, 0, 1, 1),
+	LIGHT_PLL_RATE(2568000000U, 2568000000U, 1, 107, 0, 1, 1),
+	LIGHT_PLL_RATE(2544000000U, 2544000000U, 1, 106, 0, 1, 1),
+	LIGHT_PLL_RATE(2520000000U, 2520000000U, 1, 105, 0, 1, 1),
+	LIGHT_PLL_RATE(2496000000U, 2496000000U, 1, 104, 0, 1, 1),
+	LIGHT_PLL_RATE(2472000000U, 2472000000U, 1, 103, 0, 1, 1),
+	LIGHT_PLL_RATE(2448000000U, 2448000000U, 1, 102, 0, 1, 1),
+	LIGHT_PLL_RATE(2424000000U, 2424000000U, 1, 101, 0, 1, 1),
+	LIGHT_PLL_RATE(2400000000U, 2400000000U, 1, 100, 0, 1, 1),
+	LIGHT_PLL_RATE(2376000000U, 2376000000U, 1, 99,  0, 1, 1),
+	LIGHT_PLL_RATE(2352000000U, 2352000000U, 1, 98,  0, 1, 1),
+	LIGHT_PLL_RATE(2328000000U, 2328000000U, 1, 97,  0, 1, 1),
+	LIGHT_PLL_RATE(2304000000U, 2304000000U, 1, 96,  0, 1, 1),
+	LIGHT_PLL_RATE(2280000000U, 2280000000U, 1, 95,  0, 1, 1),
+	LIGHT_PLL_RATE(2256000000U, 2256000000U, 1, 94,  0, 1, 1),
+	LIGHT_PLL_RATE(2232000000U, 2232000000U, 1, 93,  0, 1, 1),
+	LIGHT_PLL_RATE(2208000000U, 2208000000U, 1, 92,  0, 1, 1),
+	LIGHT_PLL_RATE(2184000000U, 2184000000U, 1, 91,  0, 1, 1),
+	LIGHT_PLL_RATE(2160000000U, 2160000000U, 1, 90,  0, 1, 1),
+	LIGHT_PLL_RATE(2136000000U, 2136000000U, 1, 89,  0, 1, 1),
+	LIGHT_PLL_RATE(2112000000U, 2112000000U, 1, 88,  0, 1, 1),
+	LIGHT_PLL_RATE(2088000000U, 2088000000U, 1, 87,  0, 1, 1),
+	LIGHT_PLL_RATE(2064000000U, 2064000000U, 1, 86,  0, 1, 1),
+	LIGHT_PLL_RATE(2040000000U, 2040000000U, 1, 85,  0, 1, 1),
+	LIGHT_PLL_RATE(2016000000U, 2016000000U, 1, 84,  0, 1, 1),
+	LIGHT_PLL_RATE(1992000000U, 1992000000U, 1, 83,  0, 1, 1),
+	LIGHT_PLL_RATE(1968000000U, 1968000000U, 1, 82,  0, 1, 1),
+	LIGHT_PLL_RATE(1944000000U, 1944000000U, 1, 81,  0, 1, 1),
+	LIGHT_PLL_RATE(1920000000U, 1920000000U, 1, 80,  0, 1, 1),
+	LIGHT_PLL_RATE(1896000000U, 1896000000U, 1, 79,  0, 1, 1),
+	LIGHT_PLL_RATE(1872000000U, 1872000000U, 1, 78,  0, 1, 1),
+	LIGHT_PLL_RATE(1848000000U, 1848000000U, 1, 77,  0, 1, 1),
+	LIGHT_PLL_RATE(1824000000U, 1824000000U, 1, 76,  0, 1, 1),
+	LIGHT_PLL_RATE(1800000000U, 1800000000U, 1, 75,  0, 1, 1),
+	LIGHT_PLL_RATE(1776000000U, 1776000000U, 1, 74,  0, 1, 1),
+	LIGHT_PLL_RATE(1752000000U, 1752000000U, 1, 73,  0, 1, 1),
+	LIGHT_PLL_RATE(1728000000U, 1728000000U, 1, 72,  0, 1, 1),
+	LIGHT_PLL_RATE(1704000000U, 1704000000U, 1, 71,  0, 1, 1),
+	LIGHT_PLL_RATE(1680000000U, 1680000000U, 1, 70,  0, 1, 1),
+	LIGHT_PLL_RATE(1656000000U, 1656000000U, 1, 69,  0, 1, 1),
+	LIGHT_PLL_RATE(1632000000U, 1632000000U, 1, 68,  0, 1, 1),
+	LIGHT_PLL_RATE(1608000000U, 1608000000U, 1, 67,  0, 1, 1),
+	LIGHT_PLL_RATE(1584000000U, 1584000000U, 1, 66,  0, 1, 1),
+	LIGHT_PLL_RATE(1560000000U, 1560000000U, 1, 65,  0, 1, 1),
+	LIGHT_PLL_RATE(1536000000U, 1536000000U, 1, 64,  0, 1, 1),
+	LIGHT_PLL_RATE(1512000000U, 1512000000U, 1, 63,  0, 1, 1),
+	LIGHT_PLL_RATE(3000000000U, 1500000000U, 1, 125, 0, 2, 1),
+	LIGHT_PLL_RATE(2976000000U, 1488000000U, 1, 124, 0, 2, 1),
+	LIGHT_PLL_RATE(2952000000U, 1476000000U, 1, 123, 0, 2, 1),
+	LIGHT_PLL_RATE(2928000000U, 1464000000U, 1, 122, 0, 2, 1),
+	LIGHT_PLL_RATE(2904000000U, 1452000000U, 1, 121, 0, 2, 1),
+	LIGHT_PLL_RATE(2880000000U, 1440000000U, 1, 120, 0, 2, 1),
+	LIGHT_PLL_RATE(2856000000U, 1428000000U, 1, 119, 0, 2, 1),
+	LIGHT_PLL_RATE(2832000000U, 1416000000U, 1, 118, 0, 2, 1),
+	LIGHT_PLL_RATE(2808000000U, 1404000000U, 1, 117, 0, 2, 1),
+	LIGHT_PLL_RATE(2784000000U, 1392000000U, 1, 116, 0, 2, 1),
+	LIGHT_PLL_RATE(2760000000U, 1380000000U, 1, 115, 0, 2, 1),
+	LIGHT_PLL_RATE(2736000000U, 1368000000U, 1, 114, 0, 2, 1),
+	LIGHT_PLL_RATE(2712000000U, 1356000000U, 1, 113, 0, 2, 1),
+	LIGHT_PLL_RATE(2688000000U, 1344000000U, 1, 112, 0, 2, 1),
+	LIGHT_PLL_RATE(2664000000U, 1332000000U, 1, 111, 0, 2, 1),
+	LIGHT_PLL_RATE(2640000000U, 1320000000U, 1, 110, 0, 2, 1),
+	LIGHT_PLL_RATE(2616000000U, 1308000000U, 1, 109, 0, 2, 1),
+	LIGHT_PLL_RATE(2592000000U, 1296000000U, 1, 108, 0, 2, 1),
+	LIGHT_PLL_RATE(2568000000U, 1284000000U, 1, 107, 0, 2, 1),
+	LIGHT_PLL_RATE(2544000000U, 1272000000U, 1, 106, 0, 2, 1),
+	LIGHT_PLL_RATE(2520000000U, 1260000000U, 1, 105, 0, 2, 1),
+	LIGHT_PLL_RATE(2496000000U, 1248000000U, 1, 104, 0, 2, 1),
+	LIGHT_PLL_RATE(2472000000U, 1236000000U, 1, 103, 0, 2, 1),
+	LIGHT_PLL_RATE(2448000000U, 1224000000U, 1, 102, 0, 2, 1),
+	LIGHT_PLL_RATE(2424000000U, 1212000000U, 1, 101, 0, 2, 1),
+	LIGHT_PLL_RATE(2400000000U, 1200000000U, 1, 100, 0, 2, 1),
+	LIGHT_PLL_RATE(2376000000U, 1188000000U, 1, 99,  0, 2, 1),
+	LIGHT_PLL_RATE(2352000000U, 1176000000U, 1, 98,  0, 2, 1),
+	LIGHT_PLL_RATE(2328000000U, 1164000000U, 1, 97,  0, 2, 1),
+	LIGHT_PLL_RATE(2304000000U, 1152000000U, 1, 96,  0, 2, 1),
+	LIGHT_PLL_RATE(2280000000U, 1140000000U, 1, 95,  0, 2, 1),
+	LIGHT_PLL_RATE(2256000000U, 1128000000U, 1, 94,  0, 2, 1),
+	LIGHT_PLL_RATE(2232000000U, 1116000000U, 1, 93,  0, 2, 1),
+	LIGHT_PLL_RATE(2208000000U, 1104000000U, 1, 92,  0, 2, 1),
+	LIGHT_PLL_RATE(2184000000U, 1092000000U, 1, 91,  0, 2, 1),
+	LIGHT_PLL_RATE(2160000000U, 1080000000U, 1, 90,  0, 2, 1),
+	LIGHT_PLL_RATE(2136000000U, 1068000000U, 1, 89,  0, 2, 1),
+	LIGHT_PLL_RATE(2112000000U, 1056000000U, 1, 88,  0, 2, 1),
+	LIGHT_PLL_RATE(2088000000U, 1044000000U, 1, 87,  0, 2, 1),
+	LIGHT_PLL_RATE(2064000000U, 1032000000U, 1, 86,  0, 2, 1),
+	LIGHT_PLL_RATE(2040000000U, 1020000000U, 1, 85,  0, 2, 1),
+	LIGHT_PLL_RATE(2016000000U, 1008000000U, 1, 84,  0, 2, 1),
+	LIGHT_PLL_RATE(3000000000U, 1000000000U, 1, 125, 0, 3, 1),
+	LIGHT_PLL_RATE(2976000000U, 992000000U,  1, 124, 0, 3, 1),
+	LIGHT_PLL_RATE(2952000000U, 984000000U,  1, 123, 0, 3, 1),
+	LIGHT_PLL_RATE(2928000000U, 976000000U,  1, 122, 0, 3, 1),
+	LIGHT_PLL_RATE(2904000000U, 968000000U,  1, 121, 0, 3, 1),
+	LIGHT_PLL_RATE(2880000000U, 960000000U,  1, 120, 0, 3, 1),
+	LIGHT_PLL_RATE(2856000000U, 952000000U,  1, 119, 0, 3, 1),
+	LIGHT_PLL_RATE(2832000000U, 944000000U,  1, 118, 0, 3, 1),
+	LIGHT_PLL_RATE(2808000000U, 936000000U,  1, 117, 0, 3, 1),
+	LIGHT_PLL_RATE(2784000000U, 928000000U,  1, 116, 0, 3, 1),
+	LIGHT_PLL_RATE(2760000000U, 920000000U,  1, 115, 0, 3, 1),
+	LIGHT_PLL_RATE(2736000000U, 912000000U,  1, 114, 0, 3, 1),
+	LIGHT_PLL_RATE(2712000000U, 904000000U,  1, 113, 0, 3, 1),
+	LIGHT_PLL_RATE(1800000000U, 900000000U,  1, 75,  0, 2, 1),
+	LIGHT_PLL_RATE(2688000000U, 896000000U,  1, 112, 0, 3, 1),
+	LIGHT_PLL_RATE(2664000000U, 888000000U,  1, 111, 0, 3, 1),
+	LIGHT_PLL_RATE(2640000000U, 880000000U,  1, 110, 0, 3, 1),
+	LIGHT_PLL_RATE(2616000000U, 872000000U,  1, 109, 0, 3, 1),
+	LIGHT_PLL_RATE(2592000000U, 864000000U,  1, 108, 0, 3, 1),
+	LIGHT_PLL_RATE(2568000000U, 856000000U,  1, 107, 0, 3, 1),
+	LIGHT_PLL_RATE(2544000000U, 848000000U,  1, 106, 0, 3, 1),
+	LIGHT_PLL_RATE(2520000000U, 840000000U,  1, 105, 0, 3, 1),
+	LIGHT_PLL_RATE(2496000000U, 832000000U,  1, 104, 0, 3, 1),
+	LIGHT_PLL_RATE(2472000000U, 824000000U,  1, 103, 0, 3, 1),
+	LIGHT_PLL_RATE(2448000000U, 816000000U,  1, 102, 0, 3, 1),
+	LIGHT_PLL_RATE(2424000000U, 808000000U,  1, 101, 0, 3, 1),
+	LIGHT_PLL_RATE(2400000000U, 800000000U,  1, 100, 0, 3, 1),
+	LIGHT_PLL_RATE(2376000000U, 792000000U,  1, 99,  0, 3, 1),
+	LIGHT_PLL_RATE(2352000000U, 784000000U,  1, 98,  0, 3, 1),
+	LIGHT_PLL_RATE(2328000000U, 776000000U,  1, 97,  0, 3, 1),
+	LIGHT_PLL_RATE(2304000000U, 768000000U,  1, 96,  0, 3, 1),
+	LIGHT_PLL_RATE(2280000000U, 760000000U,  1, 95,  0, 3, 1),
+	LIGHT_PLL_RATE(2256000000U, 752000000U,  1, 94,  0, 3, 1),
+	LIGHT_PLL_RATE(2232000000U, 744000000U,  1, 93,  0, 3, 1),
+	LIGHT_PLL_RATE(2208000000U, 736000000U,  1, 92,  0, 3, 1),
+	LIGHT_PLL_RATE(2184000000U, 728000000U,  1, 91,  0, 3, 1),
+	LIGHT_PLL_RATE(2160000000U, 720000000U,  1, 90,  0, 3, 1),
+	LIGHT_PLL_RATE(2136000000U, 712000000U,  1, 89,  0, 3, 1),
+	LIGHT_PLL_RATE(2808000000U, 702000000U,  1, 117, 0, 4, 1),
+	LIGHT_PLL_RATE(2760000000U, 690000000U,  1, 115, 0, 4, 1),
+	LIGHT_PLL_RATE(2712000000U, 678000000U,  1, 113, 0, 4, 1),
+	LIGHT_PLL_RATE(2664000000U, 666000000U,  1, 111, 0, 4, 1),
+	LIGHT_PLL_RATE(2616000000U, 654000000U,  1, 109, 0, 4, 1),
+	LIGHT_PLL_RATE(2568000000U, 642000000U,  1, 107, 0, 4, 1),
+	LIGHT_PLL_RATE(2520000000U, 630000000U,  1, 105, 0, 4, 1),
+	LIGHT_PLL_RATE(2472000000U, 618000000U,  1, 103, 0, 4, 1),
+	LIGHT_PLL_RATE(2424000000U, 606000000U,  1, 101, 0, 4, 1),
+	LIGHT_PLL_RATE(3000000000U, 600000000U,  1, 125, 0, 5, 1),
+	LIGHT_PLL_RATE(2952000000U, 590400000U,  1, 123, 0, 5, 1),
+	LIGHT_PLL_RATE(2904000000U, 580800000U,  1, 121, 0, 5, 1),
+	LIGHT_PLL_RATE(2856000000U, 571200000U,  1, 119, 0, 5, 1),
+	LIGHT_PLL_RATE(2808000000U, 561600000U,  1, 117, 0, 5, 1),
+	LIGHT_PLL_RATE(2760000000U, 552000000U,  1, 115, 0, 5, 1),
+	LIGHT_PLL_RATE(2712000000U, 542400000U,  1, 113, 0, 5, 1),
+	LIGHT_PLL_RATE(2664000000U, 532800000U,  1, 111, 0, 5, 1),
+	LIGHT_PLL_RATE(2616000000U, 523200000U,  1, 109, 0, 5, 1),
+	LIGHT_PLL_RATE(2568000000U, 513600000U,  1, 107, 0, 5, 1),
+	LIGHT_PLL_RATE(2520000000U, 504000000U,  1, 105, 0, 5, 1),
+	LIGHT_PLL_RATE(3000000000U, 500000000U,  1, 125, 0, 6, 1),
+	LIGHT_PLL_RATE(2952000000U, 492000000U,  1, 123, 0, 6, 1),
+	LIGHT_PLL_RATE(2904000000U, 484000000U,  1, 121, 0, 6, 1),
+	LIGHT_PLL_RATE(2856000000U, 476000000U,  1, 119, 0, 6, 1),
+	LIGHT_PLL_RATE(2808000000U, 468000000U,  1, 117, 0, 6, 1),
+	LIGHT_PLL_RATE(2760000000U, 460000000U,  1, 115, 0, 6, 1),
+	LIGHT_PLL_RATE(2712000000U, 452000000U,  1, 113, 0, 6, 1),
+	LIGHT_PLL_RATE(2664000000U, 444000000U,  1, 111, 0, 6, 1),
+	LIGHT_PLL_RATE(2616000000U, 436000000U,  1, 109, 0, 6, 1),
+	LIGHT_PLL_RATE(2568000000U, 428000000U,  1, 107, 0, 6, 1),
+	LIGHT_PLL_RATE(2520000000U, 420000000U,  1, 105, 0, 6, 1),
+	LIGHT_PLL_RATE(2472000000U, 412000000U,  1, 103, 0, 6, 1),
+	LIGHT_PLL_RATE(2400000000U, 400000000U,  1, 100, 0, 3, 2),
+	LIGHT_PLL_RATE(2352000000U, 392000000U,  1, 98,  0, 3, 2),
+	LIGHT_PLL_RATE(2304000000U, 384000000U,  1, 96,  0, 3, 2),
+	LIGHT_PLL_RATE(2256000000U, 376000000U,  1, 94,  0, 3, 2),
+	LIGHT_PLL_RATE(2208000000U, 368000000U,  1, 92,  0, 3, 2),
+	LIGHT_PLL_RATE(2160000000U, 360000000U,  1, 90,  0, 3, 2),
+	LIGHT_PLL_RATE(2112000000U, 352000000U,  1, 88,  0, 3, 2),
+	LIGHT_PLL_RATE(2064000000U, 344000000U,  1, 86,  0, 3, 2),
+	LIGHT_PLL_RATE(2016000000U, 336000000U,  1, 84,  0, 3, 2),
+	LIGHT_PLL_RATE(1968000000U, 328000000U,  1, 82,  0, 3, 2),
+	LIGHT_PLL_RATE(1920000000U, 320000000U,  1, 80,  0, 3, 2),
+	LIGHT_PLL_RATE(1872000000U, 312000000U,  1, 78,  0, 3, 2),
+	LIGHT_PLL_RATE(1824000000U, 304000000U,  1, 76,  0, 3, 2),
+	LIGHT_PLL_RATE(3000000000U, 300000000U,  1, 125, 0, 5, 2),
+	LIGHT_PLL_RATE(2880000000U, 288000000U,  1, 120, 0, 5, 2),
+	LIGHT_PLL_RATE(2760000000U, 276000000U,  1, 115, 0, 5, 2),
+	LIGHT_PLL_RATE(2640000000U, 264000000U,  1, 110, 0, 5, 2),
+	LIGHT_PLL_RATE(2520000000U, 252000000U,  1, 105, 0, 5, 2),
+	LIGHT_PLL_RATE(2400000000U, 240000000U,  1, 100, 0, 5, 2),
+	LIGHT_PLL_RATE(2280000000U, 228000000U,  1, 95,  0, 5, 2),
+	LIGHT_PLL_RATE(2160000000U, 216000000U,  1, 90,  0, 5, 2),
+	LIGHT_PLL_RATE(2040000000U, 204000000U,  1, 85,  0, 5, 2),
+	LIGHT_PLL_RATE(3000000000U, 200000000U,  1, 125, 0, 5, 3),
+	LIGHT_PLL_RATE(2880000000U, 192000000U,  1, 120, 0, 5, 3),
+	LIGHT_PLL_RATE(2760000000U, 184000000U,  1, 115, 0, 5, 3),
+	LIGHT_PLL_RATE(2640000000U, 176000000U,  1, 110, 0, 5, 3),
+	LIGHT_PLL_RATE(2520000000U, 168000000U,  1, 105, 0, 5, 3),
+	LIGHT_PLL_RATE(2400000000U, 160000000U,  1, 100, 0, 5, 3),
+	LIGHT_PLL_RATE(2280000000U, 152000000U,  1, 95,  0, 5, 3),
+	LIGHT_PLL_RATE(2160000000U, 144000000U,  1, 90,  0, 5, 3),
+	LIGHT_PLL_RATE(2040000000U, 136000000U,  1, 85,  0, 5, 3),
+	LIGHT_PLL_RATE(1920000000U, 128000000U,  1, 80,  0, 5, 3),
+	LIGHT_PLL_RATE(3000000000U, 125000000U,  1, 125, 0, 6, 4),
+	LIGHT_PLL_RATE(2760000000U, 115000000U,  1, 115, 0, 6, 4),
+	LIGHT_PLL_RATE(2520000000U, 105000000U,  1, 105, 0, 6, 4),
+	LIGHT_PLL_RATE(2280000000U, 95000000U,   1, 95,  0, 6, 4),
+	LIGHT_PLL_RATE(2040000000U, 85000000U,   1, 85,  0, 6, 4),
+	LIGHT_PLL_RATE(1800000000U, 75000000U,   1, 75,  0, 6, 4),
+	LIGHT_PLL_RATE(1560000000U, 65000000U,   1, 65,  0, 6, 4),
+	LIGHT_PLL_RATE(1320000000U, 55000000U,   1, 55,  0, 6, 4),
+};
+
+static const struct light_pll_rate_table light_dpupll_tbl[] = {
+	LIGHT_PLL_RATE(2376000000U, 1188000000U, 1, 99, 0, 2, 1),
+	LIGHT_PLL_RATE(1980000000U, 990000000U, 2, 165, 0, 2, 1),
+	LIGHT_PLL_RATE(2970000000U, 742500000U, 4, 495, 0, 4, 1),
+	LIGHT_PLL_RATE(2304000000U, 1152000000U, 1, 96, 0, 2, 1),
+	LIGHT_PLL_RATE(1512000000U, 504000000U, 1, 63, 0, 3, 1),
+	LIGHT_PLL_RATE(1512000000U, 503500000U, 1, 63, 0, 3, 1),
+	LIGHT_PLL_RATE(2898000000U, 483000000U, 4, 483, 0, 6, 1),
+	LIGHT_PLL_RATE(2592000000U, 648000000U, 1, 108, 0, 4, 1),
+	LIGHT_PLL_RATE(2772000000U, 924000000U, 2, 231, 0, 3, 1),
+	LIGHT_PLL_RATE(2856000000U, 476000000U, 1, 119, 0, 6, 1),
+	LIGHT_PLL_RATE(2130000000U, 355000000U, 4, 355, 0, 6, 1),
+	LIGHT_PLL_RATE(3192000000U, 456000000U, 1, 133, 0, 7, 1),
+	LIGHT_PLL_RATE(2730000000U, 390000000U, 4, 455, 0, 7, 1),
+	LIGHT_PLL_RATE(1680000000U, 240000000U, 1, 70, 0, 7, 1),
+	LIGHT_PLL_RATE(2832000000U, 708000000U, 1, 118, 0, 4, 1),
+	LIGHT_PLL_RATE(1026000000U, 342000000U, 4, 171, 0, 3, 1),
+	LIGHT_PLL_RATE(1260000000U, 630000000U, 4, 210, 0, 2, 1),
+};
+
+static struct light_pll_clk light_cpu_pll0div = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_CPU_PLL0,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+static struct light_pll_clk light_cpu_pll1div = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_CPU_PLL1,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+static struct light_pll_clk light_dpu0_plldiv = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_DPU0_PLL,
+	.rate_table = light_dpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_dpupll_tbl),
+};
+
+static struct light_pll_clk light_dpu1_plldiv = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_DPU1_PLL,
+	.rate_table = light_dpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_dpupll_tbl),
+};
+
+static int light_clocks_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	void __iomem *ap_base;
+	int ret;
+	const bool *teesys = of_device_get_match_data(dev);
+
+	/* Clock source */
+	clks[CLK_DUMMY] = thead_clk_fixed("dummy", 0);
+	clks[OSC_32K] = of_clk_get_by_name(np, "osc_32k");
+	clks[OSC_24M] = of_clk_get_by_name(np, "osc_24m");
+	clks[RC_24M] = of_clk_get_by_name(np, "rc_24m");
+
+	np = dev->of_node;
+	ap_base = devm_platform_ioremap_resource(pdev, 0);
+	if (WARN_ON(IS_ERR(ap_base))) {
+		ret = PTR_ERR(ap_base);
+		goto unregister_clks;
+	}
+
+	/* Light Fullmask AP PLL clocks */
+	clks[CPU_PLL0_FOUTPOSTDIV] = thead_light_pll("cpu_pll0_foutpostdiv", "osc_24m", ap_base, &light_cpu_pll0div);
+	clks[CPU_PLL1_FOUTPOSTDIV] = thead_light_pll("cpu_pll1_foutpostdiv", "osc_24m", ap_base, &light_cpu_pll1div);
+
+	clks[DPU0_PLL_FOUTPOSTDIV] = thead_light_pll("dpu0_pll_foutpostdiv", "osc_24m", ap_base, &light_dpu0_plldiv);
+	clks[DPU1_PLL_FOUTPOSTDIV] = thead_light_pll("dpu1_pll_foutpostdiv", "osc_24m", ap_base, &light_dpu1_plldiv);
+
+	/* Light Fullmask AP Fixed PLL */
+	clks[GMAC_PLL_FOUTPOSTDIV] = thead_clk_fixed("gmac_pll_foutpostdiv", 1000000000);
+	clks[VIDEO_PLL_FOUTPOSTDIV] = thead_clk_fixed("video_pll_foutpostdiv", 792000000);
+	clks[VIDEO_PLL_FOUTVCO] = thead_clk_fixed("video_pll_foutvco", 2376000000);
+	clks[TEE_PLL_FOUTPOSTDIV] = thead_clk_fixed("tee_pll_foutpostdiv", 792000000);
+	clks[CLKGEN_PERI_I2S_SRC_CLK_0] = thead_clk_fixed("clkgen_peri_i2s_src_clk_0", 294912000);	//from audio_pll_foutpostdiv
+	clks[CLKGEN_PERI_I2S_SRC_CLK_1] = thead_clk_fixed("clkgen_peri_i2s_src_clk_1", 135475200);	//from sys_pll_foutpostdiv
+	clks[CLKGEN_C910_BUS_CLK_NO_ICG] = thead_clk_fixed("clkgen_c910_bus_clk_no_icg", 750000000);
+	clks[AONSYS_BUS_CLK] = thead_clk_fixed("aonsys_hclk", 101606400);	//from sys_pll, maybe change ?
+
+	/* Light Fullmask AP MUX */
+	clks[CPU_PLL0_BYPASS] = thead_light_clk_mux_flags("cpu_pll0_bypass", ap_base + 0x4, 30, 1, cpu_pll0_bypass_sels, ARRAY_SIZE(cpu_pll0_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[CPU_PLL1_BYPASS] = thead_light_clk_mux_flags("cpu_pll1_bypass", ap_base + 0x14, 30, 1, cpu_pll1_bypass_sels, ARRAY_SIZE(cpu_pll1_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[GMAC_PLL_BYPASS] = thead_light_clk_mux_flags("gmac_pll_bypass", ap_base + 0x24, 30, 1, gmac_pll_bypass_sels, ARRAY_SIZE(gmac_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[VIDEO_PLL_BYPASS] = thead_light_clk_mux_flags("video_pll_bypass", ap_base + 0x34, 30, 1, video_pll_bypass_sels, ARRAY_SIZE(video_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[TEE_PLL_BYPASS] = thead_light_clk_mux_flags("tee_pll_bypass", ap_base + 0x64, 30, 1, tee_pll_bypass_sels, ARRAY_SIZE(tee_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[DPU0_PLL_BYPASS] = thead_light_clk_mux_flags("dpu0_pll_bypass", ap_base + 0x44, 30, 1, dpu0_pll_bypass_sels, ARRAY_SIZE(dpu0_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[DPU1_PLL_BYPASS] = thead_light_clk_mux_flags("dpu1_pll_bypass", ap_base + 0x54, 30, 1, dpu1_pll_bypass_sels, ARRAY_SIZE(dpu1_pll_bypass_sels), CLK_SET_RATE_PARENT);
+
+	clks[AHB2_CPUSYS_HCLK] = thead_light_clk_mux_flags("ahb2_cpusys_hclk", ap_base + 0x120, 5, 1, ahb2_cpusys_hclk_sels, ARRAY_SIZE(ahb2_cpusys_hclk_sels), CLK_SET_RATE_PARENT);
+	clks[C910_CCLK_I0] = thead_light_clk_mux_flags("c910_cclk_i0", ap_base + 0x100, 1, 1, c910_cclk_i0_sels, ARRAY_SIZE(c910_cclk_i0_sels), CLK_SET_RATE_PARENT);
+	clks[C910_CCLK] = thead_light_clk_mux_flags("c910_cclk", ap_base + 0x100, 0, 1, c910_cclk_sels, ARRAY_SIZE(c910_cclk_sels), CLK_SET_RATE_PARENT);
+	clks[CFG_AXI_ACLK] = thead_light_clk_mux_flags("cfg_axi_aclk", ap_base + 0x138, 5, 1, cfg_axi_aclk_sels, ARRAY_SIZE(cfg_axi_aclk_sels), CLK_SET_RATE_PARENT);
+
+	if (teesys)
+		clks[TEESYS_HCLK] = thead_light_clk_mux_flags("teesys_hclk", ap_base + 0x1cc, 13, 1, teesys_hclk_sels, ARRAY_SIZE(teesys_hclk_sels), CLK_SET_RATE_PARENT); //just for teesys!!!
+
+	clks[PERISYS_AHB_HCLK] = thead_light_clk_mux_flags("perisys_ahb_hclk", ap_base + 0x140, 5, 1, perisys_ahb_hclk_sels, ARRAY_SIZE(perisys_ahb_hclk_sels), CLK_SET_RATE_PARENT);
+	clks[CLK_OUT_1] = thead_light_clk_mux_flags("clk_out_1", ap_base + 0x1b4, 4, 1, clk_out_1_sels, ARRAY_SIZE(clk_out_1_sels), CLK_SET_RATE_PARENT);
+	clks[CLK_OUT_2] = thead_light_clk_mux_flags("clk_out_2", ap_base + 0x1b8, 4, 1, clk_out_2_sels, ARRAY_SIZE(clk_out_2_sels), CLK_SET_RATE_PARENT);
+	clks[CLK_OUT_3] = thead_light_clk_mux_flags("clk_out_3", ap_base + 0x1bc, 4, 1, clk_out_3_sels, ARRAY_SIZE(clk_out_3_sels), CLK_SET_RATE_PARENT);
+	clks[CLK_OUT_4] = thead_light_clk_mux_flags("clk_out_4", ap_base + 0x1c0, 4, 1, clk_out_4_sels, ARRAY_SIZE(clk_out_4_sels), CLK_SET_RATE_PARENT);
+	clks[PERI_I2S_SRC_CLK] = thead_light_clk_mux_flags("peri_i2s_src_clk", ap_base + 0x1f0, 0, 1, peri_i2s_src_clk_sels, ARRAY_SIZE(peri_i2s_src_clk_sels), CLK_SET_RATE_PARENT);
+	clks[NPU_CCLK] = thead_light_clk_mux_flags("npu_cclk", ap_base + 0x1c8, 6, 1, npu_cclk_sels, ARRAY_SIZE(npu_cclk_sels), CLK_SET_RATE_PARENT);
+	clks[CFG_APB_PCLK] = thead_light_clk_mux_flags("cfg_apb_pclk", ap_base + 0x1c4, 7, 1, cfg_apb_pclk_sels, ARRAY_SIZE(cfg_apb_pclk_sels), CLK_SET_RATE_PARENT);
+	clks[UART_SCLK] = thead_light_clk_mux_flags("uart_sclk", ap_base + 0x210, 0, 1, uart_sclk_sels, ARRAY_SIZE(uart_sclk_sels), CLK_SET_RATE_PARENT);
+
+	/* Light Fullmask AP Divider */
+	clks[AHB2_CPUSYS_HCLK_OUT_DIV] = thead_clk_light_divider("ahb2_cpusys_hclk_out_div", "gmac_pll_fout1ph0", ap_base + 0x120, 0, 3, 4, MUX_TYPE_DIV, 2, 7);
+	clks[APB3_CPUSYS_PCLK] = thead_clk_light_divider("apb3_cpusys_pclk", "ahb2_cpusys_hclk", ap_base + 0x130, 0, 3, 3, MUX_TYPE_CDE, 1, 7);
+	clks[AXI4_CPUSYS2_ACLK] = thead_clk_light_divider("axi4_cpusys2_aclk", "gmac_pll_foutpostdiv", ap_base + 0x134, 0, 3, 4, MUX_TYPE_DIV, 2, 7);
+	clks[CFG_AXI_ACLK_OUT_DIV] = thead_clk_light_divider("cfg_axi_aclk_out_div", "video_pll_foutpostdiv", ap_base + 0x138, 0, 4, 4, MUX_TYPE_DIV, 2, 15);
+
+	if (teesys) {
+		clks[TEESYS_I0_HCLK] = thead_clk_light_divider("teesys_i0_hclk", "tee_pll_foutpostdiv", ap_base + 0x1cc, 0, 4, 4, MUX_TYPE_DIV, 2, 15); //just for teesys!!!
+		clks[TEESYS_I1_HCLK] = thead_clk_light_divider("teesys_i1_hclk", "video_pll_foutpostdiv", ap_base + 0x1cc, 8, 4, 12, MUX_TYPE_DIV, 2, 15); //just for teesys!!!
+	}
+
+	clks[PERISYS_AHB_HCLK_OUT_DIV] = thead_clk_light_divider("perisys_ahb_hclk_out_div", "gmac_pll_fout1ph0", ap_base + 0x140, 0, 4, 4, MUX_TYPE_DIV, 2, 7);
+	clks[PERISYS_APB_PCLK] = thead_clk_light_divider("perisys_apb_pclk", "perisys_ahb_hclk", ap_base + 0x150, 0, 3, 3, MUX_TYPE_CDE, 3, 7);
+	clks[PERI2SYS_APB_PCLK] = thead_clk_light_divider("peri2sys_apb_pclk", "gmac_pll_fout4", ap_base + 0x150, 4, 3, 8, MUX_TYPE_DIV, 2, 7);
+	clks[CLK_OUT_1_OUT_DIV] = thead_clk_light_divider("clk_out_1_out_div", "osc_24m", ap_base + 0x1b4, 0, 3, 3, MUX_TYPE_DIV, 2, 4);
+	clks[CLK_OUT_2_OUT_DIV] = thead_clk_light_divider("clk_out_2_out_div", "osc_24m", ap_base + 0x1b8, 0, 3, 3, MUX_TYPE_DIV, 2, 4);
+	clks[CLK_OUT_3_OUT_DIV] = thead_clk_light_divider("clk_out_3_out_div", "osc_24m", ap_base + 0x1bc, 0, 3, 3, MUX_TYPE_DIV, 2, 4);
+	clks[CLK_OUT_4_OUT_DIV] = thead_clk_light_divider("clk_out_4_out_div", "osc_24m", ap_base + 0x1c0, 0, 3, 3, MUX_TYPE_DIV, 2, 4);
+	clks[VOSYS_ACLK_M] = thead_clk_light_divider("vosys_aclk_m", "video_pll_foutvco", ap_base + 0x1dc, 0, 4, 4, MUX_TYPE_DIV, 3, 15);
+	clks[NPU_CCLK_OUT_DIV] = thead_clk_light_divider("npu_cclk_out_div", "video_pll_foutvco", ap_base + 0x1c8, 0, 3, 3, MUX_TYPE_DIV, 3, 7);
+	clks[CFG_APB_PCLK_OUT_DIV] = thead_clk_light_divider("cfg_apb_pclk_out_div", "gmac_pll_foutpostdiv", ap_base + 0x1c4, 0, 4, 4, MUX_TYPE_DIV, 4, 15);
+	clks[VISYS_ACLK_M] = thead_clk_light_divider("visys_aclk_m", "video_pll_foutvco", ap_base + 0x1d0, 16, 4, 20, MUX_TYPE_DIV, 3, 15);
+	clks[VISYS_AHB_HCLK] = thead_clk_light_divider("visys_ahb_hclk", "video_pll_foutvco", ap_base + 0x1d0, 0, 4, 4, MUX_TYPE_DIV, 6, 15);
+	clks[VPSYS_APB_PCLK] = thead_clk_light_divider("vpsys_apb_pclk", "gmac_pll_fout1ph0", ap_base + 0x1e0, 0, 3, 4, MUX_TYPE_DIV, 2, 7);
+	clks[VPSYS_AXI_ACLK] = thead_clk_light_divider("vpsys_axi_aclk", "video_pll_foutvco", ap_base + 0x1e0, 8, 4, 12, MUX_TYPE_DIV, 3, 15);
+	clks[VENC_CCLK] = thead_clk_light_divider("venc_cclk", "gmac_pll_foutpostdiv", ap_base + 0x1e4, 0, 3, 4, MUX_TYPE_DIV, 2, 7);
+	clks[DPU0_PLL_DIV_CLK] = thead_clk_light_divider("dpu0_pll_div_clk", "dpu0_pll_foutpostdiv", ap_base + 0x1e8, 0, 8, 8, MUX_TYPE_DIV, 2, 214);
+	clks[DPU1_PLL_DIV_CLK] = thead_clk_light_divider("dpu1_pll_div_clk", "dpu1_pll_foutpostdiv", ap_base + 0x1ec, 0, 8, 8, MUX_TYPE_DIV, 2, 214);
+
+	/* Light Fullmask PLL FOUT */
+	clks[GMAC_PLL_FOUT1PH0] = thead_light_clk_fixed_factor("gmac_pll_fout1ph0", "gmac_pll_bypass", 1, 2);
+	clks[GMAC_PLL_FOUT4] = thead_light_clk_fixed_factor("gmac_pll_fout4", "gmac_pll_bypass", 1, 8);
+	clks[VIDEO_PLL_FOUT1PH0] = thead_light_clk_fixed_factor("video_pll_fout1ph0", "video_pll_bybass", 1, 2);
+	clks[VIDEO_PLL_FOUT4] = thead_light_clk_fixed_factor("video_pll_fout4", "video_pll_bypass", 1, 8);
+	clks[TEE_PLL_FOUT4] = thead_light_clk_fixed_factor("tee_pll_fout4", "tee_pll_bypass", 1, 8);
+	clks[CPU_PLL0_FOUT4] = thead_light_clk_fixed_factor("cpu_pll0_fout4", "cpu_pll0_bypass", 1, 8);
+	clks[CPU_PLL1_FOUT4] = thead_light_clk_fixed_factor("cpu_pll1_fout4", "cpu_pll1_bypass", 1, 8);
+	clks[DPU0_PLL_FOUT4] = thead_light_clk_fixed_factor("dpu0_pll_fout4", "dpu0_pll_bypass", 1, 8);
+	clks[DPU1_PLL_FOUT4] = thead_light_clk_fixed_factor("dpu1_pll_fout4", "dpu1_pll_bypass", 1, 8);
+
+	/* Light Fullmask Fixed Factor */
+	clks[C910_OSC_CLK] = thead_light_clk_fixed_factor("c910_osc_clk", "osc_24m", 1, 1);
+	clks[QSPI_SSI_CLK] = thead_light_clk_fixed_factor("qspi_ssi_clk", "video_pll_foutpostdiv", 1, 1);		/* Note: no mux to select, use default value */
+	clks[QSPI0_SSI_CLK] = thead_light_clk_fixed_factor("qspi0_ssi_clk", "qspi_ssi_clk", 1, 1);
+	clks[QSPI1_SSI_CLK] = thead_light_clk_fixed_factor("qspi1_ssi_clk", "video_pll_fout1ph0", 1, 1);
+	clks[SPI_SSI_CLK] = thead_light_clk_fixed_factor("spi_ssi_clk", "video_pll_fout1ph0", 1, 1);
+	clks[EMMC_SDIO_REF_CLK] = thead_light_clk_fixed_factor("emmc_sdio_ref_clk", "video_pll_foutpostdiv", 1, 1);	/* Note: no mux to select, use default value */
+	clks[PWM_CCLK] = thead_light_clk_fixed_factor("pwm_cclk", "osc_24m", 1, 1);
+	clks[CHIP_DBG_CCLK] = thead_light_clk_fixed_factor("chip_dbg_cclk", "osc_24m", 1, 1);
+	clks[GMAC_CCLK] = thead_light_clk_fixed_factor("gmac_cclk", "gmac_pll_fout1ph0", 1, 1);
+	clks[GPIO0_DBCLK] = thead_light_clk_fixed_factor("gpio0_dbclk", "pad_rtc_clk", 1, 1);
+	clks[GPIO1_DBCLK] = thead_light_clk_fixed_factor("gpio1_dbclk", "pad_rtc_clk", 1, 1);
+	clks[GPIO2_DBCLK] = thead_light_clk_fixed_factor("gpio2_dbclk", "pad_rtc_clk", 1, 1);
+	clks[GPIO3_DBCLK] = thead_light_clk_fixed_factor("gpio3_dbclk", "pad_rtc_clk", 1, 1);
+	clks[CLK_100M] = thead_light_clk_fixed_factor("clk_100m", "gmac_pll_foutpostdiv", 1, 10);
+	clks[I2C_IC_CLK] = thead_light_clk_fixed_factor("i2c_ic_clk", "clk_100m", 1, 2);
+	clks[TIMER_CCLK] = thead_light_clk_fixed_factor("timer_cclk", "osc_24m", 1, 1);
+	clks[AXI4_CPUSYS1_ACLK] = thead_light_clk_fixed_factor("axi4_cpusys1_aclk", "clkgen_c910_bus_clk_no_icg", 1, 1);
+	clks[CPU_BUS_DFTCLK] = thead_light_clk_fixed_factor("cpu_bus_dftclk", "cpu_pll0_foutpostdiv", 1, 2);
+	clks[CPU_PLL0_TEST_CLK] = thead_light_clk_fixed_factor("cpu_pll0_test_clk", "cpu_pll0_fout4", 1, 8);
+	clks[CPU_PLL1_TEST_CLK] = thead_light_clk_fixed_factor("cpu_pll1_test_clk", "cpu_pll1_fout4", 1, 8);
+	clks[DPU0_PLL_TEST_CLK] = thead_light_clk_fixed_factor("dpu0_pll_test_clk", "dpu0_pll_fout4", 1, 8);
+	clks[DPU1_PLL_TEST_CLK] = thead_light_clk_fixed_factor("dpu1_pll_test_clk", "dpu1_pll_fout4", 1, 8);
+	clks[GMAC_PLL_TEST_CLK] = thead_light_clk_fixed_factor("gmac_pll_test_clk", "gmac_pll_fout4", 1, 8);
+	clks[VIDEO_PLL_TEST_CLK] = thead_light_clk_fixed_factor("video_pll_test_clk", "video_pll_fout4", 1, 8);
+	clks[TEE_PLL_TEST_CLK] = thead_light_clk_fixed_factor("tee_pll_test_clk", "tee_pll_fout4", 1, 8);
+	clks[AONSYS_BUS_CLK] = thead_light_clk_fixed_factor("aonsys_bus_clk", "aonsys_hclk", 1, 1);
+
+	/* Light Fullmask Clock Gate */
+	clks[CLKGEN_AHB2_CPUSYS_HCLK] = thead_clk_light_gate("clkgen_ahb2_cpusys_hclk", "ahb2_cpusys_hclk", ap_base + 0x120, 6);
+	clks[CLKGEN_APB3_CPUSYS_HCLK] = thead_clk_light_gate("clkgen_apb3_cpusys_hclk", "ahb2_cpusys_hclk", ap_base + 0x130, 4);
+	clks[CLKGEN_C910_BROM_HCLK] = thead_clk_light_gate("clkgen_c910_brom_hclk", "ahb2_cpusys_hclk", ap_base + 0x100, 4);
+	clks[CLKGEN_SPINLOCK_HCLK] = thead_clk_light_gate("clkgen_spinlock_hclk", "ahb2_cpusys_hclk", ap_base + 0x208, 10);
+	clks[CLKGEN_MBOX0_PCLK] = thead_clk_light_gate("clkgen_mbox0_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 7);
+	clks[CLKGEN_MBOX1_PCLK] = thead_clk_light_gate("clkgen_mbox1_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 6);
+	clks[CLKGEN_MBOX2_PCLK] = thead_clk_light_gate("clkgen_mbox2_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 5);
+	clks[CLKGEN_MBOX3_PCLK] = thead_clk_light_gate("clkgen_mbox3_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 4);
+	clks[CLKGEN_WDT0_PCLK] = thead_clk_light_gate("clkgen_wdt0_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 3);
+	clks[CLKGEN_WDT1_PCLK] = thead_clk_light_gate("clkgen_wdt1_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 2);
+
+	if (teesys)
+		clks[CLKGEN_MISCSYS_TEE_CCLK] = thead_clk_light_gate("clkgen_miscsys_tee_cclk", "teesys_hclk", ap_base + 0x1cc, 25); //just for teesys!!!
+
+	clks[CLKGEN_SRAM_AXI_ACLK_2] = thead_clk_light_gate("clkgen_sram_axi_aclk_2", "axi4_cpusys1_aclk", ap_base + 0x20c, 2);
+	clks[CLKGEN_PERISYS_AHB_HCLK] = thead_clk_light_gate("clkgen_perisys_ahb_hclk", "perisys_ahb_hclk", ap_base + 0x140, 6);
+	clks[CLKGEN_PERISYS_APB1_HCLK] = thead_clk_light_gate("clkgen_perisys_apb1_hclk", "perisys_ahb_hclk", ap_base + 0x150, 9);
+	clks[CLKGEN_PERISYS_APB2_HCLK] = thead_clk_light_gate("clkgen_perisys_apb2_hclk", "perisys_ahb_hclk", ap_base + 0x150, 10);
+	clks[CLKGEN_PERISYS_APB4_HCLK] = thead_clk_light_gate("clkgen_perisys_apb4_hclk", "perisys_ahb_hclk", ap_base + 0x150, 12);
+	clks[CLKGEN_PADCTRL0_APSYS_PCLK] = thead_clk_light_gate("clkgen_padctrl0_apsys_pclk", "perisys_ahb_hclk", ap_base + 0x204, 22);
+	clks[CLKGEN_DSMART_PCLK] = thead_clk_light_gate("clkgen_dsmart_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 23);
+	clks[CLKGEN_PADCTRL1_APSYS_PCLK] = thead_clk_light_gate("clkgen_padctrl1_apsys_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 24);
+	clks[CLKGEN_CLK_OUT_1_CLK] = thead_clk_light_gate("clkgen_clk_out_1_clk", "clk_out_1", ap_base + 0x1b4, 5);
+	clks[CLKGEN_CLK_OUT_2_CLK] = thead_clk_light_gate("clkgen_clk_out_2_clk", "clk_out_2", ap_base + 0x1b8, 5);
+	clks[CLKGEN_CLK_OUT_3_CLK] = thead_clk_light_gate("clkgen_clk_out_3_clk", "clk_out_3", ap_base + 0x1bc, 5);
+	clks[CLKGEN_CLK_OUT_4_CLK] = thead_clk_light_gate("clkgen_clk_out_4_clk", "clk_out_4", ap_base + 0x1c0, 5);
+	clks[CLKGEN_NPUSYS_AXI_ACLK] = thead_clk_light_gate("clkgen_npusys_axi_aclk", "npu_cclk", ap_base + 0x1c8, 5);
+	clks[CLKGEN_SRAM_AXI_ACLK_0] = thead_clk_light_gate("clkgen_sram_axi_aclk_0", "npu_cclk", ap_base + 0x20c, 4);
+	clks[CLKGEN_APB_CPU2CFG_HCLK] = thead_clk_light_gate("clkgen_apb_cpu2cfg_hclk", "cfg_apb_pclk", ap_base + 0x1c4, 5);
+	clks[CLKGEN_SRAM_AXI_ACLK_1] = thead_clk_light_gate("clkgen_sram_axi_aclk_1", "visys_aclk_m", ap_base + 0x20c, 3);
+	clks[CLKGEN_SRAM_AXI_ACLK_3] = thead_clk_light_gate("clkgen_sram_axi_aclk_3", "vpsys_axi_aclk", ap_base + 0x20c, 1);
+	clks[CLKGEN_VPSYS_VENC_CCLK] = thead_clk_light_gate("clkgen_vpsys_venc_cclk", "venc_cclk", ap_base + 0x1e4, 5);
+	clks[CLKGEN_EMMC_SDIO_REF_CLK] = thead_clk_light_gate("clkgen_emmc_sdio_ref_clk", "emmc_sdio_ref_clk", ap_base + 0x204, 30);
+
+	clks[CLKGEN_X2H_CPUSYS_MHCLK] = thead_clk_light_gate_shared("clkgen_x2h_cpusys_mhclk", "ahb2_cpusys_hclk", ap_base + 0x120, 7, &share_cnt_x2h_cpusys_clk_en);
+	clks[CLKGEN_X2H_CPUSYS_ACLK] = thead_clk_light_gate_shared("clkgen_x2h_cpusys_aclk", "cfg_axi_aclk", ap_base + 0x120, 7, &share_cnt_x2h_cpusys_clk_en);
+	clks[CLKGEN_DMAC_CPUSYS_HCLK] = thead_clk_light_gate_shared("clkgen_dmac_cpusys_hclk", "ahb2_cpusys_hclk", ap_base + 0x208, 8, &share_cnt_dmac_cpusys_clk_en);
+	clks[CLKGEN_IOPMP_DMAC_CPUSYS_PCLK] = thead_clk_light_gate_shared("clkgen_iopmp_dmac_cpusys_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 8, &share_cnt_dmac_cpusys_clk_en);
+	clks[CLKGEN_DMAC_CPUSYS_ACLK] = thead_clk_light_gate_shared("clkgen_dmac_cpusys_aclk", "axi4_cpusys2_aclk", ap_base + 0x208, 8, &share_cnt_dmac_cpusys_clk_en);
+	clks[CLKGEN_TIMER0_PCLK] = thead_clk_light_gate_shared("clkgen_timer0_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 1, &share_cnt_timer0_clk_en);
+	clks[CLKGEN_TIMER0_CCLK] = thead_clk_light_gate_shared("clkgen_timer0_cclk", "timer_cclk", ap_base + 0x208, 1, &share_cnt_timer0_clk_en);
+	clks[CLKGEN_TIMER1_PCLK] = thead_clk_light_gate_shared("clkgen_timer1_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 0, &share_cnt_timer1_clk_en);
+	clks[CLKGEN_TIMER1_CCLK] = thead_clk_light_gate_shared("clkgen_timer1_cclk", "timer_cclk", ap_base + 0x208, 0, &share_cnt_timer1_clk_en);
+	clks[CLKGEN_AXI4_CPUSYS2_PCLK] = thead_clk_light_gate_shared("clkgen_axi4_cpusys2_pclk", "apb3_cpusys_pclk", ap_base + 0x134, 5, &share_cnt_axi4_cpusys2_clk_en);
+	clks[CLKGEN_AXI4_CPUSYS2_ACLK] = thead_clk_light_gate_shared("clkgen_axi4_cpusys2_aclk", "axi4_cpusys2_aclk", ap_base + 0x134, 5, &share_cnt_axi4_cpusys2_clk_en);
+	clks[CLKGEN_BMU_C910_PCLK] = thead_clk_light_gate_shared("clkgen_bmu_c910_pclk", "apb3_cpusys_pclk", ap_base + 0x100, 5, &share_cnt_bmu_c910_clk_en);
+	clks[CLKGEN_BMU_C910_ACLK] = thead_clk_light_gate_shared("clkgen_bmu_c910_aclk", "axi4_cpusys1_aclk", ap_base + 0x100, 5, &share_cnt_bmu_c910_clk_en);
+	clks[CLKGEN_IOPMP_AON_PCLK] = thead_clk_light_gate_shared("clkgen_iopmp_aon_pclk", "apb3_cpusys_pclk", ap_base + 0x134, 8, &share_cnt_aon2cpu_a2x_clk_en);
+	clks[CLKGEN_AON2CPU_A2X_ACLK] = thead_clk_light_gate_shared("clkgen_aon2cpu_a2x_aclk", "axi4_cpusys2_aclk", ap_base + 0x134, 8, &share_cnt_aon2cpu_a2x_clk_en);
+	clks[CLKGEN_AON2CPU_A2X_HCLK] = thead_clk_light_gate_shared("clkgen_aon2cpu_a2x_hclk", "aonsys_bus_clk", ap_base + 0x134, 8, &share_cnt_aon2cpu_a2x_clk_en);
+	clks[CLKGEN_IOPMP_CHIP_DBG_PCLK] = thead_clk_light_gate_shared("clkgen_iopmp_chip_dbg_pclk", "apb3_cpusys_pclk", ap_base + 0x208, 9, &share_cnt_chip_dbg_clk_en);
+	clks[CLKGEN_CHIP_DBG_ACLK] = thead_clk_light_gate_shared("clkgen_chip_dbg_aclk", "axi4_cpusys2_aclk", ap_base + 0x208, 9, &share_cnt_chip_dbg_clk_en);
+	clks[CLKGEN_CHIP_DBG_CCLK] = thead_clk_light_gate_shared("clkgen_chip_dbg_cclk", "chip_dbg_cclk", ap_base + 0x208, 9, &share_cnt_chip_dbg_clk_en);
+	clks[CLKGEN_X2X_CPUSYS_ACLK_M] = thead_clk_light_gate_shared("clkgen_x2x_cpusys_aclk_m", "axi4_cpusys2_aclk", ap_base + 0x134, 7, &share_cnt_x2x_cpusys_clk_en);
+	clks[CLKGEN_X2X_CPUSYS_ACLK_S] = thead_clk_light_gate_shared("clkgen_x2x_cpusys_aclk_s", "axi4_cpusys1_aclk", ap_base + 0x134, 7, &share_cnt_x2x_cpusys_clk_en);
+	clks[CLKGEN_CPU2PERI_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2peri_x2h_aclk", "axi4_cpusys1_aclk", ap_base + 0x140, 9, &share_cnt_cpu2peri_x2h_clk_en);
+	clks[CLKGEN_CPU2PERI_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2peri_x2h_mhclk", "perisys_ahb_hclk", ap_base + 0x140, 9, &share_cnt_cpu2peri_x2h_clk_en);
+	clks[CLKGEN_CPU2VI_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2vi_x2h_aclk", "axi4_cpusys1_aclk", ap_base + 0x1d0, 21, &share_cnt_cpu2vi_x2h_clk_en);
+	clks[CLKGEN_CPU2VI_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2vi_x2h_mhclk", "visys_ahb_hclk", ap_base + 0x1d0, 21, &share_cnt_cpu2vi_x2h_clk_en);
+	clks[CLKGEN_CFG2TEE_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cfg2tee_x2h_aclk", "cfg_axi_aclk", ap_base + 0x1cc, 24, &share_cnt_cfg2tee_x2h_clk_en); // just for teesys!!!
+	clks[CLKGEN_CFG2TEE_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cfg2tee_x2h_mhclk", "teesys_hclk", ap_base + 0x1cc, 24, &share_cnt_cfg2tee_x2h_clk_en); // just for teesys!!!
+	clks[CLKGEN_CPU2AON_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2aon_x2h_aclk", "cfg_axi_aclk", ap_base + 0x138, 8, &share_cnt_cpu2aon_x2h_clk_en);
+	clks[CLKGEN_CPU2AON_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2aon_x2h_mhclk", "aonsys_bus_clk", ap_base + 0x138, 8, &share_cnt_cpu2aon_x2h_clk_en);
+	clks[CLKGEN_CPU2VP_X2P_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2vp_x2p_aclk", "cfg_axi_aclk", ap_base + 0x1e0, 13, &share_cnt_cpu2vp_x2p_clk_en);
+	clks[CLKGEN_CPU2VP_X2P_PCLK] = thead_clk_light_gate_shared("clkgen_cpu2vp_x2p_pclk", "vpsys_apb_pclk", ap_base + 0x1e0, 13, &share_cnt_cpu2vp_x2p_clk_en);
+	clks[CLKGEN_TOP_AXI4S_ACLK] = thead_clk_light_gate_shared("clkgen_top_axi4s_aclk", "cfg_axi_aclk", ap_base + 0x1c8, 4, &share_cnt_npu_core_clk_en);
+	clks[CLKGEN_TOP_APB_SX_PCLK] = thead_clk_light_gate_shared("clkgen_top_apb_sx_pclk", "cfg_apb_pclk", ap_base + 0x1c8, 4, &share_cnt_npu_core_clk_en);
+	clks[CLKGEN_MISC2VP_X2X_ACLK_M] = thead_clk_light_gate_shared("clkgen_misc2vp_x2x_aclk_m", "perisys_ahb_hclk", ap_base + 0x1e0, 15, &share_cnt_vpsys_axi_aclk_en);
+	clks[CLKGEN_VPSYS_ACLK] = thead_clk_light_gate_shared("clkgen_vpsys_aclk", "vpsys_axi_aclk", ap_base + 0x1e0, 15, &share_cnt_vpsys_axi_aclk_en);
+	clks[CLKGEN_GMAC1_HCLK] = thead_clk_light_gate_shared("clkgen_gmac1_hclk", "perisys_ahb_hclk", ap_base + 0x204, 26, &share_cnt_gmac1_clk_en);
+	clks[CLKGEN_GMAC1_PCLK] = thead_clk_light_gate_shared("clkgen_gmac1_pclk", "perisys_ahb_hclk", ap_base + 0x204, 26, &share_cnt_gmac1_clk_en);
+	clks[CLKGEN_GMAC1_CCLK] = thead_clk_light_gate_shared("clkgen_gmac1_cclk", "gmac_cclk", ap_base + 0x204, 26, &share_cnt_gmac1_clk_en);
+	clks[CLKGEN_GMAC0_HCLK] = thead_clk_light_gate_shared("clkgen_gmac0_hclk", "perisys_ahb_hclk", ap_base + 0x204, 19, &share_cnt_gmac0_clk_en);
+	clks[CLKGEN_GMAC0_PCLK] = thead_clk_light_gate_shared("clkgen_gmac0_pclk", "perisys_ahb_hclk", ap_base + 0x204, 19, &share_cnt_gmac0_clk_en);
+	clks[CLKGEN_GMAC0_CCLK] = thead_clk_light_gate_shared("clkgen_gmac0_cclk", "gmac_cclk", ap_base + 0x204, 19, &share_cnt_gmac0_clk_en);
+	clks[CLKGEN_PERI2PERI1_APB_HCLK] = thead_clk_light_gate_shared("clkgen_peri2peri1_apb_hclk", "perisys_ahb_hclk", ap_base + 0x150, 11, &share_cnt_perisys_apb3_hclk_en);
+	clks[CLKGEN_PERI2PERI1_APB_PCLK] = thead_clk_light_gate_shared("clkgen_peri2peri1_apb_pclk", "peri2sys_apb_pclk", ap_base + 0x150, 11, &share_cnt_perisys_apb3_hclk_en);
+	clks[CLKGEN_QSPI0_PCLK] = thead_clk_light_gate_shared("clkgen_qspi0_pclk", "perisys_ahb_hclk", ap_base + 0x204, 17, &share_cnt_qspi0_clk_en);
+	clks[CLKGEN_QSPI0_SSI_CLK] = thead_clk_light_gate_shared("clkgen_qspi0_ssi_clk", "qspi0_ssi_clk", ap_base + 0x204, 17, &share_cnt_qspi0_clk_en);
+	clks[CLKGEN_GMAC_AXI_ACLK] = thead_clk_light_gate_shared("clkgen_gmac_axi_aclk", "perisys_ahb_hclk", ap_base + 0x204, 21, &share_cnt_gmac_axi_clk_en);
+	clks[CLKGEN_GMAC_AXI_PCLK] = thead_clk_light_gate_shared("clkgen_gmac_axi_pclk", "perisys_ahb_hclk", ap_base + 0x204, 21, &share_cnt_gmac_axi_clk_en);
+	clks[CLKGEN_GPIO0_PCLK] = thead_clk_light_gate_shared("clkgen_gpio0_pclk", "perisys_ahb_hclk", ap_base + 0x204, 8, &share_cnt_gpio0_clk_en);
+	clks[CLKGEN_GPIO0_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio0_dbclk", "gpio0_dbclk", ap_base + 0x204, 8, &share_cnt_gpio0_clk_en);
+	clks[CLKGEN_GPIO1_PCLK] = thead_clk_light_gate_shared("clkgen_gpio1_pclk", "perisys_ahb_hclk", ap_base + 0x204, 7, &share_cnt_gpio0_clk_en);
+	clks[CLKGEN_GPIO1_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio1_dbclk", "gpio1_dbclk", ap_base + 0x204, 7, &share_cnt_gpio1_clk_en);
+	clks[CLKGEN_PWM_PCLK] = thead_clk_light_gate_shared("clkgen_pwm_pclk", "perisys_apb_pclk", ap_base + 0x204, 18, &share_cnt_pwm_clk_en);
+	clks[CLKGEN_PWM_CCLK] = thead_clk_light_gate_shared("clkgen_pwm_cclk", "pwm_cclk", ap_base + 0x204, 18, &share_cnt_pwm_clk_en);
+	clks[CLKGEN_SPI_PCLK] = thead_clk_light_gate_shared("clkgen_spi_pclk", "perisys_apb_pclk", ap_base + 0x204, 15, &share_cnt_spi_clk_en);
+	clks[CLKGEN_SPI_SSI_CLK] = thead_clk_light_gate_shared("clkgen_spi_ssi_clk", "spi_ssi_clk", ap_base + 0x204, 15, &share_cnt_spi_clk_en);
+	clks[CLKGEN_UART0_PCLK] = thead_clk_light_gate_shared("clkgen_uart0_pclk", "perisys_apb_pclk", ap_base + 0x204, 14, &share_cnt_uart0_clk_en);
+	clks[CLKGEN_UART0_SCLK] = thead_clk_light_gate_shared("clkgen_uart0_sclk", "uart_sclk", ap_base + 0x204, 14, &share_cnt_uart0_clk_en);
+	clks[CLKGEN_UART2_PCLK] = thead_clk_light_gate_shared("clkgen_uart2_pclk", "perisys_apb_pclk", ap_base + 0x204, 12, &share_cnt_uart2_clk_en);
+	clks[CLKGEN_UART2_SCLK] = thead_clk_light_gate_shared("clkgen_uart2_sclk", "uart_sclk", ap_base + 0x204, 12, &share_cnt_uart2_clk_en);
+	clks[CLKGEN_I2C2_PCLK] = thead_clk_light_gate_shared("clkgen_i2c2_pclk", "perisys_apb_pclk", ap_base + 0x204, 3, &share_cnt_i2c2_clk_en);
+	clks[CLKGEN_I2C2_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c2_ic_clk", "i2c_ic_clk", ap_base + 0x204, 3, &share_cnt_i2c2_clk_en);
+	clks[CLKGEN_I2C3_PCLK] = thead_clk_light_gate_shared("clkgen_i2c3_pclk", "perisys_apb_pclk", ap_base + 0x204, 2, &share_cnt_i2c2_clk_en);
+	clks[CLKGEN_I2C3_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c3_ic_clk", "i2c_ic_clk", ap_base + 0x204, 2, &share_cnt_i2c2_clk_en);
+	clks[CLKGEN_I2S_PCLK] = thead_clk_light_gate_shared("clkgen_i2s_pclk", "perisys_apb_pclk", ap_base + 0x1f0, 1, &share_cnt_peri_i2s_clk_en);
+	clks[CLKGEN_I2S_SRC_CLK] = thead_clk_light_gate_shared("clkgen_i2s_src_clk", "peri_i2s_src_clk", ap_base + 0x1f0, 1, &share_cnt_peri_i2s_clk_en);
+	clks[CLKGEN_QSPI1_PCLK] = thead_clk_light_gate_shared("clkgen_qspi1_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 16, &share_cnt_qspi1_clk_en);
+	clks[CLKGEN_QSPI1_SSI_CLK] = thead_clk_light_gate_shared("clkgen_qspi1_ssi_clk", "qspi1_ssi_clk", ap_base + 0x204, 16, &share_cnt_qspi1_clk_en);
+	clks[CLKGEN_UART1_PCLK] = thead_clk_light_gate_shared("clkgen_uart1_pclk", "per2sys_apb_pclk", ap_base + 0x204, 13, &share_cnt_uart1_clk_en);
+	clks[CLKGEN_UART1_SCLK] = thead_clk_light_gate_shared("clkgen_uart1_sclk", "uart_sclk", ap_base + 0x204, 13, &share_cnt_uart1_clk_en);
+	clks[CLKGEN_UART3_PCLK] = thead_clk_light_gate_shared("clkgen_uart3_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 11, &share_cnt_uart3_clk_en);
+	clks[CLKGEN_UART3_SCLK] = thead_clk_light_gate_shared("clkgen_uart3_sclk", "uart_sclk", ap_base + 0x204, 11, &share_cnt_uart3_clk_en);
+	clks[CLKGEN_UART4_PCLK] = thead_clk_light_gate_shared("clkgen_uart4_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 10, &share_cnt_uart4_clk_en);
+	clks[CLKGEN_UART4_SCLK] = thead_clk_light_gate_shared("clkgen_uart4_sclk", "uart_sclk", ap_base + 0x204, 10, &share_cnt_uart4_clk_en);
+	clks[CLKGEN_UART5_PCLK] = thead_clk_light_gate_shared("clkgen_uart5_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 9, &share_cnt_uart5_clk_en);
+	clks[CLKGEN_UART5_SCLK] = thead_clk_light_gate_shared("clkgen_uart5_sclk", "uart_sclk", ap_base + 0x204, 9, &share_cnt_uart5_clk_en);
+	clks[CLKGEN_I2C0_PCLK] = thead_clk_light_gate_shared("clkgen_i2c0_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 5, &share_cnt_i2c0_clk_en);
+	clks[CLKGEN_I2C0_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c0_ic_clk", "i2c_ic_clk", ap_base + 0x204, 5, &share_cnt_i2c0_clk_en);
+	clks[CLKGEN_I2C1_PCLK] = thead_clk_light_gate_shared("clkgen_i2c1_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 4, &share_cnt_i2c1_clk_en);
+	clks[CLKGEN_I2C1_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c1_ic_clk", "i2c_ic_clk", ap_base + 0x204, 4, &share_cnt_i2c1_clk_en);
+	clks[CLKGEN_I2C4_PCLK] = thead_clk_light_gate_shared("clkgen_i2c4_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 1, &share_cnt_i2c4_clk_en);
+	clks[CLKGEN_I2C4_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c4_ic_clk", "i2c_ic_clk", ap_base + 0x204, 1, &share_cnt_i2c4_clk_en);
+	clks[CLKGEN_I2C5_PCLK] = thead_clk_light_gate_shared("clkgen_i2c5_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 0, &share_cnt_i2c5_clk_en);
+	clks[CLKGEN_I2C5_IC_CLK] = thead_clk_light_gate_shared("clkgen_i2c5_ic_clk", "i2c_ic_clk", ap_base + 0x204, 0, &share_cnt_i2c5_clk_en);
+	clks[CLKGEN_GPIO2_PCLK] = thead_clk_light_gate_shared("clkgen_gpio2_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 6, &share_cnt_gpio2_clk_en);
+	clks[CLKGEN_GPIO2_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio2_dbclk", "gpio2_dbclk", ap_base + 0x204, 6, &share_cnt_gpio2_clk_en);
+	clks[CLKGEN_GPIO3_PCLK] = thead_clk_light_gate_shared("clkgen_gpio3_pclk", "peri2sys_apb_pclk", ap_base + 0x204, 6, &share_cnt_gpio2_clk_en); //!!! gpio3 pclk is controlled by gpio2_clk_en
+	clks[CLKGEN_GPIO3_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio3_dbclk", "gpio3_dbclk", ap_base + 0x204, 20, &share_cnt_gpio3_clk_en);
+	clks[CLKGEN_VOSYS_AXI_ACLK] = thead_clk_light_gate_shared("clkgen_vosys_axi_aclk", "vosys_aclk_m", ap_base + 0x1dc, 5, &share_cnt_vosys_axi_aclk_en);
+	clks[CLKGEN_VOSYS_X2X_ACLK_S] = thead_clk_light_gate_shared("clkgen_vosys_x2x_aclk_s", "npu_cclk", ap_base + 0x1dc, 5, &share_cnt_vosys_axi_aclk_en);
+
+	clk_data.clks = clks;
+	clk_data.clk_num = ARRAY_SIZE(clks);
+
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_data);
+	if (ret < 0) {
+		dev_err(dev, "failed to register clks for light\n");
+		goto unregister_clks;
+	}
+
+#ifndef FPGA_EMU
+	/* HW defalut */
+	clk_set_parent(clks[C910_CCLK], clks[CPU_PLL1_FOUTPOSTDIV]);
+#else
+	clk_set_parent(clks[C910_CCLK_I0], clks[OSC_24M]);
+	clk_set_parent(clks[C910_CCLK], clks[C910_CCLK_I0]);
+#endif
+	dev_info(dev, "succeed to register light fullmask clock driver\n");
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(clks, ARRAY_SIZE(clks));
+	return ret;
+}
+
+
+const bool tee_sys_flag;
+
+static const struct of_device_id light_clk_of_match[] = {
+	{ .compatible = "thead,light-fm-ree-clk" },
+	{ .compatible = "thead,light-fm-tee-clk", .data = &tee_sys_flag,},
+	{ /* Sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, light_clk_of_match);
+
+static struct platform_driver light_clk_driver = {
+	.probe = light_clocks_probe,
+	.driver = {
+		.name = "light-fm-clk",
+		.of_match_table = of_match_ptr(light_clk_of_match),
+	},
+};
+
+module_platform_driver(light_clk_driver);
+MODULE_AUTHOR("wei.liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Fullmask clock driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/thead/clk-light-mpw.c b/drivers/clk/thead/clk-light-mpw.c
new file mode 100644
index 000000000000..f7356ddf4684
--- /dev/null
+++ b/drivers/clk/thead/clk-light-mpw.c
@@ -0,0 +1,492 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-mpw-clock.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+
+#include "clk.h"
+
+static struct clk *clks[LIGHT_CLK_END];
+static struct clk_onecell_data clk_data;
+
+static u32 share_cnt_cpu2cfg_x2x_clk_en;
+static u32 share_cnt_cpu2peri_x2h_clk_en;
+static u32 share_cnt_aon2cpu_a2x_clk_en;
+static u32 share_cnt_dmac_clk_en;
+static u32 share_cnt_x2h_cpusys_clk_en;
+static u32 share_cnt_cpu2tee_x2h_clk_en;
+static u32 share_cnt_cpu2aon_x2h_clk_en;
+static u32 share_cnt_cpu2cfg_x2h_clk_en;
+static u32 share_cnt_timer0_clk_en;
+static u32 share_cnt_timer1_clk_en;
+static u32 share_cnt_peri2ddr_x2x_clk_en;
+static u32 share_cnt_usb3_drd_clk_en;
+static u32 share_cnt_gmac_clk_en;
+static u32 share_cnt_emmc0_clk_en;
+static u32 share_cnt_emmc1_clk_en;
+static u32 share_cnt_pwm_clk_en;
+static u32 share_cnt_qspi0_clk_en;
+static u32 share_cnt_qspi1_clk_en;
+static u32 share_cnt_spi_clk_en;
+static u32 share_cnt_gpio0_clk_en;
+static u32 share_cnt_gpio1_clk_en;
+static u32 share_cnt_gpio2_clk_en;
+static u32 share_cnt_dmac_1_clk_en;
+static u32 share_cnt_dmac_2_clk_en;
+static u32 share_cnt_dmac_3_clk_en;
+
+#ifdef THEAD_LIGHT_AON_CLK
+static const char * const audio_pll_bypass_sels[] = {"audio_pll_foutpostdiv", "osc_24m", };
+static const char * const sys_pll_bypass_sels[] = {"sys_pll_foutpostdiv", "osc_24m", };
+#endif
+#ifdef THEAD_LIGHT_DDR_CLK
+static const char * const ddr_pll_bypass_sels[] = {"ddr_pll_foutpostdiv", "osc_24m", };
+#endif
+static const char * const cpu_pll0_bypass_sels[] = {"cpu_pll0_foutpostdiv", "osc_24m", };
+static const char * const cpu_pll1_bypass_sels[] = {"cpu_pll1_foutpostdiv", "osc_24m", };
+static const char * const gmac_pll_bypass_sels[] = {"gmac_pll_foutpostdiv", "osc_24m", };
+static const char * const video_pll_bypass_sels[] = {"video_pll_foutpostdiv", "osc_24m", };
+
+#ifdef THEAD_LIGHT_AON_CLK
+static const char * const aonsys_clk_switch_0_sels[] = {"audio_pll_fout3", "osc_24m", };
+static const char * const aonsys_clk_switch_1_sels[] = {"aonsys_clk_switch_0", "rc_24m", };
+#endif
+
+static const char * const c910_cclk_i0_sels[] = {"cpu_pll0_bypass", "osc_24m", };
+static const char * const c910_cclk_sels[] = {"c910_cclk_i0", "cpu_pll1_foutpostdiv", };
+static const char * const cpusys_ahb_hclk_sel[] = {"cpusys_ahb_hclk_div", "osc_24m"};
+static const char * const cpusys_cfg_axi_aclk_sel[] = {"cpusys_cfg_axi_aclk_div", "osc_24m"};
+static const char * const perisys_ahb_hclk_sel[] = {"perisys_ahb_hclk_div", "osc_24m"};
+static const char * const clk_out_1_sel[] = {"clk_out_1_div", "osc_24m"};
+static const char * const clk_out_2_sel[] = {"clk_out_2_div", "osc_24m"};
+static const char * const clk_out_3_sel[] = {"clk_out_3_div", "osc_24m"};
+static const char * const clk_out_4_sel[] = {"clk_out_4_div", "osc_24m"};
+
+static const struct light_pll_rate_table light_audiopll_tbl[] = {
+	LIGHT_PLL_RATE(2654208000U, 147456000U, 1, 110, 9932112,  6, 3),
+	LIGHT_PLL_RATE(884736000U,  294912000U, 1, 36,  14495600, 3, 1),
+};
+
+static const struct light_pll_rate_table light_syspll_tbl[] = {
+	LIGHT_PLL_RATE(2438553600U, 812851200U, 1, 101, 10173704, 3, 1),
+	LIGHT_PLL_RATE(884736000U,  294912000U, 1, 36,  14495600, 3, 1),
+};
+
+static const struct light_pll_rate_table light_cpupll_tbl[] = {
+	LIGHT_PLL_RATE(1800000000U, 1800000000U, 1, 75,  0, 1, 1),
+	LIGHT_PLL_RATE(3000000000U, 1500000000U, 1, 125, 0, 2, 1),
+	LIGHT_PLL_RATE(3000000000U, 1000000000U, 1, 125, 0, 3, 1),
+	LIGHT_PLL_RATE(3000000000U, 125000000U, 1, 125,  0, 6, 4),
+};
+
+#ifdef THEAD_LIGHT_DDR_CLK
+static const struct light_pll_rate_table light_ddrpll_tbl[] = {
+	LIGHT_PLL_RATE(3192000000U, 798000000U, 1, 133, 0, 4, 1),
+	LIGHT_PLL_RATE(3192000000U, 532000000U, 1, 133, 0, 6, 1),
+	LIGHT_PLL_RATE(2112000000U, 1056000000U, 1, 88, 0, 2, 1),
+};
+#endif
+
+#ifdef THEAD_LIGHT_AON_CLK
+static struct light_pll_clk light_audio_pllvco = {
+	.out_type = LIGHT_PLL_VCO,
+	.clk_type = LIGHT_AUDIO_PLL,
+	.rate_table = light_audiopll_tbl,
+	.rate_count = ARRAY_SIZE(light_audiopll_tbl),
+};
+
+static struct light_pll_clk light_audio_plldiv = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_AUDIO_PLL,
+	.rate_table = light_audiopll_tbl,
+	.rate_count = ARRAY_SIZE(light_audiopll_tbl),
+};
+
+static struct light_pll_clk light_sys_pllvco = {
+	.out_type = LIGHT_PLL_VCO,
+	.clk_type = LIGHT_SYS_PLL,
+	.rate_table = light_syspll_tbl,
+	.rate_count = ARRAY_SIZE(light_syspll_tbl),
+};
+
+static struct light_pll_clk light_sys_plldiv = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_SYS_PLL,
+	.rate_table = light_syspll_tbl,
+	.rate_count = ARRAY_SIZE(light_syspll_tbl),
+};
+#endif
+
+static struct light_pll_clk light_cpu_pll0vco = {
+	.out_type = LIGHT_PLL_VCO,
+	.clk_type = LIGHT_CPU_PLL0,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+static struct light_pll_clk light_cpu_pll0div = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_CPU_PLL0,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+static struct light_pll_clk light_cpu_pll1vco = {
+	.out_type = LIGHT_PLL_VCO,
+	.clk_type = LIGHT_CPU_PLL1,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+static struct light_pll_clk light_cpu_pll1div = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_CPU_PLL1,
+	.rate_table = light_cpupll_tbl,
+	.rate_count = ARRAY_SIZE(light_cpupll_tbl),
+};
+
+#ifdef THEAD_LIGHT_DDR_CLK
+static struct light_pll_clk light_ddr_pllvco = {
+	.out_type = LIGHT_PLL_VCO,
+	.clk_type = LIGHT_DDR_PLL,
+	.rate_table = light_ddrpll_tbl,
+	.rate_count = ARRAY_SIZE(light_ddrpll_tbl),
+};
+
+static struct light_pll_clk light_ddr_plldiv = {
+	.out_type = LIGHT_PLL_DIV,
+	.clk_type = LIGHT_DDR_PLL,
+	.rate_table = light_ddrpll_tbl,
+	.rate_count = ARRAY_SIZE(light_ddrpll_tbl),
+};
+#endif
+
+static int light_clocks_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	void __iomem *ap_base;
+#ifdef THEAD_LIGHT_DDR_CLK
+	void __iomem *ddr_base;
+#endif
+#ifdef THEAD_LIGHT_AON_CLK
+	void __iomem *aon_base;
+#endif
+	int ret;
+
+#ifdef THEAD_LIGHT_AON_CLK
+	np = of_find_compatible_node(NULL, NULL, "thead,light-aon-clk");
+	aon_base = of_iomap(np, 0);
+	if (WARN_ON(!aon_base)) {
+		ret = -ENOMEM;
+		goto unregister_clks;
+	}
+	of_node_put(np);
+#endif
+
+	/* Clock source */
+	clks[LIGHT_CLK_DUMMY] = thead_clk_fixed("dummy", 0);
+	clks[LIGHT_CLK_32K] = of_clk_get_by_name(np, "osc_32k");
+	clks[LIGHT_CLK_24M] = of_clk_get_by_name(np, "osc_24m");
+	clks[LIGHT_RC_24M] = of_clk_get_by_name(np, "rc_24m");
+
+	/* AP Fixed PLL */
+	clks[LIGHT_VIDEO_PLL_FOUTVCO] = thead_clk_fixed("video_pll_foutvco", 2376000000);
+	clks[LIGHT_VIDEO_PLL_FOUTPOSTDIV] = thead_clk_fixed("video_pll_foutpostdiv", 796000000);
+	clks[LIGHT_GMAC_PLL_FOUTVCO] = thead_clk_fixed("gmac_pll_foutvco", 2000000000);
+	clks[LIGHT_GMAC_PLL_FOUTPOSTDIV] = thead_clk_fixed("gmac_pll_foutpostdiv", 1000000000);
+
+#ifdef THEAD_LIGHT_AON_CLK
+	/* Aon PLL clocks */
+	clks[LIGHT_AUDIO_PLL_FOUTVCO] = thead_light_pll("audio_pll_foutvco", "osc_24m", aon_base, &light_audio_pllvco);
+	clks[LIGHT_AUDIO_PLL_FOUTPOSTDIV] = thead_light_pll("audio_pll_foutpostdiv", "osc_24m", aon_base, &light_audio_plldiv);
+	clks[LIGHT_SYS_PLL_FOUTVCO] = thead_light_pll("sys_pll_foutvco", "osc_24m", aon_base, &light_sys_pllvco);
+	clks[LIGHT_SYS_PLL_FOUTPOSTDIV] = thead_light_pll("sys_pll_foutpostdiv", "osc_24m", aon_base, &light_sys_plldiv);
+#endif
+
+#ifdef THEAD_LIGHT_DDR_CLK
+	np = of_find_compatible_node(NULL, NULL, "thead,light-ddr-clk");
+	ddr_base = of_iomap(np, 0);
+	if (WARN_ON(!ddr_base)) {
+		ret = -ENOMEM;
+		goto unregister_clks;
+	}
+	of_node_put(np);
+
+	/* DDR PLL */
+	clks[LIGHT_DDR_PLL_FOUTVCO] = thead_light_pll("ddr_pll_foutvco", "osc_24m", ddr_base, &light_ddr_pllvco);
+	clks[LIGHT_DDR_PLL_FOUTPOSTDIV] = thead_light_pll("ddr_pll_foutpostdiv", "osc_24m", ddr_base, &light_ddr_plldiv);
+#endif
+
+	np = dev->of_node;
+	ap_base = devm_platform_ioremap_resource(pdev, 0);
+	if (WARN_ON(IS_ERR(ap_base))) {
+		ret = PTR_ERR(ap_base);
+		goto unregister_clks;
+	}
+
+	/* AP PLL clocks */
+	clks[LIGHT_CPU_PLL0_FOUTVCO] = thead_light_pll("cpu_pll0_foutvco", "osc_24m", ap_base, &light_cpu_pll0vco);
+	clks[LIGHT_CPU_PLL0_FOUTPOSTDIV] = thead_light_pll("cpu_pll0_foutpostdiv", "osc_24m", ap_base, &light_cpu_pll0div);
+	clks[LIGHT_CPU_PLL1_FOUTVCO] = thead_light_pll("cpu_pll1_foutvco", "osc_24m", ap_base, &light_cpu_pll1vco);
+	clks[LIGHT_CPU_PLL1_FOUTPOSTDIV] = thead_light_pll("cpu_pll1_foutpostdiv", "osc_24m", ap_base, &light_cpu_pll1div);
+
+	/* PLL bypass */
+#ifdef THEAD_LIGHT_AON_CLK
+	clks[LIGHT_AUDIO_PLL_BYPASS] = thead_light_clk_mux_flags("audio_pll_bypass", aon_base + 0x4, 31, 1, audio_pll_bypass_sels, ARRAY_SIZE(audio_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_SYS_PLL_BYPASS] = thead_light_clk_mux_flags("sys_pll_bypass", aon_base + 0x14, 31, 1, sys_pll_bypass_sels, ARRAY_SIZE(sys_pll_bypass_sels), CLK_SET_RATE_PARENT);
+#endif
+#ifdef THEAD_LIGHT_DDR_CLK
+	clks[LIGHT_DDR_PLL_BYPASS] = thead_light_clk_mux_flags("ddr_pll_bypass", ddr_base + 0xc, 31, 1, ddr_pll_bypass_sels, ARRAY_SIZE(ddr_pll_bypass_sels), CLK_SET_RATE_PARENT);
+#endif
+	clks[LIGHT_CPU_PLL0_BYPASS] = thead_light_clk_mux_flags("cpu_pll0_bypass", ap_base + 0x4, 31, 1, cpu_pll0_bypass_sels, ARRAY_SIZE(cpu_pll0_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CPU_PLL1_BYPASS] = thead_light_clk_mux_flags("cpu_pll1_bypass", ap_base + 0x14, 31, 1, cpu_pll1_bypass_sels, ARRAY_SIZE(cpu_pll1_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_GMAC_PLL_BYPASS] = thead_light_clk_mux_flags("gmac_pll_bypass", ap_base + 0x24, 31, 1, gmac_pll_bypass_sels, ARRAY_SIZE(gmac_pll_bypass_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_VIDEO_PLL_BYPASS] = thead_light_clk_mux_flags("video_pll_bypass", ap_base + 0x34, 31, 1, video_pll_bypass_sels, ARRAY_SIZE(video_pll_bypass_sels), CLK_SET_RATE_PARENT);
+
+	/* PLL FOUT */
+#ifdef THEAD_LIGHT_AON_CLK
+	clks[LIGHT_AUDIO_PLL_FOUT3] = thead_light_clk_fixed_factor("audio_pll_fout3", "audio_pll_bypass", 1, 6);
+	clks[LIGHT_SYS_PLL_FOUT4] = thead_light_clk_fixed_factor("sys_pll_fout4", "sys_pll_bypass", 1, 8);
+#endif
+#ifdef THEAD_LIGHT_DDR_CLK
+	clks[LIGHT_DDR_PLL_FOUT4] = thead_light_clk_fixed_factor("ddr_pll_fout4", "ddr_pll_bypass", 1, 8);
+#endif
+	clks[LIGHT_CPU_PLL0_FOUT4] = thead_light_clk_fixed_factor("cpu_pll0_fout4", "cpu_pll0_bypass", 1, 8);
+	clks[LIGHT_CPU_PLL1_FOUT4] = thead_light_clk_fixed_factor("cpu_pll1_fout4", "cpu_pll1_bypass", 1, 8);
+	clks[LIGHT_GMAC_PLL_FOUT1PH0] = thead_light_clk_fixed_factor("gmac_pll_fout1ph0", "gmac_pll_bypass", 1, 2);
+	clks[LIGHT_GMAC_CORECLK] = thead_light_clk_fixed_factor("gmac_coreclk", "gmac_pll_fout1ph0", 1, 1);
+	clks[LIGHT_GMAC_PLL_FOUT4] = thead_light_clk_fixed_factor("gmac_pll_fout4", "gmac_pll_bypass", 1, 8);
+	clks[LIGHT_VIDEO_PLL_FOUT4] = thead_light_clk_fixed_factor("video_pll_fout4", "video_pll_bypass", 1, 8);
+	clks[LIGHT_GMAC_PLL_FOUTVCO_DIV5] = thead_light_clk_fixed_factor("gmac_pll_foutvco_div5", "gmac_pll_foutvco", 1, 5);
+	clks[LIGHT_OSC_CLK_DIV24] = thead_light_clk_fixed_factor("osc_clk_div24", "osc_24m", 1, 24);
+	clks[LIGHT_CHIP_DBG_CCLK] = thead_light_clk_fixed_factor("chip_dbg_cclk", "osc_24m", 1, 1);
+	clks[LIGHT_AXI_ACLK] = thead_light_clk_fixed_factor("cpusys_axi_aclk", "cpu_pll0_bypass", 1, 2);
+	clks[LIGHT_X2H_HCLK] = thead_light_clk_fixed_factor("aonsys_x2h_hclk", "osc_24m", 1, 1);
+	clks[LIGHT_EMMC_CLK_DIV] = thead_light_clk_fixed_factor("emmc_clk_div", "video_pll_bypass", 1, 4);
+	clks[LIGHT_EMMC0_OSC_CLK] = thead_light_clk_fixed_factor("emmc0_osc_clk", "osc_24m", 1, 1);
+	clks[LIGHT_EMMC1_OSC_CLK] = thead_light_clk_fixed_factor("emmc1_osc_clk", "osc_24m", 1, 1);
+	clks[LIGHT_PWM_CCLK] = thead_light_clk_fixed_factor("pwm_cclk", "osc_24m", 1, 1);
+	clks[LIGHT_USB3_PHY_REF_CLK] = thead_light_clk_fixed_factor("usb3_phy_ref_clk", "osc_24m", 1, 1);
+	clks[LIGHT_SPI_CLK] = thead_light_clk_fixed_factor("spi_clk", "gmac_pll_foutvco_div5", 1, 1);
+	clks[LIGHT_GPIO_DBCLK] = thead_light_clk_fixed_factor("gpio_dbclk", "osc_32k", 1, 1);
+
+#ifdef THEAD_LIGHT_AON_CLK
+	/* Aon sys mux tree */
+	clks[LIGHT_AONSYS_CLK_SWITCH_0] = thead_light_clk_mux_flags("aonsys_clk_switch_0", aon_base + 0x100, 4, 1, aonsys_clk_switch_0_sels, ARRAY_SIZE(aonsys_clk_switch_0_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_AONSYS_CLK_SWITCH_1] = thead_light_clk_mux_flags("aonsys_clk_switch_1", aon_base + 0x100, 5, 1, aonsys_clk_switch_1_sels, ARRAY_SIZE(aonsys_clk_switch_1_sels), CLK_SET_RATE_PARENT);
+
+	/* Aon sys div tree */
+	clks[LIGHT_AONSYS_CLK] = thead_clk_light_divider("aonsys_clk", "aonsys_clk_switch_1", aon_base + 0x100, 0, 3, 3, MUX_TYPE_CDE, 0, 7);
+	clks[LIGHT_SHARE_SRAM_CLK] = thead_clk_light_divider("share_sram_clk", "sys_pll_foutvco", aon_base + 0x104, 0, 4, 4, MUX_TYPE_DIV, 3, 12);
+
+	/* Aon sys gate tree */
+	clks[LIGHT_CLKGEN_RTC_PCLK] = thead_clk_light_gate("rtc_pclk_en", "aonsys_clk", aon_base + 0x120, 0);
+	clks[LIGHT_CLKGEN_AOGPIO_PCLK] = thead_clk_light_gate("aogpio_pclk_en", "aonsys_clk", aon_base + 0x120, 1);
+	clks[LIGHT_CLKGEN_AOI2C_PCLK] = thead_clk_light_gate("aoi2c_pclk_en", "aonsys_clk", aon_base + 0x120, 2);
+	clks[LIGHT_CLKGEN_PVTC_PCLK] = thead_clk_light_gate("pvtc_pclk_en", "aonsys_clk", aon_base + 0x120, 3);
+	clks[LIGHT_CLKGEN_SRAM_AXI_ACLK] = thead_clk_light_gate("share_sram_clk_en", "aonsys_clk", aon_base + 0x120, 4);
+	clks[LIGHT_CLKGEN_AOPAD_PCLK] = thead_clk_light_gate("aopad_pclk_en", "aonsys_clk", aon_base + 0x120, 5);
+	clks[LIGHT_CLKGEN_AOAPB_HCLK] = thead_clk_light_gate("aoapb_hclk_en", "aonsys_clk", aon_base + 0x120, 6);
+	clks[LIGHT_CLKGEN_AOSRAM_HCLK] = thead_clk_light_gate("aosram_hclk_en", "aonsys_clk", aon_base + 0x120, 7);
+	clks[LIGHT_CLKGEN_AOAHB_HCLK] = thead_clk_light_gate("aoahb_hclk_en", "aonsys_clk", aon_base + 0x120, 8);
+	clks[LIGHT_CLKGEN_AOGPIO_DBCLK] = thead_clk_light_gate("aogpio_dbclk_en", "aonsys_clk", aon_base + 0x120, 9);
+	clks[LIGHT_CLKGEN_AOTIMER_PCLK] = thead_clk_light_gate("aotimer_pclk_en", "aonsys_clk", aon_base + 0x120, 10);
+	clks[LIGHT_CLKGEN_AOTIMER_CCLK] = thead_clk_light_gate("aotimer_cclk_en", "aonsys_clk", aon_base + 0x120, 11);
+	clks[LIGHT_CLKGEN_CPU2RAM_X2X_ACLK_S] = thead_clk_light_gate("apsys_clk_en", "aonsys_clk", aon_base + 0x130, 0);
+#endif
+
+	/* AP sys mux tree */
+	clks[LIGHT_C910_CCLK_I0] = thead_light_clk_mux_flags("c910_cclk_i0", ap_base + 0x100, 1, 1, c910_cclk_i0_sels, ARRAY_SIZE(c910_cclk_i0_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_C910_CCLK] = thead_light_clk_mux_flags("c910_cclk", ap_base + 0x100, 0, 1, c910_cclk_sels, ARRAY_SIZE(c910_cclk_sels), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CPUSYS_AHB_HCLK] = thead_light_clk_mux_flags("cpusys_ahb_hclk", ap_base + 0x120, 5, 1, cpusys_ahb_hclk_sel, ARRAY_SIZE(cpusys_ahb_hclk_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CPUSYS_CFG_AXI_ACLK] = thead_light_clk_mux_flags("cpusys_cfg_axi_aclk", ap_base + 0x138, 5, 1, cpusys_cfg_axi_aclk_sel, ARRAY_SIZE(cpusys_cfg_axi_aclk_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_PERISYS_AHB_HCLK] = thead_light_clk_mux_flags("perisys_ahb_hclk", ap_base + 0x40, 5, 1, perisys_ahb_hclk_sel, ARRAY_SIZE(perisys_ahb_hclk_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CLK_OUT_1] = thead_light_clk_mux_flags("clk_out_1", ap_base + 0x1b4, 4, 1, clk_out_1_sel, ARRAY_SIZE(clk_out_1_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CLK_OUT_2] = thead_light_clk_mux_flags("clk_out_2", ap_base + 0x1b8, 4, 1, clk_out_2_sel, ARRAY_SIZE(clk_out_2_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CLK_OUT_3] = thead_light_clk_mux_flags("clk_out_3", ap_base + 0x1bc, 4, 1, clk_out_3_sel, ARRAY_SIZE(clk_out_3_sel), CLK_SET_RATE_PARENT);
+	clks[LIGHT_CLK_OUT_4] = thead_light_clk_mux_flags("clk_out_4", ap_base + 0x1c0, 4, 1, clk_out_4_sel, ARRAY_SIZE(clk_out_4_sel), CLK_SET_RATE_PARENT);
+
+	/* AP sys div tree */
+	clks[LIGHT_CPUSYS_AHB_HCLK_DIV] = thead_clk_light_divider("cpusys_ahb_hclk_div", "gmac_pll_fout1ph0", ap_base + 0x120, 0, 4, 4, MUX_TYPE_DIV, 2, 8);
+	clks[LIGHT_APB3_CPUSYS_PCLK] = thead_clk_light_divider("apb3_cpusys_pclk", "cpusys_ahb_hclk", ap_base + 0x130, 0, 3, 3, MUX_TYPE_CDE, 1, 7);
+	clks[LIGHT_CPUSYS_SUB_AXI_ACLK] = thead_clk_light_divider("cpusys_sub_axi_aclk", "gmac_pll_bypass", ap_base + 0x134, 0, 4, 4, MUX_TYPE_DIV, 2, 8);
+	clks[LIGHT_CPUSYS_CFG_AXI_ACLK_DIV] = thead_clk_light_divider("cpusys_cfg_axi_aclk_div", "gmac_pll_bypass", ap_base + 0x138, 0, 4, 4, MUX_TYPE_DIV, 8, 15);
+	clks[LIGHT_TEESYS_HCLK] = thead_clk_light_divider("teesys_hclk", "gmac_pll_fout1ph0", ap_base + 0x154, 0, 2, 2, MUX_TYPE_DIV, 2, 3);
+	clks[LIGHT_DMAC_1_CLK] = thead_clk_light_divider("dmac_1_clk", "video_pll_bypass", ap_base + 0x158, 0, 2, 2, MUX_TYPE_CDE, 0, 7);
+	clks[LIGHT_DMAC_2_CLK] = thead_clk_light_divider("dmac_2_clk", "video_pll_bypass", ap_base + 0x16c, 0, 2, 2, MUX_TYPE_CDE, 0, 7);
+	clks[LIGHT_DMAC_3_CLK] = thead_clk_light_divider("dmac_3_clk", "gmac_pll_bypass", ap_base + 0x160, 0, 2, 2, MUX_TYPE_CDE, 0, 7);
+	clks[LIGHT_AXI_PORT4_CLK] = thead_clk_light_divider("axi_port4_clk", "video_pll_bypass", ap_base + 0x164, 0, 2, 2, MUX_TYPE_CDE, 0, 7);
+	clks[LIGHT_PERISYS_AHB_HCLK_DIV] = thead_clk_light_divider("perisys_ahb_hclk_div", "gmac_pll_fout1ph0", ap_base + 0x140, 0, 4, 4, MUX_TYPE_DIV, 2, 8);
+	clks[LIGHT_PERISYS_APB_PCLK] = thead_clk_light_divider("perisys_apb_pclk", "perisys_ahb_hclk", ap_base + 0x150, 0, 3, 3, MUX_TYPE_CDE, 3, 7);
+	clks[LIGHT_CLK_OUT_1_DIV] = thead_clk_light_divider("clk_out_1_div", "osc_24m", ap_base + 0x1b4, 0, 3, 3, MUX_TYPE_DIV, 2, 7);
+	clks[LIGHT_CLK_OUT_2_DIV] = thead_clk_light_divider("clk_out_2_div", "osc_24m", ap_base + 0x1b8, 0, 3, 3, MUX_TYPE_DIV, 2, 7);
+	clks[LIGHT_CLK_OUT_3_DIV] = thead_clk_light_divider("clk_out_3_div", "osc_24m", ap_base + 0x1bc, 0, 3, 3, MUX_TYPE_DIV, 2, 7);
+	clks[LIGHT_CLK_OUT_4_DIV] = thead_clk_light_divider("clk_out_4_div", "osc_24m", ap_base + 0x1c0, 0, 3, 3, MUX_TYPE_DIV, 2, 7);
+
+	/* AP sys gate tree */
+	clks[LIGHT_CLKGEN_PERISYS_AXI_ACLK] = thead_clk_light_gate("clkgen_perisys_axi_aclk", "perisys_ahb_hclk", ap_base + 0x200, 31);
+	clks[LIGHT_CLKGEN_PERISYS_AHB_HCLK] = thead_clk_light_gate("clkgen_perisys_ahb_hclk", "perisys_ahb_hclk", ap_base + 0x200, 30);
+	clks[LIGHT_CLKGEN_PERISYS_APB1_HCLK] = thead_clk_light_gate("clkgen_perisys_apb1_hclk", "perisys_ahb_hclk", ap_base + 0x200, 29);
+	clks[LIGHT_CLKGEN_PERISYS_APB2_HCLK] = thead_clk_light_gate("clkgen_perisys_apb2_hclk", "perisys_ahb_hclk", ap_base + 0x200, 28);
+	clks[LIGHT_CLKGEN_USB3_DRD_PHY_REF_CLK] = thead_clk_light_gate("clkgen_usb3_drd_phy_ref_clk", "usb3_phy_ref_clk", ap_base + 0x200, 27);
+	clks[LIGHT_CLKGEN_USB3_DRD_CTRL_REF_CLK] = thead_clk_light_gate("clkgen_usb3_drd_ctrl_ref_clk", "usb3_ctrl_ref_clk", ap_base + 0x200, 26);
+	clks[LIGHT_CLKGEN_USB3_DRD_SPDCLK] = thead_clk_light_gate("clkgen_usb3_drd_spdclk", "osc_clk_div24", ap_base + 0x200, 25);
+	clks[LIGHT_CLKGEN_EMMC1_X2X_ACLK] = thead_clk_light_gate("clkgen_emmc1_x2x_aclk", "perisys_ahb_hclk", ap_base + 0x200, 23);
+	clks[LIGHT_CLKGEN_EMMC0_X2X_ACLK] = thead_clk_light_gate("clkgen_emmc0_x2x_aclk", "perisys_ahb_hclk", ap_base + 0x200, 22);
+	clks[LIGHT_CLKGEN_UART0_PCLK] = thead_clk_light_gate("clkgen_uart0_pclk", "perisys_apb_pclk", ap_base + 0x200, 14);
+	clks[LIGHT_CLKGEN_UART1_PCLK] = thead_clk_light_gate("clkgen_uart1_pclk", "perisys_apb_pclk", ap_base + 0x200, 13);
+	clks[LIGHT_CLKGEN_UART2_PCLK] = thead_clk_light_gate("clkgen_uart2_pclk", "perisys_apb_pclk", ap_base + 0x200, 12);
+	clks[LIGHT_CLKGEN_UART3_PCLK] = thead_clk_light_gate("clkgen_uart3_pclk", "perisys_apb_pclk", ap_base + 0x200, 11);
+	clks[LIGHT_CLKGEN_UART4_PCLK] = thead_clk_light_gate("clkgen_uart4_pclk", "perisys_apb_pclk", ap_base + 0x200, 10);
+	clks[LIGHT_CLKGEN_UART5_PCLK] = thead_clk_light_gate("clkgen_uart5_pclk", "perisys_apb_pclk", ap_base + 0x200, 9);
+	clks[LIGHT_CLKGEN_I2C0_IC_CLK] = thead_clk_light_gate("clkgen_i2c0_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 5);
+	clks[LIGHT_CLKGEN_I2C1_IC_CLK] = thead_clk_light_gate("clkgen_i2c1_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 4);
+	clks[LIGHT_CLKGEN_I2C2_IC_CLK] = thead_clk_light_gate("clkgen_i2c2_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 3);
+	clks[LIGHT_CLKGEN_I2C3_IC_CLK] = thead_clk_light_gate("clkgen_i2c3_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 2);
+	clks[LIGHT_CLKGEN_I2C4_IC_CLK] = thead_clk_light_gate("clkgen_i2c4_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 1);
+	clks[LIGHT_CLKGEN_I2C5_IC_CLK] = thead_clk_light_gate("clkgen_i2c5_ic_clk", "perisys_apb_pclk", ap_base + 0x200, 0);
+
+	clks[LIGHT_CLKGEN_AXI_DUMMY_SLV_4_ACLK] = thead_clk_light_gate("clkgen_axi_dummy_slv_4_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 28);
+	clks[LIGHT_CLKGEN_AXI_DUMMY_SLV_3_ACLK] = thead_clk_light_gate("clkgen_axi_dummy_slv_3_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 27);
+	clks[LIGHT_CLKGEN_AXI_DUMMY_SLV_2_ACLK] = thead_clk_light_gate("clkgen_axi_dummy_slv_2_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 26);
+	clks[LIGHT_CLKGEN_AXI_DUMMY_SLV_1_ACLK] = thead_clk_light_gate("clkgen_axi_dummy_slv_1_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 25);
+	clks[LIGHT_CLKGEN_APB_CPU2FG_HCLK] = thead_clk_light_gate("clkgen_apb_cpu2cfg_hclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 24);
+	clks[LIGHT_CLKGEN_CPU2RAM_X2X_ACLK_M] = thead_clk_light_gate("clkgen_cpu2ram_x2x_aclk_m", "cpusys_axi_aclk", ap_base + 0x204, 21);
+	clks[LIGHT_CLKGEN_AXI4_CPUSYS2_ACLK] = thead_clk_light_gate("clkgen_axi4_cpusys2_aclk", "cpusys_sub_axi_aclk", ap_base + 0x204, 20);
+	clks[LIGHT_CLKGEN_X2X_CPUSYS_ACLK_M] = thead_clk_light_gate("clkgen_x2x_cpusys_aclk_m", "cpusys_sub_axi_aclk", ap_base + 0x204, 19);
+	clks[LIGHT_CLKGEN_CHIP_DBG_ACLK] = thead_clk_light_gate("clkgen_chip_dbg_aclk", "cpusys_sub_axi_aclk", ap_base + 0x204, 18);
+	clks[LIGHT_CLKGEN_AXI4_CFG_BUS_ACLK] = thead_clk_light_gate("clkgen_axi4_cfg_bus_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 17);
+	clks[LIGHT_CLKGEN_AHB2_CPUSYS_HCLK] = thead_clk_light_gate("clkgen_ahb2_cpusys_hclk", "cpusys_ahb_hclk", ap_base + 0x204, 11);
+	clks[LIGHT_CLKGEN_APB3_CPUSYS_HCLK] = thead_clk_light_gate("clkgen_apb3_cpusys_hclk", "cpusys_ahb_hclk", ap_base + 0x204, 10);
+	clks[LIGHT_CLKGEN_C910_BROM_HCLK] = thead_clk_light_gate("clkgen_c910_brom_hclk", "cpusys_ahb_hclk", ap_base + 0x204, 9);
+	clks[LIGHT_CLKGEN_MBOX0_PCLK] = thead_clk_light_gate("clkgen_mbox0_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 7);
+	clks[LIGHT_CLKGEN_MBOX1_PCLK] = thead_clk_light_gate("clkgen_mbox1_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 6);
+	clks[LIGHT_CLKGEN_MBOX2_PCLK] = thead_clk_light_gate("clkgen_mbox2_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 5);
+	clks[LIGHT_CLKGEN_MBOX3_PCLK] = thead_clk_light_gate("clkgen_mbox3_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 4);
+	clks[LIGHT_CLKGEN_WDT0_PCLK] = thead_clk_light_gate("clkgen_wdt0_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 3);
+	clks[LIGHT_CLKGEN_WDT1_PCLK] = thead_clk_light_gate("clkgen_wdt1_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 2);
+
+	clks[LIGHT_CLKGEN_TRNG_RB_HCLK] = thead_clk_light_gate("clkgen_trng_rb_hclk", "teesys_hclk", ap_base + 0x208, 19);
+	clks[LIGHT_CLKGEN_ADC_PCLK] = thead_clk_light_gate("clkgen_adc_pclk", "perisys_apb_pclk", ap_base + 0x208, 18);
+	clks[LIGHT_CLKGEN_AXI_ACLK_4] = thead_clk_light_gate("axi_aclk_4", "axi_port4_clk", ap_base + 0x208, 17);
+	clks[LIGHT_CLKGEN_AXI_ACLK_3] = thead_clk_light_gate("axi_aclk_3", "dmac_3_clk", ap_base + 0x208, 16);
+	clks[LIGHT_CLKGEN_AXI_ACLK_2] = thead_clk_light_gate("axi_aclk_2", "dmac_2_clk", ap_base + 0x208, 15);
+	clks[LIGHT_CLKGEN_AXI_ACLK_1] = thead_clk_light_gate("axi_aclk_1", "dmac_1_clk", ap_base + 0x208, 14);
+	clks[LIGHT_CLKGEN_AXI_ACLK_0] = thead_clk_light_gate("axi_aclk_0", "cpusys_axi_aclk", ap_base + 0x208, 13);
+	clks[LIGHT_CLKGEN_SRAM_AXI_PCLK] = thead_clk_light_gate("clkgen_sram_axi_pclk", "cpusys_cfg_axi_aclk", ap_base + 0x208, 9);
+	clks[LIGHT_CLKGEN_AHB2_TEESYS_HCLK] = thead_clk_light_gate("clkgen_ahb2_teesys_hclk", "teesys_hclk", ap_base + 0x208, 8);
+	clks[LIGHT_CLKGEN_EFUSE_MPW_PCLK] = thead_clk_light_gate("clkgen_efuse_mpw_pclk", "perisys_apb_pclk", ap_base + 0x208, 7);
+	clks[LIGHT_CLKGEN_CLK_OUT_4_CLK] = thead_clk_light_gate("clkgen_clk_out_4_clk", "clk_out_4", ap_base + 0x208, 6);
+	clks[LIGHT_CLKGEN_CLK_OUT_3_CLK] = thead_clk_light_gate("clkgen_clk_out_3_clk", "clk_out_3", ap_base + 0x208, 5);
+	clks[LIGHT_CLKGEN_CLK_OUT_2_CLK] = thead_clk_light_gate("clkgen_clk_out_2_clk", "clk_out_2", ap_base + 0x208, 4);
+	clks[LIGHT_CLKGEN_CLK_OUT_1_CLK] = thead_clk_light_gate("clkgen_clk_out_1_clk", "clk_out_1", ap_base + 0x208, 3);
+	clks[LIGHT_CLKGEN_DDR_APB_PCLK] = thead_clk_light_gate("clkgen_ddr_apb_pclk", "cpusys_cfg_axi_aclk", ap_base + 0x208, 2);
+	clks[LIGHT_CLKGEN_PADCTRL_APSYS_PCLK] = thead_clk_light_gate("clkgen_padctrl_apsys_pclk", "cpusys_cfg_axi_aclk", ap_base + 0x208, 1);
+	clks[LIGHT_CLKGEN_CHIP_DBG_CCLK] = thead_clk_light_gate("clkgen_chip_dbg_cclk", "chip_dbg_cclk", ap_base + 0x208, 0);
+
+	/* register AP shared gate */
+	clks[LIGHT_CLKGEN_CPU2CFG_X2X_ACLK_M] = thead_clk_light_gate_shared("clkgen_cpu2cfg_x2x_aclk_m", "cpusys_axi_aclk", ap_base + 0x204, 22, &share_cnt_cpu2cfg_x2x_clk_en);
+	clks[LIGHT_CLKGEN_CPU2CFG_X2X_ACLK_S] = thead_clk_light_gate_shared("clkgen_cpu2cfg_x2x_aclk_s", "cpusys_cfg_axi_aclk", ap_base + 0x204, 22, &share_cnt_cpu2cfg_x2x_clk_en);
+	clks[LIGHT_CLKGEN_CPU2PERI_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2peri_x2h_mhclk", "perisys_ahb_hclk", ap_base + 0x204, 12, &share_cnt_cpu2peri_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2CFG_X2H_ACLK_S] = thead_clk_light_gate_shared("clkgen_cpu2peri_x2h_aclk", "cpusys_axi_aclk", ap_base + 0x204, 12, &share_cnt_cpu2peri_x2h_clk_en);
+	clks[LIGHT_CLKGEN_AON2CPU_A2X_ACLK] = thead_clk_light_gate_shared("clkgen_aon2cpu_a2x_aclk", "cpusys_sub_axi_aclk", ap_base + 0x204, 23, &share_cnt_aon2cpu_a2x_clk_en);
+	clks[LIGHT_CLKGEN_AON2CPU_A2X_HCLK] = thead_clk_light_gate_shared("clkgen_aon2cpu_a2x_hclk", "aonsys_x2h_hclk", ap_base + 0x204, 23, &share_cnt_aon2cpu_a2x_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_ACLK] = thead_clk_light_gate_shared("clkgen_dmac_aclk", "cpusys_sub_axi_aclk", ap_base + 0x204, 8, &share_cnt_dmac_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_HCLK] = thead_clk_light_gate_shared("clkgen_dmac_hclk", "cpusys_ahb_hclk", ap_base + 0x204, 8, &share_cnt_dmac_clk_en);
+	clks[LIGHT_CLKGEN_X2H_CPUSYS_ACLK] = thead_clk_light_gate_shared("clkgen_x2h_cpusys_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 16, &share_cnt_x2h_cpusys_clk_en);
+	clks[LIGHT_CLKGEN_X2H_CPUSYS_MHCLK] = thead_clk_light_gate_shared("clkgen_x2h_cpusys_mhclk", "cpusys_ahb_hclk", ap_base + 0x204, 16, &share_cnt_x2h_cpusys_clk_en);
+	clks[LIGHT_CLKGEN_CPU2TEE_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2tee_x2h_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 15, &share_cnt_cpu2tee_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2TEE_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2tee_x2h_mhclk", "teesys_hclk", ap_base + 0x204, 15, &share_cnt_cpu2tee_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2AON_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2aon_x2h_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 14, &share_cnt_cpu2aon_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2AON_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2aon_x2h_mhclk", "aonsys_x2h_hclk", ap_base + 0x204, 14, &share_cnt_cpu2aon_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2CFG_X2H_ACLK] = thead_clk_light_gate_shared("clkgen_cpu2cfg_x2h_aclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 13, &share_cnt_cpu2cfg_x2h_clk_en);
+	clks[LIGHT_CLKGEN_CPU2CFG_X2H_MHCLK] = thead_clk_light_gate_shared("clkgen_cpu2cfg_x2h_mhclk", "cpusys_cfg_axi_aclk", ap_base + 0x204, 13, &share_cnt_cpu2cfg_x2h_clk_en);
+	clks[LIGHT_CLKGEN_TIMER0_CCLK] = thead_clk_light_gate_shared("clkgen_timer0_cclk", "apb3_cpusys_pclk", ap_base + 0x204, 1, &share_cnt_timer0_clk_en);
+	clks[LIGHT_CLKGEN_TIMER0_PCLK] = thead_clk_light_gate_shared("clkgen_timer0_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 1, &share_cnt_timer0_clk_en);
+	clks[LIGHT_CLKGEN_TIMER1_CCLK] = thead_clk_light_gate_shared("clkgen_timer1_cclk", "apb3_cpusys_pclk", ap_base + 0x204, 0, &share_cnt_timer1_clk_en);
+	clks[LIGHT_CLKGEN_TIMER1_PCLK] = thead_clk_light_gate_shared("clkgen_timer1_pclk", "apb3_cpusys_pclk", ap_base + 0x204, 0, &share_cnt_timer1_clk_en);
+	clks[LIGHT_CLKGEN_PERI2DDR_X2X_ACLK_M] = thead_clk_light_gate_shared("clkgen_peri2ddr_x2x_aclk_m", "perisys_ahb_hclk", ap_base + 0x204, 29, &share_cnt_peri2ddr_x2x_clk_en);
+	clks[LIGHT_CLKGEN_PERI2DDR_X2X_ACLK_S] = thead_clk_light_gate_shared("clkgen_peri2ddr_x2x_aclk_s", "axi_port4_clk", ap_base + 0x204, 29, &share_cnt_peri2ddr_x2x_clk_en);
+	clks[LIGHT_CLKGEN_USB3_DRD_ACLK] = thead_clk_light_gate_shared("clkgen_usb3_drd_aclk", "perisys_ahb_hclk", ap_base + 0x200, 24, &share_cnt_usb3_drd_clk_en);
+	clks[LIGHT_CLKGEN_USB3_DRD_PCLK] = thead_clk_light_gate_shared("clkgen_usb3_drd_pclk", "perisys_apb_pclk", ap_base + 0x200, 24, &share_cnt_usb3_drd_clk_en);
+	clks[LIGHT_CLKGEN_GMAC_HCLK] = thead_clk_light_gate_shared("clkgen_gmac_hclk", "perisys_ahb_hclk", ap_base + 0x200, 19, &share_cnt_gmac_clk_en);
+	clks[LIGHT_CLKGEN_GMAC_ACLK] = thead_clk_light_gate_shared("clkgen_gmac_aclk", "perisys_ahb_hclk", ap_base + 0x200, 19, &share_cnt_gmac_clk_en);
+	clks[LIGHT_CLKGEN_GMAC_PCLK] = thead_clk_light_gate_shared("clkgen_gmac_pclk", "perisys_apb_pclk", ap_base + 0x200, 19, &share_cnt_gmac_clk_en);
+	clks[LIGHT_CLKGEN_GMAC_CCLK] = thead_clk_light_gate_shared("clkgen_gmac_cclk", "gmac_coreclk", ap_base + 0x200, 19, &share_cnt_gmac_clk_en);
+	clks[LIGHT_CLKGEN_EMMC0_HCLK] = thead_clk_light_gate_shared("clkgen_emmc0_hclk", "perisys_ahb_hclk", ap_base + 0x200, 21, &share_cnt_emmc0_clk_en);
+	clks[LIGHT_CLKGEN_EMMC0_ACLK] = thead_clk_light_gate_shared("clkgen_emmc0_aclk", "perisys_ahb_hclk", ap_base + 0x200, 21, &share_cnt_emmc0_clk_en);
+	clks[LIGHT_CLKGEN_EMMC0_REF_CLK] = thead_clk_light_gate_shared("clkgen_emmc0_ref_clk", "emmc_clk_div", ap_base + 0x200, 21, &share_cnt_emmc0_clk_en);
+	clks[LIGHT_CLKGEN_EMMC0_OSC_CLK] = thead_clk_light_gate_shared("clkgen_emmc0_osc_clk", "emmc0_osc_clk", ap_base + 0x200, 21, &share_cnt_emmc0_clk_en);
+	clks[LIGHT_CLKGEN_EMMC1_HCLK] = thead_clk_light_gate_shared("clkgen_emmc1_hclk", "perisys_ahb_hclk", ap_base + 0x200, 20, &share_cnt_emmc1_clk_en);
+	clks[LIGHT_CLKGEN_EMMC1_ACLK] = thead_clk_light_gate_shared("clkgen_emmc1_aclk", "perisys_ahb_hclk", ap_base + 0x200, 20, &share_cnt_emmc1_clk_en);
+	clks[LIGHT_CLKGEN_EMMC1_REF_CLK] = thead_clk_light_gate_shared("clkgen_emmc1_ref_clk", "emmc_clk_div", ap_base + 0x200, 20, &share_cnt_emmc1_clk_en);
+	clks[LIGHT_CLKGEN_EMMC1_OSC_CLK] = thead_clk_light_gate_shared("clkgen_emmc1_osc_clk", "emmc1_osc_clk", ap_base + 0x200, 20, &share_cnt_emmc1_clk_en);
+	clks[LIGHT_CLKGEN_PWM_PCLK] = thead_clk_light_gate_shared("clkgen_pwm_pclk", "perisys_ahb_hclk", ap_base + 0x200, 18, &share_cnt_pwm_clk_en);
+	clks[LIGHT_CLKGEN_PWM_CCLK] = thead_clk_light_gate_shared("clkgen_pwm_cclk", "pwm_cclk", ap_base + 0x200, 18, &share_cnt_pwm_clk_en);
+	clks[LIGHT_CLKGEN_QSPI0_PCLK] = thead_clk_light_gate_shared("clkgen_qspi0_pclk", "perisys_apb_pclk", ap_base + 0x200, 17, &share_cnt_qspi0_clk_en);
+	clks[LIGHT_CLKGEN_QSPI0_SSI_CLK] = thead_clk_light_gate_shared("clkgen_qspi0_ssi_clk", "spi_clk", ap_base + 0x200, 17, &share_cnt_qspi0_clk_en);
+	clks[LIGHT_CLKGEN_QSPI1_PCLK] = thead_clk_light_gate_shared("clkgen_qspi1_pclk", "perisys_apb_pclk", ap_base + 0x200, 16, &share_cnt_qspi1_clk_en);
+	clks[LIGHT_CLKGEN_QSPI1_SSI_CLK] = thead_clk_light_gate_shared("clkgen_qspi1_ssi_clk", "spi_clk", ap_base + 0x200, 16, &share_cnt_qspi0_clk_en);
+	clks[LIGHT_CLKGEN_SPI_PCLK] = thead_clk_light_gate_shared("clkgen_spi_pclk", "perisys_apb_pclk", ap_base + 0x200, 15, &share_cnt_spi_clk_en);
+	clks[LIGHT_CLKGEN_SPI_SSI_CLK] = thead_clk_light_gate_shared("clkgen_spi_ssi_clk", "spi_clk", ap_base + 0x200, 15, &share_cnt_spi_clk_en);
+	clks[LIGHT_CLKGEN_GPIO0_PCLK] = thead_clk_light_gate_shared("clkgen_gpio0_pclk", "perisys_apb_pclk", ap_base + 0x200, 8, &share_cnt_gpio0_clk_en);
+	clks[LIGHT_CLKGEN_GPIO0_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio0_dbclk", "gpio_dbclk", ap_base + 0x200, 8, &share_cnt_gpio0_clk_en);
+	clks[LIGHT_CLKGEN_GPIO1_PCLK] = thead_clk_light_gate_shared("clkgen_gpio1_pclk", "perisys_apb_pclk", ap_base + 0x200, 7, &share_cnt_gpio1_clk_en);
+	clks[LIGHT_CLKGEN_GPIO1_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio1_dbclk", "gpio_dbclk", ap_base + 0x200, 7, &share_cnt_gpio1_clk_en);
+	clks[LIGHT_CLKGEN_GPIO2_PCLK] = thead_clk_light_gate_shared("clkgen_gpio2_pclk", "perisys_apb_pclk", ap_base + 0x200, 6, &share_cnt_gpio2_clk_en);
+	clks[LIGHT_CLKGEN_GPIO2_DBCLK] = thead_clk_light_gate_shared("clkgen_gpio2_dbclk", "gpio_dbclk", ap_base + 0x200, 6, &share_cnt_gpio2_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_1_ACLK] = thead_clk_light_gate_shared("clkgen_dmac_1_aclk", "dmac_1_clk", ap_base + 0x208, 12, &share_cnt_dmac_1_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_1_HCLK] = thead_clk_light_gate_shared("clkgen_dmac_1_hclk", "teesys_hclk", ap_base + 0x208, 12, &share_cnt_dmac_1_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_2_ACLK] = thead_clk_light_gate_shared("clkgen_dmac_2_aclk", "dmac_2_clk", ap_base + 0x208, 11, &share_cnt_dmac_2_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_2_HCLK] = thead_clk_light_gate_shared("clkgen_dmac_2_hclk", "teesys_hclk", ap_base + 0x208, 11, &share_cnt_dmac_2_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_3_ACLK] = thead_clk_light_gate_shared("clkgen_dmac_3_aclk", "dmac_3_clk", ap_base + 0x208, 10, &share_cnt_dmac_3_clk_en);
+	clks[LIGHT_CLKGEN_DMAC_3_HCLK] = thead_clk_light_gate_shared("clkgen_dmac_3_hclk", "teesys_hclk", ap_base + 0x208, 10, &share_cnt_dmac_3_clk_en);
+
+	clk_data.clks = clks;
+	clk_data.clk_num = ARRAY_SIZE(clks);
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_data);
+
+	if (ret < 0) {
+		dev_err(dev, "failed to register clks for light\n");
+		goto unregister_clks;
+	}
+
+	/* HW defalut */
+	clk_set_parent(clks[LIGHT_C910_CCLK], clks[LIGHT_CPU_PLL1_FOUTPOSTDIV]);
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(clks, ARRAY_SIZE(clks));
+	return ret;
+}
+
+static const struct of_device_id light_clk_of_match[] = {
+	{ .compatible = "thead,light-mpw-clk" },
+	{ /* Sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, light_clk_of_match);
+
+static struct platform_driver light_clk_driver = {
+	.probe = light_clocks_probe,
+	.driver = {
+		.name = "light-mpw-clk",
+		.of_match_table = of_match_ptr(light_clk_of_match),
+	},
+};
+
+module_platform_driver(light_clk_driver);
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light MPW clock driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/thead/clk.c b/drivers/clk/thead/clk.c
new file mode 100644
index 000000000000..2e181a9fd180
--- /dev/null
+++ b/drivers/clk/thead/clk.c
@@ -0,0 +1,739 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+#include <linux/clk.h>
+#include <linux/clk-provider.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/iopoll.h>
+#include <linux/of.h>
+#include <linux/slab.h>
+#include <linux/spinlock.h>
+
+#include "clk.h"
+
+#define LIGHT_PLL_CFG0		0x0
+#define LIGHT_PLL_CFG1		0x04
+#define LIGHT_PLL_CFG2		0x8
+#define LIGHT_POSTDIV2_SHIFT	24
+#define LIGHT_POSTDIV2_MASK	GENMASK(26, 24)
+#define LIGHT_POSTDIV1_SHIFT	20
+#define LIGHT_POSTDIV1_MASK	GENMASK(22, 20)
+#define LIGHT_FBDIV_SHIFT	8
+#define LIGHT_FBDIV_MASK	GENMASK(19, 8)
+#define LIGHT_REFDIV_SHIFT	0
+#define LIGHT_REFDIV_MASK	GENMASK(5, 0)
+#define LIGHT_BYPASS_MASK	BIT(30)
+#define LIGHT_RST_MASK		BIT(29)
+#define LIGHT_DSMPD_MASK	BIT(24)
+#define LIGHT_DACPD_MASK	BIT(25)
+#define LIGHT_FRAC_MASK		GENMASK(23, 0)
+#define LIGHT_FRAC_SHIFT	0
+#define LIGHT_FRAC_DIV		BIT(24)
+
+#define LOCK_TIMEOUT_US		10000
+
+#define div_mask(d)	((1 << (d->width)) - 1)
+
+DEFINE_SPINLOCK(thead_light_clk_lock);
+
+enum light_pll_mode {
+        PLL_MODE_FRAC,
+        PLL_MODE_INT,
+};
+
+struct clk_lightpll {
+	struct clk_hw			hw;
+	void __iomem			*base;
+	enum light_pll_clktype		clk_type;
+	enum light_pll_outtype		out_type;
+	enum light_pll_mode		pll_mode;
+	const struct light_pll_rate_table *rate_table;
+	int rate_count;
+
+	u32 cfg0_reg_off;
+	u32 pll_sts_off;
+	int pll_lock_bit;
+
+	/* Light MPW Aon/ddr pll define bypass:rst bits as: 31:30
+	 * but AP pll define bypass:rst bits as: 30:29
+	 *
+	 * Light Fullmask align these register field define, all pll
+	 * define bypss:rst bits as: 30:29
+	 */
+	int pll_rst_bit;
+	int pll_bypass_bit;
+};
+
+struct clk_lightdiv {
+	struct clk_divider divider;
+	enum light_div_type div_type;
+	u16 min_div;
+	u16 max_div;
+	u8 sync_en;
+	const struct clk_ops *ops;
+};
+
+struct clk_lightgate {
+	struct clk_gate gate;
+	unsigned int *share_count;
+	const struct clk_ops *ops;
+};
+
+#define to_clk_lightpll(_hw) container_of(_hw, struct clk_lightpll, hw)
+
+void thead_unregister_clocks(struct clk *clks[], unsigned int count)
+{
+        unsigned int i;
+
+        for (i = 0; i < count; i++)
+                clk_unregister(clks[i]);
+}
+
+static void clk_light_pll_cfg_init(struct clk_lightpll *pll)
+{
+	switch (pll->clk_type) {
+	case LIGHT_AUDIO_PLL:
+		pll->cfg0_reg_off = 0x0;
+		pll->pll_sts_off = 0x90;
+		pll->pll_lock_bit = BIT(0);
+		pll->pll_bypass_bit = BIT(31);
+		pll->pll_rst_bit = BIT(30);
+		pll->pll_mode = PLL_MODE_FRAC;
+		break;
+	case LIGHT_SYS_PLL:
+		pll->cfg0_reg_off = 0x10;
+		pll->pll_sts_off = 0x90;
+		pll->pll_lock_bit = BIT(1);
+		pll->pll_bypass_bit = BIT(31);
+		pll->pll_rst_bit = BIT(30);
+		pll->pll_mode = PLL_MODE_FRAC;
+		break;
+	case LIGHT_CPU_PLL0:
+		pll->cfg0_reg_off = 0x0;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(1);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_CPU_PLL1:
+		pll->cfg0_reg_off = 0x10;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(4);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_GMAC_PLL:
+		pll->cfg0_reg_off = 0x20;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(3);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_VIDEO_PLL:
+		pll->cfg0_reg_off = 0x30;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(7);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_DDR_PLL:
+		pll->cfg0_reg_off = 0x8;
+		pll->pll_sts_off = 0x18;
+		pll->pll_lock_bit = BIT(0);
+		pll->pll_bypass_bit = BIT(31);
+		pll->pll_rst_bit = BIT(30);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_DPU0_PLL:
+		pll->cfg0_reg_off = 0x40;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(8);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	case LIGHT_DPU1_PLL:
+		pll->cfg0_reg_off = 0x50;
+		pll->pll_sts_off = 0x80;
+		pll->pll_lock_bit = BIT(9);
+		pll->pll_bypass_bit = BIT(30);
+		pll->pll_rst_bit = BIT(29);
+		pll->pll_mode = PLL_MODE_INT;
+		break;
+	default:
+		pr_err("%s: Unknown pll type\n", __func__);
+	};
+}
+
+static int clk_light_pll_wait_lock(struct clk_lightpll *pll)
+{
+	u32 val;
+
+	return readl_poll_timeout(pll->base + pll->pll_sts_off, val,
+				  val & pll->pll_lock_bit, 0,
+				  LOCK_TIMEOUT_US);
+}
+
+static int clk_light_pll_prepare(struct clk_hw *hw)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	void __iomem *cfg1_off;
+	u32 val;
+	int ret;
+
+	cfg1_off = pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1;
+	val = readl_relaxed(cfg1_off);
+	if (!(val & pll->pll_rst_bit))
+		return 0;
+
+	/* Enable RST */
+	val |= pll->pll_rst_bit;
+	writel_relaxed(val, cfg1_off);
+
+	udelay(3);
+
+	/* Disable RST */
+	val &= ~pll->pll_rst_bit;
+	writel_relaxed(val, cfg1_off);
+
+	ret = clk_light_pll_wait_lock(pll);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int clk_light_pll_is_prepared(struct clk_hw *hw)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	u32 val;
+
+	val = readl_relaxed(pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+
+	return (val & pll->pll_rst_bit) ? 0 : 1;
+}
+
+static void clk_light_pll_unprepare(struct clk_hw *hw)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	u32 val;
+
+	val = readl_relaxed(pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+	val |= pll->pll_rst_bit;
+	writel_relaxed(val, pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+}
+
+static unsigned long clk_light_pll_recalc_rate(struct clk_hw *hw,
+					       unsigned long parent_rate)
+{
+#ifndef CONFIG_LIGHT_CLK_EMU
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	u32 refdiv, fbdiv, postdiv1, postdiv2, frac;
+	u32 pll_cfg0, pll_cfg1;
+	u64 fvco = 0;
+
+	pll_cfg0 = readl_relaxed(pll->base + pll->cfg0_reg_off);
+	pll_cfg1 = readl_relaxed(pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+	refdiv = (pll_cfg0 & LIGHT_REFDIV_MASK) >> LIGHT_REFDIV_SHIFT;
+	fbdiv = (pll_cfg0 & LIGHT_FBDIV_MASK) >> LIGHT_FBDIV_SHIFT;
+	postdiv1 = (pll_cfg0 & LIGHT_POSTDIV1_MASK) >> LIGHT_POSTDIV1_SHIFT;
+	postdiv2 = (pll_cfg0 & LIGHT_POSTDIV2_MASK) >> LIGHT_POSTDIV2_SHIFT;
+	frac = (pll_cfg1 & LIGHT_FRAC_MASK) >> LIGHT_FRAC_SHIFT;
+
+	/* rate calculation:
+	 * INT mode: FOUTVCO = FREE * FBDIV / REFDIV
+	 * FRAC mode:FOUTVCO = (FREE * FBDIV + FREE * FRAC/BIT(24)) / REFDIV
+	 */
+	if (pll->pll_mode == PLL_MODE_FRAC)
+		fvco = (parent_rate * frac) / LIGHT_FRAC_DIV;
+
+	fvco += (parent_rate * fbdiv);
+	do_div(fvco, refdiv);
+
+	if (pll->out_type == LIGHT_PLL_DIV)
+		do_div(fvco, postdiv1 * postdiv2);
+
+	return fvco;
+#else
+
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	const struct light_pll_rate_table *rate_table = pll->rate_table;
+
+	/* return minimum supported value */
+	if (pll->out_type == LIGHT_PLL_DIV)
+		return rate_table[0].rate;
+
+	return rate_table[0].vco_rate;
+#endif
+}
+
+static const struct light_pll_rate_table *light_get_pll_div_settings(
+		struct clk_lightpll *pll, unsigned long rate)
+{
+	const struct light_pll_rate_table *rate_table = pll->rate_table;
+	int i;
+
+	for (i = 0; i < pll->rate_count; i++)
+		if (rate == rate_table[i].rate)
+			return &rate_table[i];
+
+	return NULL;
+}
+
+static const struct light_pll_rate_table *light_get_pll_vco_settings(
+		struct clk_lightpll *pll, unsigned long rate)
+{
+	const struct light_pll_rate_table *rate_table = pll->rate_table;
+	int i;
+
+	for (i = 0; i < pll->rate_count; i++)
+		if (rate == rate_table[i].vco_rate)
+			return &rate_table[i];
+
+	return NULL;
+}
+
+static inline bool clk_light_pll_change(struct clk_lightpll *pll,
+					const struct light_pll_rate_table *rate)
+{
+	u32 refdiv_old, fbdiv_old, postdiv1_old, postdiv2_old, frac_old;
+	u32 cfg0, cfg1;
+	bool pll_changed;
+
+	cfg0 = readl_relaxed(pll->base + pll->cfg0_reg_off);
+	cfg1 = readl_relaxed(pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+
+	refdiv_old = (cfg0 & LIGHT_REFDIV_MASK) >> LIGHT_REFDIV_SHIFT;
+	fbdiv_old = (cfg0 & LIGHT_FBDIV_MASK) >> LIGHT_FBDIV_SHIFT;
+	postdiv1_old = (cfg0 & LIGHT_POSTDIV1_MASK) >> LIGHT_POSTDIV1_SHIFT;
+	postdiv2_old = (cfg0 & LIGHT_POSTDIV2_MASK) >> LIGHT_POSTDIV2_SHIFT;
+	frac_old = (cfg1 & LIGHT_FRAC_MASK) >> LIGHT_FRAC_SHIFT;
+
+	pll_changed = rate->refdiv != refdiv_old || rate->fbdiv != fbdiv_old ||
+		      rate->postdiv1 != postdiv1_old || rate->postdiv2 != postdiv2_old;
+	if (pll->pll_mode == PLL_MODE_FRAC)
+		pll_changed |= (rate->frac != frac_old);
+
+	return pll_changed;
+}
+
+static int clk_light_pll_set_rate(struct clk_hw *hw, unsigned long drate,
+				 unsigned long prate)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	const struct light_pll_rate_table *rate;
+	void __iomem *cfg1_off;
+	u32 tmp, div_val;
+	int ret;
+
+	if (pll->out_type == LIGHT_PLL_VCO) {
+		rate = light_get_pll_vco_settings(pll, drate);
+		if (!rate) {
+			pr_err("%s: Invalid rate : %lu for pll clk %s\n", __func__,
+				drate, clk_hw_get_name(hw));
+			return -EINVAL;
+		}
+	} else {
+		rate = light_get_pll_div_settings(pll, drate);
+		if (!rate) {
+			pr_err("%s: Invalid rate : %lu for pll clk %s\n", __func__,
+				drate, clk_hw_get_name(hw));
+			return -EINVAL;
+		}
+	}
+
+	if (!clk_light_pll_change(pll, rate))
+		return 0;
+
+	/* Enable RST */
+	cfg1_off = pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1;
+	tmp = readl_relaxed(cfg1_off);
+	tmp |= pll->pll_rst_bit;
+	writel_relaxed(tmp, cfg1_off);
+
+	div_val = (rate->refdiv << LIGHT_REFDIV_SHIFT) |
+		  (rate->fbdiv << LIGHT_FBDIV_SHIFT) |
+		  (rate->postdiv1 << LIGHT_POSTDIV1_SHIFT) |
+		  (rate->postdiv2 << LIGHT_POSTDIV2_SHIFT);
+	writel_relaxed(div_val, pll->base + pll->cfg0_reg_off);
+
+	if (pll->pll_mode == PLL_MODE_FRAC) {
+		tmp &= ~(LIGHT_FRAC_MASK << LIGHT_FRAC_SHIFT);
+		tmp |= rate->frac;
+		writel_relaxed(tmp, cfg1_off);
+	}
+
+	udelay(3);
+
+	/* Disable RST */
+	tmp &= ~pll->pll_rst_bit;
+	writel_relaxed(tmp, cfg1_off);
+
+	/* Wait Lock, ~20us cost */
+	ret = clk_light_pll_wait_lock(pll);
+	if (ret)
+		return ret;
+
+	/* HW requires 30us for pll stable */
+	udelay(30);
+
+	return 0;
+}
+
+static long clk_light_pllvco_round_rate(struct clk_hw *hw, unsigned long rate,
+					unsigned long *prate)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	const struct light_pll_rate_table *rate_table = pll->rate_table;
+	unsigned long best = 0, now = 0;
+	unsigned int i, best_i = 0;
+
+	for (i = 0; i < pll->rate_count; i++) {
+		now = rate_table[i].vco_rate;
+
+		if (rate == now) {
+			return rate_table[i].vco_rate;
+		} else if (abs(now - rate) < abs(best - rate)) {
+			best = now;
+			best_i = i;
+		}
+	}
+
+	/* return minimum supported value */
+	return rate_table[best_i].vco_rate;
+}
+
+static long clk_light_plldiv_round_rate(struct clk_hw *hw, unsigned long rate,
+					unsigned long *prate)
+{
+	struct clk_lightpll *pll = to_clk_lightpll(hw);
+	const struct light_pll_rate_table *rate_table = pll->rate_table;
+	unsigned long best = 0, now = 0;
+	unsigned int i, best_i = 0;
+
+	for (i = 0; i < pll->rate_count; i++) {
+		now = rate_table[i].rate;
+
+		if (rate == now) {
+			return rate_table[i].rate;
+		} else if (abs(now - rate) < abs(best - rate)) {
+			best = now;
+			best_i = i;
+		}
+	}
+
+	/* return minimum supported value */
+	return rate_table[best_i].rate;
+}
+
+static const struct clk_ops clk_light_pll_def_ops = {
+	.recalc_rate	= clk_light_pll_recalc_rate,
+};
+
+static const struct clk_ops clk_light_pllvco_ops = {
+	.prepare	= clk_light_pll_prepare,
+	.unprepare	= clk_light_pll_unprepare,
+	.is_prepared	= clk_light_pll_is_prepared,
+	.recalc_rate	= clk_light_pll_recalc_rate,
+	.round_rate	= clk_light_pllvco_round_rate,
+	.set_rate	= clk_light_pll_set_rate,
+};
+
+static const struct clk_ops clk_light_plldiv_ops = {
+	.prepare	= clk_light_pll_prepare,
+	.unprepare	= clk_light_pll_unprepare,
+	.is_prepared	= clk_light_pll_is_prepared,
+	.recalc_rate	= clk_light_pll_recalc_rate,
+	.round_rate	= clk_light_plldiv_round_rate,
+	.set_rate	= clk_light_pll_set_rate,
+};
+
+struct clk *thead_light_pll(const char *name, const char *parent_name,
+			    void __iomem *base,
+			    const struct light_pll_clk *pll_clk)
+{
+	struct clk_lightpll *pll;
+	struct clk *clk;
+	struct clk_init_data init;
+	u32 val;
+
+	pll = kzalloc(sizeof(*pll), GFP_KERNEL);
+	if (!pll)
+		return ERR_PTR(-ENOMEM);
+
+	init.name = name;
+	init.flags = pll_clk->flags;
+	init.parent_names = &parent_name;
+	init.num_parents = 1;
+
+	switch (pll_clk->out_type) {
+	case LIGHT_PLL_VCO:
+		if (pll_clk->rate_table)
+			init.ops = &clk_light_pllvco_ops;
+		break;
+	case LIGHT_PLL_DIV:
+		if (pll_clk->rate_table)
+			init.ops = &clk_light_plldiv_ops;
+		break;
+	default:
+		pr_err("%s: Unknown pll out type for pll clk %s\n",
+		       __func__, name);
+	};
+
+	if (!pll_clk->rate_table)
+		init.ops = &clk_light_pll_def_ops;
+
+	pll->base = base;
+	pll->hw.init = &init;
+	pll->out_type = pll_clk->out_type;
+	pll->clk_type = pll_clk->clk_type;
+	pll->rate_table = pll_clk->rate_table;
+	pll->rate_count = pll_clk->rate_count;
+
+	clk_light_pll_cfg_init(pll);
+
+	val = readl_relaxed(pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+	val &= ~pll->pll_bypass_bit;
+	val |= LIGHT_DACPD_MASK;
+	val |= LIGHT_DSMPD_MASK;
+	if (pll->pll_mode == PLL_MODE_FRAC) {
+		val &= ~LIGHT_DSMPD_MASK;
+		val &= ~LIGHT_DACPD_MASK;
+	}
+	writel_relaxed(val, pll->base + pll->cfg0_reg_off + LIGHT_PLL_CFG1);
+
+	clk = clk_register(NULL, &pll->hw);
+	if (IS_ERR(clk)) {
+		pr_err("%s: failed to register pll %s %lu\n",
+			__func__, name, PTR_ERR(clk));
+		kfree(pll);
+	}
+
+	return clk;
+}
+
+static inline struct clk_lightdiv *to_clk_lightdiv(struct clk_hw *hw)
+{
+	struct clk_divider *divider = to_clk_divider(hw);
+
+	return container_of(divider, struct clk_lightdiv, divider);
+}
+
+static unsigned long clk_lightdiv_recalc_rate(struct clk_hw *hw,
+					 unsigned long parent_rate)
+{
+	struct clk_lightdiv *light_div = to_clk_lightdiv(hw);
+
+	return light_div->ops->recalc_rate(&light_div->divider.hw, parent_rate);
+}
+
+static long clk_lightdiv_round_rate(struct clk_hw *hw, unsigned long rate,
+			       unsigned long *prate)
+{
+	struct clk_lightdiv *light_div = to_clk_lightdiv(hw);
+
+	return light_div->ops->round_rate(&light_div->divider.hw, rate, prate);
+}
+
+static int clk_lightdiv_set_rate(struct clk_hw *hw, unsigned long rate,
+				 unsigned long parent_rate)
+{
+	struct clk_lightdiv *light_div = to_clk_lightdiv(hw);
+	struct clk_divider *div = to_clk_divider(hw);
+	unsigned int divider, value;
+	unsigned long flags = 0;
+	u32 val;
+
+	divider = parent_rate / rate;
+
+	/* DIV is zero based divider, but CDE is not */
+	if (light_div->div_type == MUX_TYPE_DIV)
+		value = divider;
+	else
+		value = divider - 1;
+
+	/* handle the div valid range */
+	if (value > light_div->max_div)
+		value = light_div->max_div;
+	if (value < light_div->min_div)
+		value = light_div->min_div;
+
+	spin_lock_irqsave(div->lock, flags);
+
+	val = readl(div->reg);
+	val &= ~BIT(light_div->sync_en);
+	writel(val, div->reg);
+
+	udelay(1);
+
+	val &= ~(div_mask(div) << div->shift);
+	val |= value << div->shift;
+	writel(val, div->reg);
+
+	udelay(1);
+
+	val |= BIT(light_div->sync_en);
+	writel(val, div->reg);
+
+	spin_unlock_irqrestore(div->lock, flags);
+
+	return 0;
+}
+
+static const struct clk_ops clk_lightdiv_ops = {
+	.recalc_rate = clk_lightdiv_recalc_rate,
+	.round_rate = clk_lightdiv_round_rate,
+	.set_rate = clk_lightdiv_set_rate,
+};
+
+struct clk *thead_clk_light_divider(const char *name, const char *parent,
+				       void __iomem *reg, u8 shift, u8 width,
+				       u8 sync, enum light_div_type div_type,
+				       u16 min, u16 max)
+{
+	struct clk_lightdiv *light_div;
+	struct clk_hw *hw;
+	struct clk_init_data init;
+	int ret;
+
+	light_div = kzalloc(sizeof(*light_div), GFP_KERNEL);
+	if (!light_div)
+		return ERR_PTR(-ENOMEM);
+
+	init.name = name;
+	init.ops = &clk_lightdiv_ops;
+	init.flags = CLK_SET_RATE_PARENT;
+	init.parent_names = parent ? &parent : NULL;
+	init.num_parents = parent ? 1 : 0;
+
+	light_div->divider.reg = reg;
+	light_div->divider.shift = shift;
+	light_div->divider.width = width;
+	light_div->divider.lock = &thead_light_clk_lock;
+	light_div->divider.hw.init = &init;
+	light_div->ops = &clk_divider_ops;
+	light_div->sync_en = sync;
+	light_div->div_type = div_type;
+	if (light_div->div_type == MUX_TYPE_DIV)
+		light_div->divider.flags = CLK_DIVIDER_ONE_BASED;
+	light_div->min_div = min > ((1 << width) - 1) ?
+			     ((1 << width) - 1) : min;
+	light_div->max_div = max > ((1 << width) - 1) ?
+			     ((1 << width) - 1) : max;
+
+	hw = &light_div->divider.hw;
+
+	ret = clk_hw_register(NULL, hw);
+	if (ret) {
+		kfree(light_div);
+		return ERR_PTR(ret);
+	}
+
+	return hw->clk;
+}
+
+static inline struct clk_lightgate *to_clk_lightgate(struct clk_hw *hw)
+{
+	struct clk_gate *gate = to_clk_gate(hw);
+
+	return container_of(gate, struct clk_lightgate, gate);
+}
+
+static int clk_light_gate_share_is_enabled(struct clk_hw *hw)
+{
+	struct clk_lightgate *light_gate = to_clk_lightgate(hw);
+
+	return light_gate->ops->is_enabled(hw);
+}
+
+static int clk_light_gate_share_enable(struct clk_hw *hw)
+{
+	struct clk_lightgate *light_gate = to_clk_lightgate(hw);
+
+	if (light_gate->share_count && (*light_gate->share_count)++ > 0) {
+		pr_debug("[%s,%d]share_count = %d\n", __func__, __LINE__, (*light_gate->share_count));
+		return 0;
+	}
+
+	pr_debug("[%s,%d]share_count = %d\n", __func__, __LINE__, (*light_gate->share_count));
+
+	return light_gate->ops->enable(hw);
+}
+
+static void clk_light_gate_share_disable(struct clk_hw *hw)
+{
+	struct clk_lightgate *light_gate = to_clk_lightgate(hw);
+
+	if (light_gate->share_count) {
+		if (WARN_ON(*light_gate->share_count == 0))
+			return;
+		else if (--(*light_gate->share_count) > 0) {
+			pr_debug("[%s,%d]share_count = %d\n", __func__, __LINE__, (*light_gate->share_count));
+			return;
+		}
+	}
+
+	pr_debug("[%s,%d]share_count = %d\n", __func__, __LINE__, (*light_gate->share_count));
+
+	light_gate->ops->disable(hw);
+}
+
+static void clk_light_gate_share_disable_unused(struct clk_hw *hw)
+{
+	struct clk_lightgate *light_gate = to_clk_lightgate(hw);
+
+	if (!light_gate->share_count || *light_gate->share_count == 0)
+		return light_gate->ops->disable(hw);
+}
+
+static const struct clk_ops clk_lightgate_share_ops = {
+	.enable = clk_light_gate_share_enable,
+	.disable = clk_light_gate_share_disable,
+	.disable_unused = clk_light_gate_share_disable_unused,
+	.is_enabled = clk_light_gate_share_is_enabled,
+};
+
+struct clk *thead_clk_light_register_gate_shared(const char *name, const char *parent,
+						 unsigned long flags, void __iomem *reg,
+						 u8 shift, spinlock_t *lock,
+						 unsigned int *share_count)
+{
+	struct clk_lightgate *light_gate;
+	struct clk_hw *hw;
+	struct clk_init_data init;
+	int ret;
+
+	light_gate = kzalloc(sizeof(*light_gate), GFP_KERNEL);
+	if (!light_gate)
+		return ERR_PTR(-ENOMEM);
+
+	light_gate->gate.reg = reg;
+	light_gate->gate.bit_idx = shift;
+	light_gate->gate.flags = 0;
+	light_gate->gate.lock = lock;
+	light_gate->gate.hw.init = &init;
+	light_gate->ops = &clk_gate_ops;
+	light_gate->share_count = share_count;
+
+	init.name = name;
+	init.ops = &clk_lightgate_share_ops;
+	init.flags = flags;
+	init.parent_names = parent ? &parent : NULL;
+	init.num_parents = parent ? 1 : 0;
+
+	hw = &light_gate->gate.hw;
+
+	ret = clk_hw_register(NULL, hw);
+	if (ret) {
+		kfree(light_gate);
+		return ERR_PTR(ret);
+	}
+
+	return hw->clk;
+}
diff --git a/drivers/clk/thead/clk.h b/drivers/clk/thead/clk.h
new file mode 100644
index 000000000000..cad975e8ede4
--- /dev/null
+++ b/drivers/clk/thead/clk.h
@@ -0,0 +1,117 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#ifndef __MACH_THEAD_CLK_H
+#define __MACH_THEAD_CLK_H
+
+#include <linux/spinlock.h>
+#include <linux/clk-provider.h>
+
+extern spinlock_t thead_light_clk_lock;
+
+#define LIGHT_PLL_RATE(_vco, _rate, _r, _b, _f, _p, _k)	\
+	{						\
+		.vco_rate	=	(_vco),		\
+		.rate		=	(_rate),	\
+		.refdiv		=	(_r),		\
+		.fbdiv		=	(_b),		\
+		.frac		=	(_f),		\
+		.postdiv1	=	(_p),		\
+		.postdiv2	=	(_k),		\
+	}
+
+enum light_pll_outtype {
+	LIGHT_PLL_VCO,
+	LIGHT_PLL_DIV,
+};
+
+enum light_div_type {
+        MUX_TYPE_DIV,
+        MUX_TYPE_CDE,
+};
+
+enum light_pll_clktype {
+	LIGHT_AUDIO_PLL,
+	LIGHT_SYS_PLL,
+	LIGHT_CPU_PLL0,
+	LIGHT_CPU_PLL1,
+	LIGHT_GMAC_PLL,
+	LIGHT_VIDEO_PLL,
+	LIGHT_DDR_PLL,
+	LIGHT_DPU0_PLL,
+	LIGHT_DPU1_PLL,
+};
+
+struct light_pll_rate_table {
+	unsigned long vco_rate;
+	unsigned long rate;
+	unsigned int refdiv;
+	unsigned int fbdiv;
+	unsigned int frac;
+	unsigned int postdiv1;
+	unsigned int postdiv2;
+};
+
+struct light_pll_clk {
+	enum light_pll_outtype out_type;
+	enum light_pll_clktype clk_type;
+	const struct light_pll_rate_table *rate_table;
+	int rate_count;
+	int flags;
+};
+
+static inline struct clk *thead_light_clk_fixed_factor(const char *name,
+		const char *parent, unsigned int mult, unsigned int div)
+{
+	return clk_register_fixed_factor(NULL, name, parent,
+			CLK_SET_RATE_PARENT, mult, div);
+}
+
+struct clk *thead_light_pll(const char *name, const char *parent_name,
+			    void __iomem *base,
+			    const struct light_pll_clk *pll_clk);
+
+static inline struct clk *thead_clk_light_gate(const char *name, const char *parent,
+					       void __iomem *reg, u8 shift)
+{
+	return clk_register_gate(NULL, name, parent, CLK_SET_RATE_PARENT, reg,
+			shift, 0, &thead_light_clk_lock);
+}
+
+struct clk *thead_clk_light_register_gate_shared(const char *name, const char *parent,
+						 unsigned long flags, void __iomem *reg,
+						 u8 shift, spinlock_t *lock,
+						 unsigned int *share_count);
+
+struct clk *thead_clk_light_divider(const char *name, const char *parent,
+				    void __iomem *reg, u8 shift, u8 width,
+				    u8 sync, enum light_div_type div_type,
+				    u16 min, u16 max);
+
+void thead_unregister_clocks(struct clk *clks[], unsigned int count);
+
+static inline struct clk *thead_clk_fixed(const char *name, unsigned long rate)
+{
+	return clk_register_fixed_rate(NULL, name, NULL, 0, rate);
+}
+
+static inline struct clk *thead_clk_light_gate_shared(const char *name, const char *parent,
+					void __iomem *reg, u8 shift,
+					unsigned int *share_count)
+{
+	return thead_clk_light_register_gate_shared(name, parent, CLK_SET_RATE_PARENT, reg,
+						    shift, &thead_light_clk_lock, share_count);
+}
+
+static inline struct clk *thead_light_clk_mux_flags(const char *name,
+			void __iomem *reg, u8 shift, u8 width,
+			const char * const *parents, int num_parents,
+			unsigned long flags)
+{
+	return clk_register_mux(NULL, name, parents, num_parents,
+			flags | CLK_SET_RATE_NO_REPARENT, reg, shift, width, 0,
+			&thead_light_clk_lock);
+}
+#endif
diff --git a/drivers/clk/thead/gate/Makefile b/drivers/clk/thead/gate/Makefile
new file mode 100644
index 000000000000..b0ad8b2011c0
--- /dev/null
+++ b/drivers/clk/thead/gate/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier: GPL-2.0
+
+obj-$(CONFIG_CLK_LIGHT_FM) += thead-gate.o visys-gate.o vpsys-gate.o vosys-gate.o dspsys-gate.o
diff --git a/drivers/clk/thead/gate/clk-gate.h b/drivers/clk/thead/gate/clk-gate.h
new file mode 100644
index 000000000000..ebb190374a0e
--- /dev/null
+++ b/drivers/clk/thead/gate/clk-gate.h
@@ -0,0 +1,35 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef CLK_GATE_H
+#define CLK_GATE_H
+
+#include <linux/clk-provider.h>
+#include <linux/mfd/syscon.h>
+
+enum clk_gate_type {
+	GATE_NOT_SHARED,
+	GATE_SHARED,
+};
+
+struct thead_clk_gate {
+	struct clk_hw hw;
+	struct regmap *regmap;
+	u32 offset;
+	u8 bit;
+	bool shared;
+	u32 *share_count;
+};
+
+struct clk *thead_gate_clk_register(const char *name,
+				    const char *parent_name,
+				    struct regmap *regmap,
+				    int offset,
+				    u8 bit,
+				    bool shared,
+				    u32 *share_count,
+				    struct device *dev);
+
+#endif
diff --git a/drivers/clk/thead/gate/dspsys-gate.c b/drivers/clk/thead/gate/dspsys-gate.c
new file mode 100644
index 000000000000..e68a5d4e6151
--- /dev/null
+++ b/drivers/clk/thead/gate/dspsys-gate.c
@@ -0,0 +1,109 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-dspsys.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/mfd/syscon.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+#include "clk-gate.h"
+#include "../clk.h"
+
+static struct clk *gates[LIGHT_CLKGEN_DSPSYS_CLK_END];
+static struct clk_onecell_data clk_gate_data;
+
+static int light_dspsys_clk_probe(struct platform_device *pdev)
+{
+	struct regmap *dspsys_regmap, *tee_dspsys_regmap;
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	int ret;
+
+	dspsys_regmap = syscon_regmap_lookup_by_phandle(np, "dspsys-regmap");
+	if (IS_ERR(dspsys_regmap)) {
+		dev_err(&pdev->dev, "cannot find regmap for dsp system register\n");
+		return PTR_ERR(dspsys_regmap);
+	}
+
+	tee_dspsys_regmap = syscon_regmap_lookup_by_phandle(np, "tee-dspsys-regmap");
+	if (IS_ERR(tee_dspsys_regmap)) {
+		dev_warn(&pdev->dev, "cannot find regmap for tee dsp system register\n");
+		tee_dspsys_regmap = NULL;
+	}
+
+	gates[CLKGEN_DSP0_PCLK] = thead_gate_clk_register("clkgen_dsp0_pclk", NULL, dspsys_regmap,
+							  0x24, 0, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_DSP1_PCLK] = thead_gate_clk_register("clkgen_dsp1_pclk", NULL, dspsys_regmap,
+							  0x24, 1, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_DSP1_CCLK] = thead_gate_clk_register("clkgen_dsp1_cclk", NULL, dspsys_regmap,
+							  0x24, 2, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_DSP0_CCLK] = thead_gate_clk_register("clkgen_dsp0_cclk", NULL, dspsys_regmap,
+							  0x24, 3, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_X2X_DSP2_ACLK_S] = thead_gate_clk_register("clkgen_x2x_dsp2_aclk_s", NULL, dspsys_regmap,
+							  0x24, 4, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_X2X_DSP0_ACLK_S] = thead_gate_clk_register("clkgen_x2x_dsp0_aclk_s", NULL, dspsys_regmap,
+							  0x24, 5, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_X2X_X4_DSPSLV_DSP1_ACLK_M] = thead_gate_clk_register("clkgen_x2x_x4_dspslv_dsp1_aclk_m",
+							  NULL, dspsys_regmap, 0x24, 6, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_X2X_X4_DSPSLV_DSP0_ACLK_M] = thead_gate_clk_register("clkgen_x2x_x4_dspslv_dsp0_aclk_m",
+							  NULL, dspsys_regmap, 0x24, 7, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_AXI4_DSPSYS_SLV_ACLK] = thead_gate_clk_register("clkgen_axi4_dspsys_slv_aclk", NULL, dspsys_regmap,
+							  0x24, 20, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_AXI4_DSPSYS_SLV_PCLK] = thead_gate_clk_register("clkgen_axi4_dspsys_slv_pclk", NULL, dspsys_regmap,
+							  0x24, 21, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_AXI4_DSPSYS_ACLK] = thead_gate_clk_register("clkgen_axi4_dspsys_aclk", NULL, dspsys_regmap,
+							  0x24, 23, GATE_NOT_SHARED, NULL, dev);
+	gates[CLKGEN_AXI4_DSPSYS_PCLK] = thead_gate_clk_register("clkgen_axi4_dspsys_pclk", NULL, dspsys_regmap,
+							  0x24, 24, GATE_NOT_SHARED, NULL, dev);
+	if (tee_dspsys_regmap) {
+		gates[CLKGEN_IOPMP_DSP1_PCLK] = thead_gate_clk_register("clkgen_iopmp_dsp1_pclk", NULL, tee_dspsys_regmap,
+							  0x24, 25, GATE_NOT_SHARED, NULL, dev);
+		gates[CLKGEN_IOPMP_DSP0_PCLK] = thead_gate_clk_register("clkgen_iopmp_dsp0_pclk", NULL, tee_dspsys_regmap,
+							  0x24, 26, GATE_NOT_SHARED, NULL, dev);
+	}
+
+	clk_gate_data.clks = gates;
+	clk_gate_data.clk_num = ARRAY_SIZE(gates);
+
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_gate_data);
+	if (ret < 0) {
+		dev_err(dev, "failed to register gate clks for light dspsys\n");
+		goto unregister_clks;
+	}
+
+	dev_info(dev, "succeed to register dspsys gate clock provider\n");
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(gates, ARRAY_SIZE(gates));
+	return ret;
+}
+
+static const struct of_device_id dspsys_clk_gate_of_match[] = {
+	{ .compatible = "thead,dspsys-gate-controller" },
+	{ /* sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, dspsys_clk_gate_of_match);
+
+static struct platform_driver light_dspsys_clk_driver = {
+	.probe = light_dspsys_clk_probe,
+	.driver = {
+		.name = "dspsys-clk-gate-provider",
+		.of_match_table = of_match_ptr(dspsys_clk_gate_of_match),
+	},
+};
+
+module_platform_driver(light_dspsys_clk_driver);
+MODULE_AUTHOR("wei.liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Fullmask dspsys clock gate provider");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/thead/gate/thead-gate.c b/drivers/clk/thead/gate/thead-gate.c
new file mode 100644
index 000000000000..372c11dee1b9
--- /dev/null
+++ b/drivers/clk/thead/gate/thead-gate.c
@@ -0,0 +1,114 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/types.h>
+#include <linux/regmap.h>
+#include "clk-gate.h"
+
+#define to_thead_clk_gate(_hw)	container_of(_hw, struct thead_clk_gate, hw)
+
+static int thead_clk_gate_is_enabled(struct clk_hw *hw)
+{
+	struct thead_clk_gate *tcg = to_thead_clk_gate(hw);
+	u32 val;
+
+	regmap_read(tcg->regmap, tcg->offset, &val);
+
+	val &= BIT(tcg->bit);
+
+	return val != 0;
+}
+
+static void thead_clk_gate_disable(struct clk_hw *hw)
+{
+	struct thead_clk_gate *tcg = to_thead_clk_gate(hw);
+
+	if (!tcg->shared)
+		goto out;
+
+	if (tcg->share_count) {
+		if (WARN_ON(*tcg->share_count == 0))
+			return;
+		else if (--(*tcg->share_count) > 0) {
+			pr_info("[%s,%d]share_count = %d\n", __func__, __LINE__,
+					(*tcg->share_count));
+			return;
+		}
+	}
+
+out:
+	regmap_update_bits(tcg->regmap, tcg->offset,
+			   BIT(tcg->bit), 0);
+}
+
+static int thead_clk_gate_enable(struct clk_hw *hw)
+{
+	struct thead_clk_gate *tcg = to_thead_clk_gate(hw);
+
+	if (!tcg->shared)
+		goto out;
+
+	if (tcg->share_count && (*tcg->share_count)++ > 0) {
+		pr_info("[%s,%d]share_count = %d\n", __func__, __LINE__, (*tcg->share_count));
+		return 0;
+	}
+
+out:
+	return regmap_update_bits(tcg->regmap, tcg->offset,
+				  BIT(tcg->bit), BIT(tcg->bit));
+}
+
+const struct clk_ops thead_gate_clk_ops = {
+	.enable = thead_clk_gate_enable,
+	.disable = thead_clk_gate_disable,
+	.is_enabled = thead_clk_gate_is_enabled,
+};
+
+struct clk *thead_gate_clk_register(const char *name,
+				    const char *parent_name,
+				    struct regmap *regmap,
+				    int offset,
+				    u8 bit,
+				    bool shared,
+				    u32 *share_count,
+				    struct device *dev)
+{
+	struct thead_clk_gate *tcg;
+	struct clk *clk;
+	struct clk_init_data init = {};
+
+	tcg = kzalloc(sizeof(*tcg), GFP_KERNEL);
+	if (!tcg)
+		return ERR_PTR(-ENOMEM);
+
+	tcg->regmap = regmap;
+	tcg->offset = offset;
+	tcg->bit = bit;
+	tcg->shared = shared;
+	tcg->share_count = share_count;
+
+	init.name = name;
+	init.flags = CLK_SET_RATE_PARENT;
+	init.parent_names = parent_name ? &parent_name : NULL;
+	init.num_parents = parent_name ? 1 : 0;
+	init.ops = &thead_gate_clk_ops;
+
+	tcg->hw.init = &init;
+
+	clk = clk_register(dev, &tcg->hw);
+	if (IS_ERR(clk))
+		kfree(tcg);
+
+	return clk;
+}
diff --git a/drivers/clk/thead/gate/visys-gate.c b/drivers/clk/thead/gate/visys-gate.c
new file mode 100644
index 000000000000..b023e42b8269
--- /dev/null
+++ b/drivers/clk/thead/gate/visys-gate.c
@@ -0,0 +1,144 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-fm-ap-clock.h>
+#include <dt-bindings/clock/light-visys.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+#include "clk-gate.h"
+#include "../clk.h"
+
+static struct clk *gates[LIGHT_CLKGEN_VISYS_CLK_END];
+static struct clk_onecell_data clk_gate_data;
+
+static u32 share_cnt_isp0_hclk_en;
+static u32 share_cnt_isp0_aclk_en;
+
+static int light_visys_clk_probe(struct platform_device *pdev)
+{
+	struct regmap *visys_regmap;
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	int ret;
+
+	visys_regmap = syscon_regmap_lookup_by_phandle(np, "visys-regmap");
+	if (IS_ERR(visys_regmap)) {
+		dev_err(&pdev->dev, "cannot find regmap for vi system register\n");
+		return PTR_ERR(visys_regmap);
+	}
+
+	/* we assume that the gate clock is a root clock  */
+	gates[LIGHT_CLKGEN_DW200_ACLK] = thead_gate_clk_register("clkgen_dw200_aclk", NULL,
+									visys_regmap, 0xa0, 27, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_AXI4_VISYS1_ACLK] = thead_gate_clk_register("clkgen_axi4_visys1_aclk", NULL,
+									visys_regmap, 0xa0, 26, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_AXI4_VISYS2_ACLK] = thead_gate_clk_register("clkgen_axi4_visys2_aclk", NULL,
+									visys_regmap, 0xa0, 25, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_AXI4_VISYS3_ACLK] = thead_gate_clk_register("clkgen_axi4_visys3_aclk", NULL,
+									visys_regmap, 0xa0, 24, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP_RY_ACLK] = thead_gate_clk_register("clkgen_isp_ry_aclk", NULL,
+									visys_regmap, 0xa0, 22, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP_VENC_SHAKE_ACLK] = thead_gate_clk_register("clkgen_isp_venc_shake_aclk", NULL,
+									visys_regmap, 0xa0, 30, GATE_NOT_SHARED, NULL, dev);
+
+	gates[LIGHT_CLKGEN_VIPRE_ACLK] = thead_gate_clk_register("clkgen_vipre_aclk", NULL,
+									visys_regmap, 0xa0, 31, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_DW200_HCLK] = thead_gate_clk_register("clkgen_dw200_hclk", NULL,
+									visys_regmap, 0xa0, 13, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP_RY_HCLK] = thead_gate_clk_register("clkgen_isp_ry_hclk", NULL,
+									visys_regmap, 0xa0, 12, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI0_PCLK] = thead_gate_clk_register("clkgen_mipi_csi0_pclk", NULL,
+									visys_regmap, 0xa0, 18, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI1_PCLK] = thead_gate_clk_register("clkgen_mipi_csi1_pclk", NULL,
+									visys_regmap, 0xa0, 17, GATE_NOT_SHARED, NULL, dev);
+
+	gates[LIGHT_CLKGEN_MIPI_CSI2_PCLK] = thead_gate_clk_register("clkgen_mipi_csi2_pclk", NULL,
+									visys_regmap, 0xa0, 16, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_VIPRE_PCLK] = thead_gate_clk_register("clkgen_vipre_pclk", NULL,
+									visys_regmap, 0xa0, 15, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP_VENC_SHAKE_PCLK] = thead_gate_clk_register("clkgen_isp_venc_shake_pclk", NULL,
+									visys_regmap, 0xa0, 29, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI0_PIXCLK] = thead_gate_clk_register("clkgen_mipi_csi0_pixclk", NULL,
+									visys_regmap, 0xa0, 11, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI1_PIXCLK] = thead_gate_clk_register("clkgen_mipi_csi1_pixclk", NULL,
+									visys_regmap, 0xa0, 10, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI2_PIXCLK] = thead_gate_clk_register("clkgen_mipi_csi2_pixclk", NULL,
+									visys_regmap, 0xa0, 9, GATE_NOT_SHARED, NULL, dev);
+
+	gates[LIGHT_CLKGEN_VIPRE_PIXELCLK] = thead_gate_clk_register("clkgen_vipre_pixelclk", NULL,
+									visys_regmap, 0xa4, 23, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI0_CFG_CLK] = thead_gate_clk_register("clkgen_mipi_csi0_cfg_clk", NULL,
+									visys_regmap, 0xa0, 8, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI1_CFG_CLK] = thead_gate_clk_register("clkgen_mipi_csi1_cfg_clk", NULL,
+									visys_regmap, 0xa0, 6, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_MIPI_CSI2_CFG_CLK] = thead_gate_clk_register("clkgen_mipi_csi2_cfg_clk", NULL,
+									visys_regmap, 0xa0, 7, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_DW200_CLK_VSE] = thead_gate_clk_register("clkgen_dw200_clk_vse", NULL,
+									visys_regmap, 0xa0, 5, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_DW200_CLK_DWE] = thead_gate_clk_register("clkgen_dw200_clk_dwe", NULL,
+									visys_regmap, 0xa0, 4, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP0_CLK] = thead_gate_clk_register("clkgen_isp_clk_0", NULL,
+									visys_regmap, 0xa4, 31, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP1_CLK] = thead_gate_clk_register("clkgen_isp_clk_1", NULL,
+									visys_regmap, 0xa4, 30, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP_RY_CCLK] = thead_gate_clk_register("clkgen_isp_ry_cclk", NULL,
+									visys_regmap, 0xa0, 21, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP1_PIXELCLK] = thead_gate_clk_register("clkgen_isp1_pixelclk", NULL,
+									visys_regmap, 0xa4, 28, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP0_PIXELCLK] = thead_gate_clk_register("clkgen_isp0_pixelclk", NULL,
+									visys_regmap, 0xa4, 29, GATE_NOT_SHARED, NULL, dev);
+	gates[LIGHT_CLKGEN_ISP1_HCLK] = thead_gate_clk_register("clkgen_isp1_hclk", NULL,
+									visys_regmap, 0xa0, 1, GATE_SHARED, &share_cnt_isp0_hclk_en, dev);
+	gates[LIGHT_CLKGEN_ISP0_HCLK] = thead_gate_clk_register("clkgen_isp0_hclk", NULL,
+									visys_regmap, 0xa0, 1, GATE_SHARED, &share_cnt_isp0_hclk_en, dev);
+	gates[LIGHT_CLKGEN_ISP1_ACLK] = thead_gate_clk_register("clkgen_isp1_aclk", NULL,
+									visys_regmap, 0xa0, 3, GATE_SHARED, &share_cnt_isp0_aclk_en, dev);
+	gates[LIGHT_CLKGEN_ISP0_ACLK] = thead_gate_clk_register("clkgen_isp0_aclk", NULL,
+									visys_regmap, 0xa0, 3, GATE_SHARED, &share_cnt_isp0_aclk_en, dev);
+
+	clk_gate_data.clks = gates;
+	clk_gate_data.clk_num = ARRAY_SIZE(gates);
+
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_gate_data);
+	if (ret < 0) {
+		dev_err(dev, "failed to register gate clks for light visys\n");
+		goto unregister_clks;
+	}
+
+	dev_info(dev, "succeed to register visys gate clock provider\n");
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(gates, ARRAY_SIZE(gates));
+	return ret;
+}
+
+static const struct of_device_id visys_clk_gate_of_match[] = {
+	{ .compatible = "thead,visys-gate-controller" },
+	{ /* sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, visys_clk_gate_of_match);
+
+static struct platform_driver light_visys_clk_driver = {
+	.probe = light_visys_clk_probe,
+	.driver = {
+		.name = "visys-clk-gate-provider",
+		.of_match_table = of_match_ptr(visys_clk_gate_of_match),
+	},
+};
+
+module_platform_driver(light_visys_clk_driver);
+MODULE_AUTHOR("wei.liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Fullmask visys clock gate provider");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/thead/gate/vosys-gate.c b/drivers/clk/thead/gate/vosys-gate.c
new file mode 100644
index 000000000000..e53ba1a3e763
--- /dev/null
+++ b/drivers/clk/thead/gate/vosys-gate.c
@@ -0,0 +1,111 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-fm-ap-clock.h>
+#include <dt-bindings/clock/light-vosys.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+#include "../clk.h"
+
+static struct clk *gates[LIGHT_CLKGEN_VOSYS_CLK_END];
+static struct clk_onecell_data clk_gate_data;
+
+static int light_vosys_clk_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	void __iomem *gate_base;
+	int ret;
+
+	gate_base = devm_platform_ioremap_resource(pdev, 0);
+	if (WARN_ON(IS_ERR(gate_base)))
+		return PTR_ERR(gate_base);
+
+	/* we assume that the gate clock is a root clock  */
+	gates[LIGHT_CLKGEN_AXI4_VO_PCLK] = thead_clk_light_gate("clkgen_axi4_vo_pclk", NULL,
+								gate_base + 0x50, 22);
+	gates[LIGHT_CLKGEN_IOPMP_VOSYS_DPU_PCLK] = thead_clk_light_gate("clkgen_iopmp_dpu_pclk", NULL,
+								gate_base + 0x50, 23);
+	gates[LIGHT_CLKGEN_IOPMP_VOSYS_DPU1_PCLK] = thead_clk_light_gate("clkgen_iopmp_dpu1_pclk", NULL,
+								gate_base + 0x50, 24);
+	gates[LIGHT_CLKGEN_IOPMP_VOSYS_GPU_PCLK] = thead_clk_light_gate("clkgen_iopmp_gpu_pclk", NULL,
+								gate_base + 0x50, 25);
+	gates[LIGHT_CLKGEN_HDMI_PCLK] = thead_clk_light_gate("clkgen_hdmi_pclk", NULL, gate_base + 0x50, 11);
+	gates[LIGHT_CLKGEN_MIPIDSI0_PCLK] = thead_clk_light_gate("clkgen_mipidsi0_pclk", NULL,
+								  gate_base + 0x50, 13);
+	gates[LIGHT_CLKGEN_MIPIDSI1_PCLK] = thead_clk_light_gate("clkgen_mipidsi1_pclk", NULL,
+								  gate_base + 0x50, 14);
+	gates[LIGHT_CLKGEN_AXI4_VO_ACLK] = thead_clk_light_gate("clkgen_axi4_vo_aclk", NULL,
+								  gate_base + 0x50, 0);
+	gates[LIGHT_CLKGEN_IOPMP_GPU_ACLK] = thead_clk_light_gate("clkgen_iopmp_gpu_aclk", NULL,
+								  gate_base + 0x50, 29);
+	gates[LIGHT_CLKGEN_IOPMP_DPU_ACLK] = thead_clk_light_gate("clkgen_iopmp_dpu_aclk", NULL,
+								  gate_base + 0x50, 28);
+	gates[LIGHT_CLKGEN_IOPMP_DPU1_ACLK] = thead_clk_light_gate("clkgen_iopmp_dpu1_aclk", NULL,
+								  gate_base + 0x50, 27);
+	gates[LIGHT_CLKGEN_X2H_DPU_ACLK] = thead_clk_light_gate("clkgen_x2h_dpu_aclk", NULL, gate_base + 0x50, 21);
+	gates[LIGHT_CLKGEN_X2H_DPU1_ACLK] = thead_clk_light_gate("clkgen_x2h_dpu1_aclk", NULL, gate_base + 0x50, 20);
+	gates[LIGHT_CLKGEN_MIPIDSI0_PIXCLK] = thead_clk_light_gate("clkgen_mipidsi0_pixclk", NULL, gate_base + 0x50, 30);
+	gates[LIGHT_CLKGEN_HDMI_PIXCLK] = thead_clk_light_gate("clkgen_hdmi_pixclk", NULL, gate_base + 0x54, 0);
+	gates[LIGHT_CLKGEN_MIPIDSI1_PIXCLK] = thead_clk_light_gate("clkgen_mipidsi1_pixclk", NULL, gate_base + 0x50, 31);
+	gates[LIGHT_CLKGEN_HDMI_SFR_CLK] = thead_clk_light_gate("clkgen_hdmi_sfr_clk", NULL, gate_base + 0x50, 10);
+	gates[LIGHT_CLKGEN_HDMI_CEC_CLK] = thead_clk_light_gate("clkgen_hdmi_cec_cclk", NULL, gate_base + 0x50, 12);
+	gates[LIGHT_CLKGEN_HDMI_I2S_CLK] = thead_clk_light_gate("clkgen_hdmi_i2s_clk", NULL, gate_base + 0x50, 19);
+	gates[LIGHT_CLKGEN_MIPIDSI0_CFG_CLK] = thead_clk_light_gate("clkgen_mipidsi0_cfg_clk", NULL, gate_base + 0x50, 15);
+	gates[LIGHT_CLKGEN_MIPIDSI1_CFG_CLK] = thead_clk_light_gate("clkgen_mipidsi1_cfg_clk", NULL, gate_base + 0x50, 16);
+	gates[LIGHT_CLKGEN_MIPIDSI0_REFCLK] = thead_clk_light_gate("clkgen_mipidsi0_refclk", NULL, gate_base + 0x50, 17);
+	gates[LIGHT_CLKGEN_MIPIDSI1_REFCLK] = thead_clk_light_gate("clkgen_mipidsi1_refclk", NULL, gate_base + 0x50, 18);
+	gates[LIGHT_CLKGEN_GPU_CORE_CLK] = thead_clk_light_gate("clkgen_gpu_core_clk", NULL, gate_base + 0x50, 3);
+	gates[LIGHT_CLKGEN_GPU_CFG_ACLK] = thead_clk_light_gate("clkgen_gpu_cfg_aclk", NULL, gate_base + 0x50, 4);
+	gates[LIGHT_CLKGEN_DPU_HCLK] = thead_clk_light_gate("clkgen_dpu_hclk", NULL, gate_base + 0x50, 7);
+	gates[LIGHT_CLKGEN_DPU_ACLK] = thead_clk_light_gate("clkgen_dpu_aclk", NULL, gate_base + 0x50, 8);
+	gates[LIGHT_CLKGEN_DPU_CCLK] = thead_clk_light_gate("clkgen_dpu_cclk", NULL, gate_base + 0x50, 9);
+	gates[LIGHT_CLKGEN_DPU_PIXCLK0] = thead_clk_light_gate("clkgen_dpu_pixclk0", NULL, gate_base + 0x50, 5);
+	gates[LIGHT_CLKGEN_DPU_PIXCLK1] = thead_clk_light_gate("clkgen_dpu_pixclk1", NULL, gate_base + 0x50, 6);
+
+	clk_gate_data.clks = gates;
+	clk_gate_data.clk_num = ARRAY_SIZE(gates);
+
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_gate_data);
+	if (ret < 0) {
+		dev_err(dev, "failed to register gate clks for light vosys\n");
+		goto unregister_clks;
+	}
+
+	dev_info(dev, "succeed to register vosys gate clock provider\n");
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(gates, ARRAY_SIZE(gates));
+	return ret;
+}
+
+static const struct of_device_id vosys_clk_gate_of_match[] = {
+	{ .compatible = "thead,vosys-gate-controller" },
+	{ /* sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, vosys_clk_gate_of_match);
+
+static struct platform_driver light_vosys_clk_driver = {
+	.probe = light_vosys_clk_probe,
+	.driver = {
+		.name = "vosys-clk-gate-provider",
+		.of_match_table = of_match_ptr(vosys_clk_gate_of_match),
+	},
+};
+
+module_platform_driver(light_vosys_clk_driver);
+MODULE_AUTHOR("wei.liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Fullmask vosys clock gate provider");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/thead/gate/vpsys-gate.c b/drivers/clk/thead/gate/vpsys-gate.c
new file mode 100644
index 000000000000..78613188da70
--- /dev/null
+++ b/drivers/clk/thead/gate/vpsys-gate.c
@@ -0,0 +1,94 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/clock/light-fm-ap-clock.h>
+#include <dt-bindings/clock/light-vpsys.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/types.h>
+#include "../clk.h"
+
+static struct clk *gates[LIGHT_VPSYS_CLK_END];
+static struct clk_onecell_data clk_gate_data;
+
+static u32 share_cnt_g2d_clk_en;
+static u32 share_cnt_fce_clk_en;
+
+static int light_vpsys_clk_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	void __iomem *gate_base;
+	int ret;
+
+	gate_base = devm_platform_ioremap_resource(pdev, 0);
+	if (WARN_ON(IS_ERR(gate_base)))
+		return PTR_ERR(gate_base);
+
+	/* we assume that the gate clock is a root clock  */
+	gates[LIGHT_VPSYS_G2D_PCLK] = thead_clk_light_gate_shared("clkgen_vpsys_g2d_pclk", NULL,
+								   gate_base + 0x20, 3, &share_cnt_g2d_clk_en);
+	gates[LIGHT_VPSYS_G2D_ACLK] = thead_clk_light_gate_shared("clkgen_vpsys_g2d_aclk", NULL,
+								   gate_base + 0x20, 3, &share_cnt_g2d_clk_en);
+	gates[LIGHT_VPSYS_G2D_CCLK] = thead_clk_light_gate_shared("clkgen_vpsys_g2d_cclk", NULL,
+								   gate_base + 0x20, 3, &share_cnt_g2d_clk_en);
+
+
+	gates[LIGHT_VPSYS_FCE_PCLK] = thead_clk_light_gate_shared("clkgen_vpsys_fce_pclk", NULL,
+								   gate_base + 0x20, 2, &share_cnt_fce_clk_en);
+	gates[LIGHT_VPSYS_FCE_ACLK] = thead_clk_light_gate_shared("clkgen_vpsys_fce_aclk", NULL,
+								   gate_base + 0x20, 2, &share_cnt_fce_clk_en);
+
+	gates[LIGHT_VPSYS_VDEC_ACLK] = thead_clk_light_gate("clkgen_vdec_aclk", NULL, gate_base + 0x20, 4);
+	gates[LIGHT_VPSYS_VDEC_CCLK] = thead_clk_light_gate("clkgen_vdec_cclk", NULL, gate_base + 0x20, 5);
+	gates[LIGHT_VPSYS_VDEC_PCLK] = thead_clk_light_gate("clkgen_vdec_pclk", NULL, gate_base + 0x20, 6);
+
+	gates[LIGHT_VPSYS_VENC_CCLK] = thead_clk_light_gate("clkgen_venc_cclk", NULL, gate_base + 0x20, 8);
+	gates[LIGHT_VPSYS_VENC_PCLK] = thead_clk_light_gate("clkgen_venc_pclk", NULL, gate_base + 0x20, 9);
+	gates[LIGHT_VPSYS_VENC_ACLK] = thead_clk_light_gate("clkgen_venc_aclk", NULL, gate_base + 0x20, 7);
+
+	clk_gate_data.clks = gates;
+	clk_gate_data.clk_num = ARRAY_SIZE(gates);
+
+	ret = of_clk_add_provider(np, of_clk_src_onecell_get, &clk_gate_data);
+	if (ret < 0) {
+		dev_err(dev, "failed to register gate clks for light vpsys\n");
+		goto unregister_clks;
+	}
+
+	dev_info(dev, "succeed to register vpsys gate clock provider\n");
+
+	return 0;
+
+unregister_clks:
+	thead_unregister_clocks(gates, ARRAY_SIZE(gates));
+	return ret;
+}
+
+static const struct of_device_id vpsys_clk_gate_of_match[] = {
+	{ .compatible = "thead,vpsys-gate-controller" },
+	{ /* sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, vpsys_clk_gate_of_match);
+
+static struct platform_driver light_vpsys_clk_driver = {
+	.probe = light_vpsys_clk_probe,
+	.driver = {
+		.name = "vpsys-clk-gate-provider",
+		.of_match_table = of_match_ptr(vpsys_clk_gate_of_match),
+	},
+};
+
+module_platform_driver(light_vpsys_clk_driver);
+MODULE_AUTHOR("wei.liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Fullmask vpsys clock gate provider");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clocksource/dw_apb_timer_of.c b/drivers/clocksource/dw_apb_timer_of.c
index 3245eb0c602d..1ef476b80044 100644
--- a/drivers/clocksource/dw_apb_timer_of.c
+++ b/drivers/clocksource/dw_apb_timer_of.c
@@ -107,9 +107,30 @@ static int __init add_clockevent(struct device_node *event_timer)
 	return 0;
 }
 
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+void __iomem *sched_io_base;
+EXPORT_SYMBOL_GPL(sched_io_base);
+static struct dw_apb_clocksource *cs_g;
+#else
 static void __iomem *sched_io_base;
+#endif
 static u32 sched_rate;
 
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+u64 dw_timer_read_counter(void)
+{
+	return ~readl_relaxed(sched_io_base);
+}
+EXPORT_SYMBOL_GPL(dw_timer_read_counter);
+
+void dw_cs_get_mult_shift(u32 *mult, u32 *shift)
+{
+	*mult = cs_g->cs.mult;
+	*shift = cs_g->cs.shift;
+}
+EXPORT_SYMBOL_GPL(dw_cs_get_mult_shift);
+#endif
+
 static int __init add_clocksource(struct device_node *source_timer)
 {
 	void __iomem *iobase;
@@ -135,6 +156,9 @@ static int __init add_clocksource(struct device_node *source_timer)
 	 */
 	sched_io_base = iobase + 0x04;
 	sched_rate = rate;
+#ifdef CONFIG_SOPHGO_MULTI_CHIP_CLOCK_SYNC
+	cs_g = cs;
+#endif
 
 	return 0;
 }
diff --git a/drivers/cpufreq/Kconfig b/drivers/cpufreq/Kconfig
index d1fdea27eb0d..4c67dd5991d1 100644
--- a/drivers/cpufreq/Kconfig
+++ b/drivers/cpufreq/Kconfig
@@ -346,5 +346,15 @@ config QORIQ_CPUFREQ
 	  This adds the CPUFreq driver support for Freescale QorIQ SoCs
 	  which are capable of changing the CPU's frequency dynamically.
 
+config RISCV_THEAD_LIGHT_CPUFREQ
+	tristate "CPU frequency scaling driver for Thead light SoCs"
+	depends on OF && COMMON_CLK
+	select CLK_LIGHT
+	select PM_OPP
+	help
+	  This adds the CPUFreq driver support for Thead light SoCs
+	  which are capable of changing the CPU's frequency dynamically.
+
+
 endif
 endmenu
diff --git a/drivers/cpufreq/Makefile b/drivers/cpufreq/Makefile
index f9c1c9012ce7..4c87824d45eb 100644
--- a/drivers/cpufreq/Makefile
+++ b/drivers/cpufreq/Makefile
@@ -110,3 +110,4 @@ obj-$(CONFIG_SPARC_US2E_CPUFREQ)	+= sparc-us2e-cpufreq.o
 obj-$(CONFIG_SPARC_US3_CPUFREQ)		+= sparc-us3-cpufreq.o
 obj-$(CONFIG_SW64_CPUFREQ)		+= sw64_cpufreq.o
 obj-$(CONFIG_SW64_CPUFREQ_DEBUGFS)	+= sw64_cpufreq_debugfs.o
+obj-$(CONFIG_RISCV_THEAD_LIGHT_CPUFREQ)  += light-mpw-cpufreq.o
diff --git a/drivers/cpufreq/light-mpw-cpufreq.c b/drivers/cpufreq/light-mpw-cpufreq.c
new file mode 100644
index 000000000000..72f8b348778c
--- /dev/null
+++ b/drivers/cpufreq/light-mpw-cpufreq.c
@@ -0,0 +1,491 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/clk.h>
+#include <linux/cpu.h>
+#include <linux/cpufreq.h>
+#include <linux/delay.h>
+#include <linux/err.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/pm_opp.h>
+#include <linux/platform_device.h>
+#include <linux/reboot.h>
+#include <linux/regulator/consumer.h>
+#include <linux/suspend.h>
+#include <linux/clk-provider.h>
+#include <linux/smp.h>
+#include <linux/kernel.h>
+#include <linux/notifier.h>
+
+extern struct atomic_notifier_head panic_notifier_list;
+
+static DEFINE_MUTEX(cpufreq_lock);
+
+bool cpufreq_denied = false;
+
+struct regulator *dvdd_cpu_reg;
+struct regulator *dvddm_cpu_reg;
+
+enum LIGHT_MPW_CPUFREQ_CLKS {
+	LIGHT_C910_CCLK,
+	LIGHT_C910_CCLK_I0,
+	LIGHT_CPU_PLL1_FOUTPOSTDIV,
+	LIGHT_CPU_PLL0_FOUTPOSTDIV,
+};
+
+#define LIGHT_MPW_CPUFREQ_CLK_NUM	4
+#define LIGHT_CPUFREQ_THRE		2000000
+#define LIGHT_C910_BUS_CLK_SYNC		BIT(11)
+#define LIGHT_C910_BUS_CLK_RATIO_MASK	0x700
+#define LIGHT_C910_BUS_CLK_DIV_RATIO_2	0x100
+#define LIGHT_C910_BUS_CLK_DIV_RATIO_3	0x200
+
+static int num_clks;
+static struct clk_bulk_data clks[] = {
+	{ .id = "c910_cclk" },
+	{ .id = "c910_cclk_i0" },
+	{ .id = "cpu_pll1_foutpostdiv" },
+	{ .id = "cpu_pll0_foutpostdiv" },
+};
+
+static struct device *cpu_dev;
+static struct cpufreq_frequency_table *freq_table;
+static unsigned int max_freq;
+static unsigned int transition_latency;
+static void __iomem *ap_sys_reg;
+static bool light_dvfs_sv = false;
+
+static u32 *light_dvddm_volt;
+static u32 soc_opp_count = 0;
+
+static int light_set_target(struct cpufreq_policy *policy, unsigned int index)
+{
+	struct dev_pm_opp *opp;
+	unsigned long freq_hz;
+	int volt, volt_old;
+	unsigned int old_freq, new_freq;
+	int ret;
+	u32 val;
+	u32 re_modify_bus_freq = 0;
+
+	mutex_lock(&cpufreq_lock);
+
+	if (cpufreq_denied) {
+		dev_emerg(cpu_dev, "Denied to set cpu frequency temporarily on reboot\n");
+		mutex_unlock(&cpufreq_lock);
+		return 0;
+	}
+	new_freq = freq_table[index].frequency;
+	freq_hz = new_freq * 1000;
+	old_freq = policy->cur;
+
+	opp = dev_pm_opp_find_freq_ceil(cpu_dev, &freq_hz);
+	if (IS_ERR(opp)) {
+		dev_err(cpu_dev, "failed to find OPP for %ld\n", freq_hz);
+		mutex_unlock(&cpufreq_lock);
+		return PTR_ERR(opp);
+	}
+
+	volt = dev_pm_opp_get_voltage(opp);
+	dev_pm_opp_put(opp);
+
+	volt_old = regulator_get_voltage(dvdd_cpu_reg);
+	if (volt_old < 0) {
+		dev_err(cpu_dev, "failed to get cpu voltage\n");
+		mutex_unlock(&cpufreq_lock);
+		return volt_old;
+	}
+
+	dev_dbg(cpu_dev, "%u MHz, %d mV --> %u MHz, %d mV\n",
+		old_freq / 1000, volt_old / 1000,
+		new_freq / 1000, volt / 1000);
+
+	/* change AXI bus clock ratio to match: BUS_CLK = CPU_CCLK/ratio <= 750MHz */
+	val = readl(ap_sys_reg);
+	if (new_freq > LIGHT_CPUFREQ_THRE) {
+		val &= ~LIGHT_C910_BUS_CLK_RATIO_MASK;
+		val |= LIGHT_C910_BUS_CLK_DIV_RATIO_3;
+	} else {
+		val &= ~LIGHT_C910_BUS_CLK_RATIO_MASK;
+
+		if (old_freq > LIGHT_CPUFREQ_THRE) {
+			re_modify_bus_freq = 1;
+			val |= LIGHT_C910_BUS_CLK_DIV_RATIO_3;
+		}else
+			val |= LIGHT_C910_BUS_CLK_DIV_RATIO_2;
+	}
+
+	writel(val, ap_sys_reg);
+	val &= ~LIGHT_C910_BUS_CLK_SYNC;
+	writel(val, ap_sys_reg);
+	udelay(1);
+	val |= LIGHT_C910_BUS_CLK_SYNC;
+	writel(val, ap_sys_reg);
+	udelay(1);
+
+	/* scaling up?  scale voltage before frequency */
+	if (new_freq > old_freq && !light_dvfs_sv) {
+		ret = regulator_set_voltage_tol(dvddm_cpu_reg, light_dvddm_volt[index], 0);
+		if (ret) {
+			dev_err(cpu_dev, "failed to scale vddsoc up: %d\n", ret);
+			mutex_unlock(&cpufreq_lock);
+			return ret;
+		}
+		ret = regulator_set_voltage_tol(dvdd_cpu_reg, volt, 0);
+		if (ret) {
+			dev_err(cpu_dev,
+				"failed to scale vddarm up: %d\n", ret);
+			mutex_unlock(&cpufreq_lock);
+			return ret;
+		}
+	}
+
+	if (!strcmp(__clk_get_name(clk_get_parent(clks[LIGHT_C910_CCLK].clk)),
+	    __clk_get_name(clks[LIGHT_C910_CCLK_I0].clk))) {
+		clk_prepare_enable(clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk);
+		clk_set_rate(clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk, new_freq * 1000);
+		ret = clk_set_parent(clks[LIGHT_C910_CCLK].clk, clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk);
+		udelay(1);
+		if (ret)
+			clk_disable_unprepare(clks[LIGHT_CPU_PLL0_FOUTPOSTDIV].clk);
+	} else {
+		clk_prepare_enable(clks[LIGHT_CPU_PLL0_FOUTPOSTDIV].clk);
+		clk_set_rate(clks[LIGHT_CPU_PLL0_FOUTPOSTDIV].clk, new_freq * 1000);
+		ret  = clk_set_parent(clks[LIGHT_C910_CCLK].clk, clks[LIGHT_C910_CCLK_I0].clk);
+		udelay(1);
+		if (ret)
+			clk_disable_unprepare(clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk);
+	}
+
+	/*add delay for clk-switch*/
+	udelay(1);
+
+	/* Ensure the c910_cclk clock divider is what we expect */
+	ret = clk_set_rate(clks[LIGHT_C910_CCLK].clk, new_freq * 1000);
+	if (ret) {
+		int ret1;
+
+		dev_err(cpu_dev, "failed to set clock rate: %d\n", ret);
+		ret1 = regulator_set_voltage_tol(dvdd_cpu_reg, volt_old, 0);
+		if (ret1)
+			dev_err(cpu_dev, "failed to restore dvdd_cpu voltage: %d\n", ret1);
+		mutex_unlock(&cpufreq_lock);
+		return ret;
+	}
+
+	/* scaling down?  scale voltage after frequency */
+	if (new_freq < old_freq && !light_dvfs_sv) {
+		ret = regulator_set_voltage_tol(dvddm_cpu_reg, light_dvddm_volt[index], 0);
+		if (ret)
+			dev_err(cpu_dev, "failed to scale dvddm down: %d\n", ret);
+		ret = regulator_set_voltage_tol(dvdd_cpu_reg, volt, 0);
+		if (ret)
+			dev_err(cpu_dev, "failed to scale dvdd_cpu down: %d\n", ret);
+	}
+
+	val = readl(ap_sys_reg);
+	if (re_modify_bus_freq) {
+		val &= ~LIGHT_C910_BUS_CLK_RATIO_MASK;
+		val |= LIGHT_C910_BUS_CLK_DIV_RATIO_2;
+
+		writel(val, ap_sys_reg);
+		val &= ~LIGHT_C910_BUS_CLK_SYNC;
+		writel(val, ap_sys_reg);
+		udelay(1);
+		val |= LIGHT_C910_BUS_CLK_SYNC;
+		writel(val, ap_sys_reg);
+		udelay(1);
+	}
+
+	mutex_unlock(&cpufreq_lock);
+
+	return 0;
+}
+
+static int light_cpufreq_init(struct cpufreq_policy *policy)
+{
+	policy->clk = clks[LIGHT_C910_CCLK].clk;
+	policy->cur = clk_get_rate(policy->clk) / 1000;
+	cpufreq_generic_init(policy, freq_table, transition_latency);
+	policy->suspend_freq = max_freq;
+	dev_pm_opp_of_register_em(cpu_dev, policy->cpus);
+
+	return 0;
+}
+
+static int light_cpufreq_reboot_notifier(struct notifier_block *this,
+					 unsigned long event, void *ptr)
+{
+	mutex_lock(&cpufreq_lock);
+	cpufreq_denied = true;
+	mutex_unlock(&cpufreq_lock);
+
+	return NOTIFY_DONE;
+}
+
+static struct notifier_block cpufreq_reboot_notifier = {
+	.notifier_call = light_cpufreq_reboot_notifier,
+};
+
+static struct cpufreq_driver light_cpufreq_driver = {
+	.flags = CPUFREQ_NEED_INITIAL_FREQ_CHECK |
+		 CPUFREQ_IS_COOLING_DEV,
+	.verify = cpufreq_generic_frequency_table_verify,
+	.target_index = light_set_target,
+	.get = cpufreq_generic_get,
+	.init = light_cpufreq_init,
+	.name = "light-cpufreq",
+	.attr = cpufreq_generic_attr,
+	.suspend = cpufreq_generic_suspend,
+};
+
+static int light_cpufreq_pm_notify(struct notifier_block *nb,
+	unsigned long event, void *dummy)
+{
+	switch (event) {
+	case PM_SUSPEND_PREPARE:
+		/* TBD */
+		break;
+	case PM_POST_SUSPEND:
+		/* TBD */
+		break;
+	default:
+		break;
+	}
+
+	return NOTIFY_OK;
+}
+
+static struct notifier_block light_cpufreq_pm_notifier = {
+	.notifier_call = light_cpufreq_pm_notify,
+};
+
+/*
+ * Set CPU PLL1's frequency as minimum on panic
+ */
+static int panic_cpufreq_notifier_call(struct notifier_block *nb,
+				 unsigned long action, void *data)
+{
+	int cpu = smp_processor_id();
+	struct cpufreq_policy *policy = cpufreq_cpu_get(cpu);
+
+	pr_info("enter panic_cpufreq_notifier_call\n");
+
+	/*
+	 * set CPU PLL1's frequency as minimum to compatible voltage
+	 * becarefull if the PLL1 is serving the cpu core, swith to PLL0 first
+	 */
+	if (strcmp(__clk_get_name(clk_get_parent(clks[LIGHT_C910_CCLK].clk)),
+		__clk_get_name(clks[LIGHT_C910_CCLK_I0].clk))) {
+		pr_debug("[%s,%d]\n", __func__, __LINE__);
+		clk_prepare_enable(clks[LIGHT_CPU_PLL0_FOUTPOSTDIV].clk);
+		clk_set_rate(clks[LIGHT_CPU_PLL0_FOUTPOSTDIV].clk, policy->min * 1000);
+		udelay(1);
+		clk_set_parent(clks[LIGHT_C910_CCLK].clk, clks[LIGHT_C910_CCLK_I0].clk);
+
+		pr_debug("[%s,%d]\n", __func__, __LINE__);
+	}
+
+	pr_debug("[%s,%d]\n", __func__, __LINE__);
+	/*
+	 * since the clk driver will use PLL1 as the default clock source,
+	 * in order to compatible voltage which is unpredictable we should
+	 * set the CPU PLL1's frequency as minimum in advance, otherwise the
+	 * system may crash in crash kernel stage.
+	 */
+	clk_prepare_enable(clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk);
+	clk_set_rate(clks[LIGHT_CPU_PLL1_FOUTPOSTDIV].clk, policy->min * 1000);
+	udelay(1);
+
+	pr_info("finish to execute cpufreq notifier callback on panic\n");
+
+	return 0;
+}
+
+static struct notifier_block panic_cpufreq_notifier = {
+	.notifier_call = panic_cpufreq_notifier_call,
+};
+
+static int light_cpufreq_probe(struct platform_device *pdev)
+{
+	struct device_node *np;
+	int num, ret;
+	const struct property *prop;
+	const __be32 *val;
+	u32 nr, i, j;
+
+        np = of_find_compatible_node(NULL, NULL, "thead,light_sys_reg");
+	if (!np)
+		return -ENOENT;
+	ap_sys_reg = of_iomap(np, 0);
+	WARN_ON(!ap_sys_reg);
+
+	cpu_dev = get_cpu_device(0);
+	if (!cpu_dev) {
+		pr_err("failed to get cpu0 device\n");
+		return -ENODEV;
+	}
+
+	np = of_node_get(cpu_dev->of_node);
+	if (!np) {
+		dev_err(cpu_dev, "failed to find cpu0 node\n");
+		return -ENOENT;
+	}
+
+	num_clks = LIGHT_MPW_CPUFREQ_CLK_NUM;
+	ret = clk_bulk_get(cpu_dev, num_clks, clks);
+	if (ret)
+		goto put_node;
+
+	dvdd_cpu_reg = regulator_get(cpu_dev, "dvdd");
+	dvddm_cpu_reg = regulator_get(cpu_dev, "dvddm");
+	if (PTR_ERR(dvdd_cpu_reg) == -EPROBE_DEFER ||
+	    PTR_ERR(dvddm_cpu_reg) == -EPROBE_DEFER) {
+		ret = -EPROBE_DEFER;
+		dev_dbg(cpu_dev, "regulators not ready, defer\n");
+		goto put_reg;
+	}
+
+	if (IS_ERR(dvdd_cpu_reg) || IS_ERR(dvddm_cpu_reg)) {
+		dev_err(cpu_dev, "failed to get regulators\n");
+		ret = -ENOENT;
+		goto put_reg;
+	}
+
+	ret = dev_pm_opp_of_add_table(cpu_dev);
+	if (ret < 0) {
+		dev_err(cpu_dev, "failed to init OPP table: %d\n", ret);
+		goto put_reg;
+	}
+
+	num = dev_pm_opp_get_opp_count(cpu_dev);
+	if (num < 0) {
+		ret = num;
+		dev_err(cpu_dev, "no OPP table is found: %d\n", ret);
+		goto out_free_opp;
+	}
+
+	ret = dev_pm_opp_init_cpufreq_table(cpu_dev, &freq_table);
+	if (ret) {
+		dev_err(cpu_dev, "failed to init cpufreq table: %d\n", ret);
+		goto out_free_opp;
+	}
+
+	/* Make light_dvddm_volt array's size same as dvdd opp number */
+	light_dvddm_volt = devm_kcalloc(cpu_dev, num, sizeof(*light_dvddm_volt),
+				     GFP_KERNEL);
+	if (light_dvddm_volt == NULL) {
+		ret = -ENOMEM;
+		goto free_freq_table;
+	}
+
+	if (of_get_property(np, "dvfs_sv", NULL))
+		light_dvfs_sv = true;
+	else
+		light_dvfs_sv = false;
+
+	prop = of_find_property(np, "light,dvddm-operating-points", NULL);
+	if (!prop || !prop->value)
+		goto soc_opp_out;
+
+	nr = prop->length / sizeof(u32);
+	if (nr % 2 || (nr / 2) < num)
+		goto soc_opp_out;
+
+	for (j = 0; j < num; j++) {
+		val = prop->value;
+		for (i = 0; i < nr / 2; i++) {
+			unsigned long freq = be32_to_cpup(val++);
+			unsigned long volt = be32_to_cpup(val++);
+			if (freq_table[j].frequency == freq) {
+				light_dvddm_volt[soc_opp_count++] = volt;
+				break;
+			}
+		}
+	}
+
+soc_opp_out:
+	if (soc_opp_count != num)
+		dev_warn(cpu_dev, "Not find valid light,dvddm-operating-points property\n");
+
+	if (of_property_read_u32(np, "clock-latency", &transition_latency))
+		transition_latency = CPUFREQ_ETERNAL;
+
+	max_freq = freq_table[--num].frequency;
+
+	ret = cpufreq_register_driver(&light_cpufreq_driver);
+	if (ret) {
+		dev_err(cpu_dev, "failed register driver: %d\n", ret);
+		goto free_freq_table;
+	}
+
+	register_pm_notifier(&light_cpufreq_pm_notifier);
+
+	of_node_put(np);
+
+	ret = atomic_notifier_chain_register(&panic_notifier_list,
+					     &panic_cpufreq_notifier);
+	if (ret) {
+		pr_err("unable to register notifier(%d)\n", ret);
+		goto free_freq_table;
+	}
+
+	register_reboot_notifier(&cpufreq_reboot_notifier);
+
+	dev_info(cpu_dev, "finish to register cpufreq driver\n");
+
+	return 0;
+
+free_freq_table:
+	dev_pm_opp_free_cpufreq_table(cpu_dev, &freq_table);
+out_free_opp:
+	dev_pm_opp_of_remove_table(cpu_dev);
+put_reg:
+	if (!IS_ERR(dvdd_cpu_reg))
+		regulator_put(dvdd_cpu_reg);
+	if (!IS_ERR(dvddm_cpu_reg))
+		regulator_put(dvddm_cpu_reg);
+
+	clk_bulk_put(num_clks, clks);
+put_node:
+	of_node_put(np);
+
+	return ret;
+}
+
+static int light_cpufreq_remove(struct platform_device *pdev)
+{
+	cpufreq_unregister_driver(&light_cpufreq_driver);
+	dev_pm_opp_free_cpufreq_table(cpu_dev, &freq_table);
+	dev_pm_opp_of_remove_table(cpu_dev);
+	regulator_put(dvdd_cpu_reg);
+	regulator_put(dvddm_cpu_reg);
+
+	clk_bulk_put(num_clks, clks);
+
+	return 0;
+}
+
+static const struct of_device_id light_cpufreq_match[] = {
+	{ .compatible = "thead,light-mpw-cpufreq" },
+	{},
+};
+
+static struct platform_driver light_cpufreq_platdrv = {
+	.driver = {
+		.name	= "thead,light-mpw-cpufreq",
+		.of_match_table = light_cpufreq_match,
+	},
+	.probe		= light_cpufreq_probe,
+	.remove		= light_cpufreq_remove,
+};
+module_platform_driver(light_cpufreq_platdrv);
+
+MODULE_ALIAS("platform:light-cpufreq");
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light cpufreq driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/firmware/Kconfig b/drivers/firmware/Kconfig
index 9cb284a6e7a1..52f07f9c5db7 100644
--- a/drivers/firmware/Kconfig
+++ b/drivers/firmware/Kconfig
@@ -314,5 +314,6 @@ source "drivers/firmware/psci/Kconfig"
 source "drivers/firmware/smccc/Kconfig"
 source "drivers/firmware/tegra/Kconfig"
 source "drivers/firmware/xilinx/Kconfig"
+source "drivers/firmware/thead/Kconfig"
 
 endmenu
diff --git a/drivers/firmware/Makefile b/drivers/firmware/Makefile
index 28fcddcd688f..a817fe549c9f 100644
--- a/drivers/firmware/Makefile
+++ b/drivers/firmware/Makefile
@@ -38,3 +38,4 @@ obj-y				+= psci/
 obj-y				+= smccc/
 obj-y				+= tegra/
 obj-y				+= xilinx/
+obj-y				+= thead/
diff --git a/drivers/firmware/thead/Kconfig b/drivers/firmware/thead/Kconfig
new file mode 100644
index 000000000000..ad5b82dd51e8
--- /dev/null
+++ b/drivers/firmware/thead/Kconfig
@@ -0,0 +1,18 @@
+# SPDX-License-Identifier: GPL-2.0-only
+config LIGHT_AON
+	bool "Thead Light Aon Protocol driver"
+	depends on THEAD_LIGHT_MBOX
+	default y
+	help
+	  Thead light Aon is a low-level system function which runs a dedicated
+	  thead riscv E902 core to provide power, clock and resource management.
+
+	  This driver manages the IPC interface between host cpu liks thead
+	  and the Aon firmware running on thead riscv E902 core.
+
+config LIGHT_AON_PD
+	bool "Thead Light Aon Power Domain driver"
+	depends on LIGHT_AON
+	select PM_GENERIC_DOMAINS if PM
+	help
+	  The Aon power domain virtual driver.
diff --git a/drivers/firmware/thead/Makefile b/drivers/firmware/thead/Makefile
new file mode 100644
index 000000000000..6bd2afe817ef
--- /dev/null
+++ b/drivers/firmware/thead/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier: GPL-2.0
+obj-$(CONFIG_LIGHT_AON)	+= light_aon.o light_aon_misc.o light_aon_test.o
+obj-$(CONFIG_LIGHT_AON_PD) += light_aon_pd.o
diff --git a/drivers/firmware/thead/light_aon.c b/drivers/firmware/thead/light_aon.c
new file mode 100644
index 000000000000..5af7de821e76
--- /dev/null
+++ b/drivers/firmware/thead/light_aon.c
@@ -0,0 +1,261 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/err.h>
+#include <linux/firmware/thead/ipc.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/kernel.h>
+#include <linux/mailbox_client.h>
+#include <linux/module.h>
+#include <linux/mutex.h>
+#include <linux/of_platform.h>
+#include <linux/platform_device.h>
+
+/* wait for response for 3000ms instead of 300ms (fix me pls)*/
+#define MAX_RX_TIMEOUT		(msecs_to_jiffies(3000))
+#define MAX_TX_TIMEOUT		(msecs_to_jiffies(500))
+
+struct light_aon_chan {
+	struct light_aon_ipc *aon_ipc;
+
+	struct mbox_client cl;
+	struct mbox_chan *ch;
+	struct completion tx_done;
+};
+
+struct light_aon_ipc {
+	struct light_aon_chan chans;
+	struct device *dev;
+	struct mutex lock;
+	struct completion done;
+	u32 *msg;
+};
+
+/*
+ * This type is used to indicate error response for most functions.
+ */
+enum light_aon_error_codes {
+	LIGHT_AON_ERR_NONE = 0,	/* Success */
+	LIGHT_AON_ERR_VERSION = 1,	/* Incompatible API version */
+	LIGHT_AON_ERR_CONFIG = 2,	/* Configuration error */
+	LIGHT_AON_ERR_PARM = 3,	/* Bad parameter */
+	LIGHT_AON_ERR_NOACCESS = 4,	/* Permission error (no access) */
+	LIGHT_AON_ERR_LOCKED = 5,	/* Permission error (locked) */
+	LIGHT_AON_ERR_UNAVAILABLE = 6,	/* Unavailable (out of resources) */
+	LIGHT_AON_ERR_NOTFOUND = 7,	/* Not found */
+	LIGHT_AON_ERR_NOPOWER = 8,	/* No power */
+	LIGHT_AON_ERR_IPC = 9,		/* Generic IPC error */
+	LIGHT_AON_ERR_BUSY = 10,	/* Resource is currently busy/active */
+	LIGHT_AON_ERR_FAIL = 11,	/* General I/O failure */
+	LIGHT_AON_ERR_LAST
+};
+
+static int light_aon_linux_errmap[LIGHT_AON_ERR_LAST] = {
+	0,	 /* LIGHT_AON_ERR_NONE */
+	-EINVAL, /* LIGHT_AON_ERR_VERSION */
+	-EINVAL, /* LIGHT_AON_ERR_CONFIG */
+	-EINVAL, /* LIGHT_AON_ERR_PARM */
+	-EACCES, /* LIGHT_AON_ERR_NOACCESS */
+	-EACCES, /* LIGHT_AON_ERR_LOCKED */
+	-ERANGE, /* LIGHT_AON_ERR_UNAVAILABLE */
+	-EEXIST, /* LIGHT_AON_ERR_NOTFOUND */
+	-EPERM,	 /* LIGHT_AON_ERR_NOPOWER */
+	-EPIPE,	 /* LIGHT_AON_ERR_IPC */
+	-EBUSY,	 /* LIGHT_AON_ERR_BUSY */
+	-EIO,	 /* LIGHT_AON_ERR_FAIL */
+};
+
+static struct light_aon_ipc *light_aon_ipc_handle;
+
+static inline int light_aon_to_linux_errno(int errno)
+{
+	if (errno >= LIGHT_AON_ERR_NONE && errno < LIGHT_AON_ERR_LAST)
+		return light_aon_linux_errmap[errno];
+	return -EIO;
+}
+
+/*
+ * Get the default handle used by SCU
+ */
+int light_aon_get_handle(struct light_aon_ipc **ipc)
+{
+	if (!light_aon_ipc_handle)
+		return -EPROBE_DEFER;
+
+	*ipc = light_aon_ipc_handle;
+	return 0;
+}
+EXPORT_SYMBOL(light_aon_get_handle);
+
+static void light_aon_tx_done(struct mbox_client *cl, void *mssg, int r)
+{
+	struct light_aon_chan *aon_chan = container_of(cl, struct light_aon_chan, cl);
+
+	complete(&aon_chan->tx_done);
+}
+
+static void light_aon_rx_callback(struct mbox_client *c, void *msg)
+{
+	struct light_aon_chan *aon_chan = container_of(c, struct light_aon_chan, cl);
+	struct light_aon_ipc *aon_ipc = aon_chan->aon_ipc;
+
+	memcpy(aon_ipc->msg, msg, LIGHT_AON_RPC_MSG_NUM * sizeof(u32));
+	dev_dbg(aon_ipc->dev, "msg head: 0x%x\n", *((u32 *)msg));
+	complete(&aon_ipc->done);
+}
+
+static int light_aon_ipc_write(struct light_aon_ipc *aon_ipc, void *msg)
+{
+	struct light_aon_rpc_msg_hdr *hdr = msg;
+	struct light_aon_chan *aon_chan;
+	u32 *data = msg;
+	int ret;
+
+	/* check size, currently it requires 7 MSG in one transfer */
+	if (hdr->size != LIGHT_AON_RPC_MSG_NUM)
+		return -EINVAL;
+
+	dev_dbg(aon_ipc->dev, "RPC SVC %u FUNC %u SIZE %u\n", hdr->svc,
+		hdr->func, hdr->size);
+
+	aon_chan = &aon_ipc->chans;
+
+	if (!wait_for_completion_timeout(&aon_chan->tx_done,
+					 MAX_TX_TIMEOUT)) {
+		dev_err(aon_ipc->dev, "tx_done timeout\n");
+		return -ETIMEDOUT;
+	}
+	reinit_completion(&aon_chan->tx_done);
+
+	ret = mbox_send_message(aon_chan->ch, data);
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+/*
+ * RPC command/response
+ */
+int light_aon_call_rpc(struct light_aon_ipc *aon_ipc, void *msg, bool have_resp)
+{
+	struct light_aon_rpc_msg_hdr *hdr;
+	int ret;
+
+	if (WARN_ON(!aon_ipc || !msg))
+		return -EINVAL;
+
+	mutex_lock(&aon_ipc->lock);
+	reinit_completion(&aon_ipc->done);
+
+	if (have_resp)
+		aon_ipc->msg = msg;
+
+	ret = light_aon_ipc_write(aon_ipc, msg);
+	if (ret < 0) {
+		dev_err(aon_ipc->dev, "RPC send msg failed: %d\n", ret);
+		goto out;
+	}
+
+	if (have_resp) {
+		if (!wait_for_completion_timeout(&aon_ipc->done,
+						 MAX_RX_TIMEOUT)) {
+			dev_err(aon_ipc->dev, "RPC send msg timeout\n");
+			mutex_unlock(&aon_ipc->lock);
+			return -ETIMEDOUT;
+		}
+
+		/* response status is stored in hdr->func field */
+		hdr = msg;
+		ret = hdr->func;
+	}
+
+out:
+	mutex_unlock(&aon_ipc->lock);
+
+	dev_dbg(aon_ipc->dev, "RPC SVC done\n");
+
+	return light_aon_to_linux_errno(ret);
+}
+EXPORT_SYMBOL(light_aon_call_rpc);
+
+static int light_aon_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct light_aon_ipc *aon_ipc;
+	struct light_aon_chan *aon_chan;
+	struct mbox_client *cl;
+	int ret;
+
+	aon_ipc = devm_kzalloc(dev, sizeof(*aon_ipc), GFP_KERNEL);
+	if (!aon_ipc)
+		return -ENOMEM;
+
+	aon_chan = &aon_ipc->chans;
+	cl = &aon_chan->cl;
+	cl->dev = dev;
+	cl->tx_block = false;
+	cl->knows_txdone = true;
+	cl->rx_callback = light_aon_rx_callback;
+
+	/* Initial tx_done completion as "done" */
+	cl->tx_done = light_aon_tx_done;
+	init_completion(&aon_chan->tx_done);
+	complete(&aon_chan->tx_done);
+
+	aon_chan->aon_ipc = aon_ipc;
+	aon_chan->ch = mbox_request_channel_byname(cl, "aon");
+	if (IS_ERR(aon_chan->ch)) {
+		ret = PTR_ERR(aon_chan->ch);
+		if (ret != -EPROBE_DEFER)
+			dev_err(dev, "Failed to request aon mbox chan ret %d\n", ret);
+		return ret;
+	}
+
+	dev_dbg(dev, "request thead mbox chan: aon\n");
+
+	aon_ipc->dev = dev;
+	mutex_init(&aon_ipc->lock);
+	init_completion(&aon_ipc->done);
+
+	light_aon_ipc_handle = aon_ipc;
+
+	return devm_of_platform_populate(dev);
+}
+
+static const struct of_device_id light_aon_match[] = {
+	{ .compatible = "thead,light-aon", },
+	{ /* Sentinel */ }
+};
+
+static int __maybe_unused light_aon_resume_noirq(struct device *dev)
+{
+	struct light_aon_chan *aon_chan;
+	int ret;
+
+	aon_chan = &light_aon_ipc_handle->chans;
+
+	complete(&aon_chan->tx_done);
+	return 0;
+}
+
+static const struct dev_pm_ops light_aon_pm_ops = {
+	SET_NOIRQ_SYSTEM_SLEEP_PM_OPS(NULL,
+				      light_aon_resume_noirq)
+};
+static struct platform_driver light_aon_driver = {
+	.driver = {
+		.name = "light-aon",
+		.of_match_table = light_aon_match,
+		.pm = &light_aon_pm_ops,
+	},
+	.probe = light_aon_probe,
+};
+builtin_platform_driver(light_aon_driver);
+
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light firmware protocol driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/firmware/thead/light_aon_misc.c b/drivers/firmware/thead/light_aon_misc.c
new file mode 100644
index 000000000000..3fb689f4b261
--- /dev/null
+++ b/drivers/firmware/thead/light_aon_misc.c
@@ -0,0 +1,74 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/firmware/thead/ipc.h>
+
+struct light_aon_msg_req_misc_set_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 ctrl;
+	u32 val;
+	u16 resource;
+	u16 reserved[7];
+} __packed __aligned(4);
+
+struct light_aon_msg_req_misc_get_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 ctrl;
+	u16 resource;
+	u16 reserved[9];
+} __packed __aligned(4);
+
+struct light_aon_msg_resp_misc_get_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 val;
+	u32 reserved[5];
+} __packed __aligned(4);
+
+int light_aon_misc_set_control(struct light_aon_ipc *ipc, u16 resource,
+			    u32 ctrl, u32 val)
+{
+	struct light_aon_msg_req_misc_set_ctrl msg;
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_MISC;
+	hdr->func = (uint8_t)LIGHT_AON_MISC_FUNC_SET_CONTROL;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.ctrl = ctrl;
+	msg.val = val;
+	msg.resource = resource;
+
+	return light_aon_call_rpc(ipc, &msg, true);
+}
+EXPORT_SYMBOL(light_aon_misc_set_control);
+
+int light_aon_misc_get_control(struct light_aon_ipc *ipc, u16 resource,
+			    u32 ctrl, u32 *val)
+{
+	struct light_aon_msg_req_misc_get_ctrl msg;
+	struct light_aon_msg_resp_misc_get_ctrl *resp;
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+	int ret;
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_MISC;
+	hdr->func = (uint8_t)LIGHT_AON_MISC_FUNC_GET_CONTROL;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.ctrl = ctrl;
+	msg.resource = resource;
+
+	ret = light_aon_call_rpc(ipc, &msg, true);
+	if (ret)
+		return ret;
+
+	resp = (struct light_aon_msg_resp_misc_get_ctrl *)&msg;
+	if (val != NULL)
+		*val = resp->val;
+
+	return 0;
+}
+EXPORT_SYMBOL(light_aon_misc_get_control);
diff --git a/drivers/firmware/thead/light_aon_pd.c b/drivers/firmware/thead/light_aon_pd.c
new file mode 100644
index 000000000000..3bef67df5a0a
--- /dev/null
+++ b/drivers/firmware/thead/light_aon_pd.c
@@ -0,0 +1,417 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <dt-bindings/firmware/thead/rsrc.h>
+#include <linux/ctype.h>
+#include <linux/debugfs.h>
+#include <linux/firmware/thead/ipc.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/of_platform.h>
+#include <linux/platform_device.h>
+#include <linux/pm.h>
+#include <linux/pm_domain.h>
+#include <linux/seq_file.h>
+#include <linux/slab.h>
+
+struct light_aon_msg_req_set_resource_power_mode {
+	struct light_aon_rpc_msg_hdr hdr;
+	u16 resource;
+	u16 mode;
+	u16 reserved[10];
+} __packed __aligned(4);
+
+#define LIGHT_AONU_PD_NAME_SIZE 20
+#define LIGHT_AONU_PD_STATE_NAME_SIZE 10
+
+struct light_aon_pm_domain {
+	struct generic_pm_domain pd;
+	char name[LIGHT_AONU_PD_NAME_SIZE];
+	u16 rsrc;
+};
+
+struct light_aon_pd_range {
+	char *name;
+	u32 rsrc;
+	u8 num;
+
+	/* add domain index */
+	bool postfix;
+	u8 start_from;
+};
+
+struct light_aon_pd_soc {
+	const struct light_aon_pd_range *pd_ranges;
+	u8 num_ranges;
+};
+
+static const struct light_aon_pd_range light_aon_pd_ranges[] = {
+	/* AUDIO SS */
+	{ "audio", LIGHT_AON_AUDIO_PD, 1, false, 0 },
+	{ "vdec", LIGHT_AON_VDEC_PD, 1, false, 0},
+	{ "npu", LIGHT_AON_NPU_PD, 1, false, 0},
+	{ "venc", LIGHT_AON_VENC_PD, 1, false, 0},
+	{ "gpu", LIGHT_AON_GPU_PD, 1, false, 0},
+	{ "dsp0", LIGHT_AON_DSP0_PD, 1, false, 0},
+	{ "dsp1", LIGHT_AON_DSP1_PD, 1, false, 0},
+	{},
+};
+
+static const struct light_aon_pd_soc light_aon_pd = {
+	.pd_ranges = light_aon_pd_ranges,
+	.num_ranges = ARRAY_SIZE(light_aon_pd_ranges),
+};
+
+static struct light_aon_ipc *pm_ipc_handle;
+static struct dentry *pd_debugfs_root;
+struct dentry *pd_pde;
+struct genpd_onecell_data *genpd_data;
+
+static inline struct light_aon_pm_domain *to_light_aon_pd(struct generic_pm_domain *genpd)
+{
+	return container_of(genpd, struct light_aon_pm_domain, pd);
+}
+
+static int light_aon_pd_power(struct generic_pm_domain *domain, bool power_on)
+{
+	struct light_aon_msg_req_set_resource_power_mode msg;
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+	struct light_aon_pm_domain *pd;
+	int ret;
+
+	pd = to_light_aon_pd(domain);
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = LIGHT_AON_RPC_SVC_PM;
+	hdr->func = LIGHT_AON_PM_FUNC_SET_RESOURCE_POWER_MODE;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.resource = pd->rsrc;
+	msg.mode = power_on ? LIGHT_AON_PM_PW_MODE_ON : LIGHT_AON_PM_PW_MODE_OFF;
+
+	ret = light_aon_call_rpc(pm_ipc_handle, &msg, true);
+	if (ret)
+		dev_err(&domain->dev, "failed to power %s resource %d ret %d\n",
+			power_on ? "up" : "off", pd->rsrc, ret);
+
+	return ret;
+}
+
+static int light_aon_pd_power_on(struct generic_pm_domain *domain)
+{
+	return light_aon_pd_power(domain, true);
+}
+
+static int light_aon_pd_power_off(struct generic_pm_domain *domain)
+{
+	return light_aon_pd_power(domain, false);
+}
+
+static struct generic_pm_domain *light_aon_pd_xlate(struct of_phandle_args *spec,
+						  void *data)
+{
+	struct generic_pm_domain *domain = ERR_PTR(-ENOENT);
+	struct genpd_onecell_data *pd_data = data;
+	unsigned int i;
+
+	for (i = 0; i < pd_data->num_domains; i++) {
+		struct light_aon_pm_domain *aon_pd;
+
+		aon_pd = to_light_aon_pd(pd_data->domains[i]);
+		if (aon_pd->rsrc == spec->args[0]) {
+			domain = &aon_pd->pd;
+			break;
+		}
+	}
+
+	return domain;
+}
+
+static struct light_aon_pm_domain *
+light_aon_add_pm_domain(struct device *dev, int idx,
+		      const struct light_aon_pd_range *pd_ranges)
+{
+	struct light_aon_pm_domain *aon_pd;
+	int ret;
+
+	aon_pd = devm_kzalloc(dev, sizeof(*aon_pd), GFP_KERNEL);
+	if (!aon_pd)
+		return ERR_PTR(-ENOMEM);
+
+	aon_pd->rsrc = pd_ranges->rsrc + idx;
+	aon_pd->pd.power_off = light_aon_pd_power_off;
+	aon_pd->pd.power_on = light_aon_pd_power_on;
+
+	if (pd_ranges->postfix)
+		snprintf(aon_pd->name, sizeof(aon_pd->name),
+			 "%s%i", pd_ranges->name, pd_ranges->start_from + idx);
+	else
+		snprintf(aon_pd->name, sizeof(aon_pd->name),
+			 "%s", pd_ranges->name);
+
+	aon_pd->pd.name = aon_pd->name;
+
+#if 0
+	if (aon_pd->rsrc >= LIGHT_AON_R_LAST) {
+		dev_warn(dev, "invalid pd %s rsrc id %d found",
+			 aon_pd->name, aon_pd->rsrc);
+
+		devm_kfree(dev, aon_pd);
+		return NULL;
+	}
+#endif
+
+	ret = pm_genpd_init(&aon_pd->pd, NULL, true);
+	if (ret) {
+		dev_warn(dev, "failed to init pd %s rsrc id %d",
+			 aon_pd->name, aon_pd->rsrc);
+		devm_kfree(dev, aon_pd);
+		return NULL;
+	}
+
+	return aon_pd;
+}
+
+static int light_aon_init_pm_domains(struct device *dev,
+				    const struct light_aon_pd_soc *pd_soc)
+{
+	const struct light_aon_pd_range *pd_ranges = pd_soc->pd_ranges;
+	struct generic_pm_domain **domains;
+	struct genpd_onecell_data *pd_data;
+	struct light_aon_pm_domain *aon_pd;
+	u32 count = 0;
+	int i, j;
+
+	for (i = 0; i < pd_soc->num_ranges; i++)
+		count += pd_ranges[i].num;
+
+	domains = devm_kcalloc(dev, count, sizeof(*domains), GFP_KERNEL);
+	if (!domains)
+		return -ENOMEM;
+
+	pd_data = devm_kzalloc(dev, sizeof(*pd_data), GFP_KERNEL);
+	if (!pd_data)
+		return -ENOMEM;
+
+	count = 0;
+	for (i = 0; i < pd_soc->num_ranges; i++) {
+		for (j = 0; j < pd_ranges[i].num; j++) {
+			aon_pd = light_aon_add_pm_domain(dev, j, &pd_ranges[i]);
+			if (IS_ERR_OR_NULL(aon_pd))
+				continue;
+
+			domains[count++] = &aon_pd->pd;
+			dev_dbg(dev, "added power domain %s\n", aon_pd->pd.name);
+		}
+	}
+
+	pd_data->domains = domains;
+	pd_data->num_domains = count;
+	pd_data->xlate = light_aon_pd_xlate;
+	genpd_data = pd_data;
+
+	of_genpd_add_provider_onecell(dev->of_node, pd_data);
+
+	return 0;
+}
+
+static char *pd_get_user_string(const char __user *userbuf, size_t userlen)
+{
+	char *buffer;
+
+	buffer = vmalloc(userlen + 1);
+	if (!buffer)
+		return ERR_PTR(-ENOMEM);
+
+	if (copy_from_user(buffer, userbuf, userlen) != 0) {
+		vfree(buffer);
+		return ERR_PTR(-EFAULT);
+	}
+
+	/* got the string, now strip linefeed. */
+	if (buffer[userlen - 1] == '\n')
+		buffer[userlen -1] = '\0';
+	else
+		buffer[userlen] = '\0';
+
+	pr_debug("buffer = %s\n", buffer);
+
+	return buffer;
+}
+
+static ssize_t light_power_domain_write(struct file *file,
+					const char __user *userbuf,
+					size_t userlen, loff_t *ppos)
+{
+	char *buffer, *start, *end;
+	struct seq_file *m = (struct seq_file *)file->private_data;
+	struct genpd_onecell_data *aon_pds_data = m->private;
+	struct generic_pm_domain *hitted_pm_genpd;
+	char pd_name[LIGHT_AONU_PD_NAME_SIZE];
+	char pd_state[LIGHT_AONU_PD_STATE_NAME_SIZE];
+	int idx, ret;
+	size_t origin_len = userlen;
+
+	buffer = pd_get_user_string(userbuf, userlen);
+	if (IS_ERR(buffer))
+		return PTR_ERR(buffer);
+
+	start = skip_spaces(buffer);
+	end = start;
+	while(!isspace(*end) && *end != '\0')
+		end++;
+
+	*end = '\0';
+	strcpy(pd_name, start);
+	pr_debug("power domain name: %s\n", pd_name);
+
+	/* find the target power domain */
+	for (idx = 0; idx < aon_pds_data->num_domains; idx++) {
+		struct generic_pm_domain *domain = aon_pds_data->domains[idx];
+		pr_debug("generic pm domain name: %s, pd_name: %s, ret = %d\n",
+				domain->name, pd_name, strcmp(pd_name, domain->name));
+		if (strcmp(pd_name, domain->name))
+			continue;
+		else {
+			hitted_pm_genpd = aon_pds_data->domains[idx];
+			pr_debug("target pm power domain-%s found, index: %d\n",
+					hitted_pm_genpd->name, idx);
+			break;
+		}
+	}
+
+	if (idx >= aon_pds_data->num_domains) {
+		pr_err("no taget power domain-%s found, idx = %d, total pd numbers = %d\n",
+				pd_name, idx, aon_pds_data->num_domains);
+		userlen = -EINVAL;
+		goto out;
+	}
+
+	if (!hitted_pm_genpd->power_on && !hitted_pm_genpd->power_off) {
+		pr_err("no power operations registered for power domain-%s\n", pd_name);
+		userlen = -EINVAL;
+		goto out;
+	}
+
+	end = end + 1;
+	start = skip_spaces(end);
+	end = start;
+	while(!isspace(*end) && *end != '\0')
+		end++;
+
+	*end = '\0';
+	strcpy(pd_state, start);
+	pr_debug("power domain target state: %s\n", pd_state);
+
+	if (!strcmp(pd_state, "on")) {
+		ret = hitted_pm_genpd->power_on(hitted_pm_genpd);
+		if (ret) {
+			userlen = ret;
+			goto out;
+		}
+	} else if (!strcmp(pd_state, "off")) {
+		ret = hitted_pm_genpd->power_off(hitted_pm_genpd);
+		if (ret) {
+			userlen = ret;
+			goto out;
+		}
+	} else {
+		pr_err("invalid power domain target state, not 'on' or 'off'\n");
+		userlen = -EINVAL;
+		goto out;
+	}
+
+out:
+	memset(buffer, 0, origin_len);
+	vfree(buffer);
+
+	return userlen;
+}
+
+static int light_power_domain_show(struct seq_file *m, void *v)
+{
+	struct genpd_onecell_data *pd_data = m->private;
+	u32 count = pd_data->num_domains;
+	int idx;
+
+	seq_puts(m, "[Power domain name list]: ");
+	for(idx = 0; idx < count; idx++)
+		seq_printf(m, "%s ", pd_data->domains[idx]->name);
+	seq_printf(m, "\n");
+	seq_puts(m, "[Power on  domain usage]: echo power_name on  > domain\n");
+	seq_puts(m, "[Power off domain usage]: echo power_name off > domain\n");
+
+	return 0;
+}
+
+static int light_power_domain_open(struct inode *inode, struct file *file)
+{
+	struct genpd_onecell_data *pd_data = inode->i_private;
+
+	return single_open(file, light_power_domain_show, pd_data);
+}
+
+static const struct file_operations light_power_domain_fops = {
+	.owner	= THIS_MODULE,
+	.write	= light_power_domain_write,
+	.read	= seq_read,
+	.open	= light_power_domain_open,
+	.llseek	= generic_file_llseek,
+};
+
+static void pd_debugfs_init(struct genpd_onecell_data *aon_pds_data)
+{
+	umode_t mode = S_IRUSR | S_IWUSR | S_IFREG;
+
+	pd_debugfs_root = debugfs_create_dir("power_domain", NULL);
+	if (!pd_debugfs_root || IS_ERR(pd_debugfs_root))
+		return;
+
+	pd_pde = debugfs_create_file("domain", mode, pd_debugfs_root, (void *)aon_pds_data, &light_power_domain_fops);
+
+	pr_info("succeed to create power domain debugfs direntry\n");
+}
+
+static int light_aon_pd_probe(struct platform_device *pdev)
+{
+	const struct light_aon_pd_soc *pd_soc;
+	int ret;
+
+	ret = light_aon_get_handle(&pm_ipc_handle);
+	if (ret)
+		return ret;
+
+	pd_soc = of_device_get_match_data(&pdev->dev);
+	if (!pd_soc)
+		return -ENODEV;
+
+	ret = light_aon_init_pm_domains(&pdev->dev, pd_soc);
+	if (ret)
+		return ret;
+
+	pd_debugfs_init(genpd_data);
+
+	return 0;
+}
+
+static const struct of_device_id light_aon_pd_match[] = {
+	{ .compatible = "thead,light-aon-pd", &light_aon_pd},
+	{ /* sentinel */ }
+};
+
+static struct platform_driver light_aon_pd_driver = {
+	.driver = {
+		.name = "light-aon-pd",
+		.of_match_table = light_aon_pd_match,
+	},
+	.probe = light_aon_pd_probe,
+};
+builtin_platform_driver(light_aon_pd_driver);
+
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light firmware protocol driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/firmware/thead/light_aon_test.c b/drivers/firmware/thead/light_aon_test.c
new file mode 100644
index 000000000000..172025430853
--- /dev/null
+++ b/drivers/firmware/thead/light_aon_test.c
@@ -0,0 +1,163 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/debugfs.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/uaccess.h>
+#include <linux/firmware/thead/ipc.h>
+
+#define MBOX_MAX_MSG_LEN		28
+
+static struct dentry *root_debugfs_dir;
+
+struct light_aon_msg_req_misc_set_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 ctrl;
+	u32 val;
+	u16 resource;
+	u16 reserved[7];
+} __packed __aligned(4);
+
+struct light_aon_msg_req_misc_get_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 ctrl;
+	u16 resource;
+	u16 reserved[9];
+} __packed __aligned(4);
+
+struct light_aon_msg_resp_misc_get_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 val;
+	u32 reserved[5];
+} __packed __aligned(4);
+
+struct light_aon_device {
+	struct device		*dev;
+	char			*test_buf;
+	struct light_aon_ipc	*ipc_handle;
+};
+
+static ssize_t light_aon_test_buf_write(struct file *filp,
+				      const char __user *userbuf,
+				      size_t count, loff_t *ppos)
+{
+	struct light_aon_device *tdev = filp->private_data;
+	int ret;
+
+	if (count > MBOX_MAX_MSG_LEN)
+		count = MBOX_MAX_MSG_LEN;
+
+	ret = copy_from_user(tdev->test_buf, userbuf, count);
+	if (ret) {
+		ret = -EFAULT;
+		goto out;
+	}
+
+	ret = light_aon_misc_set_control(tdev->ipc_handle, 0x1, 0x2, 0x3);
+	ret |= light_aon_misc_set_control(tdev->ipc_handle, 0x11, 0x12, 0x13);
+	ret |= light_aon_misc_set_control(tdev->ipc_handle, 0x21, 0x22, 0x23);
+	ret |= light_aon_misc_set_control(tdev->ipc_handle, 0x31, 0x32, 0x33);
+	if (ret)
+		dev_err(tdev->dev, "failed to set control\n");
+
+	//print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->test_buf, MBOX_MAX_MSG_LEN, true);
+
+out:
+	return ret < 0 ? ret : count;
+}
+
+static ssize_t light_aon_test_buf_read(struct file *filp,
+				      char __user *userbuf,
+				      size_t count, loff_t *ppos)
+{
+	struct light_aon_device *tdev = filp->private_data;
+
+	//print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->test_buf, MBOX_MAX_MSG_LEN, true);
+	memset(tdev->test_buf, 0, MBOX_MAX_MSG_LEN);
+
+	return MBOX_MAX_MSG_LEN;
+}
+
+static const struct file_operations light_aon_test_buf_ops = {
+	.write	= light_aon_test_buf_write,
+	.read	= light_aon_test_buf_read,
+	.open	= simple_open,
+	.llseek	= generic_file_llseek,
+};
+
+static int light_aon_add_debugfs(struct platform_device *pdev, struct light_aon_device *tdev)
+{
+	root_debugfs_dir = debugfs_create_dir("light_aon",NULL);
+	if (!root_debugfs_dir) {
+		dev_err(&pdev->dev, "Failed to create light_aon_test debugfs\n");
+		return -EINVAL;
+	}
+
+	debugfs_create_file("test", 0600, root_debugfs_dir, tdev, &light_aon_test_buf_ops);
+	return 0;
+}
+
+static int light_aon_probe(struct platform_device *pdev)
+{
+	struct light_aon_device *tdev;
+	int ret;
+
+	tdev = devm_kzalloc(&pdev->dev, sizeof(*tdev), GFP_KERNEL);
+	if (!tdev)
+		return -ENOMEM;
+
+	tdev->dev = &pdev->dev;
+	platform_set_drvdata(pdev, tdev);
+
+	tdev->test_buf = devm_kzalloc(&pdev->dev, MBOX_MAX_MSG_LEN, GFP_KERNEL);
+	if (!tdev->test_buf)
+		return -ENOMEM;
+
+	ret = light_aon_get_handle(&(tdev->ipc_handle));
+	if (ret) {
+		dev_err(&pdev->dev, "failed to get ipc_handle\n");
+		return ret;
+	}
+
+	ret = light_aon_add_debugfs(pdev, tdev);
+	if (ret)
+		return ret;
+
+	dev_info(&pdev->dev, "Successfully registered\n");
+
+	return 0;
+}
+
+static int light_aon_remove(struct platform_device *pdev)
+{
+	debugfs_remove_recursive(root_debugfs_dir);
+	return 0;
+}
+
+static const struct of_device_id light_aon_match[] = {
+	{ .compatible = "thead,light-aon-test" },
+	{},
+};
+
+static struct platform_driver light_aon_driver = {
+	.driver = {
+		.name = "thead,light-aon-test",
+		.of_match_table = light_aon_match,
+	},
+	.probe  = light_aon_probe,
+	.remove = light_aon_remove,
+};
+module_platform_driver(light_aon_driver);
+
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light firmware protocol test driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/gpio/gpio-dwapb.c b/drivers/gpio/gpio-dwapb.c
index 6b7d47a52b10..8a63ff1e5f73 100644
--- a/drivers/gpio/gpio-dwapb.c
+++ b/drivers/gpio/gpio-dwapb.c
@@ -415,13 +415,12 @@ static int dwapb_gpio_set_debounce(struct gpio_chip *gc,
 static int dwapb_gpio_set_config(struct gpio_chip *gc, unsigned offset,
 				 unsigned long config)
 {
-	u32 debounce;
-
-	if (pinconf_to_config_param(config) != PIN_CONFIG_INPUT_DEBOUNCE)
-		return -ENOTSUPP;
+	if (pinconf_to_config_param(config) == PIN_CONFIG_INPUT_DEBOUNCE) {
+		u32 debounce = pinconf_to_config_argument(config);
+		return dwapb_gpio_set_debounce(gc, offset, debounce);
+	}
 
-	debounce = pinconf_to_config_argument(config);
-	return dwapb_gpio_set_debounce(gc, offset, debounce);
+	return gpiochip_generic_config(gc, offset, config);
 }
 
 static int dwapb_convert_irqs(struct dwapb_gpio_port_irqchip *pirq,
@@ -531,10 +530,14 @@ static int dwapb_gpio_add_port(struct dwapb_gpio *gpio,
 	port->gc.fwnode = pp->fwnode;
 	port->gc.ngpio = pp->ngpio;
 	port->gc.base = pp->gpio_base;
+	port->gc.request = gpiochip_generic_request;
+	port->gc.free = gpiochip_generic_free;
 
 	/* Only port A support debounce */
 	if (pp->idx == 0)
 		port->gc.set_config = dwapb_gpio_set_config;
+	else
+		port->gc.set_config = gpiochip_generic_config;
 
 	/* Only port A can provide interrupts in all configurations of the IP */
 	if (pp->idx == 0)
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
index 062d78818da1..57fc15a0d2df 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
@@ -1109,6 +1109,8 @@ int amdgpu_device_resize_fb_bar(struct amdgpu_device *adev)
 	u16 cmd;
 	int r;
 
+	return 0;
+
 	if (!IS_ENABLED(CONFIG_PHYS_ADDR_T_64BIT))
 		return 0;
 
diff --git a/drivers/gpu/drm/amd/display/Kconfig b/drivers/gpu/drm/amd/display/Kconfig
index 901d1961b739..90489b55efa7 100644
--- a/drivers/gpu/drm/amd/display/Kconfig
+++ b/drivers/gpu/drm/amd/display/Kconfig
@@ -9,6 +9,7 @@ config DRM_AMD_DC
 	select SND_HDA_COMPONENT if SND_HDA_CORE
 	# !CC_IS_CLANG: https://github.com/ClangBuiltLinux/linux/issues/1752
 	select DRM_AMD_DC_FP if (X86 || LOONGARCH || (PPC64 && ALTIVEC) || (ARM64 && KERNEL_MODE_NEON && !CC_IS_CLANG))
+	select DRM_AMD_DC_DCN if RISCV && FPU
 	help
 	  Choose this option if you want to use the new display engine
 	  support for AMDGPU. This adds required support for Vega and
diff --git a/drivers/gpu/drm/amd/display/amdgpu_dm/dc_fpu.c b/drivers/gpu/drm/amd/display/amdgpu_dm/dc_fpu.c
index 172aa10a8800..53a7122ba98d 100644
--- a/drivers/gpu/drm/amd/display/amdgpu_dm/dc_fpu.c
+++ b/drivers/gpu/drm/amd/display/amdgpu_dm/dc_fpu.c
@@ -35,6 +35,8 @@
 #include <asm/neon.h>
 #elif defined(CONFIG_LOONGARCH)
 #include <asm/fpu.h>
+#elif defined(CONFIG_RISCV)
+#include <asm/switch_to.h>
 #endif
 
 /**
@@ -90,7 +92,7 @@ void dc_fpu_begin(const char *function_name, const int line)
 	*pcpu += 1;
 
 	if (*pcpu == 1) {
-#if defined(CONFIG_X86) || defined(CONFIG_LOONGARCH)
+#if defined(CONFIG_X86) || defined(CONFIG_LOONGARCH) || defined(CONFIG_RISCV)
 		migrate_disable();
 		kernel_fpu_begin();
 #elif defined(CONFIG_PPC64)
@@ -130,7 +132,7 @@ void dc_fpu_end(const char *function_name, const int line)
 	pcpu = get_cpu_ptr(&fpu_recursion_depth);
 	*pcpu -= 1;
 	if (*pcpu <= 0) {
-#if defined(CONFIG_X86) || defined(CONFIG_LOONGARCH)
+#if defined(CONFIG_X86) || defined(CONFIG_LOONGARCH) || defined(CONFIG_RISCV)
 		kernel_fpu_end();
 		migrate_enable();
 #elif defined(CONFIG_PPC64)
diff --git a/drivers/gpu/drm/amd/display/dc/dml/Makefile b/drivers/gpu/drm/amd/display/dc/dml/Makefile
index 0ba9a7997d56..abd04d13997d 100644
--- a/drivers/gpu/drm/amd/display/dc/dml/Makefile
+++ b/drivers/gpu/drm/amd/display/dc/dml/Makefile
@@ -43,6 +43,12 @@ dml_ccflags := -mfpu=64
 dml_rcflags := -msoft-float
 endif
 
+ifdef CONFIG_RISCV
+include $(srctree)/arch/riscv/Makefile.isa
+# Remove V from the ISA string, like in arch/riscv/Makefile, but keep F and D.
+dml_ccflags := -march=$(subst v0p7,,$(riscv-march-y))
+endif
+
 ifdef CONFIG_CC_IS_GCC
 ifneq ($(call gcc-min-version, 70100),y)
 IS_OLD_GCC = 1
diff --git a/drivers/gpu/drm/drm_gem_vram_helper.c b/drivers/gpu/drm/drm_gem_vram_helper.c
index b67eafa55715..5ebe418bd383 100644
--- a/drivers/gpu/drm/drm_gem_vram_helper.c
+++ b/drivers/gpu/drm/drm_gem_vram_helper.c
@@ -870,7 +870,7 @@ static struct ttm_tt *bo_driver_ttm_tt_create(struct ttm_buffer_object *bo,
 	if (!tt)
 		return NULL;
 
-	ret = ttm_tt_init(tt, bo, page_flags, ttm_cached, 0);
+	ret = ttm_tt_init(tt, bo, page_flags, ttm_write_combined, 0);
 	if (ret < 0)
 		goto err_ttm_tt_init;
 
diff --git a/drivers/gpu/drm/radeon/radeon_drv.c b/drivers/gpu/drm/radeon/radeon_drv.c
index 7bf08164140e..b0476feba79c 100644
--- a/drivers/gpu/drm/radeon/radeon_drv.c
+++ b/drivers/gpu/drm/radeon/radeon_drv.c
@@ -36,6 +36,7 @@
 #include <linux/vga_switcheroo.h>
 #include <linux/mmu_notifier.h>
 #include <linux/pci.h>
+#include <linux/kexec.h>
 
 #include <drm/drm_aperture.h>
 #include <drm/drm_drv.h>
@@ -336,10 +337,10 @@ radeon_pci_remove(struct pci_dev *pdev)
 static void
 radeon_pci_shutdown(struct pci_dev *pdev)
 {
-	/* if we are running in a VM, make sure the device
-	 * torn down properly on reboot/shutdown
+	/* if we are running in a VM or kexec another kernel,
+	 * make sure the device torn down properly on reboot/shutdown
 	 */
-	if (radeon_device_is_virtual())
+	if (radeon_device_is_virtual() || kexec_in_progress)
 		radeon_pci_remove(pdev);
 
 #if defined(CONFIG_PPC64) || defined(CONFIG_MACH_LOONGSON64)
diff --git a/drivers/gpu/drm/radeon/radeon_irq_kms.c b/drivers/gpu/drm/radeon/radeon_irq_kms.c
index c4dda908666c..33b56ca7af6f 100644
--- a/drivers/gpu/drm/radeon/radeon_irq_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_irq_kms.c
@@ -250,10 +250,12 @@ static bool radeon_msi_ok(struct radeon_device *rdev)
 	 * of address for "64-bit" MSIs which breaks on some platforms, notably
 	 * IBM POWER servers, so we limit them
 	 */
+#if 0
 	if (rdev->family < CHIP_BONAIRE) {
 		dev_info(rdev->dev, "radeon: MSI limited to 32-bit\n");
 		rdev->pdev->no_64bit_msi = 1;
 	}
+#endif
 
 	/* force MSI on */
 	if (radeon_msi == 1)
diff --git a/drivers/gpu/drm/ttm/ttm_bo_util.c b/drivers/gpu/drm/ttm/ttm_bo_util.c
index 0b3f4267130c..f469067c8187 100644
--- a/drivers/gpu/drm/ttm/ttm_bo_util.c
+++ b/drivers/gpu/drm/ttm/ttm_bo_util.c
@@ -354,6 +354,7 @@ static int ttm_bo_kmap_ttm(struct ttm_buffer_object *bo,
 	if (ret)
 		return ret;
 
+#if 0
 	if (num_pages == 1 && ttm->caching == ttm_cached &&
 	    !(man->use_tt && (ttm->page_flags & TTM_TT_FLAG_DECRYPTED))) {
 		/*
@@ -364,7 +365,9 @@ static int ttm_bo_kmap_ttm(struct ttm_buffer_object *bo,
 		map->bo_kmap_type = ttm_bo_map_kmap;
 		map->page = ttm->pages[start_page];
 		map->virtual = kmap(map->page);
-	} else {
+	} else
+#endif
+	{
 		/*
 		 * We need to use vmap to get the desired page protection
 		 * or to make the buffer object look contiguous.
diff --git a/drivers/gpu/drm/ttm/ttm_module.c b/drivers/gpu/drm/ttm/ttm_module.c
index b3fffe7b5062..aa137ead5cc5 100644
--- a/drivers/gpu/drm/ttm/ttm_module.c
+++ b/drivers/gpu/drm/ttm/ttm_module.c
@@ -74,7 +74,8 @@ pgprot_t ttm_prot_from_caching(enum ttm_caching caching, pgprot_t tmp)
 #endif /* CONFIG_UML */
 #endif /* __i386__ || __x86_64__ */
 #if defined(__ia64__) || defined(__arm__) || defined(__aarch64__) || \
-	defined(__powerpc__) || defined(__mips__) || defined(__loongarch__)
+	defined(__powerpc__) || defined(__mips__) || defined(__loongarch__) || \
+	defined(__riscv)
 	if (caching == ttm_write_combined)
 		tmp = pgprot_writecombine(tmp);
 	else
diff --git a/drivers/gpu/drm/ttm/ttm_resource.c b/drivers/gpu/drm/ttm/ttm_resource.c
index 46ff9c75bb12..63a9b8d41b94 100644
--- a/drivers/gpu/drm/ttm/ttm_resource.c
+++ b/drivers/gpu/drm/ttm/ttm_resource.c
@@ -187,7 +187,7 @@ void ttm_resource_init(struct ttm_buffer_object *bo,
 	res->bus.addr = NULL;
 	res->bus.offset = 0;
 	res->bus.is_iomem = false;
-	res->bus.caching = ttm_cached;
+	res->bus.caching = ttm_write_combined;
 	res->bo = bo;
 
 	man = ttm_manager_type(bo->bdev, place->mem_type);
@@ -670,17 +670,18 @@ ttm_kmap_iter_linear_io_init(struct ttm_kmap_iter_linear_io *iter_io,
 	} else {
 		iter_io->needs_unmap = true;
 		memset(&iter_io->dmap, 0, sizeof(iter_io->dmap));
-		if (mem->bus.caching == ttm_write_combined)
+		if (mem->bus.caching == ttm_write_combined  || mem->bus.caching == ttm_cached)
 			iosys_map_set_vaddr_iomem(&iter_io->dmap,
 						  ioremap_wc(mem->bus.offset,
 							     mem->size));
+#if 0
 		else if (mem->bus.caching == ttm_cached)
 			iosys_map_set_vaddr(&iter_io->dmap,
 					    memremap(mem->bus.offset, mem->size,
 						     MEMREMAP_WB |
 						     MEMREMAP_WT |
 						     MEMREMAP_WC));
-
+#endif
 		/* If uncached requested or if mapping cached or wc failed */
 		if (iosys_map_is_null(&iter_io->dmap))
 			iosys_map_set_vaddr_iomem(&iter_io->dmap,
diff --git a/drivers/gpu/drm/ttm/ttm_tt.c b/drivers/gpu/drm/ttm/ttm_tt.c
index 43eaffa7faae..507c27f2270a 100644
--- a/drivers/gpu/drm/ttm/ttm_tt.c
+++ b/drivers/gpu/drm/ttm/ttm_tt.c
@@ -154,7 +154,7 @@ static void ttm_tt_init_fields(struct ttm_tt *ttm,
 	ttm->dma_address = NULL;
 	ttm->swap_storage = NULL;
 	ttm->sg = bo->sg;
-	ttm->caching = caching;
+	ttm->caching = ttm_write_combined;
 }
 
 int ttm_tt_init(struct ttm_tt *ttm, struct ttm_buffer_object *bo,
diff --git a/drivers/mailbox/Kconfig b/drivers/mailbox/Kconfig
index bc2e265cb02d..ca9cfa3ac9f7 100644
--- a/drivers/mailbox/Kconfig
+++ b/drivers/mailbox/Kconfig
@@ -295,4 +295,12 @@ config QCOM_IPCC
 	  acts as an interrupt controller for receiving interrupts from clients.
 	  Say Y here if you want to build this driver.
 
+config THEAD_LIGHT_MBOX
+		bool "Thead light Mailbox"
+		depends on ARCH_THEAD || COMPILE_TEST
+		default y
+		help
+		  Mailbox implementation for Thead light SoCs.
+
+
 endif
diff --git a/drivers/mailbox/Makefile b/drivers/mailbox/Makefile
index fc9376117111..7e82b9edccd4 100644
--- a/drivers/mailbox/Makefile
+++ b/drivers/mailbox/Makefile
@@ -62,3 +62,6 @@ obj-$(CONFIG_SPRD_MBOX)		+= sprd-mailbox.o
 obj-$(CONFIG_QCOM_IPCC)		+= qcom-ipcc.o
 
 obj-$(CONFIG_APPLE_MAILBOX)	+= apple-mailbox.o
+
+obj-$(CONFIG_THEAD_LIGHT_MBOX)  += light-mailbox.o
+#obj-$(CONFIG_THEAD_LIGHT_MBOX) += light-mailbox-client.o
diff --git a/drivers/mailbox/light-mailbox-client.c b/drivers/mailbox/light-mailbox-client.c
new file mode 100644
index 000000000000..10cf7ae15cbc
--- /dev/null
+++ b/drivers/mailbox/light-mailbox-client.c
@@ -0,0 +1,242 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/debugfs.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/mailbox_client.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/uaccess.h>
+
+#define MBOX_MAX_MSG_LEN	28
+#define WJ_MBOX_SEND_MAX_MESSAGE_LENGTH 28
+#define HEXDUMP_BYTES_PER_LINE	28
+#define HEXDUMP_LINE_LEN	((HEXDUMP_BYTES_PER_LINE * 4) + 2)
+#define HEXDUMP_MAX_LEN		(HEXDUMP_LINE_LEN *		\
+				(MBOX_MAX_MSG_LEN / HEXDUMP_BYTES_PER_LINE))
+
+static struct dentry *root_debugfs_dir;
+
+struct mbox_client_light_device {
+	struct device		*dev;
+	void __iomem		*tx_mmio;
+	void __iomem		*rx_mmio;
+	struct mbox_chan	*tx_channel;
+	struct mbox_chan	*rx_channel;
+	char			*rx_buffer;
+	char	*message;
+	spinlock_t		lock;
+};
+
+static ssize_t mbox_client_light_message_write(struct file *filp,
+					      const char __user *userbuf,
+					      size_t count, loff_t *ppos)
+{
+	struct mbox_client_light_device *tdev = filp->private_data;
+	void *data;
+	int ret;
+
+	if (!tdev->tx_channel) {
+		dev_err(tdev->dev, "Channel cannot do Tx\n");
+		return -EINVAL;
+	}
+
+	if (count > WJ_MBOX_SEND_MAX_MESSAGE_LENGTH)
+		count = WJ_MBOX_SEND_MAX_MESSAGE_LENGTH;
+
+	tdev->message = kzalloc(MBOX_MAX_MSG_LEN, GFP_KERNEL);
+	if (!tdev->message)
+		return -ENOMEM;
+
+	ret = copy_from_user(tdev->message, userbuf, count);
+	if (ret) {
+		ret = -EFAULT;
+		goto out;
+	}
+
+	data = tdev->message;
+	print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->message, MBOX_MAX_MSG_LEN, true);
+
+	ret = mbox_send_message(tdev->tx_channel, data);
+	if (ret < 0)
+		dev_err(tdev->dev, "Failed to send message via mailbox\n");
+
+out:
+	kfree(tdev->message);
+	return ret < 0 ? ret : count;
+}
+
+static ssize_t mbox_client_light_message_read(struct file *filp,
+					     char __user *userbuf,
+					     size_t count, loff_t *ppos)
+{
+	struct mbox_client_light_device *tdev = filp->private_data;
+	unsigned long flags;
+
+	print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->rx_buffer, MBOX_MAX_MSG_LEN, true);
+	spin_lock_irqsave(&tdev->lock, flags);
+	memset(tdev->rx_buffer, 0, MBOX_MAX_MSG_LEN);
+	spin_unlock_irqrestore(&tdev->lock, flags);
+
+	return MBOX_MAX_MSG_LEN;
+}
+
+static const struct file_operations mbox_client_light_message_ops = {
+	.write	= mbox_client_light_message_write,
+	.read	= mbox_client_light_message_read,
+	.open	= simple_open,
+	.llseek	= generic_file_llseek,
+};
+
+static int index_names = 0;
+static bool debugfs_dir_created = false;
+static const char* file_names[] = {"mbox-client0", "mbox-client1"};
+
+static int mbox_client_light_add_debugfs(struct platform_device *pdev,
+					struct mbox_client_light_device *tdev)
+{
+	if (!debugfs_initialized())
+		return 0;
+
+	if (index_names > 2) {
+		dev_err(&pdev->dev, "Max device index is 2\n");
+		return 0;
+	}
+
+	if (!debugfs_dir_created) {
+		root_debugfs_dir = debugfs_create_dir("mailbox",NULL);
+		if (!root_debugfs_dir) {
+			dev_err(&pdev->dev,
+				"Failed to create mailbox debugfs\n");
+			return -EINVAL;
+		}
+		debugfs_dir_created = true;
+	}
+
+	debugfs_create_file(file_names[index_names], 0600, root_debugfs_dir,
+			    tdev, &mbox_client_light_message_ops);
+
+	index_names++;
+	return 0;
+}
+
+static void mbox_client_light_receive_message(struct mbox_client *client,
+					     void *message)
+{
+	struct mbox_client_light_device *tdev = dev_get_drvdata(client->dev);
+	char *data = message;
+
+	spin_lock(&tdev->lock);
+	memcpy(tdev->rx_buffer, data, MBOX_MAX_MSG_LEN);
+	spin_unlock(&tdev->lock);
+	print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->rx_buffer, MBOX_MAX_MSG_LEN, true);
+}
+
+static struct mbox_chan *
+mbox_client_light_request_channel(struct platform_device *pdev,
+				 const char *name)
+{
+	struct mbox_client *client;
+	struct mbox_chan *channel;
+
+	client = devm_kzalloc(&pdev->dev, sizeof(*client), GFP_KERNEL);
+	if (!client)
+		return ERR_PTR(-ENOMEM);
+
+	client->dev		= &pdev->dev;
+	client->tx_block	= true;
+	client->knows_txdone	= false;
+	client->tx_tout		= 500;
+	client->rx_callback	= mbox_client_light_receive_message;
+
+	channel = mbox_request_channel_byname(client, name);
+	if (IS_ERR(channel)) {
+		devm_kfree(&pdev->dev, client);
+		dev_warn(&pdev->dev, "Failed to request %s channel\n", name);
+		return NULL;
+	}
+
+	return channel;
+}
+
+static int mbox_client_light_probe(struct platform_device *pdev)
+{
+	struct mbox_client_light_device *tdev;
+	int ret;
+	static int chan_idx = 0;
+
+	tdev = devm_kzalloc(&pdev->dev, sizeof(*tdev), GFP_KERNEL);
+	if (!tdev)
+		return -ENOMEM;
+
+	if (!chan_idx)
+		tdev->tx_channel = mbox_client_light_request_channel(pdev, "902");
+	else
+		tdev->tx_channel = mbox_client_light_request_channel(pdev, "906");
+	if (!tdev->tx_channel) {
+		dev_err(&pdev->dev, "Request channel failed\n");
+		return -EPROBE_DEFER;
+	}
+	chan_idx++;
+	/* In fact, rx_channel is same with tx_channel in C-SKY's mailbox */
+	tdev->rx_channel = tdev->tx_channel;
+
+	tdev->dev = &pdev->dev;
+	platform_set_drvdata(pdev, tdev);
+
+	spin_lock_init(&tdev->lock);
+
+	tdev->rx_buffer = devm_kzalloc(&pdev->dev,
+					MBOX_MAX_MSG_LEN, GFP_KERNEL);
+	if (!tdev->rx_buffer)
+		return -ENOMEM;
+
+	ret = mbox_client_light_add_debugfs(pdev, tdev);
+	if (ret)
+		return ret;
+
+	dev_info(&pdev->dev, "Successfully registered\n");
+
+	return 0;
+}
+
+static int mbox_client_light_remove(struct platform_device *pdev)
+{
+	struct mbox_client_light_device *tdev = platform_get_drvdata(pdev);
+
+	debugfs_remove_recursive(root_debugfs_dir);
+
+	if (tdev->tx_channel)
+		mbox_free_channel(tdev->tx_channel);
+
+	if (tdev->rx_channel && tdev->rx_channel != tdev->tx_channel)
+		mbox_free_channel(tdev->rx_channel);
+
+	return 0;
+}
+
+static const struct of_device_id mbox_client_light_match[] = {
+	{ .compatible = "thead,light-mbox-client" },
+	{},
+};
+
+static struct platform_driver mbox_client_light_driver = {
+	.driver = {
+		.name = "thead,light-mbox-client",
+		.of_match_table = mbox_client_light_match,
+	},
+	.probe  = mbox_client_light_probe,
+	.remove = mbox_client_light_remove,
+};
+module_platform_driver(mbox_client_light_driver);
+
+MODULE_AUTHOR("Alibaba Group Holding Limited");
+MODULE_DESCRIPTION("Thead Light mailbox IPC client driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/mailbox/light-mailbox.c b/drivers/mailbox/light-mailbox.c
new file mode 100644
index 000000000000..f3d34d947ec4
--- /dev/null
+++ b/drivers/mailbox/light-mailbox.c
@@ -0,0 +1,507 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/clk.h>
+#include <linux/interrupt.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/mailbox_controller.h>
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/slab.h>
+
+/* Status Register */
+#define LIGHT_MBOX_STA		0x0
+#define LIGHT_MBOX_CLR		0x4
+#define LIGHT_MBOX_MASK		0xc
+
+/* Transmit/receive data register:
+ * INFO0 ~ INFO6
+ */
+#define LIGHT_MBOX_INFO_NUM		8
+#define LIGHT_MBOX_DATA_INFO_NUM	7
+#define LIGHT_MBOX_INFO0	0x14
+/* Transmit ack register: INFO7 */
+#define LIGHT_MBOX_INFO7	0x30
+
+/* Generate remote icu IRQ Register */
+#define LIGHT_MBOX_GEN		0x10
+#define LIGHT_MBOX_GEN_RX_DATA	BIT(6)
+#define LIGHT_MBOX_GEN_TX_ACK	BIT(7)
+
+#define LIGHT_MBOX_CHAN_RES_SIZE	0x1000
+#define LIGHT_MBOX_CHANS		4
+#define LIGHT_MBOX_CHAN_NAME_SIZE	20
+
+#define LIGHT_MBOX_ACK_MAGIC		0xdeadbeaf
+
+enum light_mbox_chan_type {
+	LIGHT_MBOX_TYPE_TXRX,	/* Tx & Rx chan */
+	LIGHT_MBOX_TYPE_DB,	/* Tx & Rx doorbell */
+};
+
+enum light_mbox_icu_cpu_id {
+	LIGHT_MBOX_ICU_CPU0,		/* 910T */
+	LIGHT_MBOX_ICU_CPU1,            /* 902 */
+	LIGHT_MBOX_ICU_CPU2,            /* 906 */
+	LIGHT_MBOX_ICU_CPU3,            /* 910R */
+};
+
+struct light_mbox_con_priv {
+	enum light_mbox_icu_cpu_id	idx;
+	enum light_mbox_chan_type	type;
+	void __iomem			*comm_local_base;
+	void __iomem			*comm_remote_base;
+	char				irq_desc[LIGHT_MBOX_CHAN_NAME_SIZE];
+	struct mbox_chan		*chan;
+	struct tasklet_struct		txdb_tasklet;
+};
+
+struct light_mbox_priv {
+	struct device			*dev;
+	void __iomem			*local_icu[LIGHT_MBOX_CHANS];
+	void __iomem			*remote_icu[LIGHT_MBOX_CHANS - 1];
+	void __iomem			*cur_cpu_ch_base;
+	enum light_mbox_icu_cpu_id	cur_icu_cpu_id;
+	spinlock_t			mbox_lock; /* control register lock */
+
+	struct mbox_controller		mbox;
+	struct mbox_chan		mbox_chans[LIGHT_MBOX_CHANS];
+
+	struct light_mbox_con_priv  	con_priv[LIGHT_MBOX_CHANS];
+	struct clk			*clk;
+	int				irq;
+};
+
+static struct light_mbox_priv *to_light_mbox_priv(struct mbox_controller *mbox)
+{
+	return container_of(mbox, struct light_mbox_priv, mbox);
+}
+
+static void light_mbox_write(struct light_mbox_priv *priv, u32 val, u32 offs)
+{
+	iowrite32(val, priv->cur_cpu_ch_base + offs);
+}
+
+static u32 light_mbox_read(struct light_mbox_priv *priv, u32 offs)
+{
+	return ioread32(priv->cur_cpu_ch_base + offs);
+}
+
+static u32 light_mbox_rmw(struct light_mbox_priv *priv, u32 off, u32 set, u32 clr)
+{
+	unsigned long flags;
+	u32 val;
+
+	spin_lock_irqsave(&priv->mbox_lock, flags);
+	val = light_mbox_read(priv, off);
+	val &= ~clr;
+	val |= set;
+	light_mbox_write(priv, val, off);
+	spin_unlock_irqrestore(&priv->mbox_lock, flags);
+
+	return val;
+}
+
+static void light_mbox_chan_write(struct light_mbox_con_priv *cp, u32 val, u32 offs, bool is_remote)
+{
+	if (is_remote)
+		iowrite32(val, cp->comm_remote_base + offs);
+	else
+		iowrite32(val, cp->comm_local_base + offs);
+}
+
+static u32 light_mbox_chan_read(struct light_mbox_con_priv *cp, u32 offs, bool is_remote)
+{
+	if (is_remote)
+		return ioread32(cp->comm_remote_base + offs);
+	else
+		return ioread32(cp->comm_local_base + offs);
+}
+
+static void light_mbox_chan_rmw(struct light_mbox_con_priv *cp, u32 off, u32 set, u32 clr, bool is_remote)
+{
+	struct light_mbox_priv *priv = to_light_mbox_priv(cp->chan->mbox);
+	unsigned long flags;
+	u32 val;
+
+	spin_lock_irqsave(&priv->mbox_lock, flags);
+	val = light_mbox_chan_read(cp, off, is_remote);
+	val &= ~clr;
+	val |= set;
+	light_mbox_chan_write(cp, val, off, is_remote);
+	spin_unlock_irqrestore(&priv->mbox_lock, flags);
+}
+
+static void light_mbox_chan_rd_data(struct light_mbox_con_priv *cp, void *data, bool is_remote)
+{
+	u32 off = LIGHT_MBOX_INFO0;
+	u32 *arg = data;
+	u32 i;
+
+	/* read info0 ~ info6, totally 28 bytes
+	 * requires data memory size is 28 bytes
+	 */
+	for (i = 0; i < LIGHT_MBOX_DATA_INFO_NUM; i++) {
+		*arg = light_mbox_chan_read(cp, off, is_remote);
+		off += 4;
+		arg++;
+	}
+}
+
+static void light_mbox_chan_wr_data(struct light_mbox_con_priv *cp, void *data, bool is_remote)
+{
+	u32 off = LIGHT_MBOX_INFO0;
+	u32 *arg = data;
+	u32 i;
+
+	/* write info0 ~ info6, totally 28 bytes
+	 * requires data memory is 28 bytes valid data
+	 */
+	for (i = 0; i < LIGHT_MBOX_DATA_INFO_NUM; i++) {
+		light_mbox_chan_write(cp, *arg, off, is_remote);
+		off += 4;
+		arg++;
+	}
+}
+
+static void light_mbox_chan_wr_ack(struct light_mbox_con_priv *cp, void *data, bool is_remote)
+{
+	u32 off = LIGHT_MBOX_INFO7;
+	u32 *arg = data;
+
+	light_mbox_chan_write(cp, *arg, off, is_remote);
+}
+
+static int light_mbox_chan_id_to_mapbit(struct light_mbox_con_priv *cp)
+{
+	struct light_mbox_priv *priv = to_light_mbox_priv(cp->chan->mbox);
+	int mapbit = 0;
+	int i;
+
+	for (i = 0; i < LIGHT_MBOX_CHANS; i++) {
+		if (i == cp->idx)
+			return mapbit;
+
+		if (i != priv->cur_icu_cpu_id)
+			mapbit++;
+	}
+
+	if (i == LIGHT_MBOX_CHANS)
+		dev_err(cp->chan->mbox->dev, "convert to mapbit failed\n");
+
+	return 0;
+}
+
+static void light_mbox_txdb_tasklet(unsigned long data)
+{
+	struct light_mbox_con_priv *cp = (struct light_mbox_con_priv *)data;
+
+	mbox_chan_txdone(cp->chan, 0);
+}
+
+static irqreturn_t light_mbox_isr(int irq, void *p)
+{
+	struct mbox_chan *chan = p;
+	struct light_mbox_priv *priv = to_light_mbox_priv(chan->mbox);
+	struct light_mbox_con_priv *cp = chan->con_priv;
+	int mapbit = light_mbox_chan_id_to_mapbit(cp);
+	u32 sta, dat[LIGHT_MBOX_DATA_INFO_NUM];
+	u32 ack_magic = LIGHT_MBOX_ACK_MAGIC;
+	u32 info0_data, info7_data;
+
+	sta = light_mbox_read(priv, LIGHT_MBOX_STA);
+	if (!(sta & BIT(mapbit)))
+		return IRQ_NONE;
+
+	/* clear chan irq bit in STA register */
+	light_mbox_rmw(priv, LIGHT_MBOX_CLR, BIT(mapbit), 0);
+
+	/* rx doorbell */
+	if (cp->type == LIGHT_MBOX_TYPE_DB) {
+		mbox_chan_received_data(cp->chan, NULL);
+		return IRQ_HANDLED;
+	}
+
+	/* info0 is the protocol word, shoud not be zero! */
+	info0_data = light_mbox_chan_read(cp, LIGHT_MBOX_INFO0, false);
+	if (info0_data) {
+		/* read info0~info6 data */
+		light_mbox_chan_rd_data(cp, dat, false);
+
+		/* clear local info0 */
+		light_mbox_chan_write(cp, 0x0, LIGHT_MBOX_INFO0, false);
+
+		/* notify remote cpu */
+		light_mbox_chan_wr_ack(cp, &ack_magic, true);
+		/* CPU1 902/906 use polling mode to monitor info7 */
+		if (cp->idx != LIGHT_MBOX_ICU_CPU1 && cp->idx != LIGHT_MBOX_ICU_CPU2)
+			light_mbox_chan_rmw(cp, LIGHT_MBOX_GEN, LIGHT_MBOX_GEN_TX_ACK, 0, true);
+
+		/* transfer the data to client */
+		mbox_chan_received_data(chan, (void *)dat);
+	}
+
+	/* info7 magic value mean the real ack signal, not generate bit7 */
+	info7_data = light_mbox_chan_read(cp, LIGHT_MBOX_INFO7, false);
+	if (info7_data == LIGHT_MBOX_ACK_MAGIC) {
+		/* clear local info7 */
+		light_mbox_chan_write(cp, 0x0, LIGHT_MBOX_INFO7, false);
+
+		/* notify framework the last TX has completed */
+		mbox_chan_txdone(chan, 0);
+	}
+
+	if (!info0_data && !info7_data)
+		return IRQ_NONE;
+
+	return IRQ_HANDLED;
+}
+
+static int light_mbox_send_data(struct mbox_chan *chan, void *data)
+{
+	struct light_mbox_con_priv *cp = chan->con_priv;
+
+	if (cp->type == LIGHT_MBOX_TYPE_DB)
+		tasklet_schedule(&cp->txdb_tasklet);
+	else
+		light_mbox_chan_wr_data(cp, data, true);
+	light_mbox_chan_rmw(cp, LIGHT_MBOX_GEN, LIGHT_MBOX_GEN_RX_DATA, 0, true);
+	return 0;
+}
+
+static int light_mbox_startup(struct mbox_chan *chan)
+{
+	struct light_mbox_priv *priv = to_light_mbox_priv(chan->mbox);
+	struct light_mbox_con_priv *cp = chan->con_priv;
+	u32 data[8] = {0};
+	int mask_bit;
+	int ret;
+
+	/* clear local and remote generate and info0~info7 */
+	light_mbox_chan_rmw(cp, LIGHT_MBOX_GEN, 0x0, 0xff, true);
+	light_mbox_chan_rmw(cp, LIGHT_MBOX_GEN, 0x0, 0xff, false);
+	light_mbox_chan_wr_ack(cp, &data[7], true);
+	light_mbox_chan_wr_ack(cp, &data[7], false);
+	light_mbox_chan_wr_data(cp, &data[0], true);
+	light_mbox_chan_wr_data(cp, &data[0], false);
+
+	/* enable the chan mask */
+	mask_bit = light_mbox_chan_id_to_mapbit(cp);
+	light_mbox_rmw(priv, LIGHT_MBOX_MASK, BIT(mask_bit), 0);
+
+	if (cp->type == LIGHT_MBOX_TYPE_DB)
+		/* tx doorbell doesn't have ACK, rx doorbell requires isr */
+		tasklet_init(&cp->txdb_tasklet, light_mbox_txdb_tasklet,
+			     (unsigned long)cp);
+
+	ret = request_irq(priv->irq, light_mbox_isr, IRQF_SHARED |
+			  IRQF_NO_SUSPEND, cp->irq_desc, chan);
+	if (ret) {
+		dev_err(priv->dev,
+			"Unable to acquire IRQ %d\n", priv->irq);
+		return ret;
+	}
+
+	return 0;
+}
+
+static void light_mbox_shutdown(struct mbox_chan *chan)
+{
+	struct light_mbox_priv *priv = to_light_mbox_priv(chan->mbox);
+	struct light_mbox_con_priv *cp = chan->con_priv;
+	int mask_bit;
+
+	/* clear the chan mask */
+	mask_bit = light_mbox_chan_id_to_mapbit(cp);
+	light_mbox_rmw(priv, LIGHT_MBOX_MASK, 0, BIT(mask_bit));
+
+	free_irq(priv->irq, chan);
+}
+
+static const struct mbox_chan_ops light_mbox_ops = {
+	.send_data = light_mbox_send_data,
+	.startup = light_mbox_startup,
+	.shutdown = light_mbox_shutdown,
+};
+
+static void light_mbox_init_generic(struct light_mbox_priv *priv)
+{
+	/* Set default configuration */
+	light_mbox_write(priv, 0xff, LIGHT_MBOX_CLR);
+	light_mbox_write(priv, 0x0, LIGHT_MBOX_MASK);
+}
+
+static struct mbox_chan *light_mbox_xlate(struct mbox_controller *mbox,
+					  const struct of_phandle_args *sp)
+{
+	struct light_mbox_priv *priv = to_light_mbox_priv(mbox);
+	struct light_mbox_con_priv *cp;
+	u32 chan, type;
+
+	if (sp->args_count != 2) {
+		dev_err(mbox->dev, "Invalid argument count %d\n", sp->args_count);
+		return ERR_PTR(-EINVAL);
+	}
+
+	chan = sp->args[0]; /* comm remote channel */
+	type = sp->args[1]; /* comm channel type */
+
+	if (chan >= mbox->num_chans) {
+		dev_err(mbox->dev, "Not supported channel number: %d\n", chan);
+		return ERR_PTR(-EINVAL);
+	}
+
+	if (chan == priv->cur_icu_cpu_id) {
+		dev_err(mbox->dev, "Cannot communicate with yourself\n");
+		return ERR_PTR(-EINVAL);
+	}
+
+	if (type > LIGHT_MBOX_TYPE_DB) {
+		dev_err(mbox->dev, "Not supported the type for channel[%d]\n", chan);
+		return ERR_PTR(-EINVAL);
+	}
+
+	cp = mbox->chans[chan].con_priv;
+	cp->type = type;
+
+	return &mbox->chans[chan];
+}
+
+static int light_mbox_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct light_mbox_priv *priv;
+	struct resource *res;
+	unsigned int remote_idx = 0;
+	unsigned int i;
+	int ret;
+
+	priv = devm_kzalloc(dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	if (of_property_read_u32(np, "icu_cpu_id", &priv->cur_icu_cpu_id)) {
+		dev_err(dev, "icu_cpu_id is missing\n");
+		return -EINVAL;
+	}
+
+	if (priv->cur_icu_cpu_id != LIGHT_MBOX_ICU_CPU0 &&
+	    priv->cur_icu_cpu_id != LIGHT_MBOX_ICU_CPU3) {
+		dev_err(dev, "icu_cpu_id is invalid\n");
+		return -EINVAL;
+	}
+
+	priv->dev = dev;
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "local_base");
+	priv->local_icu[LIGHT_MBOX_ICU_CPU0] = devm_ioremap_resource(dev, res);
+	if (IS_ERR(priv->local_icu[LIGHT_MBOX_ICU_CPU0]))
+		return PTR_ERR(priv->local_icu[LIGHT_MBOX_ICU_CPU0]);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "remote_icu0");
+	priv->remote_icu[0] = devm_ioremap_resource(dev, res);
+	if (IS_ERR(priv->remote_icu[0]))
+		return PTR_ERR(priv->remote_icu[0]);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "remote_icu1");
+	priv->remote_icu[1] = devm_ioremap_resource(dev, res);
+	if (IS_ERR(priv->remote_icu[1]))
+		return PTR_ERR(priv->remote_icu[1]);
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "remote_icu2");
+	priv->remote_icu[2] = devm_ioremap_resource(dev, res);
+	if (IS_ERR(priv->remote_icu[2]))
+		return PTR_ERR(priv->remote_icu[2]);
+
+	priv->local_icu[LIGHT_MBOX_ICU_CPU1] = priv->local_icu[LIGHT_MBOX_ICU_CPU0] +
+					       LIGHT_MBOX_CHAN_RES_SIZE;
+	priv->local_icu[LIGHT_MBOX_ICU_CPU2] = priv->local_icu[LIGHT_MBOX_ICU_CPU1] +
+					       LIGHT_MBOX_CHAN_RES_SIZE;
+	priv->local_icu[LIGHT_MBOX_ICU_CPU3] = priv->local_icu[LIGHT_MBOX_ICU_CPU2] +
+					       LIGHT_MBOX_CHAN_RES_SIZE;
+
+	priv->cur_cpu_ch_base = priv->local_icu[priv->cur_icu_cpu_id];
+
+	priv->irq = platform_get_irq(pdev, 0);
+	if (priv->irq < 0)
+		return priv->irq;
+
+	priv->clk = devm_clk_get(dev, NULL);
+	if (IS_ERR(priv->clk)) {
+		if (PTR_ERR(priv->clk) != -ENOENT)
+			return PTR_ERR(priv->clk);
+
+		priv->clk = NULL;
+	}
+
+	ret = clk_prepare_enable(priv->clk);
+	if (ret) {
+		dev_err(dev, "Failed to enable clock\n");
+		return ret;
+	}
+
+	/* init the chans */
+	for (i = 0; i < LIGHT_MBOX_CHANS; i++) {
+		struct light_mbox_con_priv *cp = &priv->con_priv[i];
+
+		cp->idx = i;
+		cp->chan = &priv->mbox_chans[i];
+		priv->mbox_chans[i].con_priv = cp;
+		snprintf(cp->irq_desc, sizeof(cp->irq_desc),
+			 "light_mbox_chan[%i]", cp->idx);
+
+		cp->comm_local_base = priv->local_icu[i];
+		if (i != priv->cur_icu_cpu_id) {
+			cp->comm_remote_base = priv->remote_icu[remote_idx];
+			remote_idx++;
+		}
+	}
+
+	spin_lock_init(&priv->mbox_lock);
+
+	priv->mbox.dev = dev;
+	priv->mbox.ops = &light_mbox_ops;
+	priv->mbox.chans = priv->mbox_chans;
+	priv->mbox.num_chans = LIGHT_MBOX_CHANS;
+	priv->mbox.of_xlate = light_mbox_xlate;
+	priv->mbox.txdone_irq = true;
+
+	platform_set_drvdata(pdev, priv);
+
+	light_mbox_init_generic(priv);
+
+	return devm_mbox_controller_register(dev, &priv->mbox);
+}
+
+static int light_mbox_remove(struct platform_device *pdev)
+{
+	struct light_mbox_priv *priv = platform_get_drvdata(pdev);
+
+	clk_disable_unprepare(priv->clk);
+
+	return 0;
+}
+
+static const struct of_device_id light_mbox_dt_ids[] = {
+	{ .compatible = "thead,light-mbox" },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, light_mbox_dt_ids);
+
+static struct platform_driver light_mbox_driver = {
+	.probe		= light_mbox_probe,
+	.remove		= light_mbox_remove,
+	.driver = {
+		.name	= "light_mbox",
+		.of_match_table = light_mbox_dt_ids,
+	},
+};
+module_platform_driver(light_mbox_driver);
+
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light mailbox IPC driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/mmc/host/Kconfig b/drivers/mmc/host/Kconfig
index bc7e2ad37002..5c705adef829 100644
--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -654,6 +654,20 @@ config MMC_SDHCI_SPRD
 
 	  If unsure, say N.
 
+config MMC_SDHCI_SOPHGO
+	tristate "Sophgo/BitMain SDIO host Controller"
+	depends on MMC_SDHCI_PLTFM
+	help
+	  This selects the SDIO Host Controller in Sophgo/BitMain
+	  SoCs.
+
+	  If you have a controller with this interface, say Y or M here.
+
+	  If unsure, say N.
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called sdhci-sophgo.
+
 config MMC_TMIO_CORE
 	tristate
 
diff --git a/drivers/mmc/host/Makefile b/drivers/mmc/host/Makefile
index a693fa3d3f1c..36976786afe2 100644
--- a/drivers/mmc/host/Makefile
+++ b/drivers/mmc/host/Makefile
@@ -95,6 +95,7 @@ obj-$(CONFIG_MMC_SDHCI_MICROCHIP_PIC32)	+= sdhci-pic32.o
 obj-$(CONFIG_MMC_SDHCI_BRCMSTB)		+= sdhci-brcmstb.o
 obj-$(CONFIG_MMC_SDHCI_OMAP)		+= sdhci-omap.o
 obj-$(CONFIG_MMC_SDHCI_SPRD)		+= sdhci-sprd.o
+obj-$(CONFIG_MMC_SDHCI_SOPHGO)		+= sdhci-sophgo.o
 obj-$(CONFIG_MMC_SUNPLUS)		+= sunplus-mmc.o
 obj-$(CONFIG_MMC_CQHCI)			+= cqhci.o
 cqhci-y					+= cqhci-core.o
diff --git a/drivers/mmc/host/sdhci-of-dwcmshc.c b/drivers/mmc/host/sdhci-of-dwcmshc.c
index a0524127ca07..1a737a239d30 100644
--- a/drivers/mmc/host/sdhci-of-dwcmshc.c
+++ b/drivers/mmc/host/sdhci-of-dwcmshc.c
@@ -8,6 +8,7 @@
  */
 
 #include <linux/acpi.h>
+#include <linux/bitfield.h>
 #include <linux/clk.h>
 #include <linux/dma-mapping.h>
 #include <linux/iopoll.h>
@@ -35,6 +36,21 @@
 #define DWCMSHC_CARD_IS_EMMC		BIT(0)
 #define DWCMSHC_ENHANCED_STROBE		BIT(8)
 #define DWCMSHC_EMMC_ATCTRL		0x40
+/* Tuning and auto-tuning fields in AT_CTRL_R control register */
+#define AT_CTRL_AT_EN			BIT(0) /* autotuning is enabled */
+#define AT_CTRL_CI_SEL			BIT(1) /* interval to drive center phase select */
+#define AT_CTRL_SWIN_TH_EN		BIT(2) /* sampling window threshold enable */
+#define AT_CTRL_RPT_TUNE_ERR		BIT(3) /* enable reporting framing errors */
+#define AT_CTRL_SW_TUNE_EN		BIT(4) /* enable software managed tuning */
+#define AT_CTRL_WIN_EDGE_SEL_MASK	GENMASK(11, 8) /* bits [11:8] */
+#define AT_CTRL_WIN_EDGE_SEL		0xf /* sampling window edge select */
+#define AT_CTRL_TUNE_CLK_STOP_EN	BIT(16) /* clocks stopped during phase code change */
+#define AT_CTRL_PRE_CHANGE_DLY_MASK	GENMASK(18, 17) /* bits [18:17] */
+#define AT_CTRL_PRE_CHANGE_DLY		0x1  /* 2-cycle latency */
+#define AT_CTRL_POST_CHANGE_DLY_MASK	GENMASK(20, 19) /* bits [20:19] */
+#define AT_CTRL_POST_CHANGE_DLY		0x3  /* 4-cycle latency */
+#define AT_CTRL_SWIN_TH_VAL_MASK	GENMASK(31, 24) /* bits [31:24] */
+#define AT_CTRL_SWIN_TH_VAL		0x9  /* sampling window threshold */
 
 /* Rockchip specific Registers */
 #define DWCMSHC_EMMC_DLL_CTRL		0x800
@@ -72,6 +88,82 @@
 	(((x) & DWCMSHC_EMMC_DLL_TIMEOUT) == 0))
 #define RK35xx_MAX_CLKS 3
 
+/* PHY register area pointer */
+#define DWC_MSHC_PTR_PHY_R	0x300
+
+/* PHY general configuration */
+#define PHY_CNFG_R		(DWC_MSHC_PTR_PHY_R + 0x00)
+#define PHY_CNFG_RSTN_DEASSERT	0x1  /* Deassert PHY reset */
+#define PHY_CNFG_PAD_SP_MASK	GENMASK(19, 16) /* bits [19:16] */
+#define PHY_CNFG_PAD_SP		0x0c /* PMOS TX drive strength */
+#define PHY_CNFG_PAD_SN_MASK	GENMASK(23, 20) /* bits [23:20] */
+#define PHY_CNFG_PAD_SN		0x0c /* NMOS TX drive strength */
+
+/* PHY command/response pad settings */
+#define PHY_CMDPAD_CNFG_R	(DWC_MSHC_PTR_PHY_R + 0x04)
+
+/* PHY data pad settings */
+#define PHY_DATAPAD_CNFG_R	(DWC_MSHC_PTR_PHY_R + 0x06)
+
+/* PHY clock pad settings */
+#define PHY_CLKPAD_CNFG_R	(DWC_MSHC_PTR_PHY_R + 0x08)
+
+/* PHY strobe pad settings */
+#define PHY_STBPAD_CNFG_R	(DWC_MSHC_PTR_PHY_R + 0x0a)
+
+/* PHY reset pad settings */
+#define PHY_RSTNPAD_CNFG_R	(DWC_MSHC_PTR_PHY_R + 0x0c)
+
+/* Bitfields are common for all pad settings */
+#define PHY_PAD_RXSEL_1V8		0x1 /* Receiver type select for 1.8V */
+#define PHY_PAD_RXSEL_3V3		0x2 /* Receiver type select for 3.3V */
+
+#define PHY_PAD_WEAKPULL_MASK		GENMASK(4, 3) /* bits [4:3] */
+#define PHY_PAD_WEAKPULL_PULLUP		0x1 /* Weak pull up enabled */
+#define PHY_PAD_WEAKPULL_PULLDOWN	0x2 /* Weak pull down enabled */
+
+#define PHY_PAD_TXSLEW_CTRL_P_MASK	GENMASK(8, 5) /* bits [8:5] */
+#define PHY_PAD_TXSLEW_CTRL_P		0x3 /* Slew control for P-Type pad TX */
+#define PHY_PAD_TXSLEW_CTRL_N_MASK	GENMASK(12, 9) /* bits [12:9] */
+#define PHY_PAD_TXSLEW_CTRL_N		0x3 /* Slew control for N-Type pad TX */
+
+/* PHY CLK delay line settings */
+#define PHY_SDCLKDL_CNFG_R		(DWC_MSHC_PTR_PHY_R + 0x1d)
+#define PHY_SDCLKDL_CNFG_UPDATE	BIT(4) /* set before writing to SDCLKDL_DC */
+
+/* PHY CLK delay line delay code */
+#define PHY_SDCLKDL_DC_R		(DWC_MSHC_PTR_PHY_R + 0x1e)
+#define PHY_SDCLKDL_DC_INITIAL		0x40 /* initial delay code */
+#define PHY_SDCLKDL_DC_DEFAULT		0x32 /* default delay code */
+#define PHY_SDCLKDL_DC_HS400		0x18 /* delay code for HS400 mode */
+
+/* PHY drift_cclk_rx delay line configuration setting */
+#define PHY_ATDL_CNFG_R			(DWC_MSHC_PTR_PHY_R + 0x21)
+#define PHY_ATDL_CNFG_INPSEL_MASK	GENMASK(3, 2) /* bits [3:2] */
+#define PHY_ATDL_CNFG_INPSEL		0x3 /* delay line input source */
+
+/* PHY DLL control settings */
+#define PHY_DLL_CTRL_R			(DWC_MSHC_PTR_PHY_R + 0x24)
+#define PHY_DLL_CTRL_DISABLE		0x0 /* PHY DLL is enabled */
+#define PHY_DLL_CTRL_ENABLE		0x1 /* PHY DLL is disabled */
+
+/* PHY DLL  configuration register 1 */
+#define PHY_DLL_CNFG1_R			(DWC_MSHC_PTR_PHY_R + 0x25)
+#define PHY_DLL_CNFG1_SLVDLY_MASK	GENMASK(5, 4) /* bits [5:4] */
+#define PHY_DLL_CNFG1_SLVDLY		0x2 /* DLL slave update delay input */
+#define PHY_DLL_CNFG1_WAITCYCLE		0x5 /* DLL wait cycle input */
+
+/* PHY DLL configuration register 2 */
+#define PHY_DLL_CNFG2_R			(DWC_MSHC_PTR_PHY_R + 0x26)
+#define PHY_DLL_CNFG2_JUMPSTEP		0xa /* DLL jump step input */
+
+/* PHY DLL master and slave delay line configuration settings */
+#define PHY_DLLDL_CNFG_R		(DWC_MSHC_PTR_PHY_R + 0x28)
+#define PHY_DLLDL_CNFG_SLV_INPSEL_MASK	GENMASK(6, 5) /* bits [6:5] */
+#define PHY_DLLDL_CNFG_SLV_INPSEL	0x3 /* clock source select for slave DL */
+
+#define FLAG_IO_FIXED_1V8	BIT(0)
+
 #define BOUNDARY_OK(addr, len) \
 	((addr | (SZ_128M - 1)) == ((addr + len - 1) | (SZ_128M - 1)))
 
@@ -92,6 +184,8 @@ struct dwcmshc_priv {
 	struct clk	*bus_clk;
 	int vendor_specific_area1; /* P_VENDOR_SPECIFIC_AREA reg */
 	void *priv; /* pointer to SoC private stuff */
+	u16 delay_line;
+	u16 flags;
 };
 
 /*
@@ -157,6 +251,127 @@ static void dwcmshc_request(struct mmc_host *mmc, struct mmc_request *mrq)
 	sdhci_request(mmc, mrq);
 }
 
+static void dwcmshc_phy_1_8v_init(struct sdhci_host *host)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+	u32 val;
+
+	/* deassert phy reset & set tx drive strength */
+	val = PHY_CNFG_RSTN_DEASSERT;
+	val |= FIELD_PREP(PHY_CNFG_PAD_SP_MASK, PHY_CNFG_PAD_SP);
+	val |= FIELD_PREP(PHY_CNFG_PAD_SN_MASK, PHY_CNFG_PAD_SN);
+	sdhci_writel(host, val, PHY_CNFG_R);
+
+	/* disable delay line */
+	sdhci_writeb(host, PHY_SDCLKDL_CNFG_UPDATE, PHY_SDCLKDL_CNFG_R);
+
+	/* set delay line */
+	sdhci_writeb(host, priv->delay_line, PHY_SDCLKDL_DC_R);
+	sdhci_writeb(host, PHY_DLL_CNFG2_JUMPSTEP, PHY_DLL_CNFG2_R);
+
+	/* enable delay lane */
+	val = sdhci_readb(host, PHY_SDCLKDL_CNFG_R);
+	val &= ~(PHY_SDCLKDL_CNFG_UPDATE);
+	sdhci_writeb(host, val, PHY_SDCLKDL_CNFG_R);
+
+	/* configure phy pads */
+	val = PHY_PAD_RXSEL_1V8;
+	val |= FIELD_PREP(PHY_PAD_WEAKPULL_MASK, PHY_PAD_WEAKPULL_PULLUP);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_CMDPAD_CNFG_R);
+	sdhci_writew(host, val, PHY_DATAPAD_CNFG_R);
+	sdhci_writew(host, val, PHY_RSTNPAD_CNFG_R);
+
+	val = FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_CLKPAD_CNFG_R);
+
+	val = PHY_PAD_RXSEL_1V8;
+	val |= FIELD_PREP(PHY_PAD_WEAKPULL_MASK, PHY_PAD_WEAKPULL_PULLDOWN);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_STBPAD_CNFG_R);
+
+	/* enable data strobe mode */
+	sdhci_writeb(host, FIELD_PREP(PHY_DLLDL_CNFG_SLV_INPSEL_MASK, PHY_DLLDL_CNFG_SLV_INPSEL),
+		     PHY_DLLDL_CNFG_R);
+
+	/* enable phy dll */
+	sdhci_writeb(host, PHY_DLL_CTRL_ENABLE, PHY_DLL_CTRL_R);
+}
+
+static void dwcmshc_phy_3_3v_init(struct sdhci_host *host)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+	u32 val;
+
+	/* deassert phy reset & set tx drive strength */
+	val = PHY_CNFG_RSTN_DEASSERT;
+	val |= FIELD_PREP(PHY_CNFG_PAD_SP_MASK, PHY_CNFG_PAD_SP);
+	val |= FIELD_PREP(PHY_CNFG_PAD_SN_MASK, PHY_CNFG_PAD_SN);
+	sdhci_writel(host, val, PHY_CNFG_R);
+
+	/* disable delay line */
+	sdhci_writeb(host, PHY_SDCLKDL_CNFG_UPDATE, PHY_SDCLKDL_CNFG_R);
+
+	/* set delay line */
+	sdhci_writeb(host, priv->delay_line, PHY_SDCLKDL_DC_R);
+	sdhci_writeb(host, PHY_DLL_CNFG2_JUMPSTEP, PHY_DLL_CNFG2_R);
+
+	/* enable delay lane */
+	val = sdhci_readb(host, PHY_SDCLKDL_CNFG_R);
+	val &= ~(PHY_SDCLKDL_CNFG_UPDATE);
+	sdhci_writeb(host, val, PHY_SDCLKDL_CNFG_R);
+
+	/* configure phy pads */
+	val = PHY_PAD_RXSEL_3V3;
+	val |= FIELD_PREP(PHY_PAD_WEAKPULL_MASK, PHY_PAD_WEAKPULL_PULLUP);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_CMDPAD_CNFG_R);
+	sdhci_writew(host, val, PHY_DATAPAD_CNFG_R);
+	sdhci_writew(host, val, PHY_RSTNPAD_CNFG_R);
+
+	val = FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_CLKPAD_CNFG_R);
+
+	val = PHY_PAD_RXSEL_3V3;
+	val |= FIELD_PREP(PHY_PAD_WEAKPULL_MASK, PHY_PAD_WEAKPULL_PULLDOWN);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_P_MASK, PHY_PAD_TXSLEW_CTRL_P);
+	val |= FIELD_PREP(PHY_PAD_TXSLEW_CTRL_N_MASK, PHY_PAD_TXSLEW_CTRL_N);
+	sdhci_writew(host, val, PHY_STBPAD_CNFG_R);
+
+	/* enable phy dll */
+	sdhci_writeb(host, PHY_DLL_CTRL_ENABLE, PHY_DLL_CTRL_R);
+}
+
+static void th1520_sdhci_set_phy(struct sdhci_host *host)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+	u32 emmc_caps = MMC_CAP2_NO_SD | MMC_CAP2_NO_SDIO;
+	u16 emmc_ctrl;
+
+	/* Before power on, set PHY configs */
+	if (priv->flags & FLAG_IO_FIXED_1V8)
+		dwcmshc_phy_1_8v_init(host);
+	else
+		dwcmshc_phy_3_3v_init(host);
+
+	if ((host->mmc->caps2 & emmc_caps) == emmc_caps) {
+		emmc_ctrl = sdhci_readw(host, priv->vendor_specific_area1 + DWCMSHC_EMMC_CONTROL);
+		emmc_ctrl |= DWCMSHC_CARD_IS_EMMC;
+		sdhci_writew(host, emmc_ctrl, priv->vendor_specific_area1 + DWCMSHC_EMMC_CONTROL);
+	}
+
+	sdhci_writeb(host, FIELD_PREP(PHY_DLL_CNFG1_SLVDLY_MASK, PHY_DLL_CNFG1_SLVDLY) |
+		     PHY_DLL_CNFG1_WAITCYCLE, PHY_DLL_CNFG1_R);
+}
+
 static void dwcmshc_set_uhs_signaling(struct sdhci_host *host,
 				      unsigned int timing)
 {
@@ -189,9 +404,25 @@ static void dwcmshc_set_uhs_signaling(struct sdhci_host *host,
 		ctrl_2 |= DWCMSHC_CTRL_HS400;
 	}
 
+	if (priv->flags & FLAG_IO_FIXED_1V8)
+		ctrl_2 |= SDHCI_CTRL_VDD_180;
 	sdhci_writew(host, ctrl_2, SDHCI_HOST_CONTROL2);
 }
 
+static void th1520_set_uhs_signaling(struct sdhci_host *host,
+				     unsigned int timing)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+
+	dwcmshc_set_uhs_signaling(host, timing);
+	if (timing == MMC_TIMING_MMC_HS400)
+		priv->delay_line = PHY_SDCLKDL_DC_HS400;
+	else
+		sdhci_writeb(host, 0, PHY_DLLDL_CNFG_R);
+	th1520_sdhci_set_phy(host);
+}
+
 static void dwcmshc_hs400_enhanced_strobe(struct mmc_host *mmc,
 					  struct mmc_ios *ios)
 {
@@ -338,6 +569,79 @@ static void rk35xx_sdhci_reset(struct sdhci_host *host, u8 mask)
 	sdhci_reset(host, mask);
 }
 
+static int th1520_execute_tuning(struct sdhci_host *host, u32 opcode)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+	u32 val = 0;
+
+	if (host->flags & SDHCI_HS400_TUNING)
+		return 0;
+
+	sdhci_writeb(host, FIELD_PREP(PHY_ATDL_CNFG_INPSEL_MASK, PHY_ATDL_CNFG_INPSEL),
+		     PHY_ATDL_CNFG_R);
+	val = sdhci_readl(host, priv->vendor_specific_area1 + DWCMSHC_EMMC_ATCTRL);
+
+	/*
+	 * configure tuning settings:
+	 *  - center phase select code driven in block gap interval
+	 *  - disable reporting of framing errors
+	 *  - disable software managed tuning
+	 *  - disable user selection of sampling window edges,
+	 *    instead tuning calculated edges are used
+	 */
+	val &= ~(AT_CTRL_CI_SEL | AT_CTRL_RPT_TUNE_ERR | AT_CTRL_SW_TUNE_EN |
+		 FIELD_PREP(AT_CTRL_WIN_EDGE_SEL_MASK, AT_CTRL_WIN_EDGE_SEL));
+
+	/*
+	 * configure tuning settings:
+	 *  - enable auto-tuning
+	 *  - enable sampling window threshold
+	 *  - stop clocks during phase code change
+	 *  - set max latency in cycles between tx and rx clocks
+	 *  - set max latency in cycles to switch output phase
+	 *  - set max sampling window threshold value
+	 */
+	val |= AT_CTRL_AT_EN | AT_CTRL_SWIN_TH_EN | AT_CTRL_TUNE_CLK_STOP_EN;
+	val |= FIELD_PREP(AT_CTRL_PRE_CHANGE_DLY_MASK, AT_CTRL_PRE_CHANGE_DLY);
+	val |= FIELD_PREP(AT_CTRL_POST_CHANGE_DLY_MASK, AT_CTRL_POST_CHANGE_DLY);
+	val |= FIELD_PREP(AT_CTRL_SWIN_TH_VAL_MASK, AT_CTRL_SWIN_TH_VAL);
+
+	sdhci_writel(host, val, priv->vendor_specific_area1 + DWCMSHC_EMMC_ATCTRL);
+	val = sdhci_readl(host, priv->vendor_specific_area1 + DWCMSHC_EMMC_ATCTRL);
+
+	/* perform tuning */
+	sdhci_start_tuning(host);
+	host->tuning_err = __sdhci_execute_tuning(host, opcode);
+	if (host->tuning_err) {
+		/* disable auto-tuning upon tuning error */
+		val &= ~AT_CTRL_AT_EN;
+		sdhci_writel(host, val, priv->vendor_specific_area1 + DWCMSHC_EMMC_ATCTRL);
+		dev_err(mmc_dev(host->mmc), "tuning failed: %d\n", host->tuning_err);
+		return -EIO;
+	}
+	sdhci_end_tuning(host);
+
+	return 0;
+}
+
+static void th1520_sdhci_reset(struct sdhci_host *host, u8 mask)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct dwcmshc_priv *priv = sdhci_pltfm_priv(pltfm_host);
+	u16 ctrl_2;
+
+	sdhci_reset(host, mask);
+
+	if (priv->flags & FLAG_IO_FIXED_1V8) {
+		ctrl_2 = sdhci_readw(host, SDHCI_HOST_CONTROL2);
+		if (!(ctrl_2 & SDHCI_CTRL_VDD_180)) {
+			ctrl_2 |= SDHCI_CTRL_VDD_180;
+			sdhci_writew(host, ctrl_2, SDHCI_HOST_CONTROL2);
+		}
+	}
+}
+
 static const struct sdhci_ops sdhci_dwcmshc_ops = {
 	.set_clock		= sdhci_set_clock,
 	.set_bus_width		= sdhci_set_bus_width,
@@ -356,6 +660,17 @@ static const struct sdhci_ops sdhci_dwcmshc_rk35xx_ops = {
 	.adma_write_desc	= dwcmshc_adma_write_desc,
 };
 
+static const struct sdhci_ops sdhci_dwcmshc_th1520_ops = {
+	.set_clock		= sdhci_set_clock,
+	.set_bus_width		= sdhci_set_bus_width,
+	.set_uhs_signaling	= th1520_set_uhs_signaling,
+	.get_max_clock		= dwcmshc_get_max_clock,
+	.reset			= th1520_sdhci_reset,
+	.adma_write_desc	= dwcmshc_adma_write_desc,
+	.voltage_switch		= dwcmshc_phy_1_8v_init,
+	.platform_execute_tuning = &th1520_execute_tuning,
+};
+
 static const struct sdhci_pltfm_data sdhci_dwcmshc_pdata = {
 	.ops = &sdhci_dwcmshc_ops,
 	.quirks = SDHCI_QUIRK_CAP_CLOCK_BASE_BROKEN,
@@ -379,6 +694,12 @@ static const struct sdhci_pltfm_data sdhci_dwcmshc_rk35xx_pdata = {
 		   SDHCI_QUIRK2_CLOCK_DIV_ZERO_BROKEN,
 };
 
+static const struct sdhci_pltfm_data sdhci_dwcmshc_th1520_pdata = {
+	.ops = &sdhci_dwcmshc_th1520_ops,
+	.quirks = SDHCI_QUIRK_CAP_CLOCK_BASE_BROKEN,
+	.quirks2 = SDHCI_QUIRK2_PRESET_VALUE_BROKEN,
+};
+
 static int dwcmshc_rk35xx_init(struct sdhci_host *host, struct dwcmshc_priv *dwc_priv)
 {
 	int err;
@@ -447,6 +768,10 @@ static const struct of_device_id sdhci_dwcmshc_dt_ids[] = {
 		.compatible = "snps,dwcmshc-sdhci",
 		.data = &sdhci_dwcmshc_pdata,
 	},
+	{
+		.compatible = "thead,th1520-dwcmshc",
+		.data = &sdhci_dwcmshc_th1520_pdata,
+	},
 	{},
 };
 MODULE_DEVICE_TABLE(of, sdhci_dwcmshc_dt_ids);
@@ -542,6 +867,30 @@ static int dwcmshc_probe(struct platform_device *pdev)
 			goto err_clk;
 	}
 
+	if (pltfm_data == &sdhci_dwcmshc_th1520_pdata) {
+		priv->delay_line = PHY_SDCLKDL_DC_DEFAULT;
+
+		if ((device_property_read_bool(dev, "mmc-ddr-1_8v")) |
+		    (device_property_read_bool(dev, "mmc-hs200-1_8v")) |
+		    (device_property_read_bool(dev, "mmc-hs400-1_8v")))
+			priv->flags |= FLAG_IO_FIXED_1V8;
+		else
+			priv->flags &= ~FLAG_IO_FIXED_1V8;
+
+		/*
+		 * start_signal_voltage_switch() will try 3.3V first
+		 * then 1.8V. Use SDHCI_SIGNALING_180 rather than
+		 * SDHCI_SIGNALING_330 to avoid setting voltage to 3.3V
+		 * in sdhci_start_signal_voltage_switch().
+		 */
+		if (priv->flags & FLAG_IO_FIXED_1V8) {
+			host->flags &= ~SDHCI_SIGNALING_330;
+			host->flags |=  SDHCI_SIGNALING_180;
+		}
+
+		sdhci_enable_v4_mode(host);
+	}
+
 #ifdef CONFIG_ACPI
 	if (pltfm_data == &sdhci_dwcmshc_bf3_pdata)
 		sdhci_enable_v4_mode(host);
diff --git a/drivers/mmc/host/sdhci-sophgo.c b/drivers/mmc/host/sdhci-sophgo.c
new file mode 100644
index 000000000000..8200ccaa68f6
--- /dev/null
+++ b/drivers/mmc/host/sdhci-sophgo.c
@@ -0,0 +1,619 @@
+/*
+ * Sophgo SDHCI Platform driver
+ *
+ * Copyright (c) 2013-2014, The Linux Foundation. All rights reserved.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 and
+ * only version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ */
+
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/delay.h>
+#include <linux/mmc/mmc.h>
+#include <linux/slab.h>
+#include <linux/reset.h>
+#include "sdhci-pltfm.h"
+#include "sdhci-sophgo.h"
+
+#define DRIVER_NAME "bm"
+
+#define BM_SDHCI_VENDOR_OFFSET		0x500
+#define BM_SDHCI_VENDOR_MSHC_CTRL_R (BM_SDHCI_VENDOR_OFFSET + 0x8)
+#define BM_SDHCI_VENDOR_A_CTRL_R (BM_SDHCI_VENDOR_OFFSET + 0x40)
+#define BM_SDHCI_VENDOR_A_STAT_R (BM_SDHCI_VENDOR_OFFSET + 0x44)
+
+static void bm_sdhci_set_tap(struct sdhci_host *host, unsigned int tap)
+{
+	sdhci_writel(host, 0x0, BM_SDHCI_VENDOR_MSHC_CTRL_R);
+	sdhci_writel(host, 0x18, BM_SDHCI_VENDOR_A_CTRL_R);
+	sdhci_writel(host, tap, BM_SDHCI_VENDOR_A_STAT_R);
+}
+
+static int sdhci_bm_execute_software_tuning(struct sdhci_host *host, u32 opcode)
+{
+	unsigned int maxwidth = 0;
+	unsigned int tuntap;
+	struct {
+		unsigned int start;
+		unsigned int end;
+		unsigned int width;
+	} tunlist[4];
+	unsigned int listcount;
+	unsigned int listsel;
+
+	unsigned int tun = 0;
+	unsigned int max = 256;
+	int i;
+
+	listcount = 0;
+	for (i = 0; i < ARRAY_SIZE(tunlist); i++) {
+		while (tun < max) {
+			bm_sdhci_set_tap(host, tun);
+			if (!mmc_send_tuning(host->mmc, opcode, NULL))
+				break;
+			tun++;
+		}
+		tunlist[i].start = tun;
+		tun++;
+		while (tun < max) {
+			bm_sdhci_set_tap(host, tun);
+			if (mmc_send_tuning(host->mmc, opcode, NULL))
+				break;
+			tun++;
+		}
+		tunlist[i].end = tun-1;
+		tunlist[i].width = tunlist[i].end - tunlist[i].start;
+		listcount++;
+		tun++;
+		pr_info("%s id:%d start:%d end:%d width:%d\n", mmc_hostname(host->mmc),
+			i, tunlist[i].start, tunlist[i].end, tunlist[i].width);
+		if (tun >= max)
+			break;
+	}
+
+	//find maxwidth
+	listsel = 0;
+	for (i = 0; i < listcount; i++) {
+		if (tunlist[i].width > maxwidth) {
+			maxwidth = tunlist[i].width;
+			listsel = i;
+		}
+	}
+	tuntap = tunlist[listsel].start + (tunlist[listsel].width/2);
+
+	/* The TRM states the ideal tap value is at 75% in the passing range. */
+	bm_sdhci_set_tap(host, tuntap);
+	pr_info("%s listsel:%d tuntap:%d\n",
+		mmc_hostname(host->mmc), listsel, tuntap);
+
+	return mmc_send_tuning(host->mmc, opcode, NULL);
+}
+
+static int sdhci_bm_select_drive_strength(struct mmc_card *card,
+		unsigned int max_dtr, int host_drv,
+		int card_drv, int *drv_type)
+{
+	struct sdhci_host *host = mmc_priv(card->host);
+	struct mmc_host *mmc = host->mmc;
+	uint32_t reg;
+	int driver_type;
+
+	pr_info("%s max_dtr %d, host_drv %d, card_drv %d, drv_type %d\n",
+		mmc_hostname(mmc),
+		max_dtr, host_drv, card_drv, *drv_type);
+
+	driver_type = MMC_SET_DRIVER_TYPE_C;
+	*drv_type = MMC_SET_DRIVER_TYPE_C;
+
+	reg = (1 << PHY_CNFG_PHY_PWRGOOD) | (0xe << PHY_CNFG_PAD_SP) |
+		(0xe << PHY_CNFG_PAD_SN) | (1 << PHY_CNFG_PHY_RSTN);
+	sdhci_writel(host, reg, SDHCI_P_PHY_CNFG);
+
+	return driver_type;
+}
+
+static void sdhci_bm_set_uhs_signaling(struct sdhci_host *host, unsigned int uhs)
+{
+	struct mmc_host *mmc = host->mmc;
+	u16 ctrl_2;
+
+	ctrl_2 = sdhci_readw(host, SDHCI_HOST_CONTROL2);
+	/* Select Bus Speed Mode for host */
+	ctrl_2 &= ~SDHCI_CTRL_UHS_MASK;
+	switch (uhs) {
+	case MMC_TIMING_UHS_SDR12:
+		ctrl_2 |= SDHCI_CTRL_UHS_SDR12;
+		break;
+	case MMC_TIMING_UHS_SDR25:
+		ctrl_2 |= SDHCI_CTRL_UHS_SDR25;
+		break;
+	case MMC_TIMING_UHS_SDR50:
+		ctrl_2 |= SDHCI_CTRL_UHS_SDR50;
+		break;
+	case MMC_TIMING_MMC_HS200:
+	case MMC_TIMING_UHS_SDR104:
+		ctrl_2 |= SDHCI_CTRL_UHS_SDR104;
+		break;
+	case MMC_TIMING_UHS_DDR50:
+	case MMC_TIMING_MMC_DDR52:
+		ctrl_2 |= SDHCI_CTRL_UHS_DDR50;
+		break;
+	}
+
+	/*
+	 * When clock frequency is less than 100MHz, the feedback clock must be
+	 * provided and DLL must not be used so that tuning can be skipped. To
+	 * provide feedback clock, the mode selection can be any value less
+	 * than 3'b011 in bits [2:0] of HOST CONTROL2 register.
+	 */
+	if (host->clock <= 100000000 &&
+	    (uhs == MMC_TIMING_MMC_HS400 ||
+	     uhs == MMC_TIMING_MMC_HS200 ||
+	     uhs == MMC_TIMING_UHS_SDR104))
+		ctrl_2 &= ~SDHCI_CTRL_UHS_MASK;
+
+	dev_dbg(mmc_dev(mmc), "%s: clock=%u uhs=%u ctrl_2=0x%x\n",
+		mmc_hostname(host->mmc), host->clock, uhs, ctrl_2);
+	sdhci_writew(host, ctrl_2, SDHCI_HOST_CONTROL2);
+}
+
+static unsigned int bm_sdhci_get_min_clock(struct sdhci_host *host)
+{
+	return 200 * 1000;
+}
+
+static unsigned int bm_sdhci_get_max_clock(struct sdhci_host *host)
+{
+	return 50 * 1000 * 1000;
+}
+
+#if 0 // FIXME, SD card not working after this.
+static void bm_sdhci_hw_reset(struct sdhci_host *host)
+{
+	struct sdhci_pltfm_host *pltfm_host;
+	struct sdhci_bm_host *bm_host;
+	struct mmc_host *mmc = host->mmc;
+
+	pltfm_host = sdhci_priv(host);
+	bm_host = sdhci_pltfm_priv(pltfm_host);
+
+	pr_info("%s hardware reset\n", mmc_hostname(mmc));
+	reset_control_assert(bm_host->reset);
+	udelay(10);
+	reset_control_deassert(bm_host->reset);
+}
+#endif
+
+void bm_sdhci_reset(struct sdhci_host *host, u8 mask)
+{
+#if 0 // FIXME, SD card not working after this.
+	bm_sdhci_hw_reset(host);
+#endif
+	sdhci_reset(host, mask);
+
+	if (mask & SDHCI_RESET_ALL)
+		bm_sdhci_phy_init(host);
+}
+
+int bm_sdhci_phy_init(struct sdhci_host *host)
+{
+	// Asset reset of phy
+	sdhci_writel(host, sdhci_readl(host, SDHCI_P_PHY_CNFG) & ~(1 << PHY_CNFG_PHY_RSTN), SDHCI_P_PHY_CNFG);
+
+	// Set PAD_SN PAD_SP
+	sdhci_writel(host,
+		     (1 << PHY_CNFG_PHY_PWRGOOD) | (0x9 << PHY_CNFG_PAD_SP) | (0x8 << PHY_CNFG_PAD_SN),
+		     SDHCI_P_PHY_CNFG);
+
+	// Set CMDPAD
+	sdhci_writew(host, (0x2 << PAD_CNFG_RXSEL) | (1 << PAD_CNFG_WEAKPULL_EN) |
+			(0x3 << PAD_CNFG_TXSLEW_CTRL_P) | (0x2 << PAD_CNFG_TXSLEW_CTRL_N), SDHCI_P_CMDPAD_CNFG);
+
+	// Set DATAPAD
+	sdhci_writew(host, (0x2 << PAD_CNFG_RXSEL) | (1 << PAD_CNFG_WEAKPULL_EN) |
+			(0x3 << PAD_CNFG_TXSLEW_CTRL_P) | (0x2 << PAD_CNFG_TXSLEW_CTRL_N), SDHCI_P_DATPAD_CNFG);
+
+	// Set CLKPAD
+	sdhci_writew(host,
+		     (0x2 << PAD_CNFG_RXSEL) | (0x3 << PAD_CNFG_TXSLEW_CTRL_P) | (0x2 << PAD_CNFG_TXSLEW_CTRL_N),
+		     SDHCI_P_CLKPAD_CNFG);
+
+	// Set STB_PAD
+	sdhci_writew(host, (0x2 << PAD_CNFG_RXSEL) | (0x2 << PAD_CNFG_WEAKPULL_EN) |
+			(0x3 << PAD_CNFG_TXSLEW_CTRL_P) | (0x2 << PAD_CNFG_TXSLEW_CTRL_N), SDHCI_P_STBPAD_CNFG);
+
+	// Set RSTPAD
+	sdhci_writew(host, (0x2 << PAD_CNFG_RXSEL) | (1 << PAD_CNFG_WEAKPULL_EN) |
+			(0x3 << PAD_CNFG_TXSLEW_CTRL_P) | (0x2 << PAD_CNFG_TXSLEW_CTRL_N), SDHCI_P_RSTNPAD_CNFG);
+
+	// Set SDCLKDL_CNFG, EXTDLY_EN = 1, fix delay
+	sdhci_writeb(host, (1 << SDCLKDL_CNFG_EXTDLY_EN), SDHCI_P_SDCLKDL_CNFG);
+
+	// Add 10 * 70ps = 0.7ns for output delay
+	sdhci_writeb(host, 10, SDHCI_P_SDCLKDL_DC);
+
+	//if (host->index == 1) {
+	//	 Set SMPLDL_CNFG, Bypass
+	sdhci_writeb(host, (1 << SMPLDL_CNFG_BYPASS_EN), SDHCI_P_SMPLDL_CNFG);
+	//}
+	//else {
+	//	Set SMPLDL_CNFG, INPSEL_CNFG = 0x2
+	//sdhci_writeb(host, (0x2 << SMPLDL_CNFG_INPSEL_CNFG), SDHCI_P_SMPLDL_CNFG);
+	//}
+
+	// Set ATDL_CNFG, tuning clk not use for init
+	sdhci_writeb(host, (2 << ATDL_CNFG_INPSEL_CNFG), SDHCI_P_ATDL_CNFG);
+
+	// deasset reset of phy
+	sdhci_writel(host, sdhci_readl(host, SDHCI_P_PHY_CNFG) | (1 << PHY_CNFG_PHY_RSTN), SDHCI_P_PHY_CNFG);
+
+	return 0;
+}
+
+void bm_sdhci_set_clock(struct sdhci_host *host, unsigned int clock)
+{
+	sdhci_set_clock(host, clock);
+
+	if (clock == 0)
+		// forward tx
+		sdhci_writeb(host, 0x0, SDHCI_P_SDCLKDL_DC);
+	else
+		// revert tx
+		sdhci_writeb(host, 0x10, SDHCI_P_SDCLKDL_DC);
+}
+
+/*
+ * If DMA addr spans 128MB boundary, we split the DMA transfer into two
+ * so that each DMA transfer doesn't exceed the boundary.
+ */
+#define BOUNDARY_OK(addr, len) \
+	((addr | (SZ_128M - 1)) == ((addr + len - 1) | (SZ_128M - 1)))
+
+static void dwcmshc_adma_write_desc(struct sdhci_host *host, void **desc,
+				    dma_addr_t addr, int len, unsigned int cmd)
+{
+	int tmplen, offset;
+
+	if (likely(!len || BOUNDARY_OK(addr, len))) {
+		sdhci_adma_write_desc(host, desc, addr, len, cmd);
+		return;
+	}
+
+	offset = addr & (SZ_128M - 1);
+	tmplen = SZ_128M - offset;
+	sdhci_adma_write_desc(host, desc, addr, tmplen, cmd);
+
+	addr += tmplen;
+	len -= tmplen;
+	sdhci_adma_write_desc(host, desc, addr, len, cmd);
+}
+
+
+/* ------------- bm palludium sdcard --------------- */
+static const struct sdhci_ops sdhci_bm_pldm_sd_ops = {
+	.reset = bm_sdhci_reset,
+	.set_clock = bm_sdhci_set_clock,
+	.set_bus_width = sdhci_set_bus_width,
+	.set_uhs_signaling = sdhci_bm_set_uhs_signaling,
+	.get_max_clock = bm_sdhci_get_max_clock,
+	.get_min_clock = bm_sdhci_get_min_clock,
+	.adma_write_desc = dwcmshc_adma_write_desc,
+};
+
+static const struct sdhci_pltfm_data sdhci_bm_pldm_sd_pdata = {
+	.ops = &sdhci_bm_pldm_sd_ops,
+	.quirks = SDHCI_QUIRK_CAP_CLOCK_BASE_BROKEN | SDHCI_QUIRK_INVERTED_WRITE_PROTECT,
+	.quirks2 = SDHCI_QUIRK2_NO_1_8_V,
+};
+
+static inline bool sdhci_data_line_cmd(struct mmc_command *cmd)
+{
+	return cmd->data || cmd->flags & MMC_RSP_BUSY;
+}
+
+static void sdhci_del_timer(struct sdhci_host *host, struct mmc_request *mrq)
+{
+	if (sdhci_data_line_cmd(mrq->cmd))
+		del_timer(&host->data_timer);
+	else
+		del_timer(&host->timer);
+}
+
+int bm_platform_execute_tuning(struct sdhci_host *host, u32 opcode)
+{
+	u16 ctrl;
+	int tuning_loop_counter = 0;
+	int err = 0;
+	unsigned long flags;
+	unsigned int tuning_count = 0;
+	bool hs400_tuning;
+	int hit = 0;
+
+	spin_lock_irqsave(&host->lock, flags);
+
+	hs400_tuning = host->flags & SDHCI_HS400_TUNING;
+	host->flags &= ~SDHCI_HS400_TUNING;
+
+	if (host->tuning_mode == SDHCI_TUNING_MODE_1)
+		tuning_count = host->tuning_count;
+
+	switch (host->timing) {
+	/* HS400 tuning is done in HS200 mode */
+	case MMC_TIMING_MMC_HS400:
+		err = -EINVAL;
+		goto out_unlock;
+
+	case MMC_TIMING_MMC_HS200:
+		/*
+		 * Periodic re-tuning for HS400 is not expected to be needed, so
+		 * disable it here.
+		 */
+		if (hs400_tuning)
+			tuning_count = 0;
+		break;
+
+	case MMC_TIMING_UHS_SDR104:
+	case MMC_TIMING_UHS_DDR50:
+		break;
+
+	case MMC_TIMING_UHS_SDR50:
+		if (host->flags & SDHCI_SDR50_NEEDS_TUNING)
+			break;
+
+	default:
+		goto out_unlock;
+	}
+
+	ctrl = sdhci_readw(host, SDHCI_HOST_CONTROL2);
+	ctrl |= SDHCI_CTRL_EXEC_TUNING;
+
+	sdhci_writel(host, SDHCI_INT_DATA_AVAIL, SDHCI_INT_ENABLE);
+	sdhci_writel(host, SDHCI_INT_DATA_AVAIL, SDHCI_SIGNAL_ENABLE);
+
+	sdhci_writew(host, 0x704b | (0x3<<4) | (0x1<<3), SDHCI_HOST_CONTROL2);/*drv_strength | 1.8v*/
+
+	sdhci_writel(host, 0, SDHCI_DMA_ADDRESS);/*sdmasa*/
+	sdhci_writel(host, 0, SDHCI_MSHC_CTRL);
+
+	sdhci_writel(host, 0x18, SDHCI_AT_CTRL);
+
+	sdhci_writew(host, 0x0, SDHCI_BLOCK_COUNT);
+	sdhci_writew(host, 0x1040, SDHCI_BLOCK_SIZE);
+	sdhci_writew(host, SDHCI_TRNS_READ, SDHCI_TRANSFER_MODE);
+
+	do {
+		struct mmc_command cmd = {0};
+		struct mmc_request mrq = {NULL};
+
+		cmd.opcode = opcode;
+		cmd.arg = 0;
+		cmd.flags = MMC_RSP_R1 | MMC_CMD_ADTC;
+		cmd.retries = 0;
+		cmd.data = NULL;
+		cmd.mrq = &mrq;
+		cmd.error = 0;
+
+		sdhci_writel(host, tuning_loop_counter, SDHCI_AT_STAT);
+		mrq.cmd = &cmd;
+		sdhci_send_command(host, &cmd);
+
+		host->cmd = NULL;
+		sdhci_del_timer(host, &mrq);
+		spin_unlock_irqrestore(&host->lock, flags);
+
+		/* Wait for Buffer Read Ready interrupt */
+		wait_event_timeout(host->buf_ready_int,
+					(host->tuning_done == 1),
+					msecs_to_jiffies(10));
+
+		spin_lock_irqsave(&host->lock, flags);
+		if (host->tuning_done == 1) {
+			u16 stat;
+
+			stat = sdhci_readw(host, SDHCI_ERR_INT_STATUS) & 0x3F;
+			if (stat == 0)
+				hit = tuning_loop_counter;
+		}
+
+		host->tuning_done = 0;
+		tuning_loop_counter++;
+		sdhci_writeb(host, 0xFF, SDHCI_INT_STATUS);
+		sdhci_writeb(host, 0xFF, SDHCI_ERR_INT_STATUS);
+		sdhci_writeb(host, SDHCI_RESET_CMD | SDHCI_RESET_DATA, SDHCI_SOFTWARE_RESET);
+	} while (tuning_loop_counter < MAX_TUNING_STEP);
+
+	if (tuning_loop_counter >= MAX_TUNING_STEP) {
+		ctrl &= ~(SDHCI_CTRL_TUNED_CLK | SDHCI_CTRL_EXEC_TUNING);
+		sdhci_writew(host, ctrl, SDHCI_HOST_CONTROL2);
+	}
+
+	sdhci_writel(host, 0, SDHCI_AT_CTRL);
+	sdhci_writeb(host, 0xFF, SDHCI_INT_STATUS);/*clear normal int*/
+	sdhci_writeb(host, 0xFF, SDHCI_ERR_INT_STATUS);/*clear error int*/
+	sdhci_writel(host, sdhci_readl(host, SDHCI_AT_CTRL) | (0x1<<4), SDHCI_AT_CTRL);/*en sw_tuning_en bit*/
+	sdhci_writel(host, (sdhci_readl(host, SDHCI_AT_STAT) & (~0xFF)) | hit, SDHCI_AT_STAT);/*center_ph_code*/
+	sdhci_writel(host, sdhci_readl(host, SDHCI_AT_CTRL) & (~(0x1<<4)), SDHCI_AT_CTRL);/*dis sw_tuning_en bit*/
+	sdhci_writeb(host, SDHCI_RESET_CMD | SDHCI_RESET_DATA, SDHCI_SOFTWARE_RESET);
+
+	if (tuning_count)
+		err = 0;
+
+	host->mmc->retune_period = err ? 0 : tuning_count;
+
+	sdhci_writel(host, host->ier, SDHCI_INT_ENABLE);
+	sdhci_writel(host, host->ier, SDHCI_SIGNAL_ENABLE);
+out_unlock:
+	spin_unlock_irqrestore(&host->lock, flags);
+	return err;
+}
+
+/* ------------- bm palludium emmc --------------- */
+static const struct sdhci_ops sdhci_bm_pldm_emmc_ops = {
+	.reset = sdhci_reset,
+	.set_clock = sdhci_set_clock,
+	.set_bus_width = sdhci_set_bus_width,
+	.set_uhs_signaling = sdhci_bm_set_uhs_signaling,
+	.get_max_clock = bm_sdhci_get_max_clock,
+	.get_min_clock = bm_sdhci_get_min_clock,
+	.platform_execute_tuning = bm_platform_execute_tuning,
+	.adma_write_desc = dwcmshc_adma_write_desc,
+};
+
+static const struct sdhci_pltfm_data sdhci_bm_pldm_emmc_pdata = {
+	.ops = &sdhci_bm_pldm_emmc_ops,
+	.quirks = SDHCI_QUIRK_CAP_CLOCK_BASE_BROKEN,
+};
+
+/* ------------ bm asic ------------ */
+static const struct sdhci_ops sdhci_bm_ops = {
+	.reset = bm_sdhci_reset,
+	.set_clock = sdhci_set_clock,
+	.set_bus_width = sdhci_set_bus_width,
+	.set_uhs_signaling = sdhci_bm_set_uhs_signaling,
+	.platform_execute_tuning = sdhci_bm_execute_software_tuning,
+	.adma_write_desc = dwcmshc_adma_write_desc,
+};
+
+static const struct sdhci_pltfm_data sdhci_bm_emmc_pdata = {
+	.ops = &sdhci_bm_ops,
+	.quirks = SDHCI_QUIRK_INVERTED_WRITE_PROTECT,
+	.quirks2 = 0,
+};
+
+static const struct sdhci_pltfm_data sdhci_bm_sd_pdata = {
+	.ops = &sdhci_bm_ops,
+	.quirks = SDHCI_QUIRK_INVERTED_WRITE_PROTECT,
+	.quirks2 = 0,
+};
+
+static const struct of_device_id sdhci_bm_dt_match[] = {
+	{.compatible = "bitmain,bm-pldm-sdcard", .data = &sdhci_bm_pldm_sd_pdata},
+	{.compatible = "bitmain,bm-pldm-emmc", .data = &sdhci_bm_pldm_emmc_pdata},
+	{.compatible = "bitmain,bm-emmc", .data = &sdhci_bm_emmc_pdata},
+	{.compatible = "bitmain,bm-sd", .data = &sdhci_bm_sd_pdata},
+	{ /* sentinel */ }
+};
+
+MODULE_DEVICE_TABLE(of, sdhci_bm_dt_match);
+
+static int sdhci_bm_probe(struct platform_device *pdev)
+{
+	struct sdhci_host *host;
+	struct sdhci_pltfm_host *pltfm_host;
+	struct sdhci_bm_host *bm_host;
+	const struct of_device_id *match;
+	const struct sdhci_pltfm_data *pdata;
+	int ret;
+
+	match = of_match_device(sdhci_bm_dt_match, &pdev->dev);
+	if (!match)
+		return -EINVAL;
+
+	pdata = match->data;
+
+	host = sdhci_pltfm_init(pdev, pdata, sizeof(*bm_host));
+	if (IS_ERR(host))
+		return PTR_ERR(host);
+
+	pltfm_host = sdhci_priv(host);
+	bm_host = sdhci_pltfm_priv(pltfm_host);
+	bm_host->mmc = host->mmc;
+	bm_host->pdev = pdev;
+	bm_host->core_mem = host->ioaddr;
+
+	ret = mmc_of_parse(host->mmc);
+	if (ret)
+		goto pltfm_free;
+
+	sdhci_get_of_property(pdev);
+
+	if (host->mmc->caps2 & MMC_CAP2_NO_SD) {
+		bm_host->reset = devm_reset_control_get(&pdev->dev, "emmc");
+		if (IS_ERR(bm_host->reset)) {
+			ret = PTR_ERR(bm_host->reset);
+			goto pltfm_free;
+		}
+
+		bm_host->clkaxi = devm_clk_get(&pdev->dev, "clk_gate_axi_emmc");
+		if (IS_ERR(bm_host->clkaxi))
+			dev_err(&pdev->dev, "get emmc clk axi failed\n");
+		else
+			clk_prepare_enable(bm_host->clkaxi);
+		bm_host->clk = devm_clk_get(&pdev->dev, "clk_gate_emmc");
+		if (IS_ERR(bm_host->clk))
+			dev_err(&pdev->dev, "get emmc clk failed\n");
+		else
+			clk_prepare_enable(bm_host->clk);
+		bm_host->clk100k = devm_clk_get(&pdev->dev, "clk_gate_100k_emmc");
+		if (IS_ERR(bm_host->clk100k))
+			dev_err(&pdev->dev, "get emmc clk 100k failed\n");
+		else
+			clk_prepare_enable(bm_host->clk100k);
+	} else if (host->mmc->caps2 & MMC_CAP2_NO_MMC) {
+		bm_host->reset = devm_reset_control_get(&pdev->dev, "sdio");
+		if (IS_ERR(bm_host->reset)) {
+			ret = PTR_ERR(bm_host->reset);
+			goto pltfm_free;
+		}
+
+		bm_host->clkaxi = devm_clk_get(&pdev->dev, "clk_gate_axi_sd");
+		if (IS_ERR(bm_host->clkaxi))
+			dev_err(&pdev->dev, "get sd clk axi failed\n");
+		else
+			clk_prepare_enable(bm_host->clkaxi);
+		bm_host->clk = devm_clk_get(&pdev->dev, "clk_gate_sd");
+		if (IS_ERR(bm_host->clk))
+			dev_err(&pdev->dev, "get sd clk failed\n");
+		else
+			clk_prepare_enable(bm_host->clk);
+		bm_host->clk100k = devm_clk_get(&pdev->dev, "clk_gate_100k_sd");
+		if (IS_ERR(bm_host->clk100k))
+			dev_err(&pdev->dev, "get sd clk 100k failed\n");
+		else
+			clk_prepare_enable(bm_host->clk100k);
+	}
+
+	host->mmc_host_ops.select_drive_strength = sdhci_bm_select_drive_strength;
+
+	ret = sdhci_add_host(host);
+	if (ret)
+		goto err_add_host;
+
+	return 0;
+
+err_add_host:
+pltfm_free:
+	sdhci_pltfm_free(pdev);
+	return ret;
+}
+
+static int sdhci_bm_remove(struct platform_device *pdev)
+{
+	struct sdhci_host *host = platform_get_drvdata(pdev);
+	int dead = (readl_relaxed(host->ioaddr + SDHCI_INT_STATUS) == 0xffffffff);
+
+	sdhci_remove_host(host, dead);
+	sdhci_pltfm_free(pdev);
+	return 0;
+}
+
+static struct platform_driver sdhci_bm_driver = {
+	.probe = sdhci_bm_probe,
+	.remove = sdhci_bm_remove,
+	.driver = {
+		.name = DRIVER_NAME,
+		.of_match_table = sdhci_bm_dt_match,
+	},
+};
+
+module_platform_driver(sdhci_bm_driver);
+MODULE_DESCRIPTION("BitMain Secure Digital Host Controller Interface driver");
+MODULE_LICENSE("GPL");
diff --git a/drivers/mmc/host/sdhci-sophgo.h b/drivers/mmc/host/sdhci-sophgo.h
new file mode 100644
index 000000000000..508d0a16d71e
--- /dev/null
+++ b/drivers/mmc/host/sdhci-sophgo.h
@@ -0,0 +1,121 @@
+/*
+ * drivers/mmc/host/sdhci-bm.c - BitMain SDHCI Platform driver
+ *
+ * Copyright (c) 2013-2014, The Linux Foundation. All rights reserved.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 and
+ * only version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ */
+
+#ifndef __SDHCI_BM_H
+#define __SDHCI_BM_H
+
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/delay.h>
+#include <linux/mmc/mmc.h>
+#include <linux/slab.h>
+
+/*register macro */
+#define P_VENDOR_SPECIFIC_AREA		0xE8
+#define P_VENDOR2_SPECIFIC_AREA		0xEA
+#define VENDOR_EMMC_CTRL		0x2C
+#define SW_RST_R			0x2F
+#define SDHCI_NORMAL_INT_STATUS		0x30
+#define SDHCI_ERR_INT_STATUS		0x32
+#define SDHCI_ERR_INT_STATUS_EN		0x36
+#define SDHCI_HOST_CTRL2_R		0x3E
+#define SDHCI_MSHC_CTRL			0x508
+#define SDHCI_AT_CTRL			0x540
+#define SDHCI_AT_STAT			0x544
+
+/* PHY register */
+#define SDHCI_PHY_R_OFFSET			0x300
+
+#define SDHCI_P_PHY_CNFG           (SDHCI_PHY_R_OFFSET + 0x00)
+#define SDHCI_P_CMDPAD_CNFG        (SDHCI_PHY_R_OFFSET + 0x04)
+#define SDHCI_P_DATPAD_CNFG        (SDHCI_PHY_R_OFFSET + 0x06)
+#define SDHCI_P_CLKPAD_CNFG        (SDHCI_PHY_R_OFFSET + 0x08)
+#define SDHCI_P_STBPAD_CNFG        (SDHCI_PHY_R_OFFSET + 0x0A)
+#define SDHCI_P_RSTNPAD_CNFG       (SDHCI_PHY_R_OFFSET + 0x0C)
+#define SDHCI_P_PADTEST_CNFG       (SDHCI_PHY_R_OFFSET + 0x0E)
+#define SDHCI_P_PADTEST_OUT        (SDHCI_PHY_R_OFFSET + 0x10)
+#define SDHCI_P_PADTEST_IN         (SDHCI_PHY_R_OFFSET + 0x12)
+#define SDHCI_P_COMMDL_CNFG        (SDHCI_PHY_R_OFFSET + 0x1C)
+#define SDHCI_P_SDCLKDL_CNFG       (SDHCI_PHY_R_OFFSET + 0x1D)
+#define SDHCI_P_SDCLKDL_DC         (SDHCI_PHY_R_OFFSET + 0x1E)
+#define SDHCI_P_SMPLDL_CNFG        (SDHCI_PHY_R_OFFSET + 0x20)
+#define SDHCI_P_ATDL_CNFG          (SDHCI_PHY_R_OFFSET + 0x21)
+#define SDHCI_P_DLL_CTRL           (SDHCI_PHY_R_OFFSET + 0x24)
+#define SDHCI_P_DLL_CNFG1          (SDHCI_PHY_R_OFFSET + 0x25)
+#define SDHCI_P_DLL_CNFG2          (SDHCI_PHY_R_OFFSET + 0x26)
+#define SDHCI_P_DLLDL_CNFG         (SDHCI_PHY_R_OFFSET + 0x28)
+#define SDHCI_P_DLL_OFFST          (SDHCI_PHY_R_OFFSET + 0x29)
+#define SDHCI_P_DLLMST_TSTDC       (SDHCI_PHY_R_OFFSET + 0x2A)
+#define SDHCI_P_DLLLBT_CNFG        (SDHCI_PHY_R_OFFSET + 0x2C)
+#define SDHCI_P_DLL_STATUS         (SDHCI_PHY_R_OFFSET + 0x2E)
+#define SDHCI_P_DLLDBG_MLKDC       (SDHCI_PHY_R_OFFSET + 0x30)
+#define SDHCI_P_DLLDBG_SLKDC       (SDHCI_PHY_R_OFFSET + 0x32)
+
+#define PHY_CNFG_PHY_RSTN               0
+#define PHY_CNFG_PHY_PWRGOOD            1
+#define PHY_CNFG_PAD_SP                 16
+#define PHY_CNFG_PAD_SP_MSK             0xf
+#define PHY_CNFG_PAD_SN                 20
+#define PHY_CNFG_PAD_SN_MSK             0xf
+
+#define PAD_CNFG_RXSEL                  0
+#define PAD_CNFG_RXSEL_MSK              0x7
+#define PAD_CNFG_WEAKPULL_EN            3
+#define PAD_CNFG_WEAKPULL_EN_MSK        0x3
+#define PAD_CNFG_TXSLEW_CTRL_P          5
+#define PAD_CNFG_TXSLEW_CTRL_P_MSK      0xf
+#define PAD_CNFG_TXSLEW_CTRL_N          9
+#define PAD_CNFG_TXSLEW_CTRL_N_MSK      0xf
+
+#define COMMDL_CNFG_DLSTEP_SEL          0
+#define COMMDL_CNFG_DLOUT_EN            1
+
+#define SDCLKDL_CNFG_EXTDLY_EN          0
+#define SDCLKDL_CNFG_BYPASS_EN          1
+#define SDCLKDL_CNFG_INPSEL_CNFG        2
+#define SDCLKDL_CNFG_INPSEL_CNFG_MSK    0x3
+#define SDCLKDL_CNFG_UPDATE_DC          4
+
+#define SMPLDL_CNFG_EXTDLY_EN           0
+#define SMPLDL_CNFG_BYPASS_EN           1
+#define SMPLDL_CNFG_INPSEL_CNFG         2
+#define SMPLDL_CNFG_INPSEL_CNFG_MSK     0x3
+#define SMPLDL_CNFG_INPSEL_OVERRIDE     4
+
+#define ATDL_CNFG_EXTDLY_EN             0
+#define ATDL_CNFG_BYPASS_EN             1
+#define ATDL_CNFG_INPSEL_CNFG           2
+#define ATDL_CNFG_INPSEL_CNFG_MSK       0x3
+
+#define MAX_TUNING_STEP                           128
+
+struct sdhci_bm_host {
+	struct platform_device *pdev;
+	void __iomem *core_mem; /* bm SDCC mapped address */
+	struct clk *clk;    /* main SD/MMC bus clock */
+	struct clk *clk100k;
+	struct clk *clkaxi;
+	struct mmc_host *mmc;
+	struct reset_control *reset;
+
+	struct reset_control *clk_rst_axi_emmc_ctrl;
+	struct reset_control *clk_rst_emmc_ctrl;
+	struct reset_control *clk_rst_100k_emmc_ctrl;
+};
+
+int bm_sdhci_phy_init(struct sdhci_host *host);
+bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd);
+#endif
diff --git a/drivers/mmc/host/sdhci.c b/drivers/mmc/host/sdhci.c
index ff41aa56564e..526df8063579 100644
--- a/drivers/mmc/host/sdhci.c
+++ b/drivers/mmc/host/sdhci.c
@@ -49,7 +49,9 @@ static unsigned int debug_quirks2;
 
 static void sdhci_enable_preset_value(struct sdhci_host *host, bool enable);
 
+#ifndef CONFIG_ARCH_SOPHGO
 static bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd);
+#endif
 
 void sdhci_dumpregs(struct sdhci_host *host)
 {
@@ -1627,7 +1629,11 @@ static void sdhci_finish_data(struct sdhci_host *host)
 	__sdhci_finish_data(host, false);
 }
 
+#ifndef CONFIG_ARCH_SOPHGO
 static bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd)
+#else
+bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd)
+#endif
 {
 	int flags;
 	u32 mask;
@@ -1717,6 +1723,9 @@ static bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd)
 
 	return true;
 }
+#ifdef CONFIG_ARCH_SOPHGO
+EXPORT_SYMBOL_GPL(sdhci_send_command);
+#endif
 
 static bool sdhci_present_error(struct sdhci_host *host,
 				struct mmc_command *cmd, bool present)
@@ -2841,7 +2850,7 @@ void sdhci_send_tuning(struct sdhci_host *host, u32 opcode)
 }
 EXPORT_SYMBOL_GPL(sdhci_send_tuning);
 
-static int __sdhci_execute_tuning(struct sdhci_host *host, u32 opcode)
+int __sdhci_execute_tuning(struct sdhci_host *host, u32 opcode)
 {
 	int i;
 
@@ -2879,6 +2888,7 @@ static int __sdhci_execute_tuning(struct sdhci_host *host, u32 opcode)
 	sdhci_reset_tuning(host);
 	return -EAGAIN;
 }
+EXPORT_SYMBOL_GPL(__sdhci_execute_tuning);
 
 int sdhci_execute_tuning(struct mmc_host *mmc, u32 opcode)
 {
diff --git a/drivers/mmc/host/sdhci.h b/drivers/mmc/host/sdhci.h
index f219bdea8f28..149e699aac92 100644
--- a/drivers/mmc/host/sdhci.h
+++ b/drivers/mmc/host/sdhci.h
@@ -793,6 +793,7 @@ void sdhci_set_bus_width(struct sdhci_host *host, int width);
 void sdhci_reset(struct sdhci_host *host, u8 mask);
 void sdhci_set_uhs_signaling(struct sdhci_host *host, unsigned timing);
 int sdhci_execute_tuning(struct mmc_host *mmc, u32 opcode);
+int __sdhci_execute_tuning(struct sdhci_host *host, u32 opcode);
 void sdhci_set_ios(struct mmc_host *mmc, struct mmc_ios *ios);
 int sdhci_start_signal_voltage_switch(struct mmc_host *mmc,
 				      struct mmc_ios *ios);
@@ -823,5 +824,8 @@ void sdhci_abort_tuning(struct sdhci_host *host, u32 opcode);
 void sdhci_switch_external_dma(struct sdhci_host *host, bool en);
 void sdhci_set_data_timeout_irq(struct sdhci_host *host, bool enable);
 void __sdhci_set_timeout(struct sdhci_host *host, struct mmc_command *cmd);
+#ifdef CONFIG_ARCH_SOPHGO
+bool sdhci_send_command(struct sdhci_host *host, struct mmc_command *cmd);
+#endif
 
 #endif /* __SDHCI_HW_H */
diff --git a/drivers/mtd/spi-nor/controllers/Kconfig b/drivers/mtd/spi-nor/controllers/Kconfig
index ca45dcd3ffe8..d2138370f1fc 100644
--- a/drivers/mtd/spi-nor/controllers/Kconfig
+++ b/drivers/mtd/spi-nor/controllers/Kconfig
@@ -16,3 +16,14 @@ config SPI_NXP_SPIFI
 	  SPIFI is a specialized controller for connecting serial SPI
 	  Flash. Enable this option if you have a device with a SPIFI
 	  controller and want to access the Flash as a mtd device.
+
+config SPI_SOPHGO_SPIFMC
+	tristate "Sophgo SPI Flash Master Controller (SPIFMC)"
+	depends on ARCH_SOPHGO || COMPILE_TEST
+	depends on HAS_IOMEM
+	help
+	  Enable support for the Sophgo SPI Flash Master controller.
+
+	  SPIFMC is a master controller to control serial SPI Flash.
+	  Enable this option if you have a device with a SPIFMC controller
+	  and want to access the Flash as a mtd device.
diff --git a/drivers/mtd/spi-nor/controllers/Makefile b/drivers/mtd/spi-nor/controllers/Makefile
index 0b8e1d530913..627ac8850ab1 100644
--- a/drivers/mtd/spi-nor/controllers/Makefile
+++ b/drivers/mtd/spi-nor/controllers/Makefile
@@ -1,3 +1,4 @@
 # SPDX-License-Identifier: GPL-2.0
 obj-$(CONFIG_SPI_HISI_SFC)	+= hisi-sfc.o
 obj-$(CONFIG_SPI_NXP_SPIFI)	+= nxp-spifi.o
+obj-$(CONFIG_SPI_SOPHGO_SPIFMC) += sophgo-spifmc.o
diff --git a/drivers/mtd/spi-nor/controllers/sophgo-spifmc.c b/drivers/mtd/spi-nor/controllers/sophgo-spifmc.c
new file mode 100644
index 000000000000..f7d85cc03137
--- /dev/null
+++ b/drivers/mtd/spi-nor/controllers/sophgo-spifmc.c
@@ -0,0 +1,445 @@
+// SPDX-License-Identifier: GPL-2.0-or-later
+/*
+ * SPI Flash Master Controller (SPIFMC)
+ *
+ * Copyright (c) 2023 Sophgo.
+ */
+#include <linux/iopoll.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/clk.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/spi-nor.h>
+
+/* Hardware register definitions */
+#define SPIFMC_CTRL	0x00
+#define SPIFMC_CTRL_CPHA	BIT(12)
+#define SPIFMC_CTRL_CPOL	BIT(13)
+#define SPIFMC_CTRL_HOLD_OL	BIT(14)
+#define SPIFMC_CTRL_WP_OL	BIT(15)
+#define SPIFMC_CTRL_LSBF	BIT(20)
+#define SPIFMC_CTRL_SRST	BIT(21)
+#define SPIFMC_CTRL_SCK_DIV_SHIFT	0
+#define SPIFMC_CTRL_FRAME_LEN_SHIFT	16
+
+#define SPIFMC_CE_CTRL	0x04
+#define SPIFMC_CE_CTRL_CEMANUAL	BIT(0)
+#define SPIFMC_CE_CTRL_CEMANUAL_EN	BIT(1)
+
+#define SPIFMC_DLY_CTRL	0x08
+#define SPIFMC_CTRL_FM_INTVL_MASK	0x000f
+#define SPIFMC_CTRL_FM_INTVL	BIT(0)
+#define SPIFMC_CTRL_CET_MASK	0x0f00
+#define SPIFMC_CTRL_CET	BIT(8)
+
+#define SPIFMC_DMMR	0x0c
+
+#define SPIFMC_TRAN_CSR	0x10
+#define SPIFMC_TRAN_CSR_TRAN_MODE_MASK	0x0003
+#define SPIFMC_TRAN_CSR_TRAN_MODE_RX	BIT(0)
+#define SPIFMC_TRAN_CSR_TRAN_MODE_TX	BIT(1)
+#define SPIFMC_TRAN_CSR_CNTNS_READ	BIT(2)
+#define SPIFMC_TRAN_CSR_FAST_MODE	BIT(3)
+#define SPIFMC_TRAN_CSR_BUS_WIDTH_1_BIT	(0x00 << 4)
+#define SPIFMC_TRAN_CSR_BUS_WIDTH_2_BIT	(0x01 << 4)
+#define SPIFMC_TRAN_CSR_BUS_WIDTH_4_BIT	(0x02 << 4)
+#define SPIFMC_TRAN_CSR_DMA_EN	BIT(6)
+#define SPIFMC_TRAN_CSR_MISO_LEVEL	BIT(7)
+#define SPIFMC_TRAN_CSR_ADDR_BYTES_MASK	0x0700
+#define SPIFMC_TRAN_CSR_ADDR_BYTES_SHIFT	8
+#define SPIFMC_TRAN_CSR_WITH_CMD	BIT(11)
+#define SPIFMC_TRAN_CSR_FIFO_TRG_LVL_MASK	0x3000
+#define SPIFMC_TRAN_CSR_FIFO_TRG_LVL_1_BYTE	(0x00 << 12)
+#define SPIFMC_TRAN_CSR_FIFO_TRG_LVL_2_BYTE	(0x01 << 12)
+#define SPIFMC_TRAN_CSR_FIFO_TRG_LVL_4_BYTE	(0x02 << 12)
+#define SPIFMC_TRAN_CSR_FIFO_TRG_LVL_8_BYTE	(0x03 << 12)
+#define SPIFMC_TRAN_CSR_GO_BUSY	BIT(15)
+
+#define SPIFMC_TRAN_NUM	0x14
+#define SPIFMC_FIFO_PORT	0x18
+#define SPIFMC_FIFO_PT	0x20
+
+#define SPIFMC_INT_STS	0x28
+#define SPIFMC_INT_TRAN_DONE	BIT(0)
+#define SPIFMC_INT_RD_FIFO	BIT(2)
+#define SPIFMC_INT_WR_FIFO	BIT(3)
+#define SPIFMC_INT_RX_FRAME	BIT(4)
+#define SPIFMC_INT_TX_FRAME	BIT(5)
+
+#define SPIFMC_INT_EN	0x2c
+#define SPIFMC_INT_TRAN_DONE_EN	BIT(0)
+#define SPIFMC_INT_RD_FIFO_EN	BIT(2)
+#define SPIFMC_INT_WR_FIFO_EN	BIT(3)
+#define SPIFMC_INT_RX_FRAME_EN	BIT(4)
+#define SPIFMC_INT_TX_FRAME_EN	BIT(5)
+
+#define SPIFMC_MAX_FIFO_DEPTH	8
+
+struct sophgo_spifmc {
+	struct device *dev;
+	struct clk *clk;
+	void __iomem *io_base;
+	struct spi_nor nor;
+};
+
+static inline int sophgo_spifmc_wait_int(struct sophgo_spifmc *spifmc,
+		u8 int_type)
+{
+	u32 stat;
+
+	return readl_poll_timeout(spifmc->io_base + SPIFMC_INT_STS, stat,
+			(stat & int_type), 0, 0);
+}
+
+static inline u32 sophgo_spifmc_init_reg(struct sophgo_spifmc *spifmc)
+{
+	u32 reg;
+
+	reg = readl(spifmc->io_base + SPIFMC_TRAN_CSR);
+	reg &= ~(SPIFMC_TRAN_CSR_TRAN_MODE_MASK
+			| SPIFMC_TRAN_CSR_CNTNS_READ
+			| SPIFMC_TRAN_CSR_FAST_MODE
+			| SPIFMC_TRAN_CSR_BUS_WIDTH_2_BIT
+			| SPIFMC_TRAN_CSR_BUS_WIDTH_4_BIT
+			| SPIFMC_TRAN_CSR_DMA_EN
+			| SPIFMC_TRAN_CSR_ADDR_BYTES_MASK
+			| SPIFMC_TRAN_CSR_WITH_CMD
+			| SPIFMC_TRAN_CSR_FIFO_TRG_LVL_MASK);
+
+	return reg;
+}
+
+/*
+ * sophgo_spifmc_read_reg is a workaround function:
+ * AHB bus could only do 32-bit access to SPIFMC fifo,
+ * so cmd without 3-byte addr will leave 3-byte data in fifo.
+ * Set TX to mark that these 3-byte data would be sent out.
+ */
+static int sophgo_spifmc_read_reg(struct spi_nor *nor, u8 opcode, u8 *buf,
+				 size_t len)
+{
+	struct sophgo_spifmc *spifmc = nor->priv;
+	u32 reg;
+	int ret, i;
+
+	reg = sophgo_spifmc_init_reg(spifmc);
+	reg |= SPIFMC_TRAN_CSR_BUS_WIDTH_1_BIT;
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_1_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+	reg |= SPIFMC_TRAN_CSR_TRAN_MODE_RX | SPIFMC_TRAN_CSR_TRAN_MODE_TX;
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+	writeb(opcode, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	for (i = 0; i < len; i++)
+		writeb(0, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_INT_STS);
+	writel(len, spifmc->io_base + SPIFMC_TRAN_NUM);
+	reg |= SPIFMC_TRAN_CSR_GO_BUSY;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+
+	ret = sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_TRAN_DONE);
+	if (ret)
+		return ret;
+
+	while (len--)
+		*buf++ = readb(spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	return 0;
+}
+
+static int sophgo_spifmc_write_reg(struct spi_nor *nor, u8 opcode,
+				  const u8 *buf, size_t len)
+{
+	struct sophgo_spifmc *spifmc = nor->priv;
+	u32 reg;
+	int i;
+
+	reg = sophgo_spifmc_init_reg(spifmc);
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_1_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+
+	/*
+	 * If write values to the Status Register,
+	 * configure TRAN_CSR register as the same as sophgo_spifmc_read_reg.
+	 */
+	if (opcode == SPINOR_OP_WRSR) {
+		reg |= SPIFMC_TRAN_CSR_TRAN_MODE_RX | SPIFMC_TRAN_CSR_TRAN_MODE_TX;
+		writel(len, spifmc->io_base + SPIFMC_TRAN_NUM);
+	}
+
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+	writeb(opcode, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	for (i = 0; i < len; i++)
+		writeb(buf[i], spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_INT_STS);
+	reg |= SPIFMC_TRAN_CSR_GO_BUSY;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+	sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_TRAN_DONE);
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	return 0;
+}
+
+static ssize_t sophgo_spifmc_read(struct spi_nor *nor, loff_t from,
+		size_t len, u_char *buf)
+{
+	struct sophgo_spifmc *spifmc = nor->priv;
+	u32 reg;
+	int xfer_size, offset;
+	int i;
+
+	reg = sophgo_spifmc_init_reg(spifmc);
+	reg |= (nor->addr_nbytes) << SPIFMC_TRAN_CSR_ADDR_BYTES_SHIFT;
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_8_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+	reg |= SPIFMC_TRAN_CSR_TRAN_MODE_RX;
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+	writeb(nor->read_opcode, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	for (i = nor->addr_nbytes - 1; i >= 0; i--)
+		writeb((from >> i * 8) & 0xff, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_INT_STS);
+	writel(len, spifmc->io_base + SPIFMC_TRAN_NUM);
+	reg |= SPIFMC_TRAN_CSR_GO_BUSY;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+	sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_RD_FIFO);
+
+	offset = 0;
+	while (offset < len) {
+		xfer_size = min_t(size_t, SPIFMC_MAX_FIFO_DEPTH, len - offset);
+
+		while ((readl(spifmc->io_base + SPIFMC_FIFO_PT) & 0xf) != xfer_size)
+			;
+
+		for (i = 0; i < xfer_size; i++)
+			buf[i + offset] = readb(spifmc->io_base + SPIFMC_FIFO_PORT);
+
+		offset += xfer_size;
+	}
+
+	sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_TRAN_DONE);
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	return len;
+}
+
+static ssize_t sophgo_spifmc_write(struct spi_nor *nor, loff_t to,
+		size_t len, const u_char *buf)
+{
+	struct sophgo_spifmc *spifmc = nor->priv;
+	u32 reg;
+	int i, offset;
+	int xfer_size, wait;
+
+	reg = sophgo_spifmc_init_reg(spifmc);
+	reg |= nor->addr_nbytes << SPIFMC_TRAN_CSR_ADDR_BYTES_SHIFT;
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_8_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+	reg |= SPIFMC_TRAN_CSR_TRAN_MODE_TX;
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+	writeb(nor->program_opcode, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	for (i = nor->addr_nbytes - 1; i >= 0; i--)
+		writeb((to >> i * 8) & 0xff, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_INT_STS);
+	writel(len, spifmc->io_base + SPIFMC_TRAN_NUM);
+	reg |= SPIFMC_TRAN_CSR_GO_BUSY;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+
+	while ((readl(spifmc->io_base + SPIFMC_FIFO_PT) & 0xf) != 0)
+		;
+
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	offset = 0;
+	while (offset < len) {
+		xfer_size = min_t(size_t, SPIFMC_MAX_FIFO_DEPTH, len - offset);
+
+		wait = 0;
+		while ((readl(spifmc->io_base + SPIFMC_FIFO_PT) & 0xf) != 0) {
+			wait++;
+			udelay(10);
+			if (wait > 30000) {
+				dev_warn(spifmc->dev, "Wait to write FIFO timeout.\n");
+				return -1;
+			}
+		}
+
+		for (i = 0; i < xfer_size; i++)
+			writeb(buf[i + offset], spifmc->io_base + SPIFMC_FIFO_PORT);
+
+		offset += xfer_size;
+	}
+
+	sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_TRAN_DONE);
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	return len;
+}
+
+static int sophgo_spifmc_erase(struct spi_nor *nor, loff_t offs)
+{
+	struct sophgo_spifmc *spifmc = nor->priv;
+	u32 reg;
+	int i;
+
+	reg = sophgo_spifmc_init_reg(spifmc);
+	reg |= nor->addr_nbytes << SPIFMC_TRAN_CSR_ADDR_BYTES_SHIFT;
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_1_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+	writeb(nor->erase_opcode, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	for (i = nor->addr_nbytes - 1; i >= 0; i--)
+		writeb((offs >> i * 8) & 0xff, spifmc->io_base + SPIFMC_FIFO_PORT);
+
+	writel(0, spifmc->io_base + SPIFMC_INT_STS);
+	reg |= SPIFMC_TRAN_CSR_GO_BUSY;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+	sophgo_spifmc_wait_int(spifmc, SPIFMC_INT_TRAN_DONE);
+	writel(0, spifmc->io_base + SPIFMC_FIFO_PT);
+
+	return 0;
+}
+
+static const struct spi_nor_controller_ops sophgo_spifmc_controller_ops = {
+	.read_reg  = sophgo_spifmc_read_reg,
+	.write_reg = sophgo_spifmc_write_reg,
+	.read  = sophgo_spifmc_read,
+	.write = sophgo_spifmc_write,
+	.erase = sophgo_spifmc_erase,
+};
+
+static void sophgo_spifmc_init(struct sophgo_spifmc *spifmc)
+{
+	u32 reg;
+
+	/* disable DMMR (Direct Memory Mapping Read) */
+	writel(0, spifmc->io_base + SPIFMC_DMMR);
+	/* soft reset */
+	writel(readl(spifmc->io_base + SPIFMC_CTRL) | SPIFMC_CTRL_SRST | 0x3,
+			spifmc->io_base + SPIFMC_CTRL);
+	/* hardware CE contrl, soft reset cannot change the register */
+	writel(0, spifmc->io_base + SPIFMC_CE_CTRL);
+	reg = spifmc->nor.addr_nbytes << SPIFMC_TRAN_CSR_ADDR_BYTES_SHIFT;
+	reg |= SPIFMC_TRAN_CSR_FIFO_TRG_LVL_4_BYTE;
+	reg |= SPIFMC_TRAN_CSR_WITH_CMD;
+	writel(reg, spifmc->io_base + SPIFMC_TRAN_CSR);
+}
+
+static int sophgo_spifmc_register(struct device_node *np,
+				struct sophgo_spifmc *spifmc)
+{
+	/* TODO: support DUAL and QUAD operations */
+	const struct spi_nor_hwcaps hwcaps = {
+		.mask = SNOR_HWCAPS_READ |
+			SNOR_HWCAPS_PP,
+	};
+	int ret;
+
+	spifmc->nor.dev = spifmc->dev;
+	spi_nor_set_flash_node(&spifmc->nor, np);
+	spifmc->nor.priv = spifmc;
+	spifmc->nor.controller_ops = &sophgo_spifmc_controller_ops;
+
+	ret = spi_nor_scan(&spifmc->nor, NULL, &hwcaps);
+	if (ret) {
+		dev_err(spifmc->dev, "Device scan failed.\n");
+		return ret;
+	}
+
+	ret = mtd_device_register(&spifmc->nor.mtd, NULL, 0);
+	if (ret) {
+		dev_err(spifmc->dev, "mtd device parse failed.\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static int sophgo_spifmc_probe(struct platform_device *pdev)
+{
+	struct device_node *np;
+	struct sophgo_spifmc *spifmc;
+	int ret;
+
+	spifmc = devm_kzalloc(&pdev->dev, sizeof(*spifmc), GFP_KERNEL);
+	if (!spifmc)
+		return -ENOMEM;
+
+	spifmc->io_base = devm_platform_ioremap_resource_byname(pdev, "memory");
+	if (IS_ERR(spifmc->io_base))
+		return PTR_ERR(spifmc->io_base);
+
+	spifmc->clk = devm_clk_get(&pdev->dev, NULL);
+	if (IS_ERR(spifmc->clk)) {
+		dev_err(&pdev->dev, "AHB clock not found.\n");
+		return PTR_ERR(spifmc->clk);
+	}
+
+	ret = clk_prepare_enable(spifmc->clk);
+	if (ret) {
+		dev_err(&pdev->dev, "Unable to enable AHB clock.\n");
+		return ret;
+	}
+
+	spifmc->dev = &pdev->dev;
+	platform_set_drvdata(pdev, spifmc);
+	sophgo_spifmc_init(spifmc);
+
+	np = of_get_next_available_child(pdev->dev.of_node, NULL);
+	if (!np) {
+		dev_err(&pdev->dev, "No SPI flash device to configure.\n");
+		ret = -ENODEV;
+		goto fail;
+	}
+
+	ret = sophgo_spifmc_register(np, spifmc);
+	of_node_put(np);
+	if (ret) {
+		dev_err(&pdev->dev, "Unable to register spifmc.\n");
+		goto fail;
+	}
+
+	return ret;
+fail:
+	clk_disable_unprepare(spifmc->clk);
+	return ret;
+}
+
+static int sophgo_spifmc_remove(struct platform_device *pdev)
+{
+	struct sophgo_spifmc *spifmc = platform_get_drvdata(pdev);
+
+	mtd_device_unregister(&spifmc->nor.mtd);
+	clk_disable_unprepare(spifmc->clk);
+
+	return 0;
+}
+
+static const struct of_device_id sophgo_spifmc_match[] = {
+	{.compatible = "sophgo,spifmc"},
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, sophgo_spifmc_match);
+
+static struct platform_driver sophgo_spifmc_driver = {
+	.probe	= sophgo_spifmc_probe,
+	.remove	= sophgo_spifmc_remove,
+	.driver	= {
+		.name = "sophgo-spifmc",
+		.of_match_table = sophgo_spifmc_match,
+	},
+};
+module_platform_driver(sophgo_spifmc_driver);
+
+MODULE_DESCRIPTION("Sophgo SPI Flash Master Controller Driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/mtd/spi-nor/gigadevice.c b/drivers/mtd/spi-nor/gigadevice.c
index d57ddaf1525b..c60656702063 100644
--- a/drivers/mtd/spi-nor/gigadevice.c
+++ b/drivers/mtd/spi-nor/gigadevice.c
@@ -33,6 +33,15 @@ static const struct spi_nor_fixups gd25q256_fixups = {
 	.post_bfpt = gd25q256_post_bfpt,
 };
 
+static void gd25lb512me_default_init(struct spi_nor *nor)
+{
+	nor->params->quad_enable = spi_nor_sr1_bit6_quad_enable;
+}
+
+static const struct spi_nor_fixups gd25lb512me_fixups = {
+	.default_init = gd25lb512me_default_init,
+};
+
 static const struct flash_info gigadevice_nor_parts[] = {
 	{ "gd25q16", INFO(0xc84015, 0, 64 * 1024,  32)
 		FLAGS(SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
@@ -67,6 +76,11 @@ static const struct flash_info gigadevice_nor_parts[] = {
 		FLAGS(SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB | SPI_NOR_TB_SR_BIT6)
 		FIXUP_FLAGS(SPI_NOR_4B_OPCODES)
 		.fixups = &gd25q256_fixups },
+	{ "gd25lb512me", INFO(0xc8671a, 0, 64 * 1024, 1024)
+		FLAGS(SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+		NO_SFDP_FLAGS(SECT_4K | SPI_NOR_QUAD_READ)
+		FIXUP_FLAGS(SPI_NOR_4B_OPCODES)
+		.fixups = &gd25lb512me_fixups },
 };
 
 const struct spi_nor_manufacturer spi_nor_gigadevice = {
diff --git a/drivers/net/ethernet/intel/i40e/i40e_common.c b/drivers/net/ethernet/intel/i40e/i40e_common.c
index 4d7caa119971..0a9efd8c6471 100644
--- a/drivers/net/ethernet/intel/i40e/i40e_common.c
+++ b/drivers/net/ethernet/intel/i40e/i40e_common.c
@@ -3213,7 +3213,8 @@ static void i40e_parse_discover_capabilities(struct i40e_hw *hw, void *buff,
 			p->base_queue = phys_id;
 			break;
 		case I40E_AQ_CAP_ID_MSIX:
-			p->num_msix_vectors = number;
+			//p->num_msix_vectors = number;
+			p->num_msix_vectors = 8;
 			i40e_debug(hw, I40E_DEBUG_INIT,
 				   "HW Capability: MSIX vector count = %d\n",
 				   p->num_msix_vectors);
diff --git a/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h b/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
index 61b9774b3d31..1b18fa4eb082 100644
--- a/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
+++ b/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
@@ -2069,7 +2069,7 @@ enum {
 #define IXGBE_DEVICE_CAPS       0x2C
 #define IXGBE_SERIAL_NUMBER_MAC_ADDR 0x11
 #define IXGBE_PCIE_MSIX_82599_CAPS  0x72
-#define IXGBE_MAX_MSIX_VECTORS_82599	0x40
+#define IXGBE_MAX_MSIX_VECTORS_82599	0x09
 #define IXGBE_PCIE_MSIX_82598_CAPS  0x62
 #define IXGBE_MAX_MSIX_VECTORS_82598	0x13
 
diff --git a/drivers/net/ethernet/stmicro/stmmac/Kconfig b/drivers/net/ethernet/stmicro/stmmac/Kconfig
index 92d7d5a00b84..d86875c039a2 100644
--- a/drivers/net/ethernet/stmicro/stmmac/Kconfig
+++ b/drivers/net/ethernet/stmicro/stmmac/Kconfig
@@ -216,6 +216,17 @@ config DWMAC_SUN8I
 	  stmmac device driver. This driver is used for H3/A83T/A64
 	  EMAC ethernet controller.
 
+config DWMAC_THEAD
+	tristate "T-HEAD dwmac support"
+	depends on OF && (ARCH_THEAD || COMPILE_TEST)
+	select MFD_SYSCON
+	help
+	  Support for ethernet controllers on T-HEAD RISC-V SoCs
+
+	  This selects the T-HEAD platform specific glue layer support for
+	  the stmmac device driver. This driver is used for T-HEAD TH1520
+	  ethernet controller.
+
 config DWMAC_IMX8
 	tristate "NXP IMX8 DWMAC support"
 	default ARCH_MXC
diff --git a/drivers/net/ethernet/stmicro/stmmac/Makefile b/drivers/net/ethernet/stmicro/stmmac/Makefile
index 5b57aee19267..a071e84272e3 100644
--- a/drivers/net/ethernet/stmicro/stmmac/Makefile
+++ b/drivers/net/ethernet/stmicro/stmmac/Makefile
@@ -22,11 +22,13 @@ obj-$(CONFIG_DWMAC_MESON)	+= dwmac-meson.o dwmac-meson8b.o
 obj-$(CONFIG_DWMAC_QCOM_ETHQOS)	+= dwmac-qcom-ethqos.o
 obj-$(CONFIG_DWMAC_ROCKCHIP)	+= dwmac-rk.o
 obj-$(CONFIG_DWMAC_SOCFPGA)	+= dwmac-altr-socfpga.o
+obj-$(CONFIG_ARCH_SOPHGO)       += dwmac-sophgo.o
 obj-$(CONFIG_DWMAC_STARFIVE)	+= dwmac-starfive.o
 obj-$(CONFIG_DWMAC_STI)		+= dwmac-sti.o
 obj-$(CONFIG_DWMAC_STM32)	+= dwmac-stm32.o
 obj-$(CONFIG_DWMAC_SUNXI)	+= dwmac-sunxi.o
 obj-$(CONFIG_DWMAC_SUN8I)	+= dwmac-sun8i.o
+obj-$(CONFIG_DWMAC_THEAD)	+= dwmac-thead.o
 obj-$(CONFIG_DWMAC_DWC_QOS_ETH)	+= dwmac-dwc-qos-eth.o
 obj-$(CONFIG_DWMAC_INTEL_PLAT)	+= dwmac-intel-plat.o
 obj-$(CONFIG_DWMAC_GENERIC)	+= dwmac-generic.o
diff --git a/drivers/net/ethernet/stmicro/stmmac/dwmac-sophgo.c b/drivers/net/ethernet/stmicro/stmmac/dwmac-sophgo.c
new file mode 100644
index 000000000000..50a76c8f0df6
--- /dev/null
+++ b/drivers/net/ethernet/stmicro/stmmac/dwmac-sophgo.c
@@ -0,0 +1,268 @@
+/*
+ * DWMAC specific glue layer
+ *
+ * Copyright (c) 2018 Bitmain Ltd.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#include <linux/stmmac.h>
+#include <linux/module.h>
+#include <linux/phy.h>
+#include <linux/platform_device.h>
+#include <linux/of_net.h>
+#include <linux/of_gpio.h>
+#include <linux/io.h>
+
+#include "stmmac_platform.h"
+
+struct bm_mac {
+	struct device *dev;
+	struct reset_control *rst;
+	struct clk *clk_tx;
+	struct clk *gate_clk_tx;
+	struct clk *gate_clk_ref;
+	struct gpio_desc *reset;
+};
+
+static u64 bm_dma_mask = DMA_BIT_MASK(40);
+
+static int bm_eth_reset_phy(struct platform_device *pdev)
+{
+	struct device_node *np = pdev->dev.of_node;
+	int phy_reset_gpio;
+
+	if (!np)
+		return 0;
+
+	phy_reset_gpio = of_get_named_gpio(np, "phy-reset-gpios", 0);
+
+	if (phy_reset_gpio < 0)
+		return 0;
+
+	if (gpio_request(phy_reset_gpio, "eth-phy-reset"))
+		return 0;
+
+	/* RESET_PU */
+	gpio_direction_output(phy_reset_gpio, 0);
+	mdelay(100);
+
+	gpio_direction_output(phy_reset_gpio, 1);
+	/* RC charging time */
+	mdelay(100);
+
+	return 0;
+}
+
+static void bm_mac_fix_speed(void *priv, unsigned int speed, unsigned int mode)
+{
+	struct bm_mac *bsp_priv = priv;
+	unsigned long rate = 125000000;
+	bool needs_calibration = false;
+	int err;
+
+	switch (speed) {
+	case SPEED_1000:
+		needs_calibration = true;
+		rate = 125000000;
+		break;
+
+	case SPEED_100:
+		needs_calibration = true;
+		rate = 25000000;
+		break;
+
+	case SPEED_10:
+		needs_calibration = true;
+		rate = 2500000;
+		break;
+
+	default:
+		dev_err(bsp_priv->dev, "invalid speed %u\n", speed);
+		break;
+	}
+
+	if (needs_calibration) {
+		err = clk_set_rate(bsp_priv->clk_tx, rate);
+		if (err < 0)
+			dev_err(bsp_priv->dev, "failed to set TX rate: %d\n"
+					, err);
+	}
+}
+
+void bm_dwmac_exit(struct platform_device *pdev, void *priv)
+{
+	struct bm_mac *bsp_priv = priv;
+
+	clk_disable_unprepare(bsp_priv->gate_clk_tx);
+	clk_disable_unprepare(bsp_priv->gate_clk_ref);
+}
+
+static int bm_validate_ucast_entries(struct device *dev, int ucast_entries)
+{
+	int x = ucast_entries;
+
+	switch (x) {
+	case 1 ... 32:
+	case 64:
+	case 128:
+		break;
+	default:
+		x = 1;
+		dev_info(dev, "Unicast table entries set to unexpected value %d\n",
+			 ucast_entries);
+		break;
+	}
+	return x;
+}
+
+static int bm_validate_mcast_bins(struct device *dev, int mcast_bins)
+{
+	int x = mcast_bins;
+
+	switch (x) {
+	case HASH_TABLE_SIZE:
+	case 128:
+	case 256:
+		break;
+	default:
+		x = 0;
+		dev_info(dev, "Hash table entries set to unexpected value %d\n",
+			 mcast_bins);
+		break;
+	}
+	return x;
+}
+
+static void bm_dwmac_probe_config_dt(struct platform_device *pdev, struct plat_stmmacenet_data *plat)
+{
+	struct device_node *np = pdev->dev.of_node;
+
+	of_property_read_u32(np, "snps,multicast-filter-bins", &plat->multicast_filter_bins);
+	of_property_read_u32(np, "snps,perfect-filter-entries", &plat->unicast_filter_entries);
+	plat->unicast_filter_entries = bm_validate_ucast_entries(&pdev->dev,
+								 plat->unicast_filter_entries);
+	plat->multicast_filter_bins = bm_validate_mcast_bins(&pdev->dev,
+							     plat->multicast_filter_bins);
+	plat->flags |= (STMMAC_FLAG_TSO_EN);
+	plat->has_gmac4 = 1;
+	plat->has_gmac = 0;
+	plat->pmt = 0;
+}
+
+static int bm_dwmac_probe(struct platform_device *pdev)
+{
+	struct plat_stmmacenet_data *plat_dat;
+	struct stmmac_resources stmmac_res;
+	struct bm_mac *bsp_priv = NULL;
+	struct phy_device *phydev = NULL;
+	struct stmmac_priv *priv = NULL;
+	struct net_device *ndev = NULL;
+	int ret;
+
+	pdev->dev.dma_mask = &bm_dma_mask;
+	pdev->dev.coherent_dma_mask = bm_dma_mask;
+
+	bm_eth_reset_phy(pdev);
+
+	ret = stmmac_get_platform_resources(pdev, &stmmac_res);
+	if (ret)
+		return ret;
+
+	plat_dat = stmmac_probe_config_dt(pdev, stmmac_res.mac);
+	if (IS_ERR(plat_dat))
+		return PTR_ERR(plat_dat);
+
+	bm_dwmac_probe_config_dt(pdev, plat_dat);
+	ret = stmmac_dvr_probe(&pdev->dev, plat_dat, &stmmac_res);
+	if (ret)
+		goto err_remove_config_dt;
+
+	bsp_priv = devm_kzalloc(&pdev->dev, sizeof(*bsp_priv), GFP_KERNEL);
+	if (!bsp_priv)
+		return PTR_ERR(bsp_priv);
+
+	bsp_priv->dev = &pdev->dev;
+
+	/* clock setup */
+	bsp_priv->clk_tx = devm_clk_get(&pdev->dev,
+					"clk_tx");
+	if (IS_ERR(bsp_priv->clk_tx))
+		dev_warn(&pdev->dev, "Cannot get mac tx clock!\n");
+	else
+		plat_dat->fix_mac_speed = bm_mac_fix_speed;
+
+	bsp_priv->gate_clk_tx = devm_clk_get(&pdev->dev, "gate_clk_tx");
+	if (IS_ERR(bsp_priv->gate_clk_tx))
+		dev_warn(&pdev->dev, "Cannot get mac tx gating clock!\n");
+	else
+		clk_prepare_enable(bsp_priv->gate_clk_tx);
+
+	bsp_priv->gate_clk_ref = devm_clk_get(&pdev->dev, "gate_clk_ref");
+	if (IS_ERR(bsp_priv->gate_clk_ref))
+		dev_warn(&pdev->dev, "Cannot get mac ref gating clock!\n");
+	else
+		clk_prepare_enable(bsp_priv->gate_clk_ref);
+
+	plat_dat->bsp_priv = bsp_priv;
+	plat_dat->exit = bm_dwmac_exit;
+
+	ndev = dev_get_drvdata(&pdev->dev);
+	priv = netdev_priv(ndev);
+	phydev = mdiobus_get_phy(priv->mii, 0);
+	if (phydev == NULL) {
+		dev_err(&pdev->dev, "Can not get phy in addr 0\n");
+		goto err_remove_config_dt;
+	}
+
+	/* set green LED0 active for transmit, yellow LED1 for link*/
+	ret = phy_write_paged(phydev, 0, 0x1f, 0xd04);
+	if (ret < 0)
+		dev_err(&pdev->dev, "Can not select page 0xd04\n");
+	ret = phy_write_paged(phydev, 0xd04, 0x10, 0x617f);
+	if (ret < 0)
+		dev_err(&pdev->dev, "Can not alter LED Configuration\n");
+	/* disable eee LED function */
+	ret = phy_write_paged(phydev, 0xd04, 0x11, 0x0);
+	if (ret < 0)
+		dev_err(&pdev->dev, "Can not disable EEE Configuration\n");
+	ret = phy_write_paged(phydev, 0, 0x1f, 0);
+	if (ret < 0)
+		dev_err(&pdev->dev, "Can not select page 0\n");
+
+	return 0;
+
+err_remove_config_dt:
+	stmmac_remove_config_dt(pdev, plat_dat);
+
+	return ret;
+}
+
+static const struct of_device_id bm_dwmac_match[] = {
+	{ .compatible = "bitmain,ethernet" },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, bm_dwmac_match);
+
+static struct platform_driver bm_dwmac_driver = {
+	.probe  = bm_dwmac_probe,
+	.remove_new = stmmac_pltfr_remove,
+	.driver = {
+		.name           = "bm-dwmac",
+		.pm		= &stmmac_pltfr_pm_ops,
+		.of_match_table = bm_dwmac_match,
+	},
+};
+module_platform_driver(bm_dwmac_driver);
+
+MODULE_AUTHOR("Wei Huang<wei.huang01@bitmain.com>");
+MODULE_DESCRIPTION("Bitmain DWMAC specific glue layer");
+MODULE_LICENSE("GPL");
diff --git a/drivers/net/ethernet/stmicro/stmmac/dwmac-thead.c b/drivers/net/ethernet/stmicro/stmmac/dwmac-thead.c
new file mode 100644
index 000000000000..fec27f78a417
--- /dev/null
+++ b/drivers/net/ethernet/stmicro/stmmac/dwmac-thead.c
@@ -0,0 +1,289 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * T-HEAD DWMAC platform driver
+ *
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ * Copyright (C) 2023 Jisheng Zhang <jszhang@kernel.org>
+ *
+ */
+
+#include <linux/bitfield.h>
+#include <linux/mfd/syscon.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/of_net.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+
+#include "stmmac_platform.h"
+
+#define GMAC_CLK_EN			0x00
+#define  GMAC_TX_CLK_EN			BIT(1)
+#define  GMAC_TX_CLK_N_EN		BIT(2)
+#define  GMAC_TX_CLK_OUT_EN		BIT(3)
+#define  GMAC_RX_CLK_EN			BIT(4)
+#define  GMAC_RX_CLK_N_EN		BIT(5)
+#define  GMAC_EPHY_REF_CLK_EN		BIT(6)
+#define GMAC_RXCLK_DELAY_CTRL		0x04
+#define  GMAC_RXCLK_BYPASS		BIT(15)
+#define  GMAC_RXCLK_INVERT		BIT(14)
+#define  GMAC_RXCLK_DELAY_MASK		GENMASK(4, 0)
+#define  GMAC_RXCLK_DELAY_VAL(x)	FIELD_PREP(GMAC_RXCLK_DELAY_MASK, (x))
+#define GMAC_TXCLK_DELAY_CTRL		0x08
+#define  GMAC_TXCLK_BYPASS		BIT(15)
+#define  GMAC_TXCLK_INVERT		BIT(14)
+#define  GMAC_TXCLK_DELAY_MASK		GENMASK(4, 0)
+#define  GMAC_TXCLK_DELAY_VAL(x)	FIELD_PREP(GMAC_RXCLK_DELAY_MASK, (x))
+#define GMAC_PLLCLK_DIV			0x0c
+#define  GMAC_PLLCLK_DIV_EN		BIT(31)
+#define  GMAC_PLLCLK_DIV_MASK		GENMASK(7, 0)
+#define  GMAC_PLLCLK_DIV_NUM(x)		FIELD_PREP(GMAC_PLLCLK_DIV_MASK, (x))
+#define GMAC_GTXCLK_SEL			0x18
+#define  GMAC_GTXCLK_SEL_PLL		BIT(0)
+#define GMAC_INTF_CTRL			0x1c
+#define  PHY_INTF_MASK			BIT(0)
+#define  PHY_INTF_RGMII			FIELD_PREP(PHY_INTF_MASK, 1)
+#define  PHY_INTF_MII_GMII		FIELD_PREP(PHY_INTF_MASK, 0)
+#define GMAC_TXCLK_OEN			0x20
+#define  TXCLK_DIR_MASK			BIT(0)
+#define  TXCLK_DIR_OUTPUT		FIELD_PREP(TXCLK_DIR_MASK, 0)
+#define  TXCLK_DIR_INPUT		FIELD_PREP(TXCLK_DIR_MASK, 1)
+
+#define GMAC_GMII_RGMII_RATE	125000000
+#define GMAC_MII_RATE		25000000
+
+struct thead_dwmac {
+	struct plat_stmmacenet_data *plat;
+	struct regmap *apb_regmap;
+	struct device *dev;
+	u32 rx_delay;
+	u32 tx_delay;
+};
+
+static int thead_dwmac_set_phy_if(struct plat_stmmacenet_data *plat)
+{
+	struct thead_dwmac *dwmac = plat->bsp_priv;
+	u32 phyif;
+
+	switch (plat->mac_interface) {
+	case PHY_INTERFACE_MODE_MII:
+		phyif = PHY_INTF_MII_GMII;
+		break;
+	case PHY_INTERFACE_MODE_RGMII:
+	case PHY_INTERFACE_MODE_RGMII_ID:
+	case PHY_INTERFACE_MODE_RGMII_TXID:
+	case PHY_INTERFACE_MODE_RGMII_RXID:
+		phyif = PHY_INTF_RGMII;
+		break;
+	default:
+		dev_err(dwmac->dev, "unsupported phy interface %d\n",
+			plat->mac_interface);
+		return -EINVAL;
+	};
+
+	regmap_write(dwmac->apb_regmap, GMAC_INTF_CTRL, phyif);
+
+	return 0;
+}
+
+static int thead_dwmac_set_txclk_dir(struct plat_stmmacenet_data *plat)
+{
+	struct thead_dwmac *dwmac = plat->bsp_priv;
+	u32 txclk_dir;
+
+	switch (plat->mac_interface) {
+	case PHY_INTERFACE_MODE_MII:
+		txclk_dir = TXCLK_DIR_INPUT;
+		break;
+	case PHY_INTERFACE_MODE_RGMII:
+	case PHY_INTERFACE_MODE_RGMII_ID:
+	case PHY_INTERFACE_MODE_RGMII_TXID:
+	case PHY_INTERFACE_MODE_RGMII_RXID:
+		txclk_dir = TXCLK_DIR_OUTPUT;
+		break;
+	default:
+		dev_err(dwmac->dev, "unsupported phy interface %d\n",
+			plat->mac_interface);
+		return -EINVAL;
+	};
+
+	regmap_write(dwmac->apb_regmap, GMAC_TXCLK_OEN, txclk_dir);
+
+	return 0;
+}
+
+static void thead_dwmac_fix_speed(void *priv, unsigned int speed, unsigned int mode)
+{
+	struct thead_dwmac *dwmac = priv;
+	struct plat_stmmacenet_data *plat = dwmac->plat;
+	unsigned long rate;
+	u32 div;
+
+	switch (plat->mac_interface) {
+	/* For MII, rxc/txc is provided by phy */
+	case PHY_INTERFACE_MODE_MII:
+		return;
+
+	case PHY_INTERFACE_MODE_RGMII:
+	case PHY_INTERFACE_MODE_RGMII_ID:
+	case PHY_INTERFACE_MODE_RGMII_RXID:
+	case PHY_INTERFACE_MODE_RGMII_TXID:
+		rate = clk_get_rate(plat->stmmac_clk);
+		if (!rate || rate % GMAC_GMII_RGMII_RATE != 0 ||
+		    rate % GMAC_MII_RATE != 0) {
+			dev_err(dwmac->dev, "invalid gmac rate %ld\n", rate);
+			return;
+		}
+
+		regmap_update_bits(dwmac->apb_regmap, GMAC_PLLCLK_DIV, GMAC_PLLCLK_DIV_EN, 0);
+
+		switch (speed) {
+		case SPEED_1000:
+			div = rate / GMAC_GMII_RGMII_RATE;
+			break;
+		case SPEED_100:
+			div = rate / GMAC_MII_RATE;
+			break;
+		case SPEED_10:
+			div = rate * 10 / GMAC_MII_RATE;
+			break;
+		default:
+			dev_err(dwmac->dev, "invalid speed %u\n", speed);
+			return;
+		}
+		regmap_update_bits(dwmac->apb_regmap, GMAC_PLLCLK_DIV,
+				   GMAC_PLLCLK_DIV_MASK, GMAC_PLLCLK_DIV_NUM(div));
+
+		regmap_update_bits(dwmac->apb_regmap, GMAC_PLLCLK_DIV,
+				   GMAC_PLLCLK_DIV_EN, GMAC_PLLCLK_DIV_EN);
+		break;
+	default:
+		dev_err(dwmac->dev, "unsupported phy interface %d\n",
+			plat->mac_interface);
+		return;
+	}
+}
+
+static int thead_dwmac_enable_clk(struct plat_stmmacenet_data *plat)
+{
+	struct thead_dwmac *dwmac = plat->bsp_priv;
+	u32 reg;
+
+	switch (plat->mac_interface) {
+	case PHY_INTERFACE_MODE_MII:
+		reg = GMAC_RX_CLK_EN | GMAC_TX_CLK_EN;
+		break;
+
+	case PHY_INTERFACE_MODE_RGMII:
+	case PHY_INTERFACE_MODE_RGMII_ID:
+	case PHY_INTERFACE_MODE_RGMII_RXID:
+	case PHY_INTERFACE_MODE_RGMII_TXID:
+		/* use pll */
+		regmap_write(dwmac->apb_regmap, GMAC_GTXCLK_SEL, GMAC_GTXCLK_SEL_PLL);
+
+		reg = GMAC_TX_CLK_EN | GMAC_TX_CLK_N_EN | GMAC_TX_CLK_OUT_EN |
+		      GMAC_RX_CLK_EN | GMAC_RX_CLK_N_EN;
+		break;
+
+	default:
+		dev_err(dwmac->dev, "unsupported phy interface %d\n",
+			plat->mac_interface);
+		return -EINVAL;
+	}
+
+	regmap_write(dwmac->apb_regmap, GMAC_CLK_EN, reg);
+
+	return 0;
+}
+
+static int thead_dwmac_init(struct platform_device *pdev,
+			    struct plat_stmmacenet_data *plat)
+{
+	struct thead_dwmac *dwmac = plat->bsp_priv;
+	int ret;
+
+	ret = thead_dwmac_set_phy_if(plat);
+	if (ret)
+		return ret;
+
+	ret = thead_dwmac_set_txclk_dir(plat);
+	if (ret)
+		return ret;
+
+	regmap_write(dwmac->apb_regmap, GMAC_RXCLK_DELAY_CTRL,
+		     GMAC_RXCLK_DELAY_VAL(dwmac->rx_delay));
+	regmap_write(dwmac->apb_regmap, GMAC_TXCLK_DELAY_CTRL,
+		     GMAC_TXCLK_DELAY_VAL(dwmac->tx_delay));
+
+	thead_dwmac_fix_speed(dwmac, SPEED_1000, 0);
+
+	return thead_dwmac_enable_clk(plat);
+}
+
+static int thead_dwmac_probe(struct platform_device *pdev)
+{
+	struct plat_stmmacenet_data *plat;
+	struct stmmac_resources stmmac_res;
+	struct thead_dwmac *dwmac;
+	struct device_node *np = pdev->dev.of_node;
+	u32 delay_ps;
+	int ret;
+
+	ret = stmmac_get_platform_resources(pdev, &stmmac_res);
+	if (ret)
+		return dev_err_probe(&pdev->dev, ret,
+				     "failed to get resources\n");
+
+	plat = devm_stmmac_probe_config_dt(pdev, stmmac_res.mac);
+	if (IS_ERR(plat))
+		return dev_err_probe(&pdev->dev, PTR_ERR(plat),
+				     "dt configuration failed\n");
+
+	dwmac = devm_kzalloc(&pdev->dev, sizeof(*dwmac), GFP_KERNEL);
+	if (!dwmac)
+		return -ENOMEM;
+
+	if (!of_property_read_u32(np, "rx-internal-delay-ps", &delay_ps))
+		dwmac->rx_delay = delay_ps;
+	if (!of_property_read_u32(np, "tx-internal-delay-ps", &delay_ps))
+		dwmac->tx_delay = delay_ps;
+
+	dwmac->apb_regmap = syscon_regmap_lookup_by_phandle(np, "thead,gmacapb");
+	if (IS_ERR(dwmac->apb_regmap))
+		return dev_err_probe(&pdev->dev, PTR_ERR(dwmac->apb_regmap),
+				     "Failed to get gmac apb syscon\n");
+
+	dwmac->dev = &pdev->dev;
+	dwmac->plat = plat;
+	plat->bsp_priv = dwmac;
+	plat->fix_mac_speed = thead_dwmac_fix_speed;
+
+	ret = thead_dwmac_init(pdev, plat);
+	if (ret)
+		return ret;
+
+	return stmmac_dvr_probe(&pdev->dev, plat, &stmmac_res);
+}
+
+static const struct of_device_id thead_dwmac_match[] = {
+	{ .compatible = "thead,th1520-dwmac" },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, thead_dwmac_match);
+
+static struct platform_driver thead_dwmac_driver = {
+	.probe = thead_dwmac_probe,
+	.remove_new = stmmac_pltfr_remove,
+	.driver = {
+		.name = "thead-dwmac",
+		.pm = &stmmac_pltfr_pm_ops,
+		.of_match_table = thead_dwmac_match,
+	},
+};
+module_platform_driver(thead_dwmac_driver);
+
+MODULE_AUTHOR("T-HEAD");
+MODULE_AUTHOR("Jisheng Zhang <jszhang@kernel.org>");
+MODULE_DESCRIPTION("T-HEAD dwmac platform driver");
+MODULE_LICENSE("GPL");
diff --git a/drivers/pci/controller/cadence/Kconfig b/drivers/pci/controller/cadence/Kconfig
index 291d12711363..25c768d5afb4 100644
--- a/drivers/pci/controller/cadence/Kconfig
+++ b/drivers/pci/controller/cadence/Kconfig
@@ -42,6 +42,17 @@ config PCIE_CADENCE_PLAT_EP
 	  endpoint mode. This PCIe controller may be embedded into many
 	  different vendors SoCs.
 
+config PCIE_CADENCE_SOPHGO
+	bool "Cadence Sophgo PCIe Host controller"
+	depends on OF
+	select IRQ_DOMAIN
+	select PCIE_CADENCE
+	help
+	  Say Y here if you want to support the Cadence PCIe controller in host mode
+	  for Sophgo SoCs. this PCIe controller is from cadence, integrated into the
+	  Sophgo SoCs. PCIe is one of subsystems, it is choisable, Don't be
+	  care of this if it is not used in your systems.
+
 config PCI_J721E
 	bool
 
diff --git a/drivers/pci/controller/cadence/Makefile b/drivers/pci/controller/cadence/Makefile
index 9bac5fb2f13d..edac7c5e94a3 100644
--- a/drivers/pci/controller/cadence/Makefile
+++ b/drivers/pci/controller/cadence/Makefile
@@ -4,3 +4,4 @@ obj-$(CONFIG_PCIE_CADENCE_HOST) += pcie-cadence-host.o
 obj-$(CONFIG_PCIE_CADENCE_EP) += pcie-cadence-ep.o
 obj-$(CONFIG_PCIE_CADENCE_PLAT) += pcie-cadence-plat.o
 obj-$(CONFIG_PCI_J721E) += pci-j721e.o
+obj-$(CONFIG_PCIE_CADENCE_SOPHGO) += pcie-cadence-sophgo.o
diff --git a/drivers/pci/controller/cadence/pcie-cadence-sophgo.c b/drivers/pci/controller/cadence/pcie-cadence-sophgo.c
new file mode 100644
index 000000000000..c0dd61e31adc
--- /dev/null
+++ b/drivers/pci/controller/cadence/pcie-cadence-sophgo.c
@@ -0,0 +1,972 @@
+// SPDX-License-Identifier: GPL-2.0
+// Copyright (c) 2017 Cadence
+// Cadence PCIe host controller driver.
+// Author: Cyrille Pitchen <cyrille.pitchen@free-electrons.com>
+
+#include <linux/kernel.h>
+#include <linux/of_address.h>
+#include <linux/of_pci.h>
+#include <linux/msi.h>
+#include <linux/irq.h>
+#include <linux/irqdomain.h>
+#include <linux/irqchip/chained_irq.h>
+#include <linux/platform_device.h>
+#include <linux/pm_runtime.h>
+
+#include "pcie-cadence.h"
+#include "pcie-cadence-sophgo.h"
+
+#define MAX_MSI_IRQS			512
+#define MAX_MSI_IRQS_PER_CTRL		1
+#define MAX_MSI_CTRLS			(MAX_MSI_IRQS / MAX_MSI_IRQS_PER_CTRL)
+#define MSI_DEF_NUM_VECTORS		512
+#define BYTE_NUM_PER_MSI_VEC		4
+
+// mango sideband signals
+#define CDNS_PCIE_CFG_MANGO_APB     0x1800000
+#define CDNS_PCIE_IRS_REG0400       0x0400
+#define CDNS_PCIE_IRS_REG0404       0x0404
+#define CDNS_PCIE_IRS_REG0418       0x0418
+#define CDNS_PCIE_IRS_REG041C       0x041C
+#define CDNS_PCIE_IRS_REG0804       0x0804
+#define CDNS_PCIE_IRS_REG080C       0x080C
+#define CDNS_PCIE_IRS_REG0810       0x0810
+#define CDNS_PCIE_IRS_REG085C       0x085C
+#define CDNS_PCIE_IRS_REG0860       0x0860
+#define CDNS_PCIE_IRS_REG0864       0x0864
+#define CDNS_PCIE_IRS_REG0868       0x0868
+#define CDNS_PCIE_IRS_REG086C       0x086C
+
+#define CDNS_PCIE_IRS_REG0804_CLR_LINK0_MSI_IN_BIT		2
+#define CDNS_PCIE_IRS_REG0804_CLR_LINK1_MSI_IN_BIT		3
+#define CDNS_PCIE_IRS_REG0810_ST_LINK0_MSI_IN_BIT		2
+#define CDNS_PCIE_IRS_REG0810_ST_LINK1_MSI_IN_BIT		3
+
+#define CDNS_PLAT_CPU_TO_BUS_ADDR       0xCFFFFFFFFF
+
+struct cdns_pcie_database {
+	void __iomem *pcie_reg_base;
+};
+
+static struct cdns_pcie_database cdns_pcie_db;
+
+static inline void cdns_pcie_rp_writel(struct cdns_pcie *pcie,
+				       u32 reg, u32 value)
+{
+	writel(value, pcie->reg_base + CDNS_PCIE_RP_BASE + reg);
+}
+
+static inline u32 cdns_pcie_rp_readl(struct cdns_pcie *pcie,
+				       u32 reg)
+{
+	return readl(pcie->reg_base + CDNS_PCIE_RP_BASE + reg);
+}
+
+/**
+ * struct cdns_mango_pcie_rc - private data for this PCIe Root Complex driver
+ * @pcie: Cadence PCIe controller
+ * @dev: pointer to PCIe device
+ * @cfg_res: start/end offsets in the physical system memory to map PCI
+ *           configuration space accesses
+ * @bus_range: first/last buses behind the PCIe host controller
+ * @cfg_base: IO mapped window to access the PCI configuration space of a
+ *            single function at a time
+ * @max_regions: maximum number of regions supported by the hardware
+ * @no_bar_nbits: Number of bits to keep for inbound (PCIe -> CPU) address
+ *                translation (nbits sets into the "no BAR match" register)
+ * @vendor_id: PCI vendor ID
+ * @device_id: PCI device ID
+ */
+struct cdns_mango_pcie_rc {
+	struct cdns_pcie	pcie;
+	struct device		*dev;
+	struct resource		*cfg_res;
+	struct resource		*bus_range;
+	void __iomem		*cfg_base;
+	u32			max_regions;
+	u32			no_bar_nbits;
+	u16			vendor_id;
+	u16			device_id;
+	u16			pcie_id;
+	u16			link_id;
+	u32			top_intc_used;
+	u32			msix_supported;
+	struct irq_domain	*msi_domain;
+	int			msi_irq;
+	struct irq_domain	*irq_domain;
+	dma_addr_t		msi_data;
+	void			*msi_page;
+	struct irq_chip		*msi_irq_chip;
+	u32			num_vectors;
+	u32			num_applied_vecs;
+	u32			irq_mask[MAX_MSI_CTRLS];
+	struct pci_bus		*root_bus;
+	raw_spinlock_t		lock;
+	DECLARE_BITMAP(msi_irq_in_use, MAX_MSI_IRQS);
+};
+
+static u64 cdns_mango_cpu_addr_fixup(struct cdns_pcie *pcie, u64 cpu_addr)
+{
+	return cpu_addr & CDNS_PLAT_CPU_TO_BUS_ADDR;
+}
+
+static const struct cdns_pcie_ops cdns_mango_ops = {
+	.cpu_addr_fixup = cdns_mango_cpu_addr_fixup,
+};
+
+static void __iomem *cdns_mango_pci_map_bus(struct pci_bus *bus, unsigned int devfn,
+					    int where)
+{
+	struct pci_host_bridge *bridge = pci_find_host_bridge(bus);
+	struct cdns_mango_pcie_rc *rc = pci_host_bridge_priv(bridge);
+	struct cdns_pcie *pcie = &rc->pcie;
+	unsigned int busn = bus->number;
+	u32 addr0, desc0;
+
+	if (pci_is_root_bus(bus)) {
+		/*
+		 * Only the root port (devfn == 0) is connected to this bus.
+		 * All other PCI devices are behind some bridge hence on another
+		 * bus.
+		 */
+		if (devfn)
+			return NULL;
+
+		return pcie->reg_base + CDNS_PCIE_RP_BASE + (where & 0xfff);
+	}
+	/* Check that the link is up */
+	if (!(cdns_pcie_readl(pcie, CDNS_PCIE_LM_BASE) & 0x1))
+		return NULL;
+	/* Clear AXI link-down status */
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_LINKDOWN, 0x0);
+
+	/* Update Output registers for AXI region 0. */
+	addr0 = CDNS_PCIE_AT_OB_REGION_PCI_ADDR0_NBITS(12) |
+		CDNS_PCIE_AT_OB_REGION_PCI_ADDR0_DEVFN(devfn) |
+		CDNS_PCIE_AT_OB_REGION_PCI_ADDR0_BUS(busn);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_PCI_ADDR0(0), addr0);
+
+	/* Configuration Type 0 or Type 1 access. */
+	desc0 = CDNS_PCIE_AT_OB_REGION_DESC0_HARDCODED_RID |
+		CDNS_PCIE_AT_OB_REGION_DESC0_DEVFN(0);
+	/*
+	 * The bus number was already set once for all in desc1 by
+	 * cdns_pcie_host_init_address_translation().
+	 */
+	if (busn == bridge->busnr + 1)
+		desc0 |= CDNS_PCIE_AT_OB_REGION_DESC0_TYPE_CONF_TYPE0;
+	else
+		desc0 |= CDNS_PCIE_AT_OB_REGION_DESC0_TYPE_CONF_TYPE1;
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_DESC0(0), desc0);
+
+	return rc->cfg_base + (where & 0xfff);
+}
+
+int cdns_pcie_config_read(struct pci_bus *bus, unsigned int devfn,
+			    int where, int size, u32 *val)
+{
+	unsigned long addr;
+	unsigned int value, offset;
+	void __iomem *aligned_addr;
+
+	if ((bus->number != 0) && (bus->number != 0x40) &&
+	    (bus->number != 0x80) && (bus->number != 0xc0))
+		return pci_generic_config_read(bus, devfn, where, size, val);
+
+	addr = (unsigned long)bus->ops->map_bus(bus, devfn, where);
+	if (!addr) {
+		*val = ~0;
+		return PCIBIOS_DEVICE_NOT_FOUND;
+	}
+
+	if (size == 1) {
+		offset = addr & 0x3;
+		aligned_addr = (void __iomem *)(addr & ~0x3UL);
+		value = readl(aligned_addr);
+		*val = (value >> (8 * offset)) & 0xff;
+	} else if (size == 2) {
+		WARN_ON((addr & 0x1) != 0); // address should be aligned to 2 bytes
+		offset = addr & 0x3;
+		aligned_addr = (void __iomem *)(addr & ~0x3UL);
+		value = readl(aligned_addr);
+		*val = (value >> (8 * offset)) & 0xffff;
+	} else {
+		WARN_ON((addr & 0x3) != 0); // address should be aligned to 4 bytes
+		*val = readl((void __iomem *)(addr));
+	}
+
+	return PCIBIOS_SUCCESSFUL;
+}
+
+int cdns_pcie_config_write(struct pci_bus *bus, unsigned int devfn,
+			     int where, int size, u32 val)
+{
+	unsigned long addr;
+	unsigned int value, offset;
+	void __iomem *aligned_addr;
+
+	if ((bus->number != 0) && (bus->number != 0x40) &&
+	    (bus->number != 0x80) && (bus->number != 0xc0))
+		return pci_generic_config_write(bus, devfn, where, size, val);
+
+	addr = (unsigned long)bus->ops->map_bus(bus, devfn, where);
+	if (!addr)
+		return PCIBIOS_DEVICE_NOT_FOUND;
+
+	if (size == 1) {
+		offset = addr & 0x3;
+		aligned_addr = (void __iomem *)(addr & ~0x3UL);
+		value = readl(aligned_addr);
+		value &= ~(0xFF << (8 * offset));
+		value |= ((val << (8 * offset)) & (0xFF << (8 * offset)));
+		writel(value, aligned_addr);
+	} else if (size == 2) {
+		WARN_ON((addr & 0x1) != 0);
+		offset = addr & 0x3;
+		aligned_addr = (void __iomem *)(addr & ~0x3UL);
+		value = readl(aligned_addr);
+		value &= ~(0xFFFF << (8 * offset));
+		value |= ((val << (8 * offset)) & (0xFFFF << (8 * offset)));
+		writel(value, aligned_addr);
+	} else {
+		WARN_ON((addr & 0x3) != 0);
+		writel(val, (void __iomem *)(addr));
+	}
+
+	return PCIBIOS_SUCCESSFUL;
+}
+
+
+static struct pci_ops cdns_pcie_host_ops = {
+	.map_bus	= cdns_mango_pci_map_bus,
+	.read		= cdns_pcie_config_read,
+	.write		= cdns_pcie_config_write,
+};
+
+static const struct of_device_id cdns_pcie_host_of_match[] = {
+	{ .compatible = "sophgo,cdns-pcie-host" },
+
+	{ },
+};
+
+static int cdns_pcie_host_init_root_port(struct cdns_mango_pcie_rc *rc)
+{
+	struct cdns_pcie *pcie = &rc->pcie;
+	u32 value, ctrl;
+	u32 id;
+
+	/*
+	 * Set the root complex BAR configuration register:
+	 * - disable both BAR0 and BAR1.
+	 * - enable Prefetchable Memory Base and Limit registers in type 1
+	 *   config space (64 bits).
+	 * - enable IO Base and Limit registers in type 1 config
+	 *   space (32 bits).
+	 */
+	ctrl = CDNS_PCIE_LM_BAR_CFG_CTRL_DISABLED;
+	value = CDNS_PCIE_LM_RC_BAR_CFG_BAR0_CTRL(ctrl) |
+		CDNS_PCIE_LM_RC_BAR_CFG_BAR1_CTRL(ctrl) |
+		CDNS_PCIE_LM_RC_BAR_CFG_PREFETCH_MEM_ENABLE |
+		CDNS_PCIE_LM_RC_BAR_CFG_PREFETCH_MEM_64BITS |
+		CDNS_PCIE_LM_RC_BAR_CFG_IO_ENABLE |
+		CDNS_PCIE_LM_RC_BAR_CFG_IO_32BITS;
+	cdns_pcie_writel(pcie, CDNS_PCIE_LM_RC_BAR_CFG, value);
+
+	/* Set root port configuration space */
+	if (rc->vendor_id != 0xffff) {
+		id = CDNS_PCIE_LM_ID_VENDOR(rc->vendor_id) |
+			CDNS_PCIE_LM_ID_SUBSYS(rc->vendor_id);
+		cdns_pcie_writel(pcie, CDNS_PCIE_LM_ID, id);
+	}
+
+	if (rc->device_id != 0xffff) {
+		value = cdns_pcie_rp_readl(pcie, PCI_VENDOR_ID);
+		value &= 0x0000FFFF;
+		value |= (rc->device_id << 16);
+		cdns_pcie_rp_writel(pcie, PCI_VENDOR_ID, value);
+	}
+
+	cdns_pcie_rp_writel(pcie, PCI_CLASS_REVISION, PCI_CLASS_BRIDGE_PCI << 16);
+
+	return 0;
+}
+
+static int cdns_pcie_host_init_address_translation(struct cdns_mango_pcie_rc *rc)
+{
+	struct cdns_pcie *pcie = &rc->pcie;
+	struct pci_host_bridge *bridge = pci_host_bridge_from_priv(rc);
+	struct resource *cfg_res = rc->cfg_res;
+	struct resource_entry *entry = NULL;
+	u32 addr0, addr1, desc1;
+	u64 cpu_addr;
+	int r, busnr = 0;
+
+	entry = resource_list_first_type(&bridge->windows, IORESOURCE_BUS);
+	if (entry)
+		busnr = entry->res->start;
+
+	/*
+	 * Reserve region 0 for PCI configure space accesses:
+	 * OB_REGION_PCI_ADDR0 and OB_REGION_DESC0 are updated dynamically by
+	 * cdns_pci_map_bus(), other region registers are set here once for all.
+	 */
+	addr1 = 0; /* Should be programmed to zero. */
+	desc1 = CDNS_PCIE_AT_OB_REGION_DESC1_BUS(busnr);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_PCI_ADDR1(0), addr1);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_DESC1(0), desc1);
+
+	cpu_addr = cfg_res->start;
+	addr0 = CDNS_PCIE_AT_OB_REGION_CPU_ADDR0_NBITS(12) |
+		(lower_32_bits(cpu_addr) & GENMASK(31, 8));
+	addr1 = upper_32_bits(cpu_addr);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_CPU_ADDR0(0), addr0);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_OB_REGION_CPU_ADDR1(0), addr1);
+
+	r = 1;
+	resource_list_for_each_entry(entry, &bridge->windows) {
+		struct resource *res = entry->res;
+		u64 pci_addr = res->start - entry->offset;
+
+		if (resource_type(res) == IORESOURCE_IO)
+			cdns_pcie_set_outbound_region(pcie, busnr, 0, r,
+						      true,
+						      pci_pio_to_address(res->start),
+						      pci_addr,
+						      resource_size(res));
+		else
+			cdns_pcie_set_outbound_region(pcie, busnr, 0, r,
+						      false,
+						      res->start,
+						      pci_addr,
+						      resource_size(res));
+
+		r++;
+	}
+
+	/*
+	 * Set Root Port no BAR match Inbound Translation registers:
+	 * needed for MSI and DMA.
+	 * Root Port BAR0 and BAR1 are disabled, hence no need to set their
+	 * inbound translation registers.
+	 */
+	addr0 = CDNS_PCIE_AT_IB_RP_BAR_ADDR0_NBITS(rc->no_bar_nbits);
+	addr1 = 0;
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_IB_RP_BAR_ADDR0(RP_NO_BAR), addr0);
+	cdns_pcie_writel(pcie, CDNS_PCIE_AT_IB_RP_BAR_ADDR1(RP_NO_BAR), addr1);
+
+	return 0;
+}
+
+static int cdns_pcie_msi_init(struct cdns_mango_pcie_rc *rc)
+{
+	struct device *dev = rc->dev;
+	struct cdns_pcie *pcie = &rc->pcie;
+	u32 apb_base = CDNS_PCIE_CFG_MANGO_APB;
+	u64 msi_target = 0;
+	u32 value = 0;
+
+	// support 512 msi vectors
+	rc->msi_page = dma_alloc_coherent(dev, 2048, &rc->msi_data,
+					  (GFP_KERNEL|GFP_DMA32|__GFP_ZERO));
+	if (rc->msi_page == NULL)
+		return -1;
+
+	dev_info(dev, "msi_data is 0x%llx\n", rc->msi_data);
+	msi_target = (u64)rc->msi_data;
+
+	if (rc->link_id == 1) {
+		apb_base -= 0x800000;
+		/* Program the msi_data */
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0868),
+				 lower_32_bits(msi_target));
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG086C),
+				 upper_32_bits(msi_target));
+
+		value = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG080C));
+		value = (value & 0xffff0000) | MAX_MSI_IRQS;
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG080C), value);
+	} else {
+		/* Program the msi_data */
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0860),
+				 lower_32_bits(msi_target));
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0864),
+				 upper_32_bits(msi_target));
+
+		value = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG085C));
+		value = (value & 0x0000ffff) | (MAX_MSI_IRQS << 16);
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG085C), value);
+	}
+
+	return 0;
+}
+
+static int cdns_pcie_host_init(struct device *dev, struct cdns_mango_pcie_rc *rc)
+{
+	int err;
+
+	err = cdns_pcie_host_init_root_port(rc);
+	if (err)
+		return err;
+
+	err = cdns_pcie_host_init_address_translation(rc);
+	if (err)
+		return err;
+
+	if (rc->top_intc_used == 0) {
+		rc->num_vectors = MSI_DEF_NUM_VECTORS;
+		rc->num_applied_vecs = 0;
+		if (IS_ENABLED(CONFIG_PCI_MSI)) {
+			err = cdns_pcie_msi_init(rc);
+			if (err)
+				return err;
+		}
+	}
+	return 0;
+}
+
+
+static void cdns_pcie_msi_ack_irq(struct irq_data *d)
+{
+	irq_chip_ack_parent(d);
+}
+
+static void cdns_pcie_msi_mask_irq(struct irq_data *d)
+{
+	pci_msi_mask_irq(d);
+	irq_chip_mask_parent(d);
+}
+
+static void cdns_pcie_msi_unmask_irq(struct irq_data *d)
+{
+	pci_msi_unmask_irq(d);
+	irq_chip_unmask_parent(d);
+}
+
+static struct irq_chip cdns_pcie_msi_irq_chip = {
+	.name = "cdns-msi",
+	.irq_ack = cdns_pcie_msi_ack_irq,
+	.irq_mask = cdns_pcie_msi_mask_irq,
+	.irq_unmask = cdns_pcie_msi_unmask_irq,
+};
+
+static struct msi_domain_info cdns_pcie_msi_domain_info = {
+	.flags	= (MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS),
+	.chip	= &cdns_pcie_msi_irq_chip,
+};
+
+static struct msi_domain_info cdns_pcie_top_intr_msi_domain_info = {
+	.flags	= (MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS
+		   | MSI_FLAG_PCI_MSIX),
+	.chip	= &cdns_pcie_msi_irq_chip,
+};
+
+struct vendor_id_list vendor_id_list[] = {
+	{"Inter X520", 0x8086, 0x10fb},
+	{"Inter I40E", 0x8086, 0x1572},
+	//{"WangXun RP1000", 0x8088},
+	{"Switchtec", 0x11f8,0x4052},
+};
+
+size_t vendor_id_list_num = ARRAY_SIZE(vendor_id_list);
+
+int check_vendor_id(struct pci_dev *dev, struct vendor_id_list vendor_id_list[],
+			size_t vendor_id_list_num)
+{
+	uint16_t device_vendor_id;
+	uint16_t device_id;
+
+	if (pci_read_config_word(dev, PCI_VENDOR_ID, &device_vendor_id) != 0) {
+		pr_err("Failed to read device vendor ID\n");
+		return 0;
+	}
+
+	if (pci_read_config_word(dev, PCI_DEVICE_ID, &device_id) != 0) {
+		pr_err("Failed to read device vendor ID\n");
+		return 0;
+	}
+
+	for (int i = 0; i < vendor_id_list_num; ++i) {
+		if (device_vendor_id == vendor_id_list[i].vendor_id && device_id == vendor_id_list[i].device_id) {
+			pr_info("dev: %s vendor ID: 0x%04x device ID: 0x%04x Enable MSI-X IRQ\n",
+				vendor_id_list[i].name, device_vendor_id, device_id);
+			return 1;
+		}
+	}
+	return 0;
+}
+
+
+static int cdns_pcie_msi_setup_for_top_intc(struct cdns_mango_pcie_rc *rc, int intc_id)
+{
+	struct irq_domain *irq_parent = cdns_pcie_get_parent_irq_domain(intc_id);
+	struct fwnode_handle *fwnode = of_node_to_fwnode(rc->dev->of_node);
+
+	if (rc->msix_supported == 1) {
+		rc->msi_domain = pci_msi_create_irq_domain(fwnode,
+							   &cdns_pcie_top_intr_msi_domain_info,
+							   irq_parent);
+	} else {
+		rc->msi_domain = pci_msi_create_irq_domain(fwnode,
+							   &cdns_pcie_msi_domain_info,
+							   irq_parent);
+	}
+
+	if (!rc->msi_domain) {
+		dev_err(rc->dev, "create msi irq domain failed\n");
+		return -ENODEV;
+	}
+
+	return 0;
+}
+
+/* MSI int handler */
+irqreturn_t cdns_handle_msi_irq(struct cdns_mango_pcie_rc *rc)
+{
+	u32 i, pos, irq;
+	unsigned long val;
+	u32 status, num_vectors;
+	irqreturn_t ret = IRQ_NONE;
+
+	num_vectors = rc->num_applied_vecs;
+	for (i = 0; i <= num_vectors; i++) {
+		status = readl((void *)(rc->msi_page + i * BYTE_NUM_PER_MSI_VEC));
+		if (!status)
+			continue;
+
+		ret = IRQ_HANDLED;
+		val = status;
+		pos = 0;
+		while ((pos = find_next_bit(&val, MAX_MSI_IRQS_PER_CTRL,
+					    pos)) != MAX_MSI_IRQS_PER_CTRL) {
+			irq = irq_find_mapping(rc->irq_domain,
+					       (i * MAX_MSI_IRQS_PER_CTRL) +
+					       pos);
+			generic_handle_irq(irq);
+			pos++;
+		}
+		writel(0, ((void *)(rc->msi_page) + i * BYTE_NUM_PER_MSI_VEC));
+	}
+	if (ret == IRQ_NONE) {
+		ret = IRQ_HANDLED;
+		for (i = 0; i <= num_vectors; i++) {
+			for (pos = 0; pos < MAX_MSI_IRQS_PER_CTRL; pos++) {
+				irq = irq_find_mapping(rc->irq_domain,
+						       (i * MAX_MSI_IRQS_PER_CTRL) +
+						       pos);
+				if (!irq)
+					continue;
+				generic_handle_irq(irq);
+			}
+		}
+	}
+
+	return ret;
+}
+
+static irqreturn_t cdns_pcie_irq_handler(int irq, void *arg)
+{
+	struct cdns_mango_pcie_rc *rc = arg;
+	struct cdns_pcie *pcie = &rc->pcie;
+	u32 apb_base = CDNS_PCIE_CFG_MANGO_APB;
+	u32 status = 0;
+	u32 st_msi_in_bit = 0;
+	u32 clr_msi_in_bit = 0;
+
+	if (rc->link_id == 1) {
+		apb_base -= 0x800000;
+		st_msi_in_bit = CDNS_PCIE_IRS_REG0810_ST_LINK1_MSI_IN_BIT;
+		clr_msi_in_bit = CDNS_PCIE_IRS_REG0804_CLR_LINK1_MSI_IN_BIT;
+	} else {
+		st_msi_in_bit = CDNS_PCIE_IRS_REG0810_ST_LINK0_MSI_IN_BIT;
+		clr_msi_in_bit = CDNS_PCIE_IRS_REG0804_CLR_LINK0_MSI_IN_BIT;
+	}
+
+	status = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG0810));
+	if ((status >> st_msi_in_bit) & 0x1) {
+		WARN_ON(!IS_ENABLED(CONFIG_PCI_MSI));
+
+		//clear msi interrupt bit reg0810[2]
+		status = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG0804));
+		status |= ((u32)0x1 << clr_msi_in_bit);
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0804), status);
+
+		status &= ~((u32)0x1 << clr_msi_in_bit);
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0804), status);
+
+		cdns_handle_msi_irq(rc);
+	}
+
+	return IRQ_HANDLED;
+}
+
+/* Chained MSI interrupt service routine */
+static void cdns_chained_msi_isr(struct irq_desc *desc)
+{
+	struct irq_chip *chip = irq_desc_get_chip(desc);
+	struct cdns_mango_pcie_rc *rc;
+	struct cdns_pcie *pcie;
+	u32 apb_base = CDNS_PCIE_CFG_MANGO_APB;
+	u32 status = 0;
+	u32 st_msi_in_bit = 0;
+	u32 clr_msi_in_bit = 0;
+
+	chained_irq_enter(chip, desc);
+
+	rc = irq_desc_get_handler_data(desc);
+	pcie = &rc->pcie;
+	if (rc->link_id == 1) {
+		apb_base -= 0x800000;
+		st_msi_in_bit = CDNS_PCIE_IRS_REG0810_ST_LINK1_MSI_IN_BIT;
+		clr_msi_in_bit = CDNS_PCIE_IRS_REG0804_CLR_LINK1_MSI_IN_BIT;
+	} else {
+		st_msi_in_bit = CDNS_PCIE_IRS_REG0810_ST_LINK0_MSI_IN_BIT;
+		clr_msi_in_bit = CDNS_PCIE_IRS_REG0804_CLR_LINK0_MSI_IN_BIT;
+	}
+
+	status = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG0810));
+	if ((status >> st_msi_in_bit) & 0x1) {
+		WARN_ON(!IS_ENABLED(CONFIG_PCI_MSI));
+
+		//clear msi interrupt bit reg0810[2]
+		status = cdns_pcie_readl(pcie, (apb_base + CDNS_PCIE_IRS_REG0804));
+		status |= ((u32)0x1 << clr_msi_in_bit);
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0804), status);
+
+		status &= ~((u32)0x1 << clr_msi_in_bit);
+		cdns_pcie_writel(pcie, (apb_base + CDNS_PCIE_IRS_REG0804), status);
+
+		cdns_handle_msi_irq(rc);
+	}
+
+	chained_irq_exit(chip, desc);
+}
+
+static int cdns_pci_msi_set_affinity(struct irq_data *d,
+				   const struct cpumask *mask, bool force)
+{
+	return -EINVAL;
+}
+
+static void cdns_pci_bottom_mask(struct irq_data *d)
+{
+}
+
+static void cdns_pci_bottom_unmask(struct irq_data *d)
+{
+}
+
+static void cdns_pci_setup_msi_msg(struct irq_data *d, struct msi_msg *msg)
+{
+	struct cdns_mango_pcie_rc *rc = irq_data_get_irq_chip_data(d);
+	u64 msi_target;
+
+	msi_target = (u64)rc->msi_data;
+
+	msg->address_lo = lower_32_bits(msi_target) + BYTE_NUM_PER_MSI_VEC * d->hwirq;
+	msg->address_hi = upper_32_bits(msi_target);
+	msg->data = 1;
+
+	rc->num_applied_vecs = d->hwirq;
+
+	dev_err(rc->dev, "msi#%d address_hi %#x address_lo %#x\n",
+		(int)d->hwirq, msg->address_hi, msg->address_lo);
+}
+
+static void cdns_pci_bottom_ack(struct irq_data *d)
+{
+}
+
+static struct irq_chip cdns_pci_msi_bottom_irq_chip = {
+	.name = "CDNS-PCI-MSI",
+	.irq_ack = cdns_pci_bottom_ack,
+	.irq_compose_msi_msg = cdns_pci_setup_msi_msg,
+	.irq_set_affinity = cdns_pci_msi_set_affinity,
+	.irq_mask = cdns_pci_bottom_mask,
+	.irq_unmask = cdns_pci_bottom_unmask,
+};
+
+static int cdns_pcie_irq_domain_alloc(struct irq_domain *domain,
+				    unsigned int virq, unsigned int nr_irqs,
+				    void *args)
+{
+	struct cdns_mango_pcie_rc *rc = domain->host_data;
+	unsigned long flags;
+	u32 i;
+	int bit;
+
+	raw_spin_lock_irqsave(&rc->lock, flags);
+
+	bit = bitmap_find_free_region(rc->msi_irq_in_use, rc->num_vectors,
+				      order_base_2(nr_irqs));
+
+	raw_spin_unlock_irqrestore(&rc->lock, flags);
+
+	if (bit < 0)
+		return -ENOSPC;
+
+	for (i = 0; i < nr_irqs; i++)
+		irq_domain_set_info(domain, virq + i, bit + i,
+				    rc->msi_irq_chip,
+				    rc, handle_edge_irq,
+				    NULL, NULL);
+
+	return 0;
+}
+
+static void cdns_pcie_irq_domain_free(struct irq_domain *domain,
+				    unsigned int virq, unsigned int nr_irqs)
+{
+	struct irq_data *d = irq_domain_get_irq_data(domain, virq);
+	struct cdns_mango_pcie_rc *rc = irq_data_get_irq_chip_data(d);
+	unsigned long flags;
+
+	raw_spin_lock_irqsave(&rc->lock, flags);
+
+	bitmap_release_region(rc->msi_irq_in_use, d->hwirq,
+			      order_base_2(nr_irqs));
+
+	raw_spin_unlock_irqrestore(&rc->lock, flags);
+}
+
+static const struct irq_domain_ops cdns_pcie_msi_domain_ops = {
+	.alloc	= cdns_pcie_irq_domain_alloc,
+	.free	= cdns_pcie_irq_domain_free,
+};
+
+int cdns_pcie_allocate_domains(struct cdns_mango_pcie_rc *rc)
+{
+	struct fwnode_handle *fwnode = of_node_to_fwnode(rc->dev->of_node);
+
+	rc->irq_domain = irq_domain_create_linear(fwnode, rc->num_vectors,
+					       &cdns_pcie_msi_domain_ops, rc);
+	if (!rc->irq_domain) {
+		dev_err(rc->dev, "Failed to create IRQ domain\n");
+		return -ENOMEM;
+	}
+
+	irq_domain_update_bus_token(rc->irq_domain, DOMAIN_BUS_NEXUS);
+
+	rc->msi_domain = pci_msi_create_irq_domain(fwnode,
+						   &cdns_pcie_msi_domain_info,
+						   rc->irq_domain);
+	if (!rc->msi_domain) {
+		dev_err(rc->dev, "Failed to create MSI domain\n");
+		irq_domain_remove(rc->irq_domain);
+		return -ENOMEM;
+	}
+
+	return 0;
+}
+
+void cdns_pcie_free_msi(struct cdns_mango_pcie_rc *rc)
+{
+	if (rc->msi_irq) {
+		irq_set_chained_handler(rc->msi_irq, NULL);
+		irq_set_handler_data(rc->msi_irq, NULL);
+	}
+
+	irq_domain_remove(rc->msi_domain);
+	irq_domain_remove(rc->irq_domain);
+
+	if (rc->msi_page)
+		dma_free_coherent(rc->dev, 1024, rc->msi_page, rc->msi_data);
+
+}
+
+static int cdns_pcie_msi_setup(struct cdns_mango_pcie_rc *rc)
+{
+	int ret = 0;
+
+	raw_spin_lock_init(&rc->lock);
+
+	if (IS_ENABLED(CONFIG_PCI_MSI)) {
+		rc->msi_irq_chip = &cdns_pci_msi_bottom_irq_chip;
+
+		ret = cdns_pcie_allocate_domains(rc);
+		if (ret)
+			return ret;
+
+		if (rc->msi_irq)
+			irq_set_chained_handler_and_data(rc->msi_irq, cdns_chained_msi_isr, rc);
+	}
+
+	return ret;
+}
+
+static int cdns_pcie_irq_parse_and_map_pci(const struct pci_dev *dev, u8 slot, u8 pin)
+{
+	return 0; /* Proper return code 0 == NO_IRQ */
+}
+
+static int cdns_pcie_host_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct pci_host_bridge *bridge;
+	struct cdns_mango_pcie_rc *rc;
+	struct cdns_pcie *pcie;
+	struct resource *res;
+	int ret;
+	int phy_count;
+	int top_intc_id = -1;
+
+	bridge = devm_pci_alloc_host_bridge(dev, sizeof(*rc));
+	if (!bridge)
+		return -ENOMEM;
+
+	rc = pci_host_bridge_priv(bridge);
+	rc->dev = dev;
+
+	pcie = &rc->pcie;
+	pcie->is_rc = true;
+	pcie->ops = &cdns_mango_ops;
+
+	rc->max_regions = 32;
+	of_property_read_u32(np, "cdns,max-outbound-regions", &rc->max_regions);
+
+	rc->no_bar_nbits = 32;
+	of_property_read_u32(np, "cdns,no-bar-match-nbits", &rc->no_bar_nbits);
+
+	rc->vendor_id = 0xffff;
+	of_property_read_u16(np, "vendor-id", &rc->vendor_id);
+
+	rc->device_id = 0xffff;
+	of_property_read_u16(np, "device-id", &rc->device_id);
+
+	rc->pcie_id = 0xffff;
+	of_property_read_u16(np, "pcie-id", &rc->pcie_id);
+
+	rc->link_id = 0xffff;
+	of_property_read_u16(np, "link-id", &rc->link_id);
+
+	rc->msix_supported = 0;
+	of_property_read_u32(np, "msix-supported", &rc->msix_supported);
+
+	rc->top_intc_used = 0;
+	of_property_read_u32(np, "top-intc-used", &rc->top_intc_used);
+	if (rc->top_intc_used == 1)
+		of_property_read_u32(np, "top-intc-id", &top_intc_id);
+
+	if (rc->link_id == 0) {
+		res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "reg");
+		pcie->reg_base = devm_ioremap_resource(dev, res);
+		if (IS_ERR(pcie->reg_base)) {
+			dev_err(dev, "missing \"reg\"\n");
+			return PTR_ERR(pcie->reg_base);
+		}
+		cdns_pcie_db.pcie_reg_base = pcie->reg_base;
+	} else if (rc->link_id == 1) {
+		pcie->reg_base = cdns_pcie_db.pcie_reg_base + 0x800000;
+	}
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "cfg");
+	rc->cfg_base = devm_pci_remap_cfg_resource(dev, res);
+	if (IS_ERR(rc->cfg_base)) {
+		dev_err(dev, "missing \"cfg\"\n");
+		return PTR_ERR(rc->cfg_base);
+	}
+	rc->cfg_res = res;
+
+	ret = cdns_pcie_init_phy(dev, pcie);
+	if (ret) {
+		dev_err(dev, "failed to init phy\n");
+		return ret;
+	}
+	platform_set_drvdata(pdev, pcie);
+
+	pm_runtime_enable(dev);
+	ret = pm_runtime_get_sync(dev);
+	if (ret < 0) {
+		dev_err(dev, "pm_runtime_get_sync() failed\n");
+		goto err_get_sync;
+	}
+
+	ret = cdns_pcie_host_init(dev, rc);
+	if (ret)
+		goto err_init;
+
+	if ((rc->top_intc_used == 0) && (IS_ENABLED(CONFIG_PCI_MSI))) {
+		rc->msi_irq = platform_get_irq_byname(pdev, "msi");
+		if (rc->msi_irq <= 0) {
+			dev_err(dev, "failed to get MSI irq\n");
+			goto err_init_irq;
+		}
+
+		ret = devm_request_irq(dev, rc->msi_irq, cdns_pcie_irq_handler,
+				       IRQF_SHARED | IRQF_NO_THREAD,
+				       "cdns-pcie-irq", rc);
+
+		if (ret) {
+			dev_err(dev, "failed to request MSI irq\n");
+			goto err_init_irq;
+		}
+	}
+
+	bridge->dev.parent = dev;
+	bridge->ops = &cdns_pcie_host_ops;
+	if (rc->top_intc_used == 1)
+		bridge->map_irq = of_irq_parse_and_map_pci;
+	else
+		bridge->map_irq = cdns_pcie_irq_parse_and_map_pci;
+	bridge->swizzle_irq = pci_common_swizzle;
+	if (rc->top_intc_used == 0)
+		bridge->sysdata = rc;
+
+	if (rc->top_intc_used == 0) {
+		ret = cdns_pcie_msi_setup(rc);
+		if (ret < 0)
+			goto err_host_probe;
+	} else if (rc->top_intc_used == 1) {
+		ret = cdns_pcie_msi_setup_for_top_intc(rc, top_intc_id);
+		if (ret < 0)
+			goto err_host_probe;
+	}
+
+	ret = pci_host_probe(bridge);
+	if (ret < 0)
+		goto err_host_probe;
+
+	return 0;
+
+ err_host_probe:
+ err_init_irq:
+	if ((rc->top_intc_used == 0) && pci_msi_enabled())
+		cdns_pcie_free_msi(rc);
+
+ err_init:
+	pm_runtime_put_sync(dev);
+
+ err_get_sync:
+	pm_runtime_disable(dev);
+	cdns_pcie_disable_phy(pcie);
+	phy_count = pcie->phy_count;
+	while (phy_count--)
+		device_link_del(pcie->link[phy_count]);
+
+	return ret;
+}
+
+static void cdns_pcie_shutdown(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct cdns_pcie *pcie = dev_get_drvdata(dev);
+	int ret;
+
+	ret = pm_runtime_put_sync(dev);
+	if (ret < 0)
+		dev_dbg(dev, "pm_runtime_put_sync failed\n");
+
+	pm_runtime_disable(dev);
+	cdns_pcie_disable_phy(pcie);
+}
+
+static struct platform_driver cdns_pcie_host_driver = {
+	.driver = {
+		.name = "cdns-pcie-host",
+		.of_match_table = cdns_pcie_host_of_match,
+		.pm	= &cdns_pcie_pm_ops,
+	},
+	.probe = cdns_pcie_host_probe,
+	.shutdown = cdns_pcie_shutdown,
+};
+builtin_platform_driver(cdns_pcie_host_driver);
diff --git a/drivers/pci/controller/cadence/pcie-cadence-sophgo.h b/drivers/pci/controller/cadence/pcie-cadence-sophgo.h
new file mode 100644
index 000000000000..ef46c46678ed
--- /dev/null
+++ b/drivers/pci/controller/cadence/pcie-cadence-sophgo.h
@@ -0,0 +1,17 @@
+#ifndef PCIE_CADENCE_SOPHGO
+#define PCIE_CADENCE_SOPHGO
+
+
+struct vendor_id_list {
+	const char  *name;
+	uint16_t    vendor_id;
+	uint16_t    device_id;
+};
+
+extern struct vendor_id_list vendor_id_list[];
+extern size_t vendor_id_list_num;
+
+extern struct irq_domain *cdns_pcie_get_parent_irq_domain(int intc_id);
+int check_vendor_id(struct pci_dev *dev, struct vendor_id_list vendor_id_list[],
+			size_t vendor_id_list_num);
+#endif
diff --git a/drivers/pci/msi/msi.c b/drivers/pci/msi/msi.c
index 7078200be11f..d701b49055c4 100644
--- a/drivers/pci/msi/msi.c
+++ b/drivers/pci/msi/msi.c
@@ -12,6 +12,7 @@
 
 #include "../pci.h"
 #include "msi.h"
+#include "../controller/cadence/pcie-cadence-sophgo.h"
 
 int pci_msi_enable = 1;
 int pci_msi_ignore_mask;
@@ -818,66 +819,70 @@ int __pci_enable_msix_range(struct pci_dev *dev, struct msix_entry *entries, int
 	}
 #endif
 
-	if (maxvec < minvec)
-		return -ERANGE;
+	if (check_vendor_id(dev, vendor_id_list, vendor_id_list_num)) {
+		if (maxvec < minvec)
+			return -ERANGE;
 
-	if (dev->msi_enabled) {
-		pci_info(dev, "can't enable MSI-X (MSI already enabled)\n");
-		return -EINVAL;
-	}
+		if (dev->msi_enabled) {
+			pci_info(dev, "can't enable MSI-X (MSI already enabled)\n");
+			return -EINVAL;
+		}
 
-	if (WARN_ON_ONCE(dev->msix_enabled))
-		return -EINVAL;
+		if (WARN_ON_ONCE(dev->msix_enabled))
+			return -EINVAL;
 
-	/* Check MSI-X early on irq domain enabled architectures */
-	if (!pci_msi_domain_supports(dev, MSI_FLAG_PCI_MSIX, ALLOW_LEGACY))
-		return -ENOTSUPP;
+		/* Check MSI-X early on irq domain enabled architectures */
+		if (!pci_msi_domain_supports(dev, MSI_FLAG_PCI_MSIX, ALLOW_LEGACY))
+			return -ENOTSUPP;
 
-	if (!pci_msi_supported(dev, nvec) || dev->current_state != PCI_D0)
-		return -EINVAL;
+		if (!pci_msi_supported(dev, nvec) || dev->current_state != PCI_D0)
+			return -EINVAL;
 
-	hwsize = pci_msix_vec_count(dev);
-	if (hwsize < 0)
-		return hwsize;
+		hwsize = pci_msix_vec_count(dev);
+		if (hwsize < 0)
+			return hwsize;
 
-	if (!pci_msix_validate_entries(dev, entries, nvec))
-		return -EINVAL;
+		if (!pci_msix_validate_entries(dev, entries, nvec))
+			return -EINVAL;
 
-	if (hwsize < nvec) {
-		/* Keep the IRQ virtual hackery working */
-		if (flags & PCI_IRQ_VIRTUAL)
-			hwsize = nvec;
-		else
-			nvec = hwsize;
-	}
+		if (hwsize < nvec) {
+			/* Keep the IRQ virtual hackery working */
+			if (flags & PCI_IRQ_VIRTUAL)
+				hwsize = nvec;
+			else
+				nvec = hwsize;
+		}
 
-	if (nvec < minvec)
-		return -ENOSPC;
+		if (nvec < minvec)
+			return -ENOSPC;
 
-	rc = pci_setup_msi_context(dev);
-	if (rc)
-		return rc;
+		rc = pci_setup_msi_context(dev);
+		if (rc)
+			return rc;
 
-	if (!pci_setup_msix_device_domain(dev, hwsize))
-		return -ENODEV;
+		if (!pci_setup_msix_device_domain(dev, hwsize))
+			return -ENODEV;
 
-	for (;;) {
-		if (affd) {
-			nvec = irq_calc_affinity_vectors(minvec, nvec, affd);
-			if (nvec < minvec)
-				return -ENOSPC;
-		}
+		for (;;) {
+			if (affd) {
+				nvec = irq_calc_affinity_vectors(minvec, nvec, affd);
+				if (nvec < minvec)
+					return -ENOSPC;
+			}
 
-		rc = msix_capability_init(dev, entries, nvec, affd);
-		if (rc == 0)
-			return nvec;
+			rc = msix_capability_init(dev, entries, nvec, affd);
+			if (rc == 0)
+				return nvec;
 
-		if (rc < 0)
-			return rc;
-		if (rc < minvec)
-			return -ENOSPC;
+			if (rc < 0)
+				return rc;
+			if (rc < minvec)
+				return -ENOSPC;
 
-		nvec = rc;
+			nvec = rc;
+		}
+	} else {
+		return -1;
 	}
 }
 
diff --git a/drivers/pci/pcie/portdrv.c b/drivers/pci/pcie/portdrv.c
index 46fad0d813b2..560b3a236d84 100644
--- a/drivers/pci/pcie/portdrv.c
+++ b/drivers/pci/pcie/portdrv.c
@@ -598,7 +598,7 @@ void pcie_port_service_unregister(struct pcie_port_service_driver *drv)
 }
 
 /* If this switch is set, PCIe port native services should not be enabled. */
-bool pcie_ports_disabled;
+bool pcie_ports_disabled = true;
 
 /*
  * If the user specified "pcie_ports=native", use the PCIe services regardless
diff --git a/drivers/pinctrl/Kconfig b/drivers/pinctrl/Kconfig
index 79753411b778..15ad8ada527d 100644
--- a/drivers/pinctrl/Kconfig
+++ b/drivers/pinctrl/Kconfig
@@ -22,7 +22,7 @@ config PINCONF
 	bool "Support pin configuration controllers" if COMPILE_TEST
 
 config GENERIC_PINCONF
-	bool
+	bool "GENERIC_PINCONF"
 	select PINCONF
 
 config DEBUG_PINCTRL
@@ -469,6 +469,15 @@ config PINCTRL_TB10X
 	depends on OF && ARC_PLAT_TB10X
 	select GPIOLIB
 
+config PINCTRL_TH1520
+	tristate "Pinctrl driver for the T-Head TH1520 SoC"
+	depends on ARCH_THEAD || COMPILE_TEST
+	select GENERIC_PINMUX_FUNCTIONS
+	select GENERIC_PINCONF
+	select PINMUX
+	help
+	  This selects the pinctrl driver for T-Head TH1520 RISC-V SoC.
+
 config PINCTRL_ZYNQ
 	bool "Pinctrl driver for Xilinx Zynq"
 	depends on ARCH_ZYNQ
diff --git a/drivers/pinctrl/Makefile b/drivers/pinctrl/Makefile
index 4275eca92488..f07a2ee92197 100644
--- a/drivers/pinctrl/Makefile
+++ b/drivers/pinctrl/Makefile
@@ -48,6 +48,7 @@ obj-$(CONFIG_PINCTRL_ST) 	+= pinctrl-st.o
 obj-$(CONFIG_PINCTRL_STMFX) 	+= pinctrl-stmfx.o
 obj-$(CONFIG_PINCTRL_SX150X)	+= pinctrl-sx150x.o
 obj-$(CONFIG_PINCTRL_TB10X)	+= pinctrl-tb10x.o
+obj-$(CONFIG_PINCTRL_TH1520)	+= pinctrl-th1520.o
 obj-$(CONFIG_PINCTRL_ZYNQMP)	+= pinctrl-zynqmp.o
 obj-$(CONFIG_PINCTRL_ZYNQ)	+= pinctrl-zynq.o
 
@@ -75,6 +76,7 @@ obj-$(CONFIG_SOC_STARFIVE)	+= starfive/
 obj-$(CONFIG_PINCTRL_STM32)	+= stm32/
 obj-y				+= sunplus/
 obj-$(CONFIG_PINCTRL_SUNXI)	+= sunxi/
+obj-$(CONFIG_ARCH_SOPHGO)	+= sophgo/
 obj-$(CONFIG_ARCH_TEGRA)	+= tegra/
 obj-y				+= ti/
 obj-$(CONFIG_PINCTRL_UNIPHIER)	+= uniphier/
diff --git a/drivers/pinctrl/pinctrl-th1520.c b/drivers/pinctrl/pinctrl-th1520.c
new file mode 100644
index 000000000000..6af46d59d0fa
--- /dev/null
+++ b/drivers/pinctrl/pinctrl-th1520.c
@@ -0,0 +1,860 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Pinctrl driver for the T-Head TH1520 SoC
+ *
+ * Copyright (C) 2023 Emil Renner Berthing <emil.renner.berthing@canonical.com>
+ */
+
+#include <linux/bits.h>
+#include <linux/cleanup.h>
+#include <linux/clk.h>
+#include <linux/device.h>
+#include <linux/io.h>
+#include <linux/mod_devicetable.h>
+#include <linux/module.h>
+#include <linux/mutex.h>
+#include <linux/of.h>
+#include <linux/platform_device.h>
+#include <linux/seq_file.h>
+#include <linux/spinlock.h>
+
+#include <linux/pinctrl/pinconf.h>
+#include <linux/pinctrl/pinconf-generic.h>
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/pinctrl/pinmux.h>
+
+#include "core.h"
+#include "pinmux.h"
+#include "pinconf.h"
+
+#define TH1520_PADCFG_IE	BIT(9)
+#define TH1520_PADCFG_SL	BIT(8)
+#define TH1520_PADCFG_ST	BIT(7)
+#define TH1520_PADCFG_SPU	BIT(6)
+#define TH1520_PADCFG_PS	BIT(5)
+#define TH1520_PADCFG_PE	BIT(4)
+#define TH1520_PADCFG_BIAS	(TH1520_PADCFG_SPU | TH1520_PADCFG_PS | TH1520_PADCFG_PE)
+#define TH1520_PADCFG_DS	GENMASK(3, 0)
+
+#define TH1520_PULL_DOWN_OHM	44000 /* typ. 44kOhm */
+#define TH1520_PULL_UP_OHM	48000 /* typ. 48kOhm */
+#define TH1520_PULL_STRONG_OHM	 2100 /* typ. 2.1kOhm */
+
+#define TH1520_PAD_NO_PADCFG	BIT(30)
+#define TH1520_PAD_MUXDATA	GENMASK(29, 0)
+
+struct th1520_pad_group {
+	const char *name;
+	const struct pinctrl_pin_desc *pins;
+	unsigned int npins;
+};
+
+struct th1520_pinctrl {
+	struct pinctrl_desc desc;
+	struct mutex mutex;	/* serialize adding functions */
+	raw_spinlock_t lock;	/* serialize register access */
+	void __iomem *base;
+	struct pinctrl_dev *pctl;
+};
+
+static void __iomem *th1520_padcfg(struct th1520_pinctrl *thp,
+				   unsigned int pin)
+{
+	return thp->base + 4 * (pin / 2);
+}
+
+static unsigned int th1520_padcfg_shift(unsigned int pin)
+{
+	return 16 * (pin & BIT(0));
+}
+
+static void __iomem *th1520_muxcfg(struct th1520_pinctrl *thp,
+				   unsigned int pin)
+{
+	return thp->base + 0x400 + 4 * (pin / 8);
+}
+
+static unsigned int th1520_muxcfg_shift(unsigned int pin)
+{
+	return 4 * (pin & GENMASK(2, 0));
+}
+
+enum th1520_muxtype {
+	TH1520_MUX_____,
+	TH1520_MUX_GPIO,
+	TH1520_MUX_PWM,
+	TH1520_MUX_UART,
+	TH1520_MUX_IR,
+	TH1520_MUX_I2C,
+	TH1520_MUX_SPI,
+	TH1520_MUX_QSPI,
+	TH1520_MUX_SDIO,
+	TH1520_MUX_AUD,
+	TH1520_MUX_I2S,
+	TH1520_MUX_MAC0,
+	TH1520_MUX_MAC1,
+	TH1520_MUX_DPU0,
+	TH1520_MUX_DPU1,
+	TH1520_MUX_ISP,
+	TH1520_MUX_HDMI,
+	TH1520_MUX_BSEL,
+	TH1520_MUX_DBG,
+	TH1520_MUX_CLK,
+	TH1520_MUX_JTAG,
+	TH1520_MUX_ISO,
+	TH1520_MUX_FUSE,
+	TH1520_MUX_RST,
+};
+
+static const char *const th1520_muxtype_string[] = {
+	[TH1520_MUX_GPIO] = "gpio",
+	[TH1520_MUX_PWM]  = "pwm",
+	[TH1520_MUX_UART] = "uart",
+	[TH1520_MUX_IR]   = "ir",
+	[TH1520_MUX_I2C]  = "i2c",
+	[TH1520_MUX_SPI]  = "spi",
+	[TH1520_MUX_QSPI] = "qspi",
+	[TH1520_MUX_SDIO] = "sdio",
+	[TH1520_MUX_AUD]  = "audio",
+	[TH1520_MUX_I2S]  = "i2s",
+	[TH1520_MUX_MAC0] = "gmac0",
+	[TH1520_MUX_MAC1] = "gmac1",
+	[TH1520_MUX_DPU0] = "dpu0",
+	[TH1520_MUX_DPU1] = "dpu1",
+	[TH1520_MUX_ISP]  = "isp",
+	[TH1520_MUX_HDMI] = "hdmi",
+	[TH1520_MUX_BSEL] = "bootsel",
+	[TH1520_MUX_DBG]  = "debug",
+	[TH1520_MUX_CLK]  = "clock",
+	[TH1520_MUX_JTAG] = "jtag",
+	[TH1520_MUX_ISO]  = "iso7816",
+	[TH1520_MUX_FUSE] = "efuse",
+	[TH1520_MUX_RST]  = "reset",
+};
+
+static enum th1520_muxtype th1520_muxtype_get(const char *str)
+{
+	enum th1520_muxtype mt;
+
+	for (mt = TH1520_MUX_GPIO; mt < ARRAY_SIZE(th1520_muxtype_string); mt++) {
+		if (!strcmp(str, th1520_muxtype_string[mt]))
+			return mt;
+	}
+	return TH1520_MUX_____;
+}
+
+#define TH1520_PAD(_nr, _name, m0, m1, m2, m3, m4, m5, _flags) \
+	{ .number = _nr, .name = #_name, .drv_data = (void *)((_flags) | \
+		(TH1520_MUX_##m0 <<  0) | (TH1520_MUX_##m1 <<  5) | (TH1520_MUX_##m2 << 10) | \
+		(TH1520_MUX_##m3 << 15) | (TH1520_MUX_##m4 << 20) | (TH1520_MUX_##m5 << 25)) }
+
+static const struct pinctrl_pin_desc th1520_group1_pins[] = {
+	TH1520_PAD(0,  OSC_CLK_IN,    ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(1,  OSC_CLK_OUT,   ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(2,  SYS_RST_N,     ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(3,  RTC_CLK_IN,    ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(4,  RTC_CLK_OUT,   ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	/* skip number 5 so we can calculate register offsets and shifts from the pin number */
+	TH1520_PAD(6,  TEST_MODE,     ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(7,  DEBUG_MODE,    DBG,  ____, ____, GPIO, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(8,  POR_SEL,       ____, ____, ____, ____, ____, ____, TH1520_PAD_NO_PADCFG),
+	TH1520_PAD(9,  I2C_AON_SCL,   I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(10, I2C_AON_SDA,   I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(11, CPU_JTG_TCLK,  JTAG, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(12, CPU_JTG_TMS,   JTAG, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(13, CPU_JTG_TDI,   JTAG, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(14, CPU_JTG_TDO,   JTAG, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(15, CPU_JTG_TRST,  JTAG, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(16, AOGPIO_7,      CLK,  AUD,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(17, AOGPIO_8,      UART, AUD,  IR,   GPIO, ____, ____, 0),
+	TH1520_PAD(18, AOGPIO_9,      UART, AUD,  IR,   GPIO, ____, ____, 0),
+	TH1520_PAD(19, AOGPIO_10,     CLK,  AUD,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(20, AOGPIO_11,     GPIO, AUD,  ____, ____, ____, ____, 0),
+	TH1520_PAD(21, AOGPIO_12,     GPIO, AUD,  ____, ____, ____, ____, 0),
+	TH1520_PAD(22, AOGPIO_13,     GPIO, AUD,  ____, ____, ____, ____, 0),
+	TH1520_PAD(23, AOGPIO_14,     GPIO, AUD,  ____, ____, ____, ____, 0),
+	TH1520_PAD(24, AOGPIO_15,     GPIO, AUD,  ____, ____, ____, ____, 0),
+	TH1520_PAD(25, AUDIO_PA0,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(26, AUDIO_PA1,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(27, AUDIO_PA2,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(28, AUDIO_PA3,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(29, AUDIO_PA4,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(30, AUDIO_PA5,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(31, AUDIO_PA6,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(32, AUDIO_PA7,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(33, AUDIO_PA8,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(34, AUDIO_PA9,     AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(35, AUDIO_PA10,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(36, AUDIO_PA11,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(37, AUDIO_PA12,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(38, AUDIO_PA13,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(39, AUDIO_PA14,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(40, AUDIO_PA15,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(41, AUDIO_PA16,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(42, AUDIO_PA17,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(43, AUDIO_PA27,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(44, AUDIO_PA28,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(45, AUDIO_PA29,    AUD,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(46, AUDIO_PA30,    AUD,  RST,  ____, GPIO, ____, ____, 0),
+};
+
+static const struct pinctrl_pin_desc th1520_group2_pins[] = {
+	TH1520_PAD(0,  QSPI1_SCLK,    QSPI, ISO,  ____, GPIO, FUSE, ____, 0),
+	TH1520_PAD(1,  QSPI1_CSN0,    QSPI, ____, I2C,  GPIO, FUSE, ____, 0),
+	TH1520_PAD(2,  QSPI1_D0_MOSI, QSPI, ISO,  I2C,  GPIO, FUSE, ____, 0),
+	TH1520_PAD(3,  QSPI1_D1_MISO, QSPI, ISO,  ____, GPIO, FUSE, ____, 0),
+	TH1520_PAD(4,  QSPI1_D2_WP,   QSPI, ISO,  UART, GPIO, FUSE, ____, 0),
+	TH1520_PAD(5,  QSPI1_D3_HOLD, QSPI, ISO,  UART, GPIO, ____, ____, 0),
+	TH1520_PAD(6,  I2C0_SCL,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(7,  I2C0_SDA,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(8,  I2C1_SCL,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(9,  I2C1_SDA,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(10, UART1_TXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(11, UART1_RXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(12, UART4_TXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(13, UART4_RXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(14, UART4_CTSN,    UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(15, UART4_RTSN,    UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(16, UART3_TXD,     DBG,  UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(17, UART3_RXD,     DBG,  UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(18, GPIO0_18,      GPIO, I2C,  ____, ____, ____, ____, 0),
+	TH1520_PAD(19, GPIO0_19,      GPIO, I2C,  ____, ____, ____, ____, 0),
+	TH1520_PAD(20, GPIO0_20,      GPIO, UART, IR,   ____, ____, ____, 0),
+	TH1520_PAD(21, GPIO0_21,      GPIO, UART, IR,   ____, DPU0, DPU1, 0),
+	TH1520_PAD(22, GPIO0_22,      GPIO, JTAG, I2C,  ____, DPU0, DPU1, 0),
+	TH1520_PAD(23, GPIO0_23,      GPIO, JTAG, I2C,  ____, DPU0, DPU1, 0),
+	TH1520_PAD(24, GPIO0_24,      GPIO, JTAG, QSPI, ____, DPU0, DPU1, 0),
+	TH1520_PAD(25, GPIO0_25,      GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(26, GPIO0_26,      GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(27, GPIO0_27,      GPIO, ____, I2C,  ____, DPU0, DPU1, 0),
+	TH1520_PAD(28, GPIO0_28,      GPIO, ____, I2C,  ____, DPU0, DPU1, 0),
+	TH1520_PAD(29, GPIO0_29,      GPIO, ____, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(30, GPIO0_30,      GPIO, ____, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(31, GPIO0_31,      GPIO, ____, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(32, GPIO1_0,       GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(33, GPIO1_1,       GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(34, GPIO1_2,       GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(35, GPIO1_3,       GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(36, GPIO1_4,       GPIO, JTAG, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(37, GPIO1_5,       GPIO, ____, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(38, GPIO1_6,       GPIO, ____, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(39, GPIO1_7,       GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(40, GPIO1_8,       GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(41, GPIO1_9,       GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(42, GPIO1_10,      GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(43, GPIO1_11,      GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(44, GPIO1_12,      GPIO, QSPI, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(45, GPIO1_13,      GPIO, UART, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(46, GPIO1_14,      GPIO, UART, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(47, GPIO1_15,      GPIO, UART, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(48, GPIO1_16,      GPIO, UART, ____, ____, DPU0, DPU1, 0),
+	TH1520_PAD(49, CLK_OUT_0,     BSEL, CLK,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(50, CLK_OUT_1,     BSEL, CLK,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(51, CLK_OUT_2,     BSEL, CLK,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(52, CLK_OUT_3,     BSEL, CLK,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(53, GPIO1_21,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(54, GPIO1_22,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(55, GPIO1_23,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(56, GPIO1_24,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(57, GPIO1_25,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(58, GPIO1_26,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(59, GPIO1_27,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(60, GPIO1_28,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(61, GPIO1_29,      GPIO, ____, ISP,  ____, ____, ____, 0),
+	TH1520_PAD(62, GPIO1_30,      GPIO, ____, ISP,  ____, ____, ____, 0),
+};
+
+static const struct pinctrl_pin_desc th1520_group3_pins[] = {
+	TH1520_PAD(0,  UART0_TXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(1,  UART0_RXD,     UART, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(2,  QSPI0_SCLK,    QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(3,  QSPI0_CSN0,    QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(4,  QSPI0_CSN1,    QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(5,  QSPI0_D0_MOSI, QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(6,  QSPI0_D1_MISO, QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(7,  QSPI0_D2_WP,   QSPI, PWM,  I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(8,  QSPI1_D3_HOLD, QSPI, ____, I2S,  GPIO, ____, ____, 0),
+	TH1520_PAD(9,  I2C2_SCL,      I2C,  UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(10, I2C2_SDA,      I2C,  UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(11, I2C3_SCL,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(12, I2C3_SDA,      I2C,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(13, GPIO2_13,      GPIO, SPI,  ____, ____, ____, ____, 0),
+	TH1520_PAD(14, SPI_SCLK,      SPI,  UART, IR,   GPIO, ____, ____, 0),
+	TH1520_PAD(15, SPI_CSN,       SPI,  UART, IR,   GPIO, ____, ____, 0),
+	TH1520_PAD(16, SPI_MOSI,      SPI,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(17, SPI_MISO,      SPI,  ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(18, GPIO2_18,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(19, GPIO2_19,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(20, GPIO2_20,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(21, GPIO2_21,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(22, GPIO2_22,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(23, GPIO2_23,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(24, GPIO2_24,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(25, GPIO2_25,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(26, SDIO0_WPRTN,   SDIO, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(27, SDIO0_DETN,    SDIO, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(28, SDIO1_WPRTN,   SDIO, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(29, SDIO1_DETN,    SDIO, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(30, GPIO2_30,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(31, GPIO2_31,      GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(32, GPIO3_0,       GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(33, GPIO3_1,       GPIO, MAC1, ____, ____, ____, ____, 0),
+	TH1520_PAD(34, GPIO3_2,       GPIO, PWM,  ____, ____, ____, ____, 0),
+	TH1520_PAD(35, GPIO3_3,       GPIO, PWM,  ____, ____, ____, ____, 0),
+	TH1520_PAD(36, HDMI_SCL,      HDMI, PWM,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(37, HDMI_SDA,      HDMI, PWM,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(38, HDMI_CEC,      HDMI, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(39, GMAC0_TX_CLK,  MAC0, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(40, GMAC0_RX_CLK,  MAC0, ____, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(41, GMAC0_TXEN,    MAC0, UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(42, GMAC0_TXD0,    MAC0, UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(43, GMAC0_TXD1,    MAC0, UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(44, GMAC0_TXD2,    MAC0, UART, ____, GPIO, ____, ____, 0),
+	TH1520_PAD(45, GMAC0_TXD3,    MAC0, I2C,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(46, GMAC0_RXDV,    MAC0, I2C,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(47, GMAC0_RXD0,    MAC0, I2C,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(48, GMAC0_RXD1,    MAC0, I2C,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(49, GMAC0_RXD2,    MAC0, SPI,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(50, GMAC0_RXD3,    MAC0, SPI,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(51, GMAC0_MDC,     MAC0, SPI,  MAC1, GPIO, ____, ____, 0),
+	TH1520_PAD(52, GMAC0_MDIO,    MAC0, SPI,  MAC1, GPIO, ____, ____, 0),
+	TH1520_PAD(53, GMAC0_COL,     MAC0, PWM,  ____, GPIO, ____, ____, 0),
+	TH1520_PAD(54, GMAC0_CRS,     MAC0, PWM,  ____, GPIO, ____, ____, 0),
+};
+
+static const struct th1520_pad_group th1520_group1 = {
+	.name = "th1520-group1",
+	.pins = th1520_group1_pins,
+	.npins = ARRAY_SIZE(th1520_group1_pins),
+};
+
+static const struct th1520_pad_group th1520_group2 = {
+	.name = "th1520-group2",
+	.pins = th1520_group2_pins,
+	.npins = ARRAY_SIZE(th1520_group2_pins),
+};
+
+static const struct th1520_pad_group th1520_group3 = {
+	.name = "th1520-group3",
+	.pins = th1520_group3_pins,
+	.npins = ARRAY_SIZE(th1520_group3_pins),
+};
+
+static int th1520_pinctrl_get_groups_count(struct pinctrl_dev *pctldev)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+
+	return thp->desc.npins;
+}
+
+static const char *th1520_pinctrl_get_group_name(struct pinctrl_dev *pctldev,
+						 unsigned int gsel)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+
+	return thp->desc.pins[gsel].name;
+}
+
+static int th1520_pinctrl_get_group_pins(struct pinctrl_dev *pctldev,
+					 unsigned int gsel,
+					 const unsigned int **pins,
+					 unsigned int *npins)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+
+	*pins = &thp->desc.pins[gsel].number;
+	*npins = 1;
+	return 0;
+}
+
+#ifdef CONFIG_DEBUG_FS
+static void th1520_pin_dbg_show(struct pinctrl_dev *pctldev,
+				struct seq_file *s, unsigned int pin)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	void __iomem *padcfg = th1520_padcfg(thp, pin);
+	void __iomem *muxcfg = th1520_muxcfg(thp, pin);
+	u32 pad;
+	u32 mux;
+
+	scoped_guard(raw_spinlock_irqsave, &thp->lock) {
+		pad = readl_relaxed(padcfg);
+		mux = readl_relaxed(muxcfg);
+	}
+
+	seq_printf(s, "[PADCFG_%03u:0x%x=0x%07x MUXCFG_%03u:0x%x=0x%08x]",
+		   1 + pin / 2, 0x000 + 4 * (pin / 2), pad,
+		   1 + pin / 8, 0x400 + 4 * (pin / 8), mux);
+}
+#else
+#define th1520_pin_dbg_show NULL
+#endif
+
+static void th1520_pinctrl_dt_free_map(struct pinctrl_dev *pctldev,
+				       struct pinctrl_map *map, unsigned int nmaps)
+{
+	unsigned long *seen = NULL;
+	unsigned int i;
+
+	for (i = 0; i < nmaps; i++) {
+		if (map[i].type == PIN_MAP_TYPE_CONFIGS_PIN &&
+		    map[i].data.configs.configs != seen) {
+			seen = map[i].data.configs.configs;
+			kfree(seen);
+		}
+	}
+
+	kfree(map);
+}
+
+static int th1520_pinctrl_dt_node_to_map(struct pinctrl_dev *pctldev,
+					 struct device_node *np,
+					 struct pinctrl_map **maps,
+					 unsigned int *num_maps)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	struct device_node *child;
+	struct pinctrl_map *map;
+	unsigned long *configs;
+	unsigned int nconfigs;
+	unsigned int nmaps;
+	int ret;
+
+	nmaps = 0;
+	for_each_available_child_of_node(np, child) {
+		int npins = of_property_count_strings(child, "pins");
+
+		if (npins <= 0) {
+			of_node_put(child);
+			dev_err(thp->pctl->dev, "no pins selected for %pOFn.%pOFn\n",
+				np, child);
+			return -EINVAL;
+		}
+		nmaps += npins;
+		if (of_property_present(child, "function"))
+			nmaps += npins;
+	}
+
+	map = kcalloc(nmaps, sizeof(*map), GFP_KERNEL);
+	if (!map)
+		return -ENOMEM;
+
+	nmaps = 0;
+	mutex_lock(&thp->mutex);
+	for_each_available_child_of_node(np, child) {
+		unsigned int rollback = nmaps;
+		enum th1520_muxtype muxtype;
+		struct property *prop;
+		const char *funcname;
+		const char **pgnames;
+		const char *pinname;
+		int npins;
+
+		ret = pinconf_generic_parse_dt_config(child, pctldev, &configs, &nconfigs);
+		if (ret) {
+			dev_err(thp->pctl->dev, "%pOFn.%pOFn: error parsing pin config\n",
+				np, child);
+			goto put_child;
+		}
+
+		if (!of_property_read_string(child, "function", &funcname)) {
+			muxtype = th1520_muxtype_get(funcname);
+			if (!muxtype) {
+				dev_err(thp->pctl->dev, "%pOFn.%pOFn: unknown function '%s'\n",
+					np, child, funcname);
+				ret = -EINVAL;
+				goto free_configs;
+			}
+
+			funcname = devm_kasprintf(thp->pctl->dev, GFP_KERNEL, "%pOFn.%pOFn",
+						  np, child);
+			if (!funcname) {
+				ret = -ENOMEM;
+				goto free_configs;
+			}
+
+			npins = of_property_count_strings(child, "pins");
+			pgnames = devm_kcalloc(thp->pctl->dev, npins, sizeof(*pgnames), GFP_KERNEL);
+			if (!pgnames) {
+				ret = -ENOMEM;
+				goto free_configs;
+			}
+		} else {
+			funcname = NULL;
+		}
+
+		npins = 0;
+		of_property_for_each_string(child, "pins", prop, pinname) {
+			unsigned int i;
+
+			for (i = 0; i < thp->desc.npins; i++) {
+				if (!strcmp(pinname, thp->desc.pins[i].name))
+					break;
+			}
+			if (i == thp->desc.npins) {
+				nmaps = rollback;
+				dev_err(thp->pctl->dev, "%pOFn.%pOFn: unknown pin '%s'\n",
+					np, child, pinname);
+				goto free_configs;
+			}
+
+			if (nconfigs) {
+				map[nmaps].type = PIN_MAP_TYPE_CONFIGS_PIN;
+				map[nmaps].data.configs.group_or_pin = thp->desc.pins[i].name;
+				map[nmaps].data.configs.configs = configs;
+				map[nmaps].data.configs.num_configs = nconfigs;
+				nmaps += 1;
+			}
+			if (funcname) {
+				pgnames[npins++] = thp->desc.pins[i].name;
+				map[nmaps].type = PIN_MAP_TYPE_MUX_GROUP;
+				map[nmaps].data.mux.function = funcname;
+				map[nmaps].data.mux.group = thp->desc.pins[i].name;
+				nmaps += 1;
+			}
+		}
+
+		if (funcname) {
+			ret = pinmux_generic_add_function(pctldev, funcname, pgnames,
+							  npins, (void *)muxtype);
+			if (ret < 0) {
+				dev_err(thp->pctl->dev, "error adding function %s\n", funcname);
+				goto put_child;
+			}
+		}
+	}
+
+	*maps = map;
+	*num_maps = nmaps;
+	mutex_unlock(&thp->mutex);
+	return 0;
+
+free_configs:
+	kfree(configs);
+put_child:
+	of_node_put(child);
+	th1520_pinctrl_dt_free_map(pctldev, map, nmaps);
+	mutex_unlock(&thp->mutex);
+	return ret;
+}
+
+static const struct pinctrl_ops th1520_pinctrl_ops = {
+	.get_groups_count = th1520_pinctrl_get_groups_count,
+	.get_group_name = th1520_pinctrl_get_group_name,
+	.get_group_pins = th1520_pinctrl_get_group_pins,
+	.pin_dbg_show = th1520_pin_dbg_show,
+	.dt_node_to_map = th1520_pinctrl_dt_node_to_map,
+	.dt_free_map = th1520_pinctrl_dt_free_map,
+};
+
+static int th1520_pinmux_set_mux(struct pinctrl_dev *pctldev,
+				 unsigned int fsel, unsigned int gsel)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	const struct function_desc *func = pinmux_generic_get_function(pctldev, fsel);
+	uintptr_t muxdata = (uintptr_t)thp->desc.pins[gsel].drv_data & TH1520_PAD_MUXDATA;
+	uintptr_t muxtype = (uintptr_t)func->data;
+	unsigned int pin = thp->desc.pins[gsel].number;
+	void __iomem *muxcfg = th1520_muxcfg(thp, pin);
+	unsigned int shift = th1520_muxcfg_shift(pin);
+	u32 mask, value, tmp;
+
+	for (value = 0; muxdata; muxdata >>= 5, value++) {
+		if ((muxdata & GENMASK(4, 0)) == muxtype)
+			break;
+	}
+	if (!muxdata) {
+		dev_err(thp->pctl->dev, "%s: invalid mux %s for pin %s\n",
+			func->name, th1520_muxtype_string[muxtype], thp->desc.pins[gsel].name);
+		return -EINVAL;
+	}
+
+	mask = GENMASK(3, 0) << shift;
+	value = value << shift;
+
+	scoped_guard(raw_spinlock_irqsave, &thp->lock) {
+		tmp = readl_relaxed(muxcfg);
+		tmp = (tmp & ~mask) | value;
+		writel_relaxed(tmp, muxcfg);
+	}
+	return 0;
+}
+
+static const struct pinmux_ops th1520_pinmux_ops = {
+	.get_functions_count = pinmux_generic_get_function_count,
+	.get_function_name = pinmux_generic_get_function_name,
+	.get_function_groups = pinmux_generic_get_function_groups,
+	.set_mux = th1520_pinmux_set_mux,
+	.strict = true,
+};
+
+static const u8 th1520_drive_strength_in_mA[16] = {
+	1, 2, 3, 5, 7, 8, 10, 12, 13, 15, 16, 18, 20, 21, 23, 25,
+};
+
+static u16 th1520_drive_strength_from_mA(u32 arg)
+{
+	u16 ds;
+
+	for (ds = 0; ds < TH1520_PADCFG_DS; ds++) {
+		if (arg <= th1520_drive_strength_in_mA[ds])
+			return ds;
+	}
+	return TH1520_PADCFG_DS;
+}
+
+static int th1520_padcfg_rmw(struct th1520_pinctrl *thp, unsigned int pin,
+			     u32 mask, u32 value)
+{
+	void __iomem *padcfg = th1520_padcfg(thp, pin);
+	unsigned int shift = th1520_padcfg_shift(pin);
+	u32 tmp;
+
+	mask <<= shift;
+	value <<= shift;
+
+	scoped_guard(raw_spinlock_irqsave, &thp->lock) {
+		tmp = readl_relaxed(padcfg);
+		tmp = (tmp & ~mask) | value;
+		writel_relaxed(tmp, padcfg);
+	}
+	return 0;
+}
+
+static int th1520_pinconf_get(struct pinctrl_dev *pctldev,
+			      unsigned int pin, unsigned long *config)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	const struct pin_desc *desc = pin_desc_get(pctldev, pin);
+	bool enabled;
+	int param;
+	u32 value;
+	u32 arg;
+
+	if ((uintptr_t)desc->drv_data & TH1520_PAD_NO_PADCFG)
+		return -ENOTSUPP;
+
+	value = readl_relaxed(th1520_padcfg(thp, pin));
+	value = (value >> th1520_padcfg_shift(pin)) & GENMASK(9, 0);
+
+	param = pinconf_to_config_param(*config);
+	switch (param) {
+	case PIN_CONFIG_BIAS_DISABLE:
+		enabled = !(value & (TH1520_PADCFG_SPU | TH1520_PADCFG_PE));
+		arg = 0;
+		break;
+	case PIN_CONFIG_BIAS_PULL_DOWN:
+		enabled = (value & TH1520_PADCFG_BIAS) == TH1520_PADCFG_PE;
+		arg = enabled ? TH1520_PULL_DOWN_OHM : 0;
+		break;
+	case PIN_CONFIG_BIAS_PULL_UP:
+		if (value & TH1520_PADCFG_SPU) {
+			enabled = true;
+			arg = TH1520_PULL_STRONG_OHM;
+		} else if ((value & (TH1520_PADCFG_PE | TH1520_PADCFG_PS)) ==
+				    (TH1520_PADCFG_PE | TH1520_PADCFG_PS)) {
+			enabled = true;
+			arg = TH1520_PULL_UP_OHM;
+		} else {
+			enabled = false;
+			arg = 0;
+		}
+		break;
+	case PIN_CONFIG_DRIVE_STRENGTH:
+		enabled = true;
+		arg = th1520_drive_strength_in_mA[value & TH1520_PADCFG_DS];
+		break;
+	case PIN_CONFIG_INPUT_ENABLE:
+		enabled = value & TH1520_PADCFG_IE;
+		arg = enabled ? 1 : 0;
+		break;
+	case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+		enabled = value & TH1520_PADCFG_ST;
+		arg = enabled ? 1 : 0;
+		break;
+	case PIN_CONFIG_SLEW_RATE:
+		enabled = value & TH1520_PADCFG_SL;
+		arg = enabled ? 1 : 0;
+		break;
+	default:
+		return -ENOTSUPP;
+	}
+
+	*config = pinconf_to_config_packed(param, arg);
+	return enabled ? 0 : -EINVAL;
+}
+
+static int th1520_pinconf_group_get(struct pinctrl_dev *pctldev,
+				    unsigned int gsel, unsigned long *config)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	unsigned int pin = thp->desc.pins[gsel].number;
+
+	return th1520_pinconf_get(pctldev, pin, config);
+}
+
+static int th1520_pinconf_set(struct pinctrl_dev *pctldev, unsigned int pin,
+			      unsigned long *configs, unsigned int num_configs)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	const struct pin_desc *desc = pin_desc_get(pctldev, pin);
+	unsigned int i;
+	u16 mask, value;
+
+	if ((uintptr_t)desc->drv_data & TH1520_PAD_NO_PADCFG)
+		return -ENOTSUPP;
+
+	mask = 0;
+	value = 0;
+	for (i = 0; i < num_configs; i++) {
+		int param = pinconf_to_config_param(configs[i]);
+		u32 arg = pinconf_to_config_argument(configs[i]);
+
+		switch (param) {
+		case PIN_CONFIG_BIAS_DISABLE:
+			mask |= TH1520_PADCFG_BIAS;
+			value &= ~TH1520_PADCFG_BIAS;
+			break;
+		case PIN_CONFIG_BIAS_PULL_DOWN:
+			if (arg == 0)
+				return -ENOTSUPP;
+			mask |= TH1520_PADCFG_BIAS;
+			value &= ~TH1520_PADCFG_BIAS;
+			value |= TH1520_PADCFG_PE;
+			break;
+		case PIN_CONFIG_BIAS_PULL_UP:
+			if (arg == 0)
+				return -ENOTSUPP;
+			mask |= TH1520_PADCFG_BIAS;
+			value &= ~TH1520_PADCFG_BIAS;
+			if (arg == TH1520_PULL_STRONG_OHM)
+				value |= TH1520_PADCFG_SPU;
+			else
+				value |= TH1520_PADCFG_PE | TH1520_PADCFG_PS;
+			break;
+		case PIN_CONFIG_DRIVE_STRENGTH:
+			mask |= TH1520_PADCFG_DS;
+			value &= ~TH1520_PADCFG_DS;
+			value |= th1520_drive_strength_from_mA(arg);
+			break;
+		case PIN_CONFIG_INPUT_ENABLE:
+			mask |= TH1520_PADCFG_IE;
+			if (arg)
+				value |= TH1520_PADCFG_IE;
+			else
+				value &= ~TH1520_PADCFG_IE;
+			break;
+		case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+			mask |= TH1520_PADCFG_ST;
+			if (arg)
+				value |= TH1520_PADCFG_ST;
+			else
+				value &= ~TH1520_PADCFG_ST;
+			break;
+		case PIN_CONFIG_SLEW_RATE:
+			mask |= TH1520_PADCFG_SL;
+			if (arg)
+				value |= TH1520_PADCFG_SL;
+			else
+				value &= ~TH1520_PADCFG_SL;
+			break;
+		default:
+			return -ENOTSUPP;
+		}
+	}
+
+	return th1520_padcfg_rmw(thp, pin, mask, value);
+}
+
+static int th1520_pinconf_group_set(struct pinctrl_dev *pctldev,
+				    unsigned int gsel,
+				    unsigned long *configs,
+				    unsigned int num_configs)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	unsigned int pin = thp->desc.pins[gsel].number;
+
+	return th1520_pinconf_set(pctldev, pin, configs, num_configs);
+}
+
+#ifdef CONFIG_DEBUG_FS
+static void th1520_pinconf_dbg_show(struct pinctrl_dev *pctldev,
+				    struct seq_file *s, unsigned int pin)
+{
+	struct th1520_pinctrl *thp = pinctrl_dev_get_drvdata(pctldev);
+	u32 value = readl_relaxed(th1520_padcfg(thp, pin));
+
+	value = (value >> th1520_padcfg_shift(pin)) & GENMASK(9, 0);
+
+	seq_printf(s, " [0x%03x]", value);
+}
+#else
+#define th1520_pinconf_dbg_show NULL
+#endif
+
+static const struct pinconf_ops th1520_pinconf_ops = {
+	.pin_config_get = th1520_pinconf_get,
+	.pin_config_group_get = th1520_pinconf_group_get,
+	.pin_config_set = th1520_pinconf_set,
+	.pin_config_group_set = th1520_pinconf_group_set,
+	.pin_config_dbg_show = th1520_pinconf_dbg_show,
+	.is_generic = true,
+};
+
+static int th1520_pinctrl_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	const struct th1520_pad_group *group = device_get_match_data(dev);
+	struct th1520_pinctrl *thp;
+	struct clk *clk;
+	int ret;
+
+	thp = devm_kzalloc(dev, sizeof(*thp), GFP_KERNEL);
+	if (!thp)
+		return -ENOMEM;
+
+	thp->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(thp->base))
+		return PTR_ERR(thp->base);
+
+	clk = devm_clk_get_enabled(dev, NULL);
+	if (IS_ERR(clk))
+		return dev_err_probe(dev, PTR_ERR(clk), "error getting clock\n");
+
+	thp->desc.name = group->name;
+	thp->desc.pins = group->pins;
+	thp->desc.npins = group->npins;
+	thp->desc.pctlops = &th1520_pinctrl_ops;
+	thp->desc.pmxops = &th1520_pinmux_ops;
+	thp->desc.confops = &th1520_pinconf_ops;
+	thp->desc.owner = THIS_MODULE;
+	mutex_init(&thp->mutex);
+	raw_spin_lock_init(&thp->lock);
+
+	ret = devm_pinctrl_register_and_init(dev, &thp->desc, thp, &thp->pctl);
+	if (ret)
+		return dev_err_probe(dev, ret, "could not register pinctrl driver\n");
+
+	return pinctrl_enable(thp->pctl);
+}
+
+static const struct of_device_id th1520_pinctrl_of_match[] = {
+	{ .compatible = "thead,th1520-group1-pinctrl", .data = &th1520_group1 },
+	{ .compatible = "thead,th1520-group2-pinctrl", .data = &th1520_group2 },
+	{ .compatible = "thead,th1520-group3-pinctrl", .data = &th1520_group3 },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, th1520_pinctrl_of_match);
+
+static struct platform_driver th1520_pinctrl_driver = {
+	.probe = th1520_pinctrl_probe,
+	.driver = {
+		.name = "pinctrl-th1520",
+		.of_match_table = th1520_pinctrl_of_match,
+	},
+};
+module_platform_driver(th1520_pinctrl_driver);
+
+MODULE_DESCRIPTION("Pinctrl driver for the T-Head TH1520 SoC");
+MODULE_AUTHOR("Emil Renner Berthing <emil.renner.berthing@canonical.com>");
+MODULE_LICENSE("GPL");
diff --git a/drivers/pinctrl/sophgo/Makefile b/drivers/pinctrl/sophgo/Makefile
new file mode 100644
index 000000000000..2f2cd0d5a99d
--- /dev/null
+++ b/drivers/pinctrl/sophgo/Makefile
@@ -0,0 +1,2 @@
+obj-$(CONFIG_ARCH_SOPHGO)	+= pinctrl-sophgo.o
+obj-$(CONFIG_ARCH_SOPHGO)	+= pinctrl-mango.o
diff --git a/drivers/pinctrl/sophgo/pinctrl-mango.c b/drivers/pinctrl/sophgo/pinctrl-mango.c
new file mode 100644
index 000000000000..8e7bd08a73db
--- /dev/null
+++ b/drivers/pinctrl/sophgo/pinctrl-mango.c
@@ -0,0 +1,453 @@
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/pinctrl/pinmux.h>
+#include <linux/pinctrl/pinconf.h>
+#include <linux/pinctrl/pinconf-generic.h>
+#include <linux/device.h>
+#include <linux/of.h>
+
+#include "../pinctrl-utils.h"
+#include "pinctrl-sophgo.h"
+
+#define DRV_PINCTRL_NAME "mango_pinctrl"
+#define DRV_PINMUX_NAME "mango_pinmux"
+
+#define FUNCTION(fname, gname, fmode) \
+	{ \
+		.name = #fname, \
+		.groups = gname##_group, \
+		.num_groups = ARRAY_SIZE(gname##_group), \
+		.mode = fmode, \
+	}
+
+#define PIN_GROUP(gname) \
+	{ \
+		.name = #gname "_grp", \
+		.pins = gname##_pins, \
+		.num_pins = ARRAY_SIZE(gname##_pins), \
+	}
+
+static const struct pinctrl_pin_desc mango_pins[] = {
+	PINCTRL_PIN(0,   "MIO0"),
+	PINCTRL_PIN(1,   "MIO1"),
+	PINCTRL_PIN(2,   "MIO2"),
+	PINCTRL_PIN(3,   "MIO3"),
+	PINCTRL_PIN(4,   "MIO4"),
+	PINCTRL_PIN(5,   "MIO5"),
+	PINCTRL_PIN(6,   "MIO6"),
+	PINCTRL_PIN(7,   "MIO7"),
+	PINCTRL_PIN(8,   "MIO8"),
+	PINCTRL_PIN(9,   "MIO9"),
+	PINCTRL_PIN(10,   "MIO10"),
+	PINCTRL_PIN(11,   "MIO11"),
+	PINCTRL_PIN(12,   "MIO12"),
+	PINCTRL_PIN(13,   "MIO13"),
+	PINCTRL_PIN(14,   "MIO14"),
+	PINCTRL_PIN(15,   "MIO15"),
+	PINCTRL_PIN(16,   "MIO16"),
+	PINCTRL_PIN(17,   "MIO17"),
+	PINCTRL_PIN(18,   "MIO18"),
+	PINCTRL_PIN(19,   "MIO19"),
+	PINCTRL_PIN(20,   "MIO20"),
+	PINCTRL_PIN(21,   "MIO21"),
+	PINCTRL_PIN(22,   "MIO22"),
+	PINCTRL_PIN(23,   "MIO23"),
+	PINCTRL_PIN(24,   "MIO24"),
+	PINCTRL_PIN(25,   "MIO25"),
+	PINCTRL_PIN(26,   "MIO26"),
+	PINCTRL_PIN(27,   "MIO27"),
+	PINCTRL_PIN(28,   "MIO28"),
+	PINCTRL_PIN(29,   "MIO29"),
+	PINCTRL_PIN(30,   "MIO30"),
+	PINCTRL_PIN(31,   "MIO31"),
+	PINCTRL_PIN(32,   "MIO32"),
+	PINCTRL_PIN(33,   "MIO33"),
+	PINCTRL_PIN(34,   "MIO34"),
+	PINCTRL_PIN(35,   "MIO35"),
+	PINCTRL_PIN(36,   "MIO36"),
+	PINCTRL_PIN(37,   "MIO37"),
+	PINCTRL_PIN(38,   "MIO38"),
+	PINCTRL_PIN(39,   "MIO39"),
+	PINCTRL_PIN(40,   "MIO40"),
+	PINCTRL_PIN(41,   "MIO41"),
+	PINCTRL_PIN(42,   "MIO42"),
+	PINCTRL_PIN(43,   "MIO43"),
+	PINCTRL_PIN(44,   "MIO44"),
+	PINCTRL_PIN(45,   "MIO45"),
+	PINCTRL_PIN(46,   "MIO46"),
+	PINCTRL_PIN(47,   "MIO47"),
+	PINCTRL_PIN(48,   "MIO48"),
+	PINCTRL_PIN(49,   "MIO49"),
+	PINCTRL_PIN(50,   "MIO50"),
+	PINCTRL_PIN(51,   "MIO51"),
+	PINCTRL_PIN(52,   "MIO52"),
+	PINCTRL_PIN(53,   "MIO53"),
+	PINCTRL_PIN(54,   "MIO54"),
+	PINCTRL_PIN(55,   "MIO55"),
+	PINCTRL_PIN(56,   "MIO56"),
+	PINCTRL_PIN(57,   "MIO57"),
+	PINCTRL_PIN(58,   "MIO58"),
+	PINCTRL_PIN(59,   "MIO59"),
+	PINCTRL_PIN(60,   "MIO60"),
+	PINCTRL_PIN(61,   "MIO61"),
+	PINCTRL_PIN(62,   "MIO62"),
+	PINCTRL_PIN(63,   "MIO63"),
+	PINCTRL_PIN(64,   "MIO64"),
+	PINCTRL_PIN(65,   "MIO65"),
+	PINCTRL_PIN(66,   "MIO66"),
+	PINCTRL_PIN(67,   "MIO67"),
+	PINCTRL_PIN(68,   "MIO68"),
+	PINCTRL_PIN(69,   "MIO69"),
+	PINCTRL_PIN(70,   "MIO70"),
+	PINCTRL_PIN(71,   "MIO71"),
+	PINCTRL_PIN(72,   "MIO72"),
+	PINCTRL_PIN(73,   "MIO73"),
+	PINCTRL_PIN(74,   "MIO74"),
+	PINCTRL_PIN(75,   "MIO75"),
+	PINCTRL_PIN(76,   "MIO76"),
+	PINCTRL_PIN(77,   "MIO77"),
+	PINCTRL_PIN(78,   "MIO78"),
+	PINCTRL_PIN(79,   "MIO79"),
+	PINCTRL_PIN(80,   "MIO80"),
+	PINCTRL_PIN(81,   "MIO81"),
+	PINCTRL_PIN(82,   "MIO82"),
+	PINCTRL_PIN(83,   "MIO83"),
+	PINCTRL_PIN(84,   "MIO84"),
+	PINCTRL_PIN(85,   "MIO85"),
+	PINCTRL_PIN(86,   "MIO86"),
+	PINCTRL_PIN(87,   "MIO87"),
+	PINCTRL_PIN(88,   "MIO88"),
+	PINCTRL_PIN(89,   "MIO89"),
+	PINCTRL_PIN(90,   "MIO90"),
+	PINCTRL_PIN(91,   "MIO91"),
+	PINCTRL_PIN(92,   "MIO92"),
+	PINCTRL_PIN(93,   "MIO93"),
+	PINCTRL_PIN(94,   "MIO94"),
+	PINCTRL_PIN(95,   "MIO95"),
+	PINCTRL_PIN(96,   "MIO96"),
+	PINCTRL_PIN(97,   "MIO97"),
+	PINCTRL_PIN(98,   "MIO98"),
+	PINCTRL_PIN(99,   "MIO99"),
+	PINCTRL_PIN(100,  "MIO100"),
+	PINCTRL_PIN(101,  "MIO101"),
+	PINCTRL_PIN(102,  "MIO102"),
+	PINCTRL_PIN(103,  "MIO103"),
+	PINCTRL_PIN(104,  "MIO104"),
+	PINCTRL_PIN(105,  "MIO105"),
+	PINCTRL_PIN(106,  "MIO106"),
+	PINCTRL_PIN(107,  "MIO107"),
+	PINCTRL_PIN(108,  "MIO108"),
+	PINCTRL_PIN(109,  "MIO109"),
+	PINCTRL_PIN(110,  "MIO110"),
+	PINCTRL_PIN(111,  "MIO111"),
+	PINCTRL_PIN(112,  "MIO112"),
+	PINCTRL_PIN(113,  "MIO113"),
+	PINCTRL_PIN(114,  "MIO114"),
+	PINCTRL_PIN(115,  "MIO115"),
+	PINCTRL_PIN(116,  "MIO116"),
+	PINCTRL_PIN(117,  "MIO117"),
+	PINCTRL_PIN(118,  "MIO118"),
+	PINCTRL_PIN(119,  "MIO119"),
+	PINCTRL_PIN(120,  "MIO120"),
+	PINCTRL_PIN(121,  "MIO121"),
+	PINCTRL_PIN(122,  "MIO122"),
+	PINCTRL_PIN(123,  "MIO123"),
+	PINCTRL_PIN(124,  "MIO124"),
+	PINCTRL_PIN(125,  "MIO125"),
+	PINCTRL_PIN(126,  "MIO126"),
+	PINCTRL_PIN(127,  "MIO127"),
+	PINCTRL_PIN(128,  "MIO128"),
+	PINCTRL_PIN(129,  "MIO129"),
+	PINCTRL_PIN(130,  "MIO130"),
+	PINCTRL_PIN(131,  "MIO131"),
+	PINCTRL_PIN(132,  "MIO132"),
+	PINCTRL_PIN(133,  "MIO133"),
+	PINCTRL_PIN(134,  "MIO134"),
+	PINCTRL_PIN(135,  "MIO135"),
+	PINCTRL_PIN(136,  "MIO136"),
+	PINCTRL_PIN(137,  "MIO137"),
+	PINCTRL_PIN(138,  "MIO138"),
+	PINCTRL_PIN(139,  "MIO139"),
+	PINCTRL_PIN(140,  "MIO140"),
+	PINCTRL_PIN(141,  "MIO141"),
+	PINCTRL_PIN(142,  "MIO142"),
+	PINCTRL_PIN(143,  "MIO143"),
+	PINCTRL_PIN(144,  "MIO144"),
+	PINCTRL_PIN(145,  "MIO145"),
+	PINCTRL_PIN(146,  "MIO146"),
+	PINCTRL_PIN(147,  "MIO147"),
+	PINCTRL_PIN(148,  "MIO148"),
+	PINCTRL_PIN(149,  "MIO149"),
+	PINCTRL_PIN(150,  "MIO150"),
+	PINCTRL_PIN(151,  "MIO151"),
+	PINCTRL_PIN(152,  "MIO152"),
+	PINCTRL_PIN(153,  "MIO153"),
+	PINCTRL_PIN(154,  "MIO154"),
+	PINCTRL_PIN(155,  "MIO155"),
+	PINCTRL_PIN(156,  "MIO156"),
+};
+
+static const unsigned int lpc_pins[] = {0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12};
+static const unsigned int pcie_pins[] = {13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24};
+static const unsigned int spif_pins[] = {25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40};
+static const unsigned int emmc_pins[] = {41, 42, 43, 44};
+static const unsigned int sdio_pins[] = {45, 46, 47, 48};
+static const unsigned int eth0_pins[] = {49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64};
+static const unsigned int pwm0_pins[] = {65};
+static const unsigned int pwm1_pins[] = {66};
+static const unsigned int pwm2_pins[] = {67};
+static const unsigned int pwm3_pins[] = {68};
+static const unsigned int fan0_pins[] = {69};
+static const unsigned int fan1_pins[] = {70};
+static const unsigned int fan2_pins[] = {71};
+static const unsigned int fan3_pins[] = {72};
+static const unsigned int i2c0_pins[] = {73, 74};
+static const unsigned int i2c1_pins[] = {75, 76};
+static const unsigned int i2c2_pins[] = {77, 78};
+static const unsigned int i2c3_pins[] = {79, 80};
+static const unsigned int uart0_pins[] = {81, 82, 83, 84};
+static const unsigned int uart1_pins[] = {85, 86, 87, 88};
+static const unsigned int uart2_pins[] = {89, 90, 91, 92};
+static const unsigned int uart3_pins[] = {93, 94, 95, 96};
+static const unsigned int spi0_pins[] = {97, 98, 99, 100, 101};
+static const unsigned int spi1_pins[] = {102, 103, 104, 105, 106};
+static const unsigned int jtag0_pins[] = {107, 108, 109, 110, 111, 112};
+static const unsigned int jtag1_pins[] = {113, 114, 115, 116, 117, 118};
+static const unsigned int jtag2_pins[] = {119, 120, 121, 122, 123, 124};
+static const unsigned int gpio0_pins[] = {125, 126, 127, 128, 129, 130, 131, 132, 133, 134, 135, 136, 137,\
+					 138, 139, 140, 141, 142, 143, 144, 145, 146, 147, 148, 149, 150,\
+					 151, 152, 153};
+static const unsigned int dbgi2c_pins[] = {154, 155, 156};
+
+static const char * const lpc_group[] = {"lpc_grp"};
+static const char * const pcie_group[] = {"pcie_grp"};
+static const char * const spif_group[] = {"spif_grp"};
+static const char * const emmc_group[] = {"emmc_grp"};
+static const char * const sdio_group[] = {"sdio_grp"};
+static const char * const eth0_group[] = {"eth0_grp"};
+static const char * const pwm0_group[] = {"pwm0_grp"};
+static const char * const pwm1_group[] = {"pwm1_grp"};
+static const char * const pwm2_group[] = {"pwm2_grp"};
+static const char * const pwm3_group[] = {"pwm3_grp"};
+static const char * const fan0_group[] = {"fan0_grp"};
+static const char * const fan1_group[] = {"fan1_grp"};
+static const char * const fan2_group[] = {"fan2_grp"};
+static const char * const fan3_group[] = {"fan3_grp"};
+static const char * const i2c0_group[] = {"i2c0_grp"};
+static const char * const i2c1_group[] = {"i2c1_grp"};
+static const char * const i2c2_group[] = {"i2c2_grp"};
+static const char * const i2c3_group[] = {"i2c3_grp"};
+static const char * const uart0_group[] = {"uart0_grp"};
+static const char * const uart1_group[] = {"uart1_grp"};
+static const char * const uart2_group[] = {"uart2_grp"};
+static const char * const uart3_group[] = {"uart3_grp"};
+static const char * const spi0_group[] = {"spi0_grp"};
+static const char * const spi1_group[] = {"spi1_grp"};
+static const char * const jtag0_group[] = {"jtag0_grp"};
+static const char * const jtag1_group[] = {"jtag1_grp"};
+static const char * const jtag2_group[] = {"jtag2_grp"};
+static const char * const gpio0_group[] = {"gpio0_grp"};
+static const char * const dbgi2c_group[] = {"dbgi2c_grp"};
+
+static struct mango_group mango_groups[] = {
+	PIN_GROUP(lpc),
+	PIN_GROUP(pcie),
+	PIN_GROUP(spif),
+	PIN_GROUP(emmc),
+	PIN_GROUP(sdio),
+	PIN_GROUP(eth0),
+	PIN_GROUP(pwm0),
+	PIN_GROUP(pwm1),
+	PIN_GROUP(pwm2),
+	PIN_GROUP(pwm3),
+	PIN_GROUP(fan0),
+	PIN_GROUP(fan1),
+	PIN_GROUP(fan2),
+	PIN_GROUP(fan3),
+	PIN_GROUP(i2c0),
+	PIN_GROUP(i2c1),
+	PIN_GROUP(i2c2),
+	PIN_GROUP(i2c3),
+	PIN_GROUP(uart0),
+	PIN_GROUP(uart1),
+	PIN_GROUP(uart2),
+	PIN_GROUP(uart3),
+	PIN_GROUP(spi0),
+	PIN_GROUP(spi1),
+	PIN_GROUP(jtag0),
+	PIN_GROUP(jtag1),
+	PIN_GROUP(jtag2),
+	PIN_GROUP(gpio0),
+	PIN_GROUP(dbgi2c),
+};
+
+static const struct mango_pmx_func mango_funcs[] = {
+	FUNCTION(lpc_a, lpc, FUNC_MODE0),
+	FUNCTION(lpc_r, lpc, FUNC_MODE1),
+	FUNCTION(pcie_a, pcie, FUNC_MODE0),
+	FUNCTION(pcie_r, pcie, FUNC_MODE1),
+	FUNCTION(spif_a, spif, FUNC_MODE0),
+	FUNCTION(spif_r, spif, FUNC_MODE1),
+	FUNCTION(emmc_a, emmc, FUNC_MODE0),
+	FUNCTION(emmc_r, emmc, FUNC_MODE1),
+	FUNCTION(sdio_a, sdio, FUNC_MODE0),
+	FUNCTION(sdio_r, sdio, FUNC_MODE1),
+	FUNCTION(eth0_a, eth0, FUNC_MODE1),
+	FUNCTION(eth0_r, eth0, FUNC_MODE0),
+	FUNCTION(pwm0_a, pwm0, FUNC_MODE0),
+	FUNCTION(pwm0_r, pwm0, FUNC_MODE1),
+	FUNCTION(pwm1_a, pwm1, FUNC_MODE0),
+	FUNCTION(pwm1_r, pwm1, FUNC_MODE1),
+	FUNCTION(pwm2_a, pwm2, FUNC_MODE0),
+	FUNCTION(pwm2_r, pwm2, FUNC_MODE1),
+	FUNCTION(pwm3_a, pwm3, FUNC_MODE0),
+	FUNCTION(pwm3_r, pwm3, FUNC_MODE1),
+	FUNCTION(fan0_a, fan0, FUNC_MODE1),
+	FUNCTION(fan0_r, fan0, FUNC_MODE0),
+	FUNCTION(fan1_a, fan1, FUNC_MODE1),
+	FUNCTION(fan1_r, fan1, FUNC_MODE0),
+	FUNCTION(fan2_a, fan2, FUNC_MODE1),
+	FUNCTION(fan2_r, fan2, FUNC_MODE0),
+	FUNCTION(fan3_a, fan3, FUNC_MODE1),
+	FUNCTION(fan3_r, fan3, FUNC_MODE0),
+	FUNCTION(i2c0_a, i2c0, FUNC_MODE0),
+	FUNCTION(i2c0_r, i2c0, FUNC_MODE1),
+	FUNCTION(i2c1_a, i2c1, FUNC_MODE0),
+	FUNCTION(i2c1_r, i2c1, FUNC_MODE1),
+	FUNCTION(i2c2_a, i2c2, FUNC_MODE1),
+	FUNCTION(i2c2_r, i2c2, FUNC_MODE0),
+	FUNCTION(i2c3_a, i2c3, FUNC_MODE1),
+	FUNCTION(i2c3_r, i2c3, FUNC_MODE0),
+	FUNCTION(uart0_a, uart0, FUNC_MODE0),
+	FUNCTION(uart0_r, uart0, FUNC_MODE1),
+	FUNCTION(uart1_a, uart1, FUNC_MODE0),
+	FUNCTION(uart1_r, uart1, FUNC_MODE1),
+	FUNCTION(uart2_a, uart2, FUNC_MODE1),
+	FUNCTION(uart2_r, uart2, FUNC_MODE0),
+	FUNCTION(uart3_a, uart3, FUNC_MODE1),
+	FUNCTION(uart3_r, uart3, FUNC_MODE0),
+	FUNCTION(spi0_a, spi0, FUNC_MODE1),
+	FUNCTION(spi0_r, spi0, FUNC_MODE0),
+	FUNCTION(spi1_a, spi1, FUNC_MODE0),
+	FUNCTION(spi1_r, spi1, FUNC_MODE1),
+	FUNCTION(jtag0_a, jtag0, FUNC_MODE0),
+	FUNCTION(jtag0_r, jtag0, FUNC_MODE1),
+	FUNCTION(jtag1_a, jtag1, FUNC_MODE1),
+	FUNCTION(jtag1_r, jtag1, FUNC_MODE0),
+	FUNCTION(jtag2_a, jtag2, FUNC_MODE1),
+	FUNCTION(jtag2_r, jtag2, FUNC_MODE0),
+	FUNCTION(gpio0_a, gpio0, FUNC_MODE1),
+	FUNCTION(gpio0_r, gpio0, FUNC_MODE0),
+	FUNCTION(dbgi2c_a, dbgi2c, FUNC_MODE0),
+	FUNCTION(dbgi2c_r, dbgi2c, FUNC_MODE1),
+};
+
+static struct device_attribute lpc_attr =	__ATTR(lpc, 0664, pinmux_show, pinmux_store);
+static struct device_attribute pcie_attr =	__ATTR(pcie, 0664, pinmux_show, pinmux_store);
+static struct device_attribute spif_attr =	__ATTR(spif, 0664, pinmux_show, pinmux_store);
+static struct device_attribute emmc_attr =	__ATTR(emmc, 0664, pinmux_show, pinmux_store);
+static struct device_attribute sdio_attr =	__ATTR(sdio, 0664, pinmux_show, pinmux_store);
+static struct device_attribute eth0_attr =	__ATTR(eth0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute pwm0_attr =	__ATTR(pwm0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute pwm1_attr =	__ATTR(pwm1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute pwm2_attr =	__ATTR(pwm2, 0664, pinmux_show, pinmux_store);
+static struct device_attribute pwm3_attr =	__ATTR(pwm3, 0664, pinmux_show, pinmux_store);
+static struct device_attribute fan0_attr =	__ATTR(fan0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute fan1_attr =	__ATTR(fan1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute fan2_attr =	__ATTR(fan2, 0664, pinmux_show, pinmux_store);
+static struct device_attribute fan3_attr =	__ATTR(fan3, 0664, pinmux_show, pinmux_store);
+static struct device_attribute i2c0_attr =	__ATTR(i2c0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute i2c1_attr =	__ATTR(i2c1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute i2c2_attr =	__ATTR(i2c2, 0664, pinmux_show, pinmux_store);
+static struct device_attribute i2c3_attr =	__ATTR(i2c3, 0664, pinmux_show, pinmux_store);
+static struct device_attribute uart0_attr =	__ATTR(uart0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute uart1_attr =	__ATTR(uart1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute uart2_attr =	__ATTR(uart2, 0664, pinmux_show, pinmux_store);
+static struct device_attribute uart3_attr =	__ATTR(uart3, 0664, pinmux_show, pinmux_store);
+static struct device_attribute spi0_attr =	__ATTR(spi0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute spi1_attr =	__ATTR(spi1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute jtag0_attr =	__ATTR(jtag0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute jtag1_attr =	__ATTR(jtag1, 0664, pinmux_show, pinmux_store);
+static struct device_attribute jtag2_attr =	__ATTR(jtag2, 0664, pinmux_show, pinmux_store);
+static struct device_attribute gpio0_attr =	__ATTR(gpio0, 0664, pinmux_show, pinmux_store);
+static struct device_attribute dbgi2c_attr =	__ATTR(dbgi2c, 0664, pinmux_show, pinmux_store);
+
+
+static struct attribute *pinmux_attrs[] = {
+	&lpc_attr.attr,
+	&pcie_attr.attr,
+	&spif_attr.attr,
+	&emmc_attr.attr,
+	&sdio_attr.attr,
+	&eth0_attr.attr,
+	&pwm0_attr.attr,
+	&pwm1_attr.attr,
+	&pwm2_attr.attr,
+	&pwm3_attr.attr,
+	&fan0_attr.attr,
+	&fan1_attr.attr,
+	&fan2_attr.attr,
+	&fan3_attr.attr,
+	&i2c0_attr.attr,
+	&i2c1_attr.attr,
+	&i2c2_attr.attr,
+	&i2c3_attr.attr,
+	&uart0_attr.attr,
+	&uart1_attr.attr,
+	&uart2_attr.attr,
+	&uart3_attr.attr,
+	&spi0_attr.attr,
+	&spi1_attr.attr,
+	&jtag0_attr.attr,
+	&jtag1_attr.attr,
+	&jtag2_attr.attr,
+	&gpio0_attr.attr,
+	&dbgi2c_attr.attr,
+	NULL,
+};
+ATTRIBUTE_GROUPS(pinmux);
+
+static struct class  pinmux_class = {
+	.name = "pinmux",
+	.dev_groups = pinmux_groups,
+};
+
+static struct mango_soc_pinctrl_data mango_pinctrl_data = {
+	.pins = mango_pins,
+	.npins = ARRAY_SIZE(mango_pins),
+	.groups = mango_groups,
+	.groups_count = ARRAY_SIZE(mango_groups),
+	.functions = mango_funcs,
+	.functions_count = ARRAY_SIZE(mango_funcs),
+	.p_class = &pinmux_class,
+};
+
+static const struct of_device_id mango_pinctrl_of_table[] = {
+	{
+		.compatible = "sophgo, pinctrl-mango",
+		.data = &mango_pinctrl_data,
+	},
+	{}
+};
+
+static int mango_pinctrl_probe(struct platform_device *pdev)
+{
+	return sophgo_pinctrl_probe(pdev);
+}
+
+static struct platform_driver mango_pinctrl_driver = {
+	.probe = mango_pinctrl_probe,
+	.driver = {
+		.name = DRV_PINCTRL_NAME,
+		.of_match_table = of_match_ptr(mango_pinctrl_of_table),
+	},
+};
+
+static int __init mango_pinctrl_init(void)
+{
+	return platform_driver_register(&mango_pinctrl_driver);
+}
+postcore_initcall(mango_pinctrl_init);
diff --git a/drivers/pinctrl/sophgo/pinctrl-sophgo.c b/drivers/pinctrl/sophgo/pinctrl-sophgo.c
new file mode 100644
index 000000000000..0862177d4144
--- /dev/null
+++ b/drivers/pinctrl/sophgo/pinctrl-sophgo.c
@@ -0,0 +1,292 @@
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/of_device.h>
+#include <linux/mfd/syscon.h>
+#include <linux/regmap.h>
+
+#include "pinctrl-sophgo.h"
+
+
+static int mango_get_groups(struct pinctrl_dev *pctldev, unsigned int selector,
+		const char * const **groups,
+		unsigned int * const num_groups);
+
+static struct mango_soc_pinctrl_data *get_pinmux_data(struct pinctrl_dev *pctldev)
+{
+	struct mango_pinctrl *mangopctrl = pinctrl_dev_get_drvdata(pctldev);
+
+	return mangopctrl->data;
+}
+
+static int mango_get_functions_count(struct pinctrl_dev *pctldev)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	return data->functions_count;
+}
+
+static const char *mango_get_fname(struct pinctrl_dev *pctldev,
+		unsigned int selector)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	return data->functions[selector].name;
+}
+
+static int mango_set_mux(struct pinctrl_dev *pctldev, unsigned int selector,
+		unsigned int group)
+{
+	int p;
+	unsigned int pidx;
+	u32 offset, regval, mux_offset;
+	struct mango_pinctrl *ctrl = pinctrl_dev_get_drvdata(pctldev);
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	data->groups[group].cur_func_idx = data->functions[selector].mode;
+	for (p = 0; p < data->groups[group].num_pins; p++) {
+		pidx = data->groups[group].pins[p];
+		offset = (pidx >> 1) << 2;
+		regmap_read(ctrl->syscon_pinctl,
+			ctrl->top_pinctl_offset + offset, &regval);
+		mux_offset = ((!((pidx + 1) & 1) << 4) + 4);
+
+		regval = regval & ~(3 << mux_offset);
+		regval |= data->functions[selector].mode << mux_offset;
+		regmap_write(ctrl->syscon_pinctl,
+			ctrl->top_pinctl_offset + offset, regval);
+		regmap_read(ctrl->syscon_pinctl,
+			ctrl->top_pinctl_offset + offset, &regval);
+		dev_dbg(ctrl->dev, "%s : check new reg=0x%x val=0x%x\n",
+			data->groups[group].name,
+			ctrl->top_pinctl_offset + offset, regval);
+	}
+
+	return 0;
+}
+
+static const struct pinmux_ops mango_pinmux_ops = {
+	.get_functions_count = mango_get_functions_count,
+	.get_function_name = mango_get_fname,
+	.get_function_groups = mango_get_groups,
+	.set_mux = mango_set_mux,
+	.strict = true,
+};
+
+static int mango_pinconf_cfg_get(struct pinctrl_dev *pctldev, unsigned int pin,
+		unsigned long *config)
+{
+	return 0;
+}
+
+static int mango_pinconf_cfg_set(struct pinctrl_dev *pctldev, unsigned int pin,
+		unsigned long *configs, unsigned int num_configs)
+{
+	return 0;
+}
+
+static int mango_pinconf_group_set(struct pinctrl_dev *pctldev,
+		unsigned int selector, unsigned long *configs, unsigned int num_configs)
+{
+	return 0;
+}
+
+static const struct pinconf_ops mango_pinconf_ops = {
+	.is_generic = true,
+	.pin_config_get = mango_pinconf_cfg_get,
+	.pin_config_set = mango_pinconf_cfg_set,
+	.pin_config_group_set = mango_pinconf_group_set,
+};
+
+static int mango_get_groups(struct pinctrl_dev *pctldev, unsigned int selector,
+		const char * const **groups,
+		unsigned int * const num_groups)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	*groups = data->functions[selector].groups;
+	*num_groups = data->functions[selector].num_groups;
+
+	return 0;
+}
+
+static int mango_get_groups_count(struct pinctrl_dev *pctldev)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	return data->groups_count;
+}
+
+static const char *mango_get_group_name(struct pinctrl_dev *pctldev,
+					   unsigned int selector)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	return data->groups[selector].name;
+}
+
+static int mango_get_group_pins(struct pinctrl_dev *pctldev, unsigned int selector,
+		const unsigned int **pins,
+		unsigned int *num_pins)
+{
+	struct mango_soc_pinctrl_data *data = get_pinmux_data(pctldev);
+
+	*pins = data->groups[selector].pins;
+	*num_pins = data->groups[selector].num_pins;
+
+	return 0;
+}
+
+static void mango_pin_dbg_show(struct pinctrl_dev *pctldev, struct seq_file *s,
+	unsigned int offset)
+{
+}
+
+static const struct pinctrl_ops mango_pctrl_ops = {
+	.get_groups_count = mango_get_groups_count,
+	.get_group_name = mango_get_group_name,
+	.get_group_pins = mango_get_group_pins,
+	.pin_dbg_show = mango_pin_dbg_show,
+	.dt_node_to_map = pinconf_generic_dt_node_to_map_all,
+	.dt_free_map = pinctrl_utils_free_map,
+};
+
+static struct pinctrl_desc mango_desc = {
+	.name = "mango_pinctrl",
+	.pctlops = &mango_pctrl_ops,
+	.pmxops = &mango_pinmux_ops,
+	.confops = &mango_pinconf_ops,
+	.owner = THIS_MODULE,
+};
+
+ssize_t pinmux_show(struct device *dev,
+				struct device_attribute *attr, char *buf)
+{
+	struct mango_pinctrl *mangopctrl;
+	int p, ret, group, selector = -1;
+	struct mango_soc_pinctrl_data *data;
+
+	mangopctrl = dev_get_drvdata(dev);
+	data = (struct mango_soc_pinctrl_data *)mangopctrl->data;
+
+	for (p = 0; p < data->functions_count; p++) {
+		if (!strncmp(attr->attr.name, data->functions[p].name,
+			 strlen(attr->attr.name))) {
+			selector = p;
+			break;
+		}
+	}
+	if (selector < 0)
+		return -ENXIO;
+
+	group = selector/2;
+	ret = snprintf(buf, 128, "%d\n", data->groups[group].cur_func_idx);
+	if (ret <= 0 || ret > 128) {
+		dev_err(dev, "snprintf failed %d\n", ret);
+		return -EFAULT;
+	}
+	return ret;
+}
+
+ssize_t pinmux_store(struct device *dev,
+				struct device_attribute *attr,
+				const char *buf, size_t size)
+{
+	struct mango_pinctrl *mangopctrl;
+	int p, ret, group, selector = -1;
+	unsigned long user_data;
+	struct mango_soc_pinctrl_data *data;
+
+	ret = kstrtoul(buf, 0, &user_data);
+	if (ret)
+		return -EINVAL;
+
+	if (user_data != 0 && user_data != 1)
+		return -EINVAL;
+
+	mangopctrl = dev_get_drvdata(dev);
+	data = (struct mango_soc_pinctrl_data *)mangopctrl->data;
+
+	for (p = 0; p < data->functions_count; p++) {
+		if (!strncmp(attr->attr.name, data->functions[p].name,
+				strlen(attr->attr.name)) &&
+				(user_data == data->functions[p].mode)) {
+			selector = p;
+			break;
+		}
+	}
+	if (selector < 0)
+		return -ENXIO;
+
+	group = selector/2;
+	mango_set_mux(mangopctrl->pctl, selector, group);
+
+	dev_info(dev, "pinmux store set %s to func %d\n",
+			attr->attr.name, data->functions[selector].mode);
+	return size;
+}
+
+
+int sophgo_pinctrl_probe(struct platform_device *pdev)
+{
+	struct mango_pinctrl *mangopctrl;
+	struct pinctrl_desc *desc;
+	struct mango_soc_pinctrl_data *data;
+	struct device *dev = &pdev->dev;
+	struct device *pin_dev = NULL;
+	struct device_node *np = dev->of_node, *np_top;
+	static struct regmap *syscon;
+	int ret;
+
+	data = (struct mango_soc_pinctrl_data *)of_device_get_match_data(&pdev->dev);
+	if (!data)
+		return -EINVAL;
+	mangopctrl = devm_kzalloc(&pdev->dev, sizeof(*mangopctrl), GFP_KERNEL);
+	if (!mangopctrl)
+		return -ENOMEM;
+
+	mangopctrl->dev = &pdev->dev;
+
+	np_top = of_parse_phandle(np, "subctrl-syscon", 0);
+	if (!np_top) {
+		dev_err(dev, "%s can't get subctrl-syscon node\n", __func__);
+		return -EINVAL;
+	}
+	syscon = syscon_node_to_regmap(np_top);
+	if (IS_ERR(syscon)) {
+		dev_err(dev, "cannot get regmap\n");
+		return PTR_ERR(syscon);
+	}
+	mangopctrl->syscon_pinctl = syscon;
+
+	ret = device_property_read_u32(&pdev->dev,
+		"top_pinctl_offset", &mangopctrl->top_pinctl_offset);
+	if (ret < 0) {
+		dev_err(dev, "cannot get top_pinctl_offset\n");
+		return ret;
+	}
+
+	desc = &mango_desc;
+	desc->pins = data->pins;
+	desc->npins = data->npins;
+
+	mangopctrl->data = (void *)data;
+	mangopctrl->pctl = devm_pinctrl_register(&pdev->dev, desc, mangopctrl);
+	if (IS_ERR(mangopctrl->pctl)) {
+		dev_err(&pdev->dev, "could not register Sophgo pin ctrl driver\n");
+		return PTR_ERR(mangopctrl->pctl);
+	}
+
+	platform_set_drvdata(pdev, mangopctrl);
+
+	ret = class_register(data->p_class);
+	if (ret < 0) {
+		dev_err(dev, "cannot register pinmux class\n");
+		return ret;
+	}
+	pin_dev = device_create(data->p_class, &pdev->dev, MKDEV(0, 0), mangopctrl, "mango_pinmux");
+	if (IS_ERR(pin_dev))
+		return PTR_ERR(pin_dev);
+
+	return 0;
+}
diff --git a/drivers/pinctrl/sophgo/pinctrl-sophgo.h b/drivers/pinctrl/sophgo/pinctrl-sophgo.h
new file mode 100644
index 000000000000..f3a30f0275b1
--- /dev/null
+++ b/drivers/pinctrl/sophgo/pinctrl-sophgo.h
@@ -0,0 +1,70 @@
+#ifndef __mango_PINCTRL_CORE_H__
+#define __mango_PINCTRL_CORE_H__
+
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/pinctrl/pinmux.h>
+#include <linux/pinctrl/pinconf.h>
+#include <linux/pinctrl/pinconf-generic.h>
+#include "../pinctrl-utils.h"
+#include "../core.h"
+
+enum FUNC_MODE {
+	FUNC_MODE0,
+	FUNC_MODE1,
+	FUNC_MODE2,
+	FUNC_MODE3,
+	FUNC_MASK,
+};
+
+struct mango_pinctrl {
+	struct device *dev;
+	struct pinctrl_dev *pctl;
+	u32 top_pinctl_offset;
+	struct regmap *syscon_pinctl;
+	void *data;
+};
+
+struct mango_group {
+	const char *name;
+	const unsigned int *pins;
+	const unsigned int num_pins;
+	int cur_func_idx;
+	struct mango_pmx_func *funcs;
+};
+
+struct mango_pmx_func {
+	const char *name;
+	const char * const *groups;
+	unsigned int num_groups;
+	enum FUNC_MODE mode;
+};
+
+struct mango_soc_pinmux_info {
+	const char name[16];
+	const char name_a[16];
+	const char name_r[16];
+	struct pinctrl_state *pinctrl_a;
+	struct pinctrl_state *pinctrl_r;
+	const unsigned int def_state; /* default state */
+	int (*set)(struct device *dev, unsigned int data);
+};
+
+struct mango_soc_pinctrl_data {
+	const struct pinctrl_pin_desc *pins;
+	unsigned int npins;
+	struct mango_group *groups;
+	int groups_count;
+	const struct mango_pmx_func *functions;
+	int functions_count;
+	struct class *p_class;
+};
+
+int sophgo_pinctrl_probe(struct platform_device *pdev);
+int mango_pmux_probe(struct platform_device *pdev);
+
+ssize_t pinmux_show(struct device *dev,
+			struct device_attribute *attr, char *buf);
+
+ssize_t pinmux_store(struct device *dev,
+			struct device_attribute *attr, const char *buf, size_t size);
+#endif
diff --git a/drivers/pwm/Kconfig b/drivers/pwm/Kconfig
index 8ebcddf91f7b..428fa365a19a 100644
--- a/drivers/pwm/Kconfig
+++ b/drivers/pwm/Kconfig
@@ -637,6 +637,17 @@ config PWM_TEGRA
 	  To compile this driver as a module, choose M here: the module
 	  will be called pwm-tegra.
 
+config PWM_THEAD
+	tristate "T-HEAD PWM support"
+	depends on ARCH_THEAD || COMPILE_TEST
+	depends on HAS_IOMEM
+	help
+	  Generic PWM framework driver for the PWFM controller found on THEAD
+	  SoCs.
+
+	  To compile this driver as a module, choose M here: the module
+	  will be called pwm-thead.
+
 config PWM_TIECAP
 	tristate "ECAP PWM support"
 	depends on ARCH_OMAP2PLUS || ARCH_DAVINCI_DA8XX || ARCH_KEYSTONE || ARCH_K3 || COMPILE_TEST
diff --git a/drivers/pwm/Makefile b/drivers/pwm/Makefile
index c822389c2a24..4847ffd6997d 100644
--- a/drivers/pwm/Makefile
+++ b/drivers/pwm/Makefile
@@ -50,6 +50,7 @@ obj-$(CONFIG_PWM_RZ_MTU3)	+= pwm-rz-mtu3.o
 obj-$(CONFIG_PWM_SAMSUNG)	+= pwm-samsung.o
 obj-$(CONFIG_PWM_SIFIVE)	+= pwm-sifive.o
 obj-$(CONFIG_PWM_SL28CPLD)	+= pwm-sl28cpld.o
+obj-$(CONFIG_ARCH_SOPHGO)	+= pwm-sophgo.o
 obj-$(CONFIG_PWM_SPEAR)		+= pwm-spear.o
 obj-$(CONFIG_PWM_SPRD)		+= pwm-sprd.o
 obj-$(CONFIG_PWM_STI)		+= pwm-sti.o
@@ -59,6 +60,7 @@ obj-$(CONFIG_PWM_STMPE)		+= pwm-stmpe.o
 obj-$(CONFIG_PWM_SUN4I)		+= pwm-sun4i.o
 obj-$(CONFIG_PWM_SUNPLUS)	+= pwm-sunplus.o
 obj-$(CONFIG_PWM_TEGRA)		+= pwm-tegra.o
+obj-$(CONFIG_PWM_THEAD)		+= pwm-thead.o
 obj-$(CONFIG_PWM_TIECAP)	+= pwm-tiecap.o
 obj-$(CONFIG_PWM_TIEHRPWM)	+= pwm-tiehrpwm.o
 obj-$(CONFIG_PWM_TWL)		+= pwm-twl.o
diff --git a/drivers/pwm/pwm-sophgo.c b/drivers/pwm/pwm-sophgo.c
new file mode 100644
index 000000000000..b6297175a5b7
--- /dev/null
+++ b/drivers/pwm/pwm-sophgo.c
@@ -0,0 +1,276 @@
+/*
+ * Copyright (c) 2007 Ben Dooks
+ * Copyright (c) 2008 Simtec Electronics
+ *     Ben Dooks <ben@simtec.co.uk>, <ben-linux@fluff.org>
+ * Copyright (c) 2013 Tomasz Figa <tomasz.figa@gmail.com>
+ *
+ * PWM driver for Samsung SoCs
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License.
+ */
+
+#include <linux/bitops.h>
+#include <linux/clk.h>
+#include <linux/export.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/platform_device.h>
+#include <linux/pwm.h>
+#include <linux/slab.h>
+
+
+
+#define REG_HLPERIOD		0x0
+#define REG_PERIOD			0x4
+#define REG_GROUP			0x8
+#define REG_POLARITY		0x20
+
+
+/**
+ * struct sophgo_pwm_channel - private data of PWM channel
+ * @period_ns:	current period in nanoseconds programmed to the hardware
+ * @duty_ns:	current duty time in nanoseconds programmed to the hardware
+ * @tin_ns:	time of one timer tick in nanoseconds with current timer rate
+ */
+struct sophgo_pwm_channel {
+	u32 period;
+	u32 hlperiod;
+};
+
+/**
+ * struct sophgo_pwm_chip - private data of PWM chip
+ * @chip:		generic PWM chip
+ * @variant:		local copy of hardware variant data
+ * @inverter_mask:	inverter status for all channels - one bit per channel
+ * @base:		base address of mapped PWM registers
+ * @base_clk:		base clock used to drive the timers
+ * @tclk0:		external clock 0 (can be ERR_PTR if not present)
+ * @tclk1:		external clock 1 (can be ERR_PTR if not present)
+ */
+struct sophgo_pwm_chip {
+	struct pwm_chip chip;
+	void __iomem *base;
+	struct clk *base_clk;
+	u8 polarity_mask;
+	bool no_polarity;
+};
+
+
+static inline
+struct sophgo_pwm_chip *to_sophgo_pwm_chip(struct pwm_chip *chip)
+{
+	return container_of(chip, struct sophgo_pwm_chip, chip);
+}
+
+static int pwm_sophgo_request(struct pwm_chip *chip, struct pwm_device *pwm_dev)
+{
+	struct sophgo_pwm_channel *channel;
+
+	channel = kzalloc(sizeof(*channel), GFP_KERNEL);
+	if (!channel)
+		return -ENOMEM;
+
+	return pwm_set_chip_data(pwm_dev, channel);
+}
+
+static void pwm_sophgo_free(struct pwm_chip *chip, struct pwm_device *pwm_dev)
+{
+	struct sophgo_pwm_channel *channel = pwm_get_chip_data(pwm_dev);
+
+	pwm_set_chip_data(pwm_dev, NULL);
+	kfree(channel);
+}
+
+static int pwm_sophgo_config(struct pwm_chip *chip, struct pwm_device *pwm_dev,
+			     int duty_ns, int period_ns)
+{
+	struct sophgo_pwm_chip *our_chip = to_sophgo_pwm_chip(chip);
+	struct sophgo_pwm_channel *channel = pwm_get_chip_data(pwm_dev);
+	u64 cycles;
+
+	cycles = clk_get_rate(our_chip->base_clk);
+	cycles *= period_ns;
+	do_div(cycles, NSEC_PER_SEC);
+
+	channel->period = cycles;
+	cycles = cycles * duty_ns;
+	do_div(cycles, period_ns);
+	channel->hlperiod = channel->period - cycles;
+
+	return 0;
+}
+
+static int pwm_sophgo_enable(struct pwm_chip *chip, struct pwm_device *pwm_dev)
+{
+	struct sophgo_pwm_chip *our_chip = to_sophgo_pwm_chip(chip);
+	struct sophgo_pwm_channel *channel = pwm_get_chip_data(pwm_dev);
+
+	writel(channel->period, our_chip->base + REG_GROUP * pwm_dev->hwpwm + REG_PERIOD);
+	writel(channel->hlperiod, our_chip->base + REG_GROUP * pwm_dev->hwpwm + REG_HLPERIOD);
+
+	return 0;
+}
+
+static void pwm_sophgo_disable(struct pwm_chip *chip,
+			       struct pwm_device *pwm_dev)
+{
+	struct sophgo_pwm_chip *our_chip = to_sophgo_pwm_chip(chip);
+
+	writel(0, our_chip->base + REG_GROUP * pwm_dev->hwpwm + REG_PERIOD);
+	writel(0, our_chip->base + REG_GROUP * pwm_dev->hwpwm + REG_HLPERIOD);
+}
+
+static int pwm_sophgo_apply(struct pwm_chip *chip, struct pwm_device *pwm,
+			      const struct pwm_state *state)
+{
+	int ret;
+
+	bool enabled = pwm->state.enabled;
+
+	if (state->polarity != pwm->state.polarity && pwm->state.enabled) {
+		pwm_sophgo_disable(chip, pwm);
+		enabled = false;
+	}
+
+	if (!state->enabled) {
+		if (enabled)
+			pwm_sophgo_disable(chip, pwm);
+		return 0;
+	}
+
+	ret = pwm_sophgo_config(chip, pwm, state->duty_cycle, state->period);
+	if (ret) {
+		dev_err(chip->dev, "pwm apply err\n");
+		return ret;
+	}
+	dev_dbg(chip->dev, "%s tate->enabled =%d\n", __func__, state->enabled);
+	if (state->enabled)
+		ret = pwm_sophgo_enable(chip, pwm);
+	else
+		pwm_sophgo_disable(chip, pwm);
+
+	if (ret) {
+		dev_err(chip->dev, "pwm apply failed\n");
+		return ret;
+	}
+	return ret;
+}
+
+static const struct pwm_ops pwm_sophgo_ops = {
+	.request	= pwm_sophgo_request,
+	.free		= pwm_sophgo_free,
+	.apply		= pwm_sophgo_apply,
+	.owner		= THIS_MODULE,
+};
+
+static const struct of_device_id sophgo_pwm_match[] = {
+	{ .compatible = "sophgo,sophgo-pwm" },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, sophgo_pwm_match);
+
+static int pwm_sophgo_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct sophgo_pwm_chip *chip;
+	struct resource *res;
+	int ret;
+
+	pr_info("%s\n", __func__);
+
+	chip = devm_kzalloc(&pdev->dev, sizeof(*chip), GFP_KERNEL);
+	if (chip == NULL)
+		return -ENOMEM;
+
+	chip->chip.dev = &pdev->dev;
+	chip->chip.ops = &pwm_sophgo_ops;
+	chip->chip.base = -1;
+	chip->polarity_mask = 0;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	chip->base = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(chip->base))
+		return PTR_ERR(chip->base);
+
+	chip->base_clk = devm_clk_get(&pdev->dev, NULL);
+	if (IS_ERR(chip->base_clk)) {
+		dev_err(dev, "failed to get pwm source clk\n");
+		return PTR_ERR(chip->base_clk);
+	}
+
+	ret = clk_prepare_enable(chip->base_clk);
+	if (ret < 0) {
+		dev_err(dev, "failed to enable base clock\n");
+		return ret;
+	}
+
+	//pwm-num default is 4, compatible with sg2042
+	if (of_property_read_bool(pdev->dev.of_node, "pwm-num"))
+		device_property_read_u32(&pdev->dev, "pwm-num", &chip->chip.npwm);
+	else
+		chip->chip.npwm = 4;
+
+	//no_polarity default is false(have polarity) , compatible with sg2042
+	if (of_property_read_bool(pdev->dev.of_node, "no-polarity"))
+		chip->no_polarity = true;
+	else
+		chip->no_polarity = false;
+	pr_debug("chip->chip.npwm =%d  chip->no_polarity=%d\n", chip->chip.npwm, chip->no_polarity);
+
+	platform_set_drvdata(pdev, chip);
+
+	ret = pwmchip_add(&chip->chip);
+	if (ret < 0) {
+		dev_err(dev, "failed to register PWM chip\n");
+		clk_disable_unprepare(chip->base_clk);
+		return ret;
+	}
+
+	return 0;
+}
+
+static int pwm_sophgo_remove(struct platform_device *pdev)
+{
+	struct sophgo_pwm_chip *chip = platform_get_drvdata(pdev);
+
+	pwmchip_remove(&chip->chip);
+
+	clk_disable_unprepare(chip->base_clk);
+
+	return 0;
+}
+
+#ifdef CONFIG_PM_SLEEP
+static int pwm_sophgo_suspend(struct device *dev)
+{
+	return 0;
+}
+
+static int pwm_sophgo_resume(struct device *dev)
+{
+	return 0;
+}
+#endif
+
+static SIMPLE_DEV_PM_OPS(pwm_sophgo_pm_ops, pwm_sophgo_suspend,
+			 pwm_sophgo_resume);
+
+static struct platform_driver pwm_sophgo_driver = {
+	.driver		= {
+		.name	= "sophgo-pwm",
+		.pm	= &pwm_sophgo_pm_ops,
+		.of_match_table = of_match_ptr(sophgo_pwm_match),
+	},
+	.probe		= pwm_sophgo_probe,
+	.remove		= pwm_sophgo_remove,
+};
+module_platform_driver(pwm_sophgo_driver);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("chunzhi.lin");
+MODULE_DESCRIPTION("Sophgo PWM driver");
diff --git a/drivers/pwm/pwm-thead.c b/drivers/pwm/pwm-thead.c
new file mode 100644
index 000000000000..3b4772c3b8ca
--- /dev/null
+++ b/drivers/pwm/pwm-thead.c
@@ -0,0 +1,269 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * T-HEAD PWM driver
+ *
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ * Copyright (C) 2023 Jisheng Zhang <jszhang@kernel.org>
+ *
+ * Limitations:
+ * - The THEAD_PWM_CTRL_START bit is only effective when 0 -> 1, which is used
+ *   to start the channel, 1 -> 0 doesn't change anything. so 0 % duty cycle
+ *   is used to "disable" the channel.
+ * - The THEAD_PWM_CTRL_START bit is automatically cleared once PWM channel is
+ *   started.
+ * - The THEAD_PWM_CFG_UPDATE atomically updates and only updates period and duty.
+ * - To update period and duty, THEAD_PWM_CFG_UPDATE needs to go through 0 -> 1
+ *   step, I.E if THEAD_PWM_CFG_UPDATE is already 1, it's necessary to clear it
+ *   to 0 beforehand.
+ * - Polarity can only be changed if never started before.
+ */
+
+#include <linux/bitfield.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/mod_devicetable.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/pm_runtime.h>
+#include <linux/pwm.h>
+#include <linux/slab.h>
+
+#define THEAD_PWM_MAX_NUM		6
+#define THEAD_PWM_MAX_PERIOD		GENMASK(31, 0)
+#define THEAD_PWM_MAX_DUTY		GENMASK(31, 0)
+
+#define THEAD_PWM_CHN_BASE(n)		((n) * 0x20)
+#define THEAD_PWM_CTRL(n)		(THEAD_PWM_CHN_BASE(n) + 0x00)
+#define  THEAD_PWM_CTRL_START		BIT(0)
+#define  THEAD_PWM_CTRL_SOFT_RST		BIT(1)
+#define  THEAD_PWM_CTRL_CFG_UPDATE	BIT(2)
+#define  THEAD_PWM_CTRL_INTEN		BIT(3)
+#define  THEAD_PWM_CTRL_MODE		GENMASK(5, 4)
+#define  THEAD_PWM_CTRL_MODE_CONTINUOUS	FIELD_PREP(THEAD_PWM_CTRL_MODE, 2)
+#define  THEAD_PWM_CTRL_EVTRIG		GENMASK(7, 6)
+#define  THEAD_PWM_CTRL_FPOUT		BIT(8)
+#define  THEAD_PWM_CTRL_INFACTOUT	BIT(9)
+#define THEAD_PWM_RPT(n)		(THEAD_PWM_CHN_BASE(n) + 0x04)
+#define THEAD_PWM_PER(n)		(THEAD_PWM_CHN_BASE(n) + 0x08)
+#define THEAD_PWM_FP(n)			(THEAD_PWM_CHN_BASE(n) + 0x0c)
+#define THEAD_PWM_STATUS(n)		(THEAD_PWM_CHN_BASE(n) + 0x10)
+#define  THEAD_PWM_STATUS_CYCLE		GENMASK(7, 0)
+
+struct thead_pwm_chip {
+	struct pwm_chip chip;
+	void __iomem *mmio_base;
+	struct clk *clk;
+	u8 channel_ever_started;
+};
+
+static inline struct thead_pwm_chip *thead_pwm_from_chip(struct pwm_chip *chip)
+{
+	return container_of(chip, struct thead_pwm_chip, chip);
+}
+
+static int thead_pwm_apply(struct pwm_chip *chip, struct pwm_device *pwm,
+			   const struct pwm_state *state)
+{
+	struct thead_pwm_chip *priv = thead_pwm_from_chip(chip);
+	u32 val = THEAD_PWM_CTRL_INFACTOUT | THEAD_PWM_CTRL_FPOUT | THEAD_PWM_CTRL_MODE_CONTINUOUS;
+	u64 period_cycle, duty_cycle, rate;
+	int ret;
+
+	/* if ever started, can't change the polarity */
+	if ((priv->channel_ever_started & (1 << pwm->hwpwm)) &&
+	    state->polarity != pwm->state.polarity)
+		return -EINVAL;
+
+	if (!state->enabled) {
+		if (pwm->state.enabled) {
+			val = readl(priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+			val &= ~THEAD_PWM_CTRL_CFG_UPDATE;
+			writel(val, priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+
+			writel(0, priv->mmio_base + THEAD_PWM_FP(pwm->hwpwm));
+
+			val |= THEAD_PWM_CTRL_CFG_UPDATE;
+			writel(val, priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+			pm_runtime_put_sync(chip->dev);
+		}
+		return 0;
+	}
+
+	if (!pwm->state.enabled) {
+		ret = pm_runtime_resume_and_get(chip->dev);
+		if (ret < 0)
+			return ret;
+	}
+
+	if (state->polarity == PWM_POLARITY_INVERSED)
+		val &= ~THEAD_PWM_CTRL_FPOUT;
+
+	writel(val, priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+
+	rate = clk_get_rate(priv->clk);
+	/*
+	 * The following calculations might overflow if clk is bigger
+	 * than 1 GHz. In practise it's 24MHz, so this limitation
+	 * is only theoretic.
+	 */
+	if (rate > NSEC_PER_SEC)
+		return -EINVAL;
+
+	period_cycle = mul_u64_u64_div_u64(rate, state->period, NSEC_PER_SEC);
+	if (period_cycle > THEAD_PWM_MAX_PERIOD)
+		period_cycle = THEAD_PWM_MAX_PERIOD;
+	/*
+	 * With limitation above we have period_cycle <= THEAD_PWM_MAX_PERIOD,
+	 * so this cannot overflow.
+	 */
+	writel(period_cycle, priv->mmio_base + THEAD_PWM_PER(pwm->hwpwm));
+
+	duty_cycle = mul_u64_u64_div_u64(rate, state->duty_cycle, NSEC_PER_SEC);
+	if (duty_cycle > THEAD_PWM_MAX_DUTY)
+		duty_cycle = THEAD_PWM_MAX_DUTY;
+	/*
+	 * With limitation above we have duty_cycle <= THEAD_PWM_MAX_DUTY,
+	 * so this cannot overflow.
+	 */
+	writel(duty_cycle, priv->mmio_base + THEAD_PWM_FP(pwm->hwpwm));
+
+	val |= THEAD_PWM_CTRL_CFG_UPDATE;
+	writel(val, priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+
+	if (!pwm->state.enabled) {
+		val |= THEAD_PWM_CTRL_START;
+		writel(val, priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+		priv->channel_ever_started |= 1 << pwm->hwpwm;
+	}
+
+	return 0;
+}
+
+static int thead_pwm_get_state(struct pwm_chip *chip, struct pwm_device *pwm,
+			       struct pwm_state *state)
+{
+	struct thead_pwm_chip *priv = thead_pwm_from_chip(chip);
+	u64 rate = clk_get_rate(priv->clk);
+	u32 val;
+	int ret;
+
+	ret = pm_runtime_resume_and_get(chip->dev);
+	if (ret < 0)
+		return ret;
+
+	val = readl(priv->mmio_base + THEAD_PWM_CTRL(pwm->hwpwm));
+	if (val & THEAD_PWM_CTRL_FPOUT)
+		state->polarity = PWM_POLARITY_NORMAL;
+	else
+		state->polarity = PWM_POLARITY_INVERSED;
+
+	val = readl(priv->mmio_base + THEAD_PWM_PER(pwm->hwpwm));
+	/*
+	 * val 32 bits, multiply NSEC_PER_SEC, won't overflow.
+	 */
+	state->period = DIV64_U64_ROUND_UP((u64)val * NSEC_PER_SEC, rate);
+
+	val = readl(priv->mmio_base + THEAD_PWM_FP(pwm->hwpwm));
+	state->enabled = !!val;
+	/*
+	 * val 32 bits, multiply NSEC_PER_SEC, won't overflow.
+	 */
+	state->duty_cycle = DIV64_U64_ROUND_UP((u64)val * NSEC_PER_SEC, rate);
+
+	pm_runtime_put_sync(chip->dev);
+
+	return 0;
+}
+
+static const struct pwm_ops thead_pwm_ops = {
+	.apply = thead_pwm_apply,
+	.get_state = thead_pwm_get_state,
+};
+
+static int __maybe_unused thead_pwm_runtime_suspend(struct device *dev)
+{
+	struct thead_pwm_chip *priv = dev_get_drvdata(dev);
+
+	clk_disable_unprepare(priv->clk);
+
+	return 0;
+}
+
+static int __maybe_unused thead_pwm_runtime_resume(struct device *dev)
+{
+	struct thead_pwm_chip *priv = dev_get_drvdata(dev);
+	int ret;
+
+	ret = clk_prepare_enable(priv->clk);
+	if (ret)
+		dev_err(dev, "failed to enable pwm clock(%pe)\n", ERR_PTR(ret));
+
+	return ret;
+}
+
+static int thead_pwm_probe(struct platform_device *pdev)
+{
+	struct thead_pwm_chip *priv;
+	int ret, i;
+	u32 val;
+
+	priv = devm_kzalloc(&pdev->dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, priv);
+
+	priv->mmio_base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(priv->mmio_base))
+		return PTR_ERR(priv->mmio_base);
+
+	priv->clk = devm_clk_get_enabled(&pdev->dev, NULL);
+	if (IS_ERR(priv->clk))
+		return PTR_ERR(priv->clk);
+
+	priv->chip.ops = &thead_pwm_ops;
+	priv->chip.dev = &pdev->dev;
+	priv->chip.npwm = THEAD_PWM_MAX_NUM;
+
+	/* check whether PWM is ever started or not */
+	for (i = 0; i < priv->chip.npwm; i++) {
+		val = readl(priv->mmio_base + THEAD_PWM_FP(i));
+		if (val)
+			priv->channel_ever_started |= 1 << i;
+	}
+
+	ret = devm_pwmchip_add(&pdev->dev, &priv->chip);
+	if (ret)
+		return ret;
+
+	devm_pm_runtime_enable(&pdev->dev);
+
+	return 0;
+}
+
+static const struct of_device_id thead_pwm_dt_ids[] = {
+	{.compatible = "thead,th1520-pwm",},
+	{/* sentinel */}
+};
+MODULE_DEVICE_TABLE(of, thead_pwm_dt_ids);
+
+static const struct dev_pm_ops thead_pwm_pm_ops = {
+	SET_RUNTIME_PM_OPS(thead_pwm_runtime_suspend, thead_pwm_runtime_resume, NULL)
+};
+
+static struct platform_driver thead_pwm_driver = {
+	.driver = {
+		.name = "thead-pwm",
+		.of_match_table = thead_pwm_dt_ids,
+		.pm = &thead_pwm_pm_ops,
+	},
+	.probe = thead_pwm_probe,
+};
+module_platform_driver(thead_pwm_driver);
+
+MODULE_AUTHOR("Wei Liu <lw312886@linux.alibaba.com>");
+MODULE_AUTHOR("Jisheng Zhang <jszhang@kernel.org>");
+MODULE_DESCRIPTION("T-HEAD pwm driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/regulator/Kconfig b/drivers/regulator/Kconfig
index 965d4f0c18a6..8a2c579c783c 100644
--- a/drivers/regulator/Kconfig
+++ b/drivers/regulator/Kconfig
@@ -1663,4 +1663,13 @@ config REGULATOR_QCOM_LABIBB
 	  boost regulator and IBB can be used as a negative boost regulator
 	  for LCD display panel.
 
+config REGULATOR_LIGHT_AON
+        tristate "Thead Light Aon regulator"
+        depends on LIGHT_AON
+        default y
+        help
+          This driver provides support for the thead light virtal regulators that
+          inmplemented on Light Aon system.
+
+
 endif
diff --git a/drivers/regulator/Makefile b/drivers/regulator/Makefile
index 23074714a81a..aa1d8ca59499 100644
--- a/drivers/regulator/Makefile
+++ b/drivers/regulator/Makefile
@@ -195,5 +195,6 @@ obj-$(CONFIG_REGULATOR_WM831X) += wm831x-ldo.o
 obj-$(CONFIG_REGULATOR_WM8350) += wm8350-regulator.o
 obj-$(CONFIG_REGULATOR_WM8400) += wm8400-regulator.o
 obj-$(CONFIG_REGULATOR_WM8994) += wm8994-regulator.o
+obj-$(CONFIG_REGULATOR_LIGHT_AON) += light-regulator-aon.o
 
 ccflags-$(CONFIG_REGULATOR_DEBUG) += -DDEBUG
diff --git a/drivers/regulator/light-regulator-aon.c b/drivers/regulator/light-regulator-aon.c
new file mode 100644
index 000000000000..d30cb956145b
--- /dev/null
+++ b/drivers/regulator/light-regulator-aon.c
@@ -0,0 +1,888 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/debugfs.h>
+#include <linux/err.h>
+#include <linux/slab.h>
+#include <linux/interrupt.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/platform_device.h>
+#include <linux/regulator/driver.h>
+#include <linux/regulator/machine.h>
+#include <linux/regulator/of_regulator.h>
+#include <linux/regulator/machine.h>
+#include <linux/slab.h>
+#include <linux/uaccess.h>
+#include <linux/firmware/thead/ipc.h>
+
+#define MBOX_MAX_MSG_LEN	28
+
+#define CONFIG_AON_REG_DEBUG	1
+
+struct rpc_msg_regu_vol_set {
+	u16 regu_id;                    ///< virtual regu id
+	u16 is_dual_rail;               ///< whether this regu has dual rails
+	u32 dc1;                        ///< voltage uinit in uv for single rail or first rail of dual rail
+	u32 dc2;                        ///< voltage uinit in uv for second rail of dual rail,ignore it if "is_dual_rail" is false
+	u16 reserved[6];
+} __packed __aligned(4);
+
+struct rpc_msg_regu_vol_get {
+	u16 regu_id;                    ///< virtual regu id
+	u16 is_dual_rail;               ///< whether this regu has dual rails
+	u32 dc1;                        ///< voltage uinit in uv for single rail or first rail of dual rail
+	u32 dc2;                        ///< voltage uinit in uv for second rail of dual rail,ignore it if "is_dual_rail" is false
+	u16 reserved[6];
+
+} __packed __aligned(4);
+
+struct rpc_msg_regu_pwr_set {
+	u16 regu_id;                    ///< virtual regu id
+	u16 status;                     ///< 0: power off; 1: powr on
+	u32 reserved[5];
+} __packed __aligned(4);
+
+struct rpc_msg_regu_pwr_get {
+	u16 regu_id;                    ///< virtual regu id
+	u16 status;                     ///< 0: power off; 1: powr on
+	u32 reserved[5];
+
+} __packed __aligned(4);
+
+struct light_aon_msg_regulator_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	union rpc_func_t {
+	struct rpc_msg_regu_vol_set    regu_vol_set;
+	struct rpc_msg_regu_vol_get    regu_vol_get;
+	struct rpc_msg_regu_pwr_set    regu_pwr_set;
+	struct rpc_msg_regu_pwr_get    regu_pwr_get;
+	} __packed __aligned(4) rpc;
+} __packed __aligned(4);
+
+enum pm_resource {
+	SOC_DVDD18_AON,      /*da9063:  ldo-3 */
+	SOC_AVDD33_USB3,     /*da9063:  ldo-9 */
+	SOC_DVDD08_AON,      /*da9063:  ldo-2 */
+	SOC_APCPU_DVDD_DVDDM,/*da9063:  vbcore1 & vbcore2*/
+	SOC_DVDD08_DDR,      /*da9063:  buckperi */
+	SOC_VDD_DDR_1V8,     /*da9063:  ldo-4  */
+	SOC_VDD_DDR_1V1,     /*da9063:  buckmem & buckio  */
+	SOC_VDD_DDR_0V6,     /*da9063:  buckpro */
+	SOC_DVDD18_AP,       /*da9063:  ldo-11 */
+	SOC_DVDD08_AP,       /*da9121:  da9121_ex */
+	SOC_AVDD08_MIPI_HDMI,/*da9063:  ldo-1  */
+	SOC_AVDD18_MIPI_HDMI,/*da9063:  ldo-5  */
+	SOC_DVDD33_EMMC,     /*da9063:  ldo-10 */
+	SOC_DVDD18_EMMC,     /*slg51000:ldo-3 */
+	SOC_DOVDD18_SCAN,    /*da9063:  ldo-6 */
+	SOC_VEXT_2V8,        /*da9063:  ldo-7 */
+	SOC_DVDD12_SCAN,     /*da9063:  ld0-8 */
+	SOC_AVDD28_SCAN_EN,  /*da9063: gpio4 */
+	SOC_AVDD28_RGB,      /*slg51000:ldo-1 */
+	SOC_DOVDD18_RGB,     /*slg51000:ldo-4 */
+	SOC_DVDD12_RGB,      /*slg51000:ldo-5 */
+	SOC_AVDD25_IR,       /*slg51000:ldo-2 */
+	SOC_DOVDD18_IR,      /*slg51000:ldo-7 */
+	SOC_DVDD12_IR,       /*slg51000:ldo-6 */
+	SOC_ADC_VREF,
+	SOC_LCD0_EN,
+	SOC_VEXT_1V8,
+
+
+	SOC_REGU_MAX
+};
+
+struct apcpu_vol_set {
+	u32 vdd;               ///< cpu core voltage
+	u32 vddm;              ///< cpu core-mem voltage
+};
+
+struct aon_regu_desc {
+	struct regulator_desc *regu_desc;            ///< discription of regulator
+	u32                    regu_num;             ///< element number of regulators,which point to regu-dsc-array
+};
+
+struct aon_regu_info {
+	struct device              *dev;
+	const struct apcpu_vol_set *cpu_vol;         ///< signed-off voltage of cpu
+	u32                        vddm;             ///< cpu-mem voltage
+	struct aon_regu_desc       *regu_desc;       ///< regu-desc set
+	struct light_aon_ipc       *ipc_handle;      ///< handle of mail-box
+};
+
+static struct aon_regu_info light_aon_pmic_info;
+
+#define APCPU_VOL_DEF(_vdd, _vddm) \
+	{					\
+		.vdd = _vdd,		\
+		.vddm = _vddm,		\
+	}
+
+static const struct apcpu_vol_set apcpu_volts[] = {
+	/*300Mhz*/
+	APCPU_VOL_DEF(600000U, 750000U),
+	APCPU_VOL_DEF(600000U, 800000U),
+	APCPU_VOL_DEF(650000U, 800000U),
+	APCPU_VOL_DEF(720000U, 770000U),
+	/*800Mhz*/
+	APCPU_VOL_DEF(700000U,800000U),
+	APCPU_VOL_DEF(720000U,820000U),
+	/*1500Mhz*/
+	APCPU_VOL_DEF(800000U,800000U),
+	APCPU_VOL_DEF(820000U,820000U),
+	/*1850Mhz*/
+	APCPU_VOL_DEF(1000000U,1000000U),
+};
+
+/* dc2 is valid when is_dual_rail is true
+ *
+ * dual-rail regulator means that a virtual regulator involes two hw-regulators
+ */
+static int aon_set_regulator(struct light_aon_ipc *ipc, u16 regu_id,
+			    u32 dc1, u32 dc2, u16 is_dual_rail)
+{
+	struct light_aon_msg_regulator_ctrl msg = {0};
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_PM;
+	hdr->func = (uint8_t)LIGHT_AON_PM_FUNC_SET_RESOURCE_REGULATOR;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.rpc.regu_vol_set.regu_id = regu_id;
+	msg.rpc.regu_vol_set.is_dual_rail = is_dual_rail;
+	msg.rpc.regu_vol_set.dc1 = dc1;
+	msg.rpc.regu_vol_set.dc2 = dc2;
+
+	return light_aon_call_rpc(ipc, &msg, true);
+}
+
+/* dc2 is valid when is_dual_rail is true
+ *
+ * dual-rail regulator means that a virtual regulator involes two hw-regulators
+ */
+static int aon_get_regulator(struct light_aon_ipc *ipc, u16 regu_id,
+			    u32 *dc1, u32 *dc2, u16 is_dual_rail)
+{
+	struct light_aon_msg_regulator_ctrl msg = {0};
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+	int ret;
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_PM;
+	hdr->func = (uint8_t)LIGHT_AON_PM_FUNC_GET_RESOURCE_REGULATOR;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+	msg.rpc.regu_vol_get.regu_id  = regu_id;
+	msg.rpc.regu_vol_get.is_dual_rail = is_dual_rail;
+
+	ret = light_aon_call_rpc(ipc, &msg, true);
+	if (ret)
+		return ret;
+
+	if (dc1 != NULL)
+		*dc1 = msg.rpc.regu_vol_get.dc1;
+
+	if (dc2 != NULL)
+		*dc2 = msg.rpc.regu_vol_get.dc2;
+
+	return 0;
+}
+
+static int aon_regu_power_ctrl(struct light_aon_ipc *ipc,u32 regu_id,u16 pwr_on)
+{
+	struct light_aon_msg_regulator_ctrl msg = {0};
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_PM;
+	hdr->func = (uint8_t)LIGHT_AON_PM_FUNC_PWR_SET;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.rpc.regu_pwr_set.regu_id = regu_id;
+	msg.rpc.regu_pwr_set.status  = pwr_on;
+	return light_aon_call_rpc(ipc, &msg, true);
+}
+static int aon_regu_dummy_enable(struct regulator_dev *reg)
+{
+	return 0;
+}
+static int aon_regu_dummy_disable(struct regulator_dev *reg)
+{
+	return 0;
+}
+static int aon_regu_dummy_is_enabled(struct regulator_dev *reg)
+{
+	return 0;
+}
+static int aon_regu_enable(struct regulator_dev *reg)
+{
+	u16 regu_id =(u16) rdev_get_id(reg);
+	return aon_regu_power_ctrl(light_aon_pmic_info.ipc_handle, regu_id, 1);
+}
+
+static int aon_regu_disable(struct regulator_dev *reg)
+{
+	u16 regu_id =(u16) rdev_get_id(reg);
+	return aon_regu_power_ctrl(light_aon_pmic_info.ipc_handle, regu_id, 0);
+}
+
+static int aon_regu_is_enabled(struct regulator_dev *reg)
+{
+	struct light_aon_msg_regulator_ctrl msg = {0};
+	struct light_aon_rpc_msg_hdr *hdr = &msg.hdr;
+	int ret;
+	u16 regu_id =(u16) rdev_get_id(reg);
+
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_PM;
+	hdr->func = (uint8_t)LIGHT_AON_PM_FUNC_PWR_GET;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+
+	msg.rpc.regu_pwr_get.regu_id = regu_id;
+	ret = light_aon_call_rpc(light_aon_pmic_info.ipc_handle, &msg, true);
+	if (ret < 0) {
+		return ret;
+	}
+
+	return (int) msg.rpc.regu_pwr_get.status;
+}
+
+static int aon_regu_set_voltage(struct regulator_dev *reg,
+				int minuV, int uV, unsigned *selector)
+{
+	u16 regu_id =(u16) rdev_get_id(reg);
+	u32 voltage = minuV; /* uV */
+	int err;
+
+	pr_debug("[%s,%d]minuV = %d, uV = %d\n", __func__, __LINE__, minuV, uV);
+
+	err = aon_set_regulator(light_aon_pmic_info.ipc_handle, regu_id,
+				       voltage, 0, 0);
+	if (err) {
+		pr_err("failed to set Voltages to %d!\n", minuV);
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static int aon_regu_get_voltage(struct regulator_dev *reg)
+{
+	u16 regu_id = (u16) rdev_get_id(reg);
+	int voltage, ret;
+
+	ret = aon_get_regulator(light_aon_pmic_info.ipc_handle, regu_id,
+				&voltage, NULL, 0);
+	if (ret) {
+		pr_err("failed to get voltage\n");
+		return -EINVAL;
+	}
+
+	pr_debug("[%s,%d]voltage = %d\n", __func__, __LINE__, voltage);
+
+	return voltage;
+}
+
+static const struct apcpu_vol_set *apcpu_get_matched_signed_off_voltage(u32 vdd, u32 vddm)
+{
+	int vol_count = ARRAY_SIZE(apcpu_volts);
+	int i;
+
+	for (i = 0; i < vol_count; i++)
+		if ((vdd == apcpu_volts[i].vdd) &&
+		    (vddm == apcpu_volts[i].vddm))
+			return &apcpu_volts[i];
+
+#ifdef CONFIG_AON_REG_DEBUG
+	return &apcpu_volts[2];
+#else
+	return NULL;
+#endif
+}
+
+static int apcpu_set_vdd_vddm_voltage(struct regulator_dev *reg,
+			      int minuV, int uV, unsigned *selector)
+{
+	struct aon_regu_info *info = rdev_get_drvdata(reg);
+	const struct apcpu_vol_set *cpu_vol;
+	u32 vol = minuV; /* uV */
+	u32 dc1, dc2;
+	int err;
+
+	cpu_vol = apcpu_get_matched_signed_off_voltage(vol, light_aon_pmic_info.vddm);
+	if (!cpu_vol) {
+		dev_err(info->dev, "failed to find bcore1/bcore2 matching table\n");
+#ifndef CONFIG_AON_REG_DEBUG
+		return -EINVAL;
+#endif
+	}
+
+	dc1 = cpu_vol->vdd;
+	dc2 = cpu_vol->vddm;
+	info->cpu_vol = cpu_vol;
+	info->vddm = cpu_vol->vddm;
+
+	err = aon_set_regulator(light_aon_pmic_info.ipc_handle, (u16)SOC_APCPU_DVDD_DVDDM,
+				       dc1, dc2, 1);
+	if (err) {
+		dev_err(info->dev, "failed to set Voltages to %d!\n", uV);
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static int apcpu_set_vddm_voltage(struct regulator_dev *reg,
+			      int minuV, int uV, unsigned *selector)
+{
+	struct aon_regu_info *info = rdev_get_drvdata(reg);
+	int bcore_table_count = ARRAY_SIZE(apcpu_volts);
+	u32 vol = minuV; /* uV */
+	int i;
+
+	for (i = 0; i < bcore_table_count; i++)
+		if (vol == apcpu_volts[i].vddm)
+			break;
+
+	if (i >= bcore_table_count) {
+		dev_err(info->dev, "The vol is not existed in matching table\n");
+#ifndef CONFIG_AON_REG_DEBUG
+		return -EINVAL;
+#endif
+	}
+
+	/* update the vddm */
+	info->vddm = vol;
+	return 0;
+}
+
+static int apcpu_get_voltage(struct regulator_dev *reg, bool is_vdd)
+{
+	struct aon_regu_info *info = rdev_get_drvdata(reg);
+	const struct apcpu_vol_set *cpu_vol;
+	u32 dc1, dc2;
+	int err;
+
+	err = aon_get_regulator(light_aon_pmic_info.ipc_handle, SOC_APCPU_DVDD_DVDDM,
+				       &dc1, &dc2, 1);
+	if (err) {
+		dev_err(info->dev, "failed to get Voltages!\n");
+		return -EINVAL;
+	}
+	cpu_vol = apcpu_get_matched_signed_off_voltage(dc1, dc2);
+	if (!cpu_vol) {
+		dev_err(info->dev, "Voltage [%d:%d] is not existing in matching table\n", dc1, dc2);
+		return -EINVAL;
+	}
+
+	info->cpu_vol = cpu_vol;
+
+	return is_vdd ? cpu_vol->vdd : cpu_vol->vddm;
+}
+
+static int apcpu_get_vdd_voltage(struct regulator_dev *reg)
+{
+	return apcpu_get_voltage(reg, true);
+}
+
+static int apcpu_get_vddm_voltage(struct regulator_dev *reg)
+{
+	return apcpu_get_voltage(reg, false);
+}
+
+static const struct regulator_ops regu_common_ops = {
+	.enable =        aon_regu_enable,
+	.disable =       aon_regu_disable,
+	.is_enabled =    aon_regu_is_enabled,
+	.list_voltage =  regulator_list_voltage_linear,
+	.set_voltage =   aon_regu_set_voltage,
+	.get_voltage =   aon_regu_get_voltage,
+};
+static const struct regulator_ops apcpu_dvdd_ops = {
+	.enable =        aon_regu_dummy_enable,
+	.disable =       aon_regu_dummy_disable,
+	.is_enabled =    aon_regu_dummy_is_enabled,
+	.list_voltage =  regulator_list_voltage_linear,
+	.set_voltage =   apcpu_set_vdd_vddm_voltage,
+	.get_voltage =   apcpu_get_vdd_voltage,
+};
+
+static const struct regulator_ops apcpu_dvddm_ops = {
+	.enable =        aon_regu_dummy_enable,
+	.disable =       aon_regu_dummy_disable,
+	.is_enabled =    aon_regu_dummy_is_enabled,
+	.list_voltage =  regulator_list_voltage_linear,
+	.set_voltage =   apcpu_set_vddm_voltage,
+	.get_voltage =   apcpu_get_vddm_voltage,
+};
+
+/* Macros for voltage DC/DC converters (BUCKs) for cpu */
+#define REGU_DSC_DEF(regu_id, of_math_name) \
+	.id = regu_id, \
+	.name = #regu_id, \
+	.of_match = of_match_ptr(__stringify(of_math_name)), \
+	.ops = &regu_common_ops, \
+	.type = REGULATOR_VOLTAGE, \
+	.owner = THIS_MODULE
+
+#define BUCK_APCPU_DVDD(regu_id,min_mV, step_mV, max_mV) \
+	.id = regu_id, \
+	.name = "APCPU_DVDD", \
+	.of_match = of_match_ptr("appcpu_dvdd"), \
+	.ops = &apcpu_dvdd_ops, \
+	.min_uV = (min_mV), \
+	.uV_step = (step_mV), \
+	.n_voltages = ((max_mV) - (min_mV))/(step_mV) + 1, \
+	.type = REGULATOR_VOLTAGE, \
+	.owner = THIS_MODULE
+
+#define BUCK_APCPU_DVDDM(regu_id, min_mV, step_mV, max_mV) \
+	.id = regu_id, \
+	.name = "APCPU_DVDDM", \
+	.of_match = of_match_ptr("appcpu_dvddm"), \
+	.ops = &apcpu_dvddm_ops, \
+	.min_uV = (min_mV) , \
+	.uV_step = (step_mV), \
+	.n_voltages = ((max_mV) - (min_mV))/(step_mV) + 1, \
+	.type = REGULATOR_VOLTAGE, \
+	.owner = THIS_MODULE
+
+/* regulator desc for dialog */
+static struct regulator_desc light_dialog_ant_regu_desc[] = {
+	/*cpu vdd vddm regulators, used to adjust vol dynamicaly */
+	{
+		BUCK_APCPU_DVDD(SOC_APCPU_DVDD_DVDDM, 300000, 10000, 1570000),
+	},
+	{
+		BUCK_APCPU_DVDDM(SOC_APCPU_DVDD_DVDDM, 300000, 10000, 1570000),
+	},
+
+	/*common regu ,no need to adjust vol dynamicaly */
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AON,soc_dvdd18_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD33_USB3,soc_avdd33_usb3),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AON,soc_dvdd08_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_DDR,soc_dvdd08_ddr),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V8,soc_vdd_ddr_1v8),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V1,soc_vdd_ddr_1v1),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_0V6,soc_vdd_ddr_0v6),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AP,soc_dvdd18_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AP,soc_dvdd08_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD08_MIPI_HDMI,soc_avdd08_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD18_MIPI_HDMI,soc_avdd18_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD33_EMMC,soc_dvdd33_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_EMMC,soc_dvdd18_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_DOVDD18_SCAN,soc_dovdd18_scan),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD12_SCAN,soc_dvdd12_scan),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD28_SCAN_EN,soc_avdd28_scan_en),
+	},
+};
+
+static struct regulator_desc light_dialog_regu_desc[] = {
+	/*cpu vdd vddm regulators, used to adjust vol dynamicaly */
+	{
+		BUCK_APCPU_DVDD(SOC_APCPU_DVDD_DVDDM, 300000, 10000, 1570000),
+	},
+	{
+		BUCK_APCPU_DVDDM(SOC_APCPU_DVDD_DVDDM, 300000, 10000, 1570000),
+	},
+
+	/*common regu ,no need to adjust vol dynamicaly */
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AON,soc_dvdd18_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD33_USB3,soc_avdd33_usb3),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AON,soc_dvdd08_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_DDR,soc_dvdd08_ddr),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V8,soc_vdd_ddr_1v8),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V1,soc_vdd_ddr_1v1),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_0V6,soc_vdd_ddr_0v6),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AP,soc_dvdd18_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AP,soc_dvdd08_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD08_MIPI_HDMI,soc_avdd08_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD18_MIPI_HDMI,soc_avdd18_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD33_EMMC,soc_dvdd33_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_EMMC,soc_dvdd18_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_DOVDD18_SCAN,soc_dovdd18_scan),
+	},
+	{
+		REGU_DSC_DEF(SOC_VEXT_2V8,soc_vext_2v8),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD12_SCAN,soc_dvdd12_scan),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD28_SCAN_EN,soc_avdd28_scan_en),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD28_RGB,soc_avdd28_rgb),
+	},
+	{
+		REGU_DSC_DEF(SOC_DOVDD18_RGB,soc_dovdd18_rgb),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD12_RGB,soc_dvdd12_rgb),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD25_IR,soc_avdd25_ir),
+	},
+	{
+		REGU_DSC_DEF(SOC_DOVDD18_IR,soc_dovdd18_ir),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD12_IR,soc_dvdd12_ir),
+	},
+};
+
+/* regulator desc for ricoh */
+static struct regulator_desc light_ricoh_regu_desc[] = {
+    /*cpu vdd vddm regulators, used to adjust vol dynamicaly */
+	{
+		BUCK_APCPU_DVDD(SOC_APCPU_DVDD_DVDDM, 600000, 12500, 1500000),
+	},
+	{
+		BUCK_APCPU_DVDDM(SOC_APCPU_DVDD_DVDDM, 600000, 12500, 1500000),
+	},
+
+	/*common regu ,no need to adjust vol dynamicaly */
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AON,soc_dvdd18_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD33_USB3,soc_avdd33_usb3),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AON,soc_dvdd08_aon),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_DDR,soc_dvdd08_ddr),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V8,soc_vdd_ddr_1v8),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_1V1,soc_vdd_ddr_1v1),
+	},
+	{
+		REGU_DSC_DEF(SOC_VDD_DDR_0V6,soc_vdd_ddr_0v6),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_AP,soc_dvdd18_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD08_AP,soc_dvdd08_ap),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD08_MIPI_HDMI,soc_avdd08_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_AVDD18_MIPI_HDMI,soc_avdd18_mipi_hdmi),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD33_EMMC,soc_dvdd33_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_DVDD18_EMMC,soc_dvdd18_emmc),
+	},
+	{
+		REGU_DSC_DEF(SOC_LCD0_EN,soc_lcd0_en),
+	},
+	{
+		REGU_DSC_DEF(SOC_VEXT_1V8,soc_vext_1v8),
+	},
+};
+
+#define GEN_REGISTER_SHOW(x, y)	\
+static ssize_t x##_registers_show(struct device *dev,				\
+				     struct device_attribute *attr,		\
+				     char *buf)					\
+{										\
+	struct platform_device *pdev = to_platform_device(dev);			\
+	struct aon_regu_info *info = platform_get_drvdata(pdev);	\
+	u32 dc1, dc2;								\
+	ssize_t ret;								\
+										\
+	ret = aon_get_regulator(light_aon_pmic_info.ipc_handle, y,		\
+				       &dc1, &dc2, 0);				\
+	if (ret) {								\
+		dev_err(info->dev, "failed to get Voltages!\n");		\
+		return -EINVAL;							\
+	}									\
+										\
+	ret = sprintf(buf, "%u\n", dc1);					\
+	return ret;								\
+}
+
+#define GEN_REGISTER_STORE(x, y)	\
+static ssize_t x##_register_store(struct device *dev,			\
+				      struct device_attribute *attr,		\
+				      const char *buf, size_t count)		\
+{										\
+	struct platform_device *pdev = to_platform_device(dev);			\
+	struct aon_regu_info *info = platform_get_drvdata(pdev);	\
+	unsigned long dc1, dc2 = 0;						\
+	int err;								\
+										\
+	if (kstrtoul(buf, 0, &dc1))						\
+		return -EINVAL;							\
+										\
+	err = aon_set_regulator(light_aon_pmic_info.ipc_handle, y,		\
+				       dc1, dc2, 0);				\
+	if (err) {								\
+		dev_err(info->dev, "failed to set Voltages to [%lu]!\n", dc1);	\
+		return -EINVAL;							\
+	}									\
+										\
+	return count;								\
+}
+
+static ssize_t soc_apcpu_dvdd_dvddm_registers_show(struct device *dev,
+				struct device_attribute *attr, char *buf)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct aon_regu_info *info = platform_get_drvdata(pdev);
+	size_t bufpos = 0, count = 26;
+	const struct apcpu_vol_set *cpu_vol;
+	u32 dc1, dc2;
+	int i = 0;
+	int err;
+	err = aon_get_regulator(light_aon_pmic_info.ipc_handle, SOC_APCPU_DVDD_DVDDM,
+				       &dc1, &dc2, 1);
+	if (err) {
+		dev_err(info->dev, "failed to get Voltages!\n");
+		return -EINVAL;
+	}
+	cpu_vol = apcpu_get_matched_signed_off_voltage(dc1, dc2);
+	if (!cpu_vol)
+		dev_err(info->dev, "Read [%d:%d] is not existing in matching table\n", dc1, dc2);
+	snprintf(buf + bufpos, count - bufpos, "%.*x: ", 2, i);
+	bufpos += 4;
+	snprintf(buf + bufpos, count - bufpos, "%u", dc1);
+	bufpos += 8;
+	buf[bufpos++] = '\n';
+	i++;
+	snprintf(buf + bufpos, count - bufpos, "%.*x: ", 2, i);
+	bufpos += 4;
+	snprintf(buf + bufpos, count - bufpos, "%u", dc2);
+	bufpos += 8;
+	buf[bufpos++] = '\n';
+	return bufpos;
+}
+static ssize_t soc_apcpu_dvdd_dvddm_register_store(struct device *dev,
+				 struct device_attribute *attr,
+				 const char *buf, size_t size)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct aon_regu_info *info = platform_get_drvdata(pdev);
+	const struct apcpu_vol_set *cpu_vol;
+	char *start = (char *)buf;
+	unsigned long dc1, dc2;
+	int err;
+	while (*start == ' ')
+		start++;
+	dc1 = simple_strtoul(start, &start, 0);
+	while (*start == ' ')
+		start++;
+	if (kstrtoul(start, 0, &dc2))
+		return -EINVAL;
+	cpu_vol = apcpu_get_matched_signed_off_voltage(dc1, dc2);
+	if (!cpu_vol) {
+		dev_err(info->dev, "failed to find bcore1/bcore2 matching table\n");
+#ifndef CONFIG_AON_REG_DEBUG
+		return -EINVAL;
+#endif
+	}
+	info->cpu_vol = cpu_vol;
+	info->vddm = cpu_vol->vddm;
+	err = aon_set_regulator(light_aon_pmic_info.ipc_handle, SOC_APCPU_DVDD_DVDDM,
+				       dc1, dc2, 1);
+	if (err) {
+		dev_err(info->dev, "failed to set Voltages to [%lu,%lu]!\n", dc1, dc2);
+#ifndef CONFIG_AON_REG_DEBUG
+		return -EINVAL;
+#endif
+	}
+	return size;
+}
+
+GEN_REGISTER_SHOW(soc_dvdd18_aon, SOC_DVDD18_AON)
+GEN_REGISTER_STORE(soc_dvdd18_aon, SOC_DVDD18_AON)
+GEN_REGISTER_SHOW(soc_dvdd08_ap, SOC_DVDD08_AP)
+GEN_REGISTER_STORE(soc_dvdd08_ap, SOC_DVDD08_AP)
+GEN_REGISTER_SHOW(soc_dvdd18_emmc, SOC_DVDD18_EMMC)
+GEN_REGISTER_STORE(soc_dvdd18_emmc, SOC_DVDD18_EMMC)
+GEN_REGISTER_SHOW(soc_dvdd33_emmc, SOC_DVDD33_EMMC)
+GEN_REGISTER_STORE(soc_dvdd33_emmc, SOC_DVDD33_EMMC)
+
+static DEVICE_ATTR(soc_dvdd18_aon_regs, 0644, soc_dvdd18_aon_registers_show, soc_dvdd18_aon_register_store);
+static DEVICE_ATTR(soc_dvdd08_ap_regs, 0644, soc_dvdd08_ap_registers_show, soc_dvdd08_ap_register_store);
+static DEVICE_ATTR(soc_dvdd33_emmc_regs, 0644, soc_dvdd33_emmc_registers_show, soc_dvdd33_emmc_register_store);
+static DEVICE_ATTR(soc_dvdd18_emmc_regs, 0644, soc_dvdd18_emmc_registers_show, soc_dvdd18_emmc_register_store);
+static DEVICE_ATTR(soc_apcpu_dvdd_dvddm_regs, 0644, soc_apcpu_dvdd_dvddm_registers_show, soc_apcpu_dvdd_dvddm_register_store);
+
+static struct attribute *aon_regs_sysfs_entries[] = {
+	&dev_attr_soc_dvdd18_aon_regs.attr,
+	&dev_attr_soc_dvdd08_ap_regs.attr,
+	&dev_attr_soc_dvdd33_emmc_regs.attr,
+	&dev_attr_soc_dvdd18_emmc_regs.attr,
+	&dev_attr_soc_apcpu_dvdd_dvddm_regs.attr,
+	NULL
+};
+static const struct attribute_group dev_attr_aon_regs_group = {
+	.attrs = aon_regs_sysfs_entries,
+};
+
+
+static const struct aon_regu_desc light_dialog_regus = {
+    .regu_desc = (struct regulator_desc*) &light_dialog_regu_desc,
+    .regu_num  = ARRAY_SIZE(light_dialog_regu_desc),
+};
+
+static const struct aon_regu_desc light_dialog_ant_regus = {
+    .regu_desc = (struct regulator_desc*) &light_dialog_ant_regu_desc,
+    .regu_num  = ARRAY_SIZE(light_dialog_ant_regu_desc),
+};
+
+static const struct aon_regu_desc light_ricoh_regus = {
+    .regu_desc = (struct regulator_desc*)&light_ricoh_regu_desc,
+    .regu_num  = ARRAY_SIZE(light_ricoh_regu_desc),
+};
+
+static int light_aon_regulator_probe(struct platform_device *pdev)
+{
+	struct device_node *np = pdev->dev.of_node;
+	struct regulator_config config = { };
+	int i;
+	int ret;
+	struct aon_regu_desc *regus_set = NULL;
+
+	if (!np)
+		return -ENODEV;
+
+	regus_set = (struct aon_regu_desc*)of_device_get_match_data(&pdev->dev);
+	if (!regus_set) {
+		return -ENODEV;
+	}
+
+	/*get ipc handle */
+	ret = light_aon_get_handle(&(light_aon_pmic_info.ipc_handle));
+	if (ret) {
+		dev_err(&pdev->dev, "failed to get ipc_handle\n");
+		return ret;
+	}
+
+	/*init private drv data */
+	light_aon_pmic_info.dev = &pdev->dev;
+	light_aon_pmic_info.regu_desc = regus_set;
+	light_aon_pmic_info.cpu_vol = &apcpu_volts[2]; /* pmic default voltages */
+	light_aon_pmic_info.vddm = light_aon_pmic_info.cpu_vol->vddm;
+
+	/*register all regulators*/
+	config.dev = &pdev->dev;
+	config.driver_data = &light_aon_pmic_info;
+	for (i = 0; i < regus_set->regu_num; i++) {
+		struct regulator_dev *rdev;
+		struct regulator_desc *desc;
+
+		desc = &regus_set->regu_desc[i];
+		rdev = devm_regulator_register(&pdev->dev, desc, &config);
+		if (IS_ERR(rdev)) {
+			dev_err(&pdev->dev,
+				"Failed to initialize regulator-%d\n", i);
+			return PTR_ERR(rdev);
+		}
+	}
+
+	i = sysfs_create_group(&config.dev->kobj, &dev_attr_aon_regs_group);
+	if (i) {
+		dev_err(&pdev->dev, "Failed to create aon regs debug sysfs.\n");
+		return i;
+	}
+
+	platform_set_drvdata(pdev, &light_aon_pmic_info);
+
+	return 0;
+}
+
+static const struct of_device_id light_pmic_dev_id[] = {
+	{ .compatible = "thead,light-dialog-pmic-ant", .data = &light_dialog_ant_regus},
+	{ .compatible = "thead,light-dialog-pmic", .data = &light_dialog_regus},
+	{ .compatible = "thead,light-ricoh-pmic",  .data = &light_ricoh_regus},
+	{},
+};
+MODULE_DEVICE_TABLE(of, light_pmic_dev_id);
+
+static struct platform_driver light_aon_regulator_driver = {
+	.driver = {
+		   .name = "light-aon-reg",
+		   .owner = THIS_MODULE,
+		   .of_match_table = light_pmic_dev_id,
+	},
+	.probe = light_aon_regulator_probe,
+};
+
+module_platform_driver(light_aon_regulator_driver);
+
+MODULE_AUTHOR("fugang.duan <duanfugang.dfg@linux.alibaba.com>");
+MODULE_AUTHOR("linghui.zlh <linghui.zlh@linux.alibaba.com>");
+MODULE_DESCRIPTION("Thead Light Aon regulator virtual driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/reset/Kconfig b/drivers/reset/Kconfig
index ccd59ddd7610..ec69e6bbba6e 100644
--- a/drivers/reset/Kconfig
+++ b/drivers/reset/Kconfig
@@ -253,6 +253,16 @@ config RESET_SUNXI
 	help
 	  This enables the reset driver for Allwinner SoCs.
 
+config RESET_TH1520
+	bool "TH1520 Reset Driver"
+	depends on (ARCH_THEAD || COMPILE_TEST) && OF
+	select MFD_SYSCON
+	default ARCH_THEAD
+	help
+	  Support for the T-HEAD 1520 RISC-V SoC reset controller.
+	  Say Y if you want to control reset signals provided by this
+	  controller.
+
 config RESET_TI_SCI
 	tristate "TI System Control Interface (TI-SCI) reset driver"
 	depends on TI_SCI_PROTOCOL || (COMPILE_TEST && TI_SCI_PROTOCOL=n)
diff --git a/drivers/reset/Makefile b/drivers/reset/Makefile
index 8270da8a4baa..ca0abdce468d 100644
--- a/drivers/reset/Makefile
+++ b/drivers/reset/Makefile
@@ -33,6 +33,8 @@ obj-$(CONFIG_RESET_SIMPLE) += reset-simple.o
 obj-$(CONFIG_RESET_SOCFPGA) += reset-socfpga.o
 obj-$(CONFIG_RESET_SUNPLUS) += reset-sunplus.o
 obj-$(CONFIG_RESET_SUNXI) += reset-sunxi.o
+obj-$(CONFIG_ARCH_SOPHGO) += reset-sophgo.o
+obj-$(CONFIG_RESET_TH1520) += reset-th1520.o
 obj-$(CONFIG_RESET_TI_SCI) += reset-ti-sci.o
 obj-$(CONFIG_RESET_TI_SYSCON) += reset-ti-syscon.o
 obj-$(CONFIG_RESET_TI_TPS380X) += reset-tps380x.o
diff --git a/drivers/reset/reset-sophgo.c b/drivers/reset/reset-sophgo.c
new file mode 100644
index 000000000000..3c46a43e24ba
--- /dev/null
+++ b/drivers/reset/reset-sophgo.c
@@ -0,0 +1,163 @@
+/*
+ * Sophgo SoCs Reset Controller driver
+ *
+ * Copyright (c) 2018 Bitmain Ltd.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/reset-controller.h>
+#include <linux/slab.h>
+#include <linux/spinlock.h>
+#include <linux/types.h>
+#include <linux/of_device.h>
+#include <linux/mfd/syscon.h>
+#include <linux/regmap.h>
+
+#define BITS_PER_REG	32
+
+struct bm_reset_data {
+	spinlock_t			lock;
+	void __iomem			*membase;
+	struct reset_controller_dev	rcdev;
+	struct regmap		*syscon_rst;
+	u32			top_rst_offset;
+};
+
+static int bm_reset_assert(struct reset_controller_dev *rcdev,
+			      unsigned long id)
+{
+	struct bm_reset_data *data = container_of(rcdev,
+						     struct bm_reset_data,
+						     rcdev);
+	int bank = id / BITS_PER_REG;
+	int offset = id % BITS_PER_REG;
+	unsigned long flags;
+	u32 reg;
+
+	spin_lock_irqsave(&data->lock, flags);
+
+	regmap_read(data->syscon_rst, data->top_rst_offset + (bank * 4),
+		&reg);
+	regmap_write(data->syscon_rst, data->top_rst_offset + (bank * 4),
+		reg & ~BIT(offset));
+
+	spin_unlock_irqrestore(&data->lock, flags);
+
+	return 0;
+}
+
+static int bm_reset_deassert(struct reset_controller_dev *rcdev,
+				unsigned long id)
+{
+	struct bm_reset_data *data = container_of(rcdev,
+						     struct bm_reset_data,
+						     rcdev);
+	int bank = id / BITS_PER_REG;
+	int offset = id % BITS_PER_REG;
+	unsigned long flags;
+	u32 reg;
+
+	spin_lock_irqsave(&data->lock, flags);
+
+	regmap_read(data->syscon_rst, data->top_rst_offset + (bank * 4),
+		&reg);
+	regmap_write(data->syscon_rst,  data->top_rst_offset + (bank * 4),
+		reg | BIT(offset));
+
+	spin_unlock_irqrestore(&data->lock, flags);
+
+	return 0;
+}
+
+static const struct reset_control_ops bm_reset_ops = {
+	.assert		= bm_reset_assert,
+	.deassert	= bm_reset_deassert,
+};
+
+static const struct of_device_id bm_reset_dt_ids[] = {
+	 { .compatible = "bitmain,reset", },
+	 { /* sentinel */ },
+};
+MODULE_DEVICE_TABLE(of, bm_reset_dt_ids);
+
+static int bm_reset_probe(struct platform_device *pdev)
+{
+	struct bm_reset_data *data;
+	int ret = 0;
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node, *np_top;
+	static struct regmap *syscon;
+
+	data = devm_kzalloc(&pdev->dev, sizeof(*data), GFP_KERNEL);
+	if (!data)
+		return -ENOMEM;
+
+	np_top = of_parse_phandle(np, "subctrl-syscon", 0);
+	if (!np_top) {
+		dev_err(dev, "%s can't get subctrl-syscon node\n", __func__);
+		goto out_free_devm;
+	}
+
+	syscon = syscon_node_to_regmap(np_top);
+	if (IS_ERR(syscon)) {
+		dev_err(dev, "cannot get regmap\n");
+		goto out_free_devm;
+	}
+
+	data->syscon_rst = syscon;
+	ret = device_property_read_u32(&pdev->dev, "top_rst_offset",
+		&data->top_rst_offset);
+	if (ret < 0) {
+		dev_err(dev, "cannot get top_rst_offset\n");
+		goto out_free_devm;
+	}
+
+	ret = device_property_read_u32(&pdev->dev, "nr_resets",
+		&data->rcdev.nr_resets);
+	if (ret < 0) {
+		dev_err(dev, "cannot get nr_resets\n");
+		goto out_free_devm;
+	}
+
+	spin_lock_init(&data->lock);
+
+	data->rcdev.owner = THIS_MODULE;
+	data->rcdev.ops = &bm_reset_ops;
+	data->rcdev.of_node = pdev->dev.of_node;
+
+	ret = devm_reset_controller_register(&pdev->dev, &data->rcdev);
+	if (!ret)
+		return 0;
+
+out_free_devm:
+	devm_kfree(&pdev->dev, data);
+	return ret;
+}
+
+static struct platform_driver bm_reset_driver = {
+	.probe	= bm_reset_probe,
+	.driver = {
+		.name		= "bm-reset",
+		.of_match_table	= bm_reset_dt_ids,
+	},
+};
+
+static int __init bm_reset_init(void)
+{
+	return platform_driver_register(&bm_reset_driver);
+}
+postcore_initcall(bm_reset_init);
+
+MODULE_AUTHOR("Wei Huang<wei.huang01@bitmain.com>");
+MODULE_DESCRIPTION("Bitmain SoC Reset Controoler Driver");
+MODULE_LICENSE("GPL");
diff --git a/drivers/reset/reset-th1520.c b/drivers/reset/reset-th1520.c
new file mode 100644
index 000000000000..5a89d201fc0c
--- /dev/null
+++ b/drivers/reset/reset-th1520.c
@@ -0,0 +1,109 @@
+// SPDX-License-Identifier: GPL-2.0-only
+
+#include <linux/mfd/syscon.h>
+#include <linux/of_device.h>
+#include <linux/platform_device.h>
+#include <linux/reset-controller.h>
+#include <linux/regmap.h>
+#include <dt-bindings/reset/thead,th1520-reset.h>
+
+struct th1520_rst_signal {
+	unsigned int offset, bit;
+};
+
+struct th1520_rst {
+	struct reset_controller_dev rcdev;
+	struct regmap *regmap;
+	const struct th1520_rst_signal *signals;
+};
+
+enum th1520_rst_registers {
+	RST_WDT0 = 0x0034,
+	RST_WDT1 = 0x0038,
+};
+
+static int th1520_reset_update(struct th1520_rst *rst, unsigned long id,
+			       unsigned int value)
+{
+	const struct th1520_rst_signal *signal = &rst->signals[id];
+
+	return regmap_update_bits(rst->regmap, signal->offset, signal->bit,
+				  value);
+}
+
+static const struct th1520_rst_signal th1520_rst_signals[] = {
+	[TH1520_RESET_WDT0] = { RST_WDT0, BIT(0) },
+	[TH1520_RESET_WDT1] = { RST_WDT1, BIT(0) },
+};
+
+static struct th1520_rst *to_th1520_rst(struct reset_controller_dev *rcdev)
+{
+	return container_of(rcdev, struct th1520_rst, rcdev);
+}
+
+static int th1520_reset_set(struct reset_controller_dev *rcdev,
+			    unsigned long id, bool assert)
+{
+	struct th1520_rst *rst = to_th1520_rst(rcdev);
+	const unsigned int bit = rst->signals[id].bit;
+	unsigned int value = assert ? bit : 0;
+
+	return th1520_reset_update(rst, id, value);
+}
+
+static int th1520_reset_assert(struct reset_controller_dev *rcdev,
+			       unsigned long id)
+{
+	return th1520_reset_set(rcdev, id, false);
+}
+
+static int th1520_reset_deassert(struct reset_controller_dev *rcdev,
+				 unsigned long id)
+{
+	return th1520_reset_set(rcdev, id, true);
+}
+
+static const struct reset_control_ops th1520_rst_ops = {
+	.assert = th1520_reset_assert,
+	.deassert = th1520_reset_deassert,
+};
+
+static int th1520_reset_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct th1520_rst *rst;
+	struct regmap_config config = { .name = "rst" };
+
+	rst = devm_kzalloc(dev, sizeof(*rst), GFP_KERNEL);
+	if (!rst)
+		return -ENOMEM;
+
+	rst->signals = th1520_rst_signals;
+	rst->regmap = syscon_node_to_regmap(dev->of_node);
+	if (IS_ERR(rst->regmap))
+		return PTR_ERR(rst->regmap);
+
+	regmap_attach_dev(dev, rst->regmap, &config);
+
+	rst->rcdev.owner = THIS_MODULE;
+	rst->rcdev.dev = dev;
+	rst->rcdev.of_node = dev->of_node;
+	rst->rcdev.ops = &th1520_rst_ops;
+	rst->rcdev.nr_resets = ARRAY_SIZE(th1520_rst_signals);
+
+	return devm_reset_controller_register(dev, &rst->rcdev);
+}
+
+static const struct of_device_id th1520_reset_dt_ids[] = {
+	{ .compatible = "thead,th1520-reset" },
+	{ /* sentinel */ },
+};
+
+static struct platform_driver th1520_reset_driver = {
+	.probe	= th1520_reset_probe,
+	.driver = {
+		.name		= "th1520-reset",
+		.of_match_table	= th1520_reset_dt_ids,
+	},
+};
+builtin_platform_driver(th1520_reset_driver);
diff --git a/drivers/rpmsg/Kconfig b/drivers/rpmsg/Kconfig
index d3795860f5c0..34e4d97766c3 100644
--- a/drivers/rpmsg/Kconfig
+++ b/drivers/rpmsg/Kconfig
@@ -74,6 +74,10 @@ config RPMSG_QCOM_SMD
 	  providing communication channels to remote processors in Qualcomm
 	  platforms.
 
+config RPMSG_THEAD_LIGHT
+        tristate "THEAD Light RPM Driver"
+        depends on RPMSG
+
 config RPMSG_VIRTIO
 	tristate "Virtio RPMSG bus driver"
 	depends on HAS_DMA
diff --git a/drivers/rpmsg/Makefile b/drivers/rpmsg/Makefile
index 58e3b382e316..35c46c704a7c 100644
--- a/drivers/rpmsg/Makefile
+++ b/drivers/rpmsg/Makefile
@@ -10,3 +10,4 @@ obj-$(CONFIG_RPMSG_QCOM_GLINK_RPM) += qcom_glink_rpm.o
 obj-$(CONFIG_RPMSG_QCOM_GLINK_SMEM) += qcom_glink_smem.o
 obj-$(CONFIG_RPMSG_QCOM_SMD)	+= qcom_smd.o
 obj-$(CONFIG_RPMSG_VIRTIO)	+= virtio_rpmsg_bus.o
+obj-$(CONFIG_RPMSG_THEAD_LIGHT) += light_rpmsg.o
diff --git a/drivers/rpmsg/light_rpmsg.c b/drivers/rpmsg/light_rpmsg.c
new file mode 100644
index 000000000000..cecda6e251a9
--- /dev/null
+++ b/drivers/rpmsg/light_rpmsg.c
@@ -0,0 +1,864 @@
+/*
+ * Copyright (C) 2023 Alibaba Group Holding Limited.
+ *
+ * derived from the omap-rpmsg implementation.
+ *
+ * The code contained herein is licensed under the GNU General Public
+ * License. You may obtain a copy of the GNU General Public License
+ * Version 2 or later at the following locations:
+ *
+ * http://www.opensource.org/licenses/gpl-license.html
+ * http://www.gnu.org/copyleft/gpl.html
+ */
+
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/init.h>
+#include <linux/interrupt.h>
+#include <linux/module.h>
+#include <linux/notifier.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/of_device.h>
+#include <linux/of_irq.h>
+#include <linux/platform_device.h>
+#include <linux/rpmsg.h>
+#include <linux/slab.h>
+#include <linux/virtio.h>
+#include <linux/virtio_config.h>
+#include <linux/virtio_ids.h>
+#include <linux/virtio_ring.h>
+#include <linux/light_rpmsg.h>
+#include <linux/delay.h>
+#include <linux/regmap.h>
+#include <linux/mfd/syscon.h>
+#include <linux/debugfs.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/mailbox_client.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/uaccess.h>
+#include <linux/workqueue.h>
+#include <linux/light_rpmsg.h>
+
+#define MBOX_MAX_MSG_LEN	28
+#define WJ_MBOX_SEND_MAX_MESSAGE_LENGTH 28
+#define HEXDUMP_BYTES_PER_LINE	28
+#define HEXDUMP_LINE_LEN	((HEXDUMP_BYTES_PER_LINE * 4) + 2)
+#define HEXDUMP_MAX_LEN		(HEXDUMP_LINE_LEN *		\
+				(MBOX_MAX_MSG_LEN / HEXDUMP_BYTES_PER_LINE))
+
+//extern struct light_rpmsg_vproc *pri_rpdev;
+static struct dentry *root_debugfs_dir;
+
+struct mbox_client_light_device {
+	struct device		*dev;
+	void __iomem		*tx_mmio;
+	void __iomem		*rx_mmio;
+	struct mbox_chan	*tx_channel;
+	struct mbox_chan	*rx_channel;
+	char			*rx_buffer;
+	struct regmap 		*audio_mbox_regmap;
+	char	*message;
+	spinlock_t		lock;
+};
+
+struct mbox_client_light_device *tdev_priv;
+
+static volatile uint32_t *p_mbox_reg;
+static volatile uint32_t *p_mbox_reg1;
+static volatile uint32_t *p_mbox_reg2;
+
+/*
+ * For now, allocate 256 buffers of 512 bytes for each side. each buffer
+ * will then have 16B for the msg header and 496B for the payload.
+ * This will require a total space of 256KB for the buffers themselves, and
+ * 3 pages for every vring (the size of the vring depends on the number of
+ * buffers it supports).
+ */
+#define RPMSG_NUM_BUFS		(512)
+//#define RPMSG_BUF_SIZE		(512)
+//#define RPMSG_BUFS_SPACE	(RPMSG_NUM_BUFS * RPMSG_BUF_SIZE)
+
+/*
+ * The alignment between the consumer and producer parts of the vring.
+ * Note: this is part of the "wire" protocol. If you change this, you need
+ * to update your BIOS image as well
+ */
+#define RPMSG_VRING_ALIGN	(4096)
+
+/* With 256 buffers, our vring will occupy 3 pages */
+#define RPMSG_RING_SIZE	((DIV_ROUND_UP(vring_size(RPMSG_NUM_BUFS / 2, \
+				RPMSG_VRING_ALIGN), PAGE_SIZE)) * PAGE_SIZE)
+
+#define to_light_virdev(vd) container_of(vd, struct light_virdev, vdev)
+#define to_light_rpdev(vd, id) container_of(vd, struct light_rpmsg_vproc, ivdev[id])
+
+struct light_rpmsg_vq_info {
+	__u16 num;	/* number of entries in the virtio_ring */
+	__u16 vq_id;	/* a globaly unique index of this virtqueue */
+	void *addr;	/* address where we mapped the virtio ring */
+	struct light_rpmsg_vproc *rpdev;
+};
+
+static u64 light_rpmsg_get_features(struct virtio_device *vdev)
+{
+	/* VIRTIO_RPMSG_F_NS has been made private */
+	return 1 << 0;
+}
+
+static int light_rpmsg_finalize_features(struct virtio_device *vdev)
+{
+	/* Give virtio_ring a chance to accept features */
+	vring_transport_features(vdev);
+	return 0;
+}
+
+/* kick the remote processor, and let it know which virtqueue to poke at */
+static bool light_rpmsg_notify(struct virtqueue *vq)
+{
+	unsigned int mu_rpmsg = 0;
+	int ret;
+	struct light_rpmsg_vq_info *rpvq = vq->priv;
+
+#ifdef CONFIG_PM_SLEEP
+    if(rpvq->rpdev->sleep_flag) {
+        dev_err(tdev_priv->dev, "dev in deep sleep, Channel cannot do Tx+++\n");
+		return -EINVAL;
+	}
+#endif
+
+	mu_rpmsg = rpvq->vq_id << 16;
+	mutex_lock(&rpvq->rpdev->lock);
+
+	//pr_info("light rpmsg: notify %d\n", rpvq->rpdev->first_notify);
+	if (unlikely(rpvq->rpdev->first_notify > 0)) {
+		rpvq->rpdev->first_notify--;
+        if (!tdev_priv->tx_channel) {
+            dev_err(tdev_priv->dev, "Channel cannot do Tx+++\n");
+            return -EINVAL;
+        }
+
+        ret = mbox_send_message(tdev_priv->tx_channel, "Hello, Queue!");
+	} else {
+		*p_mbox_reg1 |= 1 << 0;
+		*p_mbox_reg2 |= 1 << 0;
+	}
+	mutex_unlock(&rpvq->rpdev->lock);
+
+	return true;
+}
+
+static int light_mu_rpmsg_callback(struct notifier_block *this,
+					unsigned long index, void *data)
+{
+	u32 mu_msg = (phys_addr_t) data;
+	struct light_virdev *virdev;
+
+	virdev = container_of(this, struct light_virdev, nb);
+
+	pr_debug("light rpmsg: %s notifier_call mu_msg: 0x%x\n", __func__, mu_msg);
+	/* ignore vq indices which are clearly not for us */
+	mu_msg = mu_msg >> 16;
+	if (mu_msg < virdev->base_vq_id || mu_msg > virdev->base_vq_id + 1) {
+		pr_debug("light rpmsg: mu_msg 0x%x is invalid\n", mu_msg);
+		//return NOTIFY_DONE;
+	}
+
+	mu_msg -= virdev->base_vq_id;
+	pr_debug("%smu_msg 0x%xbase_vq_id 0x%xvirdev num_of_vqs0x%x\n", __func__, mu_msg, virdev->base_vq_id, virdev->num_of_vqs);
+
+	/*
+	 * Currently both PENDING_MSG and explicit-virtqueue-index
+	 * messaging are supported.
+	 * Whatever approach is taken, at this point 'mu_msg' contains
+	 * the index of the vring which was just triggered.
+	 */
+	//if (mu_msg < virdev->num_of_vqs)
+		vring_interrupt(mu_msg, virdev->vq[mu_msg]);
+
+	return NOTIFY_DONE;
+}
+
+static int light_mu_rpmsg_register_nb(struct light_rpmsg_vproc *rpdev,
+		struct notifier_block *nb)
+{
+	if ((rpdev == NULL) || (nb == NULL))
+		return -EINVAL;
+
+	blocking_notifier_chain_register(&(rpdev->notifier), nb);
+
+	return 0;
+}
+
+static int light_mu_rpmsg_unregister_nb(struct light_rpmsg_vproc *rpdev,
+		struct notifier_block *nb)
+{
+	if ((rpdev == NULL) || (nb == NULL))
+		return -EINVAL;
+
+	blocking_notifier_chain_unregister(&(rpdev->notifier), nb);
+
+	return 0;
+}
+
+static struct virtqueue *rp_find_vq(struct virtio_device *vdev,
+				    unsigned int index,
+				    void (*callback)(struct virtqueue *vq),
+				    const char *name,
+				    bool ctx)
+{
+	struct light_virdev *virdev = to_light_virdev(vdev);
+	struct light_rpmsg_vproc *rpdev = to_light_rpdev(virdev,
+						     virdev->base_vq_id / 2);
+	struct light_rpmsg_vq_info *rpvq;
+	struct virtqueue *vq;
+	int err;
+	//static void __iomem *brd_io;
+
+	rpvq = kmalloc(sizeof(*rpvq), GFP_KERNEL);
+	if (!rpvq)
+		return ERR_PTR(-ENOMEM);
+
+	/* ioremap'ing normal memory, so we cast away sparse's complaints */
+	//rpvq->addr = (__force void *) ioremap_nocache(virdev->vring[index],
+	//						RPMSG_RING_SIZE);
+	rpvq->addr = (__force void *) ioremap(virdev->vring[index],
+							RPMSG_RING_SIZE);
+	if (!rpvq->addr) {
+		err = -ENOMEM;
+		goto free_rpvq;
+	}
+
+	p_mbox_reg = ioremap(0xffefc48000,25);
+	p_mbox_reg1 = p_mbox_reg + 4;
+	p_mbox_reg2 = p_mbox_reg + 5;
+
+	memset_io(rpvq->addr, 0, RPMSG_RING_SIZE);
+
+	pr_debug("vring%d: phys 0x%x, virt 0x%p\n", index, virdev->vring[index],
+					rpvq->addr);
+
+	vq = vring_new_virtqueue(index, RPMSG_NUM_BUFS / 2, RPMSG_VRING_ALIGN,
+			vdev, true, ctx,
+			rpvq->addr,
+			light_rpmsg_notify, callback,
+			name);
+	if (!vq) {
+		pr_err("light rpmsg: vring_new_virtqueue failed\n");
+		err = -ENOMEM;
+		goto unmap_vring;
+	}
+
+	virdev->vq[index] = vq;
+	vq->priv = rpvq;
+	/* system-wide unique id for this virtqueue */
+	rpvq->vq_id = virdev->base_vq_id + index;
+	rpvq->rpdev = rpdev;
+	mutex_init(&rpdev->lock);
+
+	return vq;
+
+unmap_vring:
+	/* iounmap normal memory, so make sparse happy */
+	iounmap((__force void __iomem *) rpvq->addr);
+free_rpvq:
+	kfree(rpvq);
+	return ERR_PTR(err);
+}
+
+static void light_rpmsg_del_vqs(struct virtio_device *vdev)
+{
+	struct virtqueue *vq, *n;
+	struct light_virdev *virdev = to_light_virdev(vdev);
+	struct light_rpmsg_vproc *rpdev = to_light_rpdev(virdev,
+						     virdev->base_vq_id / 2);
+
+	list_for_each_entry_safe(vq, n, &vdev->vqs, list) {
+		struct light_rpmsg_vq_info *rpvq = vq->priv;
+
+		iounmap(rpvq->addr);
+		vring_del_virtqueue(vq);
+		kfree(rpvq);
+	}
+
+	if (&virdev->nb)
+		light_mu_rpmsg_unregister_nb(rpdev, &virdev->nb);
+}
+
+static int light_rpmsg_find_vqs(struct virtio_device *vdev, unsigned int nvqs,
+		       struct virtqueue *vqs[],
+		       vq_callback_t *callbacks[],
+		       const char * const names[],
+		       const bool *ctx,
+		       struct irq_affinity *desc)
+{
+	struct light_virdev *virdev = to_light_virdev(vdev);
+	struct light_rpmsg_vproc *rpdev = to_light_rpdev(virdev,
+						     virdev->base_vq_id / 2);
+	int i, err;
+
+	/* we maintain two virtqueues per remote processor (for RX and TX) */
+	if (nvqs != 2)
+		return -EINVAL;
+
+	for (i = 0; i < nvqs; ++i) {
+		vqs[i] = rp_find_vq(vdev, i, callbacks[i], names[i],
+				ctx ? ctx[i] : false);
+		if (IS_ERR(vqs[i])) {
+			err = PTR_ERR(vqs[i]);
+			goto error;
+		}
+	}
+
+	virdev->num_of_vqs = nvqs;
+
+	virdev->nb.notifier_call = light_mu_rpmsg_callback;
+	light_mu_rpmsg_register_nb(rpdev, &virdev->nb);
+
+	return 0;
+
+error:
+	light_rpmsg_del_vqs(vdev);
+	return err;
+}
+
+static void light_rpmsg_reset(struct virtio_device *vdev)
+{
+	dev_dbg(&vdev->dev, "reset!\n");
+}
+
+static u8 light_rpmsg_get_status(struct virtio_device *vdev)
+{
+	return 0;
+}
+
+static void light_rpmsg_set_status(struct virtio_device *vdev, u8 status)
+{
+	dev_dbg(&vdev->dev, "%s new status: %d\n", __func__, status);
+}
+
+static void light_rpmsg_vproc_release(struct device *dev)
+{
+	/* this handler is provided so driver core doesn't yell at us */
+}
+
+static struct virtio_config_ops light_rpmsg_config_ops = {
+	.get_features	= light_rpmsg_get_features,
+	.finalize_features = light_rpmsg_finalize_features,
+	.find_vqs	= light_rpmsg_find_vqs,
+	.del_vqs	= light_rpmsg_del_vqs,
+	.reset		= light_rpmsg_reset,
+	.set_status	= light_rpmsg_set_status,
+	.get_status	= light_rpmsg_get_status,
+};
+
+static struct light_rpmsg_vproc light_rpmsg_vprocs[] = {
+	{
+		.rproc_name	= "m4",
+	},
+	{
+		.rproc_name	= "m4",
+	},
+};
+
+static const struct of_device_id light_rpmsg_dt_ids[] = {
+	{ .compatible = "light,light-rpmsg", .data = (void *)LIGHT_RPMSG, },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, light_rpmsg_dt_ids);
+
+static int set_vring_phy_buf(struct platform_device *pdev,
+		       struct light_rpmsg_vproc *rpdev, int vdev_nums)
+{
+	struct resource *res;
+	resource_size_t size;
+	unsigned int start, end;
+	int i, ret = 0;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (res) {
+		size = resource_size(res);
+		start = res->start;
+		end = res->start + size;
+		for (i = 0; i < vdev_nums; i++) {
+			rpdev->ivdev[i].vring[0] = start;
+			rpdev->ivdev[i].vring[1] = start +
+						   0x8000;
+			start += 0x10000;
+			if (start > end) {
+				pr_err("Too small memory size %x!\n",
+						(u32)size);
+				ret = -EINVAL;
+				break;
+			}
+		}
+	} else {
+		return -ENOMEM;
+	}
+
+	return ret;
+}
+
+static void rpmsg_work_handler(struct work_struct *work)
+{
+	u32 message = 0;
+	struct delayed_work *dwork = to_delayed_work(work);
+	struct light_rpmsg_vproc *rpdev = container_of(dwork,
+			struct light_rpmsg_vproc, rpmsg_work);
+
+	//spin_lock_irqsave(&rpdev->mu_lock, flags);
+	blocking_notifier_call_chain(&(rpdev->notifier), 4,
+					(void *)(phys_addr_t)message);
+	//spin_unlock_irqrestore(&rpdev->mu_lock, flags);
+}
+
+struct light_rpmsg_vproc *pri_rpdev;
+EXPORT_SYMBOL_GPL(pri_rpdev);
+
+static int light_rpmsg_probe(struct platform_device *pdev)
+{
+	int core_id, j, ret = 0;
+	struct device *dev = &pdev->dev;
+	struct device_node *np = pdev->dev.of_node;
+	struct light_rpmsg_vproc *rpdev;
+
+	if (of_property_read_u32(np, "multi-core-id", &core_id))
+		core_id = 0;
+	rpdev = &light_rpmsg_vprocs[core_id];
+	rpdev->core_id = core_id;
+	rpdev->variant = (enum light_rpmsg_variants)of_device_get_match_data(dev);
+
+	spin_lock_init(&rpdev->mu_lock);
+
+	pri_rpdev = rpdev;
+
+	INIT_DELAYED_WORK(&(rpdev->rpmsg_work), rpmsg_work_handler);
+	BLOCKING_INIT_NOTIFIER_HEAD(&(rpdev->notifier));
+#ifdef  CONFIG_PM_SLEEP
+    sema_init(&rpdev->pm_sem, 0);
+#endif
+	pr_info("light rpmsg: Ready for cross core communication!\n");
+
+	ret = of_property_read_u32(np, "vdev-nums", &rpdev->vdev_nums);
+	if (ret) {
+		rpdev->vdev_nums = 1;
+	}
+
+	if (rpdev->vdev_nums > MAX_VDEV_NUMS) {
+		pr_err("light rpmsg: vdev-nums exceed the max %d\n", MAX_VDEV_NUMS);
+		return -EINVAL;
+	}
+
+	rpdev->first_notify = rpdev->vdev_nums;
+
+	pr_info("light rpmsg: rproc_name = %s",rpdev->rproc_name);
+	if (!strcmp(rpdev->rproc_name, "m4")) {
+		ret = set_vring_phy_buf(pdev, rpdev,
+					rpdev->vdev_nums);
+		if (ret) {
+			pr_err("light rpmsg: No vring buffer.\n");
+			return -ENOMEM;
+		}
+	} else {
+		pr_err("light rpmsg: No remote processor.\n");
+		return -ENODEV;
+	}
+
+	for (j = 0; j < rpdev->vdev_nums; j++) {
+		pr_debug("%s rpdev%d vdev%d: vring0 0x%x, vring1 0x%x\n",
+			 __func__, rpdev->core_id, rpdev->vdev_nums,
+			 rpdev->ivdev[j].vring[0],
+			 rpdev->ivdev[j].vring[1]);
+		rpdev->ivdev[j].vdev.id.device = VIRTIO_ID_RPMSG;
+		rpdev->ivdev[j].vdev.config = &light_rpmsg_config_ops;
+		rpdev->ivdev[j].vdev.dev.parent = &pdev->dev;
+		rpdev->ivdev[j].vdev.dev.release = light_rpmsg_vproc_release;
+		rpdev->ivdev[j].base_vq_id = j * 2;
+
+		ret = register_virtio_device(&rpdev->ivdev[j].vdev);
+		if (ret) {
+			pr_err("light rpmsg: %s failed to register rpdev: %d\n", __func__, ret);
+			return ret;
+		}
+
+	}
+	platform_set_drvdata(pdev, rpdev);
+
+	return ret;
+}
+
+#ifdef CONFIG_PM_SLEEP
+
+typedef enum {
+   RPMSG_MAILBOX_TYPE_PM = 0xA0,
+   RPMSG_MAILBOX_TYPE_MAX
+} rpmsg_mailbox_message_type_en;
+
+typedef enum {
+   RPMSG_PM_CTRL = 0x50,
+   RPMSG_PM_GET,
+   RPMSG_PM_STATUS,
+   RPMSG_PM_MAX
+} rpmsg_pm_message_type_en;
+
+typedef enum {
+   LIGHT_PM_DISABLE = 0xA0,
+   LIGHT_PM_OFF,
+   LIGHT_PM_HW_VAD,
+   LIGHT_PM_TYPE_MAX
+} light_pm_type_en;
+
+typedef enum {
+   LIGHT_PM_WAKEUP = 0x50,
+   LIGHT_PM_SLEEP,
+   LIGHT_PM_STATUS_MAX
+} light_pm_status_en;
+
+#define MAX_PM_NOTIFY_TIME 10
+#define MAX_PM_ASK_TIME 10
+
+static int light_rpmsg_sleep_notify(struct virtqueue *vq, light_pm_type_en type)
+{
+	int ret;
+	struct light_rpmsg_vq_info *rpvq = vq->priv;
+	uint8_t sleep_ctrl[4] = {RPMSG_MAILBOX_TYPE_PM, RPMSG_PM_CTRL, type, '\n'};
+	mutex_lock(&rpvq->rpdev->lock);
+	ret = mbox_send_message(tdev_priv->tx_channel, sleep_ctrl);
+	if(ret < 0) {
+       pr_err("sleep notify faild %d", ret);
+	   mutex_unlock(&rpvq->rpdev->lock);
+       return ret;
+	}
+	mutex_unlock(&rpvq->rpdev->lock);
+	return 0;
+}
+
+static int light_rpmsg_sleep_ask(struct virtqueue *vq)
+{
+	int ret;
+	struct light_rpmsg_vq_info *rpvq = vq->priv;
+	uint8_t sleep_get[3] = {RPMSG_MAILBOX_TYPE_PM, RPMSG_PM_GET, '\n'};
+	mutex_lock(&rpvq->rpdev->lock);
+	ret = mbox_send_message(tdev_priv->tx_channel, sleep_get);
+	if(ret < 0) {
+       pr_err("sleep ask send faild %d", ret);
+	   mutex_unlock(&rpvq->rpdev->lock);
+       return ret;
+	}
+	mutex_unlock(&rpvq->rpdev->lock);
+	return 0;
+}
+
+static int light_rpmsg_suspend(struct device *dev)
+
+{
+  int ret;
+  int try_num = 0;
+  struct light_rpmsg_vproc *rpdev = dev_get_drvdata(dev);
+
+  //clk_disable_unprepare(rpdev->mu_clk);
+  printk("%s,%d,enter",__func__,__LINE__);
+  light_rpmsg_sleep_notify(rpdev->ivdev[0].vq[0], LIGHT_PM_OFF);
+  try_num++;
+  down_timeout(&rpdev->pm_sem, msecs_to_jiffies(200));
+  while(!rpdev->sleep_flag) {
+    light_rpmsg_sleep_notify(rpdev->ivdev[0].vq[0], LIGHT_PM_OFF);
+	down_timeout(&rpdev->pm_sem, msecs_to_jiffies(200));
+	if(try_num++ > MAX_PM_NOTIFY_TIME) {
+         pr_err("sleep notify faild after try %d time", MAX_PM_NOTIFY_TIME);
+		 printk("%s,%d,try %d times, exist",__func__,__LINE__, try_num);
+		 return -1;
+	}
+  }
+  printk("%s,%d,try %d times, exist",__func__,__LINE__, try_num);
+  return 0;
+}
+
+static int light_rpmsg_resume(struct device *dev)
+{
+  struct light_rpmsg_vproc *rpdev = dev_get_drvdata(dev);
+  int ret;
+  int try_num = 0;
+  printk("%s,%d,enter",__func__,__LINE__);
+  while(rpdev->sleep_flag) {
+    ret = light_rpmsg_sleep_ask(rpdev->ivdev[0].vq[0]);
+    down_timeout(&rpdev->pm_sem, msecs_to_jiffies(200));
+	if(try_num++ > MAX_PM_ASK_TIME) {
+         pr_err("sleep status check faild after try %d time", MAX_PM_ASK_TIME);
+		 printk("%s,%d,try %d times, exist",__func__,__LINE__, try_num);
+		 return -1;
+	}
+  }
+  printk("%s,%d,try %d times, exist",__func__,__LINE__, try_num);
+  return ret;
+}
+
+#endif
+
+static SIMPLE_DEV_PM_OPS(light_rpmsg_pm_ops, light_rpmsg_suspend, light_rpmsg_resume);
+
+static struct platform_driver light_rpmsg_driver = {
+	.driver = {
+		   .owner = THIS_MODULE,
+		   .name = "light-rpmsg",
+		   .of_match_table = light_rpmsg_dt_ids,
+		   .pm = &light_rpmsg_pm_ops,
+		   },
+	.probe = light_rpmsg_probe,
+};
+
+static int __init light_rpmsg_init(void)
+{
+	int ret;
+
+	ret = platform_driver_register(&light_rpmsg_driver);
+	if (ret)
+		pr_err("light rpmsg: Unable to initialize\n");
+	else
+		pr_info("light rpmsg: driver is registered.\n");
+
+	return ret;
+}
+
+late_initcall(light_rpmsg_init);
+
+static ssize_t mbox_client_light_message_write(struct file *filp,
+					      const char __user *userbuf,
+					      size_t count, loff_t *ppos)
+{
+	struct mbox_client_light_device *tdev = filp->private_data;
+	void *data;
+	int ret;
+
+	if (!tdev->tx_channel) {
+		dev_err(tdev->dev, "Channel cannot do Tx\n");
+		return -EINVAL;
+	}
+
+	if (count > WJ_MBOX_SEND_MAX_MESSAGE_LENGTH)
+		count = WJ_MBOX_SEND_MAX_MESSAGE_LENGTH;
+
+	tdev->message = kzalloc(MBOX_MAX_MSG_LEN, GFP_KERNEL);
+	if (!tdev->message)
+		return -ENOMEM;
+
+	ret = copy_from_user(tdev->message, userbuf, count);
+	if (ret) {
+		ret = -EFAULT;
+		goto out;
+	}
+
+	data = tdev->message;
+	print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->message, MBOX_MAX_MSG_LEN, true);
+
+	ret = mbox_send_message(tdev->tx_channel, data);
+	if (ret < 0)
+		dev_err(tdev->dev, "Failed to send message via mailbox\n");
+
+out:
+	kfree(tdev->message);
+	return ret < 0 ? ret : count;
+}
+
+static ssize_t mbox_client_light_message_read(struct file *filp,
+					     char __user *userbuf,
+					     size_t count, loff_t *ppos)
+{
+	struct mbox_client_light_device *tdev = filp->private_data;
+	unsigned long flags;
+
+	print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->rx_buffer, MBOX_MAX_MSG_LEN, true);
+	spin_lock_irqsave(&tdev->lock, flags);
+	memset(tdev->rx_buffer, 0, MBOX_MAX_MSG_LEN);
+	spin_unlock_irqrestore(&tdev->lock, flags);
+
+	return MBOX_MAX_MSG_LEN;
+}
+
+static const struct file_operations mbox_client_light_message_ops = {
+	.write	= mbox_client_light_message_write,
+	.read	= mbox_client_light_message_read,
+	.open	= simple_open,
+	.llseek	= generic_file_llseek,
+};
+
+static int index_names = 0;
+static bool debugfs_dir_created = false;
+static const char* file_names[] = {"mbox-client0", "mbox-client1"};
+
+static int mbox_client_light_add_debugfs(struct platform_device *pdev,
+					struct mbox_client_light_device *tdev)
+{
+	if (!debugfs_initialized())
+		return 0;
+
+	if (index_names > 2) {
+		dev_err(&pdev->dev, "Max device index is 2\n");
+		return 0;
+	}
+
+	if (!debugfs_dir_created) {
+		root_debugfs_dir = debugfs_create_dir("mailbox",NULL);
+		if (!root_debugfs_dir) {
+			dev_err(&pdev->dev,
+				"Failed to create mailbox debugfs\n");
+			return -EINVAL;
+		}
+		debugfs_dir_created = true;
+	}
+
+	debugfs_create_file(file_names[index_names], 0600, root_debugfs_dir,
+			    tdev, &mbox_client_light_message_ops);
+
+	index_names++;
+	return 0;
+}
+
+static void mbox_client_light_receive_message(struct mbox_client *client,
+					     void *message)
+{
+	struct mbox_client_light_device *tdev = dev_get_drvdata(client->dev);
+	char *data = message;
+
+	spin_lock(&tdev->lock);
+	memcpy(tdev->rx_buffer, data, MBOX_MAX_MSG_LEN);
+	spin_unlock(&tdev->lock);
+
+	//printk("mbox_client receive rpmsg_work\n");
+	schedule_delayed_work(&(pri_rpdev->rpmsg_work), 0);
+#ifdef CONFIG_PM_SLEEP
+     if(data[0] == RPMSG_MAILBOX_TYPE_PM && data[1] == RPMSG_PM_STATUS) {
+        if(data[2] == LIGHT_PM_WAKEUP) {
+            pri_rpdev->sleep_flag = 0;
+			up(&pri_rpdev->pm_sem);
+			printk("audio wakeup");
+		} else if(data[2] == LIGHT_PM_SLEEP) {
+            pri_rpdev->sleep_flag = 1;
+			up(&pri_rpdev->pm_sem);
+			printk("audio sleep");
+		}
+	 }
+#endif
+	//print_hex_dump(KERN_INFO, __func__, DUMP_PREFIX_NONE, 16, 1, tdev->rx_buffer, MBOX_MAX_MSG_LEN, true);
+}
+
+static struct mbox_chan *
+mbox_client_light_request_channel(struct platform_device *pdev,
+				 const char *name)
+{
+	struct mbox_client *client;
+	struct mbox_chan *channel;
+
+	client = devm_kzalloc(&pdev->dev, sizeof(*client), GFP_KERNEL);
+	if (!client)
+		return ERR_PTR(-ENOMEM);
+
+	client->dev		= &pdev->dev;
+	client->tx_block	= true;
+	client->knows_txdone	= false;
+	client->tx_tout		= 500;
+	client->rx_callback	= mbox_client_light_receive_message;
+
+	channel = mbox_request_channel_byname(client, name);
+	if (IS_ERR(channel)) {
+		devm_kfree(&pdev->dev, client);
+		dev_warn(&pdev->dev, "Failed to request %s channel\n", name);
+		return NULL;
+	}
+
+	return channel;
+}
+
+static int mbox_client_light_probe(struct platform_device *pdev)
+{
+	struct mbox_client_light_device *tdev;
+	struct device_node *np = pdev->dev.of_node;
+	int ret;
+
+	static int chan_idx = 1;
+
+	tdev = devm_kzalloc(&pdev->dev, sizeof(*tdev), GFP_KERNEL);
+	if (!tdev)
+		return -ENOMEM;
+
+	tdev_priv = tdev;
+
+	if (!chan_idx)
+		tdev->tx_channel = mbox_client_light_request_channel(pdev, "902");
+	else
+		tdev->tx_channel = mbox_client_light_request_channel(pdev, "906");
+
+	if (!tdev->tx_channel) {
+		dev_err(&pdev->dev, "Request channel failed\n");
+		return -EPROBE_DEFER;
+	}
+	chan_idx++;
+
+	/* In fact, rx_channel is same with tx_channel in C-SKY's mailbox */
+	tdev->rx_channel = tdev->tx_channel;
+
+	tdev->dev = &pdev->dev;
+	platform_set_drvdata(pdev, tdev);
+
+	tdev->audio_mbox_regmap = syscon_regmap_lookup_by_phandle(np, "audio-mbox-regmap");
+	if (IS_ERR(tdev->audio_mbox_regmap)) {
+		dev_err(&pdev->dev, "cannot find regmap for audio mbox register\n");
+	} else {
+		dev_dbg(&pdev->dev, "audio_mbox_regmap ok\n");
+	}
+
+	spin_lock_init(&tdev->lock);
+
+	tdev->rx_buffer = devm_kzalloc(&pdev->dev,
+					MBOX_MAX_MSG_LEN, GFP_KERNEL);
+	if (!tdev->rx_buffer)
+		return -ENOMEM;
+
+	ret = mbox_client_light_add_debugfs(pdev, tdev);
+	if (ret)
+		return ret;
+
+	dev_err(&pdev->dev, "Successfully registered\n");
+
+	return 0;
+}
+
+static int mbox_client_light_remove(struct platform_device *pdev)
+{
+	struct mbox_client_light_device *tdev = platform_get_drvdata(pdev);
+
+	debugfs_remove_recursive(root_debugfs_dir);
+
+	if (tdev->tx_channel)
+		mbox_free_channel(tdev->tx_channel);
+
+	if (tdev->rx_channel && tdev->rx_channel != tdev->tx_channel)
+		mbox_free_channel(tdev->rx_channel);
+
+	return 0;
+}
+
+static const struct of_device_id mbox_client_light_match[] = {
+	{ .compatible = "thead,light-mbox-client" },
+	{},
+};
+
+static struct platform_driver mbox_client_light_driver = {
+	.driver = {
+		.name = "thead,light-mbox-client",
+		.of_match_table = mbox_client_light_match,
+	},
+	.probe  = mbox_client_light_probe,
+	.remove = mbox_client_light_remove,
+};
+module_platform_driver(mbox_client_light_driver);
+
+MODULE_AUTHOR("Alibaba Group Holding Limited");
+MODULE_DESCRIPTION("Thead Light mailbox IPC client driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/rtc/Kconfig b/drivers/rtc/Kconfig
index 6f270577df86..f5e30f724f74 100644
--- a/drivers/rtc/Kconfig
+++ b/drivers/rtc/Kconfig
@@ -1992,4 +1992,10 @@ config RTC_DRV_POLARFIRE_SOC
 	  This driver can also be built as a module, if so, the module
 	  will be called "rtc-mpfs".
 
+config RTC_DRV_ASTBMC
+	tristate "SG2042 server get rtc time from bmc via pci bus"
+	help
+	  This driver can also be built as a module, if so, the module
+	  will be called "rtc-astbmc".
+
 endif # RTC_CLASS
diff --git a/drivers/rtc/Makefile b/drivers/rtc/Makefile
index 7711f79787ac..441b27e2d8fd 100644
--- a/drivers/rtc/Makefile
+++ b/drivers/rtc/Makefile
@@ -189,3 +189,4 @@ obj-$(CONFIG_RTC_DRV_WM8350)	+= rtc-wm8350.o
 obj-$(CONFIG_RTC_DRV_X1205)	+= rtc-x1205.o
 obj-$(CONFIG_RTC_DRV_XGENE)	+= rtc-xgene.o
 obj-$(CONFIG_RTC_DRV_ZYNQMP)	+= rtc-zynqmp.o
+obj-$(CONFIG_RTC_DRV_ASTBMC)	+= rtc-astbmc.o
diff --git a/drivers/rtc/rtc-astbmc.c b/drivers/rtc/rtc-astbmc.c
new file mode 100644
index 000000000000..8b56090cf0f8
--- /dev/null
+++ b/drivers/rtc/rtc-astbmc.c
@@ -0,0 +1,535 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/* rtc-astbmc.c
+ *
+ * Driver for Dallas Semiconductor astbmcrtc Low Current, PCI Compatible
+ * Real Time Clock
+ *
+ * Author : Raghavendra Chandra Ganiga <ravi23ganiga@gmail.com>
+ */
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/device.h>
+#include <linux/platform_device.h>
+#include <linux/rtc.h>
+#include <linux/spi/spi.h>
+#include <linux/bcd.h>
+#include <linux/regmap.h>
+#include <linux/version.h>
+#include <linux/kernel.h>
+#include <linux/errno.h>
+#include <linux/pci.h>
+#include <linux/file.h>
+#include <linux/fs.h>
+#include <linux/interrupt.h>
+#include <linux/wait.h>
+#include <linux/workqueue.h>
+#include <linux/miscdevice.h>
+#include <linux/serial_core.h>
+#include <linux/serial_8250.h>
+#include <linux/jiffies.h>
+
+/* Registers in astbmcrtc rtc */
+
+#define ASPEED_PCI_BMC_HOST2BMC_Q1		0x30000
+#define ASPEED_PCI_BMC_HOST2BMC_Q2		0x30010
+#define ASPEED_PCI_BMC_BMC2HOST_Q1		0x30020
+#define ASPEED_PCI_BMC_BMC2HOST_Q2		0x30030
+#define ASPEED_PCI_BMC_BMC2HOST_STS		0x30040
+#define	 BMC2HOST_INT_STS_DOORBELL		BIT(31)
+#define	 BMC2HOST_ENABLE_INTB			BIT(30)
+/* */
+#define	 BMC2HOST_Q1_FULL				BIT(27)
+#define	 BMC2HOST_Q1_EMPTY				BIT(26)
+#define	 BMC2HOST_Q2_FULL				BIT(25)
+#define	 BMC2HOST_Q2_EMPTY				BIT(24)
+#define	 BMC2HOST_Q1_FULL_UNMASK		BIT(23)
+#define	 BMC2HOST_Q1_EMPTY_UNMASK		BIT(22)
+#define	 BMC2HOST_Q2_FULL_UNMASK		BIT(21)
+#define	 BMC2HOST_Q2_EMPTY_UNMASK		BIT(20)
+
+#define ASPEED_PCI_BMC_HOST2BMC_STS		0x30044
+#define	 HOST2BMC_INT_STS_DOORBELL		BIT(31)
+#define	 HOST2BMC_ENABLE_INTB			BIT(30)
+/* */
+#define	 HOST2BMC_Q1_FULL				BIT(27)
+#define	 HOST2BMC_Q1_EMPTY				BIT(26)
+#define	 HOST2BMC_Q2_FULL				BIT(25)
+#define	 HOST2BMC_Q2_EMPTY				BIT(24)
+#define	 HOST2BMC_Q1_FULL_UNMASK		BIT(23)
+#define	 HOST2BMC_Q1_EMPTY_UNMASK		BIT(22)
+#define	 HOST2BMC_Q2_FULL_UNMASK		BIT(21)
+#define	 HOST2BMC_Q2_EMPTY_UNMASK		BIT(20)
+
+struct aspeed_pci_bmc_dev {
+	struct device *dev;
+	struct miscdevice miscdev;
+
+	unsigned long mem_bar_base;
+	unsigned long mem_bar_size;
+	void __iomem *mem_bar_reg;
+
+	unsigned long message_bar_base;
+	unsigned long message_bar_size;
+	void __iomem *msg_bar_reg;
+
+	struct bin_attribute	bin0;
+	struct bin_attribute	bin1;
+
+	struct kernfs_node	*kn0;
+	struct kernfs_node	*kn1;
+
+	/* Queue waiters for idle engine */
+	wait_queue_head_t tx_wait0;
+	wait_queue_head_t tx_wait1;
+	wait_queue_head_t rx_wait0;
+	wait_queue_head_t rx_wait1;
+
+	void __iomem *sio_mbox_reg;
+	int sio_mbox_irq;
+
+	u8 IntLine;
+	int legency_irq;
+};
+
+#define HOST_BMC_QUEUE_SIZE			(16 * 4)
+#define PCIE_DEVICE_SIO_ADDR		(0x2E * 4)
+#define BMC_MULTI_MSI	32
+
+#define DRIVER_NAME "ASPEED BMC DEVICE"
+
+static struct rtc_device *rtc;
+static int time64_flag = 1;
+module_param(time64_flag, int, 0644);
+
+static struct aspeed_pci_bmc_dev *file_aspeed_bmc_device(struct file *file)
+{
+	return container_of(file->private_data, struct aspeed_pci_bmc_dev,
+			miscdev);
+}
+
+static int aspeed_pci_bmc_dev_mmap(struct file *file, struct vm_area_struct *vma)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_dev = file_aspeed_bmc_device(file);
+	unsigned long vsize = vma->vm_end - vma->vm_start;
+	pgprot_t prot = vma->vm_page_prot;
+
+	if (vma->vm_pgoff + vsize > pci_bmc_dev->mem_bar_base + 0x100000)
+		return -EINVAL;
+
+	prot = pgprot_noncached(prot);
+
+	if (remap_pfn_range(vma, vma->vm_start,
+		(pci_bmc_dev->mem_bar_base >> PAGE_SHIFT) + vma->vm_pgoff,
+		vsize, prot))
+		return -EAGAIN;
+
+	return 0;
+}
+
+static const struct file_operations aspeed_pci_bmc_dev_fops = {
+	.owner		= THIS_MODULE,
+	.mmap		= aspeed_pci_bmc_dev_mmap,
+};
+
+
+static irqreturn_t aspeed_pci_host_bmc_device_interrupt(int irq, void *dev_id)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_id;
+	u32 bmc2host_q_sts = readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS);
+
+	if (bmc2host_q_sts & BMC2HOST_INT_STS_DOORBELL)
+		writel(BMC2HOST_INT_STS_DOORBELL, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS);
+
+	if (bmc2host_q_sts & BMC2HOST_ENABLE_INTB)
+		writel(BMC2HOST_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS);
+
+	if (bmc2host_q_sts & BMC2HOST_Q1_FULL)
+		dev_info(pci_bmc_device->dev, "Q1 Full\n");
+
+	if (bmc2host_q_sts & BMC2HOST_Q2_FULL)
+		dev_info(pci_bmc_device->dev, "Q2 Full\n");
+
+
+	//check q1
+	if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS) & HOST2BMC_Q1_FULL))
+		wake_up_interruptible(&pci_bmc_device->tx_wait0);
+
+	if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q1_EMPTY))
+		wake_up_interruptible(&pci_bmc_device->rx_wait0);
+	//chech q2
+	if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS) & HOST2BMC_Q2_FULL))
+		wake_up_interruptible(&pci_bmc_device->tx_wait1);
+
+	if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q2_EMPTY))
+		wake_up_interruptible(&pci_bmc_device->rx_wait1);
+
+	return IRQ_HANDLED;
+
+}
+
+
+static int clear_r_queue1(struct device *dev, int timeout)
+{
+	u32 value;
+	unsigned long tick_end = jiffies + timeout * HZ;
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	while (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q1_EMPTY)) {
+		value = readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_Q1);
+		writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+
+		if (time_after(jiffies, tick_end)) {
+			return 0;
+		}
+	}
+	return 1;
+}
+
+
+
+static ssize_t read_8bytes_from_queue1(struct device *dev, time64_t * time_stamp, int timeout)
+{
+	int i = 0;
+	u32 * time_buf = (u32*)time_stamp;
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	unsigned long tick_end = jiffies + timeout * HZ;
+
+	while (i < 2) {
+		if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q1_EMPTY)) {
+			time_buf[i++] = readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_Q1);
+			writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+		}
+
+		if (time_after(jiffies, tick_end)) {
+			return 0;
+		}
+	}
+	return sizeof(time64_t);
+}
+
+static ssize_t read_queue1(struct device *dev, u32 * data)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	int ret;
+
+	ret = wait_event_interruptible(pci_bmc_device->rx_wait0,
+		!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q1_EMPTY));
+	if (ret)
+		return -EINTR;
+
+	* data = readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_Q1);
+	writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+	return sizeof(u32);
+}
+static ssize_t write_queue1(struct device *dev, u32 data)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	int ret;
+
+	ret = wait_event_interruptible(pci_bmc_device->tx_wait0,
+		!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS) & HOST2BMC_Q1_FULL));
+	if (ret)
+		return -EINTR;
+
+	writel(data, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_Q1);
+	//trigger to host
+	writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+
+	return sizeof(u32);
+}
+
+static ssize_t read_queue2(struct device *dev, u32 * timestamp)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	int ret;
+
+	ret = wait_event_interruptible(pci_bmc_device->rx_wait1,
+		!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_STS) & BMC2HOST_Q2_EMPTY));
+	if (ret)
+		return -EINTR;
+
+	* timestamp = readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_BMC2HOST_Q2);
+	writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+	return sizeof(u32);
+}
+static ssize_t write_queue2(struct device *dev, u32 data)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+	int ret;
+
+	ret = wait_event_interruptible(pci_bmc_device->tx_wait1,
+		!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS) & HOST2BMC_Q2_FULL));
+	if (ret)
+		return -EINTR;
+
+	writel(data, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_Q2);
+	//trigger to host
+	writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+
+
+	return sizeof(u32);
+}
+
+static ssize_t write_8bytes_to_queue2(struct device *dev, time64_t * time_stamp)
+{
+	int i = 0;
+	u32 * time_buf = (u32*)time_stamp;
+	struct aspeed_pci_bmc_dev *pci_bmc_device = dev_get_drvdata(dev);
+
+	while (i < 2) {
+		if (!(readl(pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS) & HOST2BMC_Q2_FULL)) {
+			writel(time_buf[i++], pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_Q2);
+			writel(HOST2BMC_INT_STS_DOORBELL | HOST2BMC_ENABLE_INTB, pci_bmc_device->msg_bar_reg + ASPEED_PCI_BMC_HOST2BMC_STS);
+
+		}
+	}
+	return sizeof(time64_t);
+}
+
+
+
+static int astbmc_read_time(struct device *dev, struct rtc_time *dt)
+{
+	time64_t time_stamp = 0;
+	u32 tx_cmd = 0x55555555;
+
+	clear_r_queue1(dev, 5);
+
+    write_queue1(dev, tx_cmd);
+
+	read_8bytes_from_queue1(dev, &time_stamp, 5);
+
+	rtc_time64_to_tm(time_stamp, dt);
+
+	return 0;
+}
+
+static int astbmc_set_time(struct device *dev, struct rtc_time *dt)
+{
+	time64_t time_stamp = 0;
+	u32 tx_cmd = 0xaaaaaaaa;
+
+	write_queue2(dev, tx_cmd);
+
+	time_stamp = rtc_tm_to_time64(dt);
+
+	write_8bytes_to_queue2(dev, &time_stamp);
+
+	return 0;
+}
+
+static const struct rtc_class_ops astbmc_rtc_ops = {
+	.read_time = astbmc_read_time,
+	.set_time = astbmc_set_time,
+};
+
+
+//0-unenabled 1-enabled
+static int is_bmc_rtc_device_func_enable(struct device *dev)
+{
+	time64_t time_stamp = 0;
+	u32 tx_cmd = 0x55555555;
+
+	clear_r_queue1(dev, 5);
+
+    write_queue1(dev, tx_cmd);
+
+	if (read_8bytes_from_queue1(dev, &time_stamp, 5) == 0) {
+		pr_info("BMC has not enabled rtc device func!\n");
+		return 0;
+	}
+
+	pr_info("BMC has enabled rtc device func!\n");
+	return 1;
+
+}
+
+
+#define BMC_MSI_IDX_BASE	0
+static int aspeed_pci_host_bmc_device_probe(struct pci_dev *pdev, const struct pci_device_id *ent)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_dev;
+	struct device *dev = &pdev->dev;
+	u16 config_cmd_val;
+	int nr_entries;
+	int rc = 0;
+
+	pr_info("ASPEED BMC PCI ID %04x:%04x, IRQ=%u\n", pdev->vendor, pdev->device, pdev->irq);
+
+	pci_bmc_dev = kzalloc(sizeof(*pci_bmc_dev), GFP_KERNEL);
+	if (!pci_bmc_dev) {
+		rc = -ENOMEM;
+		dev_err(&pdev->dev, "kmalloc() returned NULL memory.\n");
+		goto out_err;
+	}
+
+	rc = pci_enable_device(pdev);
+	if (rc != 0) {
+		dev_err(&pdev->dev, "pci_enable_device() returned error %d\n", rc);
+		goto out_err;
+	}
+
+	/* set PCI host mastering  */
+	pci_set_master(pdev);
+
+	nr_entries = pci_alloc_irq_vectors(pdev, 1, 1, PCI_IRQ_MSI);
+	if (nr_entries < 0) {
+		pci_bmc_dev->legency_irq = 1;
+		pci_read_config_word(pdev, PCI_COMMAND, &config_cmd_val);
+		config_cmd_val &= ~PCI_COMMAND_INTX_DISABLE;
+		pci_write_config_word((struct pci_dev *)pdev, PCI_COMMAND, config_cmd_val);
+
+	} else {
+		pci_bmc_dev->legency_irq = 0;
+		pci_read_config_word(pdev, PCI_COMMAND, &config_cmd_val);
+		config_cmd_val |= PCI_COMMAND_INTX_DISABLE;
+		pci_write_config_word((struct pci_dev *)pdev, PCI_COMMAND, config_cmd_val);
+		pdev->irq = pci_irq_vector(pdev, BMC_MSI_IDX_BASE);
+	}
+
+	pr_info("ASPEED BMC PCI ID %04x:%04x, IRQ=%u\n", pdev->vendor, pdev->device, pdev->irq);
+
+	init_waitqueue_head(&pci_bmc_dev->tx_wait0);
+	init_waitqueue_head(&pci_bmc_dev->tx_wait1);
+	init_waitqueue_head(&pci_bmc_dev->rx_wait0);
+	init_waitqueue_head(&pci_bmc_dev->rx_wait1);
+
+	//Get MEM bar
+	pci_bmc_dev->mem_bar_base = pci_resource_start(pdev, 0);
+	pci_bmc_dev->mem_bar_size = pci_resource_len(pdev, 0);
+
+	pr_info("BAR0 I/O Mapped Base Address is: %08lx End %08lx\n", pci_bmc_dev->mem_bar_base, pci_bmc_dev->mem_bar_size);
+
+	pci_bmc_dev->mem_bar_reg = pci_ioremap_bar(pdev, 0);
+	if (!pci_bmc_dev->mem_bar_reg) {
+		rc = -ENOMEM;
+		goto out_free0;
+	}
+
+    //Get MSG BAR info
+	pci_bmc_dev->message_bar_base = pci_resource_start(pdev, 1);
+	pci_bmc_dev->message_bar_size = pci_resource_len(pdev, 1);
+
+	pr_info("MSG BAR1 Memory Mapped Base Address is: %08lx End %08lx\n", pci_bmc_dev->message_bar_base, pci_bmc_dev->message_bar_size);
+
+	pci_bmc_dev->msg_bar_reg = pci_ioremap_bar(pdev, 1);
+	if (!pci_bmc_dev->msg_bar_reg) {
+		rc = -ENOMEM;
+		goto out_free1;
+	}
+
+	/* ERRTA40: dummy read */
+	(void)__raw_readl((void __iomem *)pci_bmc_dev->msg_bar_reg);
+
+
+	pci_bmc_dev->miscdev.minor = MISC_DYNAMIC_MINOR;
+	pci_bmc_dev->miscdev.name = DRIVER_NAME;
+	pci_bmc_dev->miscdev.fops = &aspeed_pci_bmc_dev_fops;
+	pci_bmc_dev->miscdev.parent = dev;
+
+	rc = misc_register(&pci_bmc_dev->miscdev);
+	if (rc) {
+		pr_err("host bmc register fail %d\n", rc);
+		goto out_free;
+	}
+
+	pci_set_drvdata(pdev, pci_bmc_dev);
+
+	rc = request_irq(pdev->irq, aspeed_pci_host_bmc_device_interrupt, IRQF_SHARED, "ASPEED BMC DEVICE", pci_bmc_dev);
+	if (rc) {
+		pr_err("host bmc device Unable to get IRQ %d\n", rc);
+		goto out_unreg;
+	}
+
+	return 0;
+
+	if (!is_bmc_rtc_device_func_enable(dev))
+		return 0;
+
+    //register rtc device
+    rtc = devm_rtc_allocate_device(dev);
+	if (IS_ERR(rtc))
+		return PTR_ERR(rtc);
+
+	rtc->ops = &astbmc_rtc_ops;
+	rtc->range_min = RTC_TIMESTAMP_BEGIN_0000;
+	rtc->range_max = RTC_TIMESTAMP_END_9999;
+
+	devm_rtc_register_device(rtc);
+
+	return 0;
+
+out_unreg:
+	misc_deregister(&pci_bmc_dev->miscdev);
+out_free1:
+	pci_release_region(pdev, 1);
+out_free0:
+	pci_release_region(pdev, 0);
+out_free:
+	kfree(pci_bmc_dev);
+out_err:
+	pci_disable_device(pdev);
+
+	return rc;
+
+}
+
+
+
+static void aspeed_pci_host_bmc_device_remove(struct pci_dev *pdev)
+{
+	struct aspeed_pci_bmc_dev *pci_bmc_dev = pci_get_drvdata(pdev);
+
+	free_irq(pdev->irq, pdev);
+	misc_deregister(&pci_bmc_dev->miscdev);
+	pci_release_regions(pdev);
+	kfree(pci_bmc_dev);
+	pci_disable_device(pdev);
+}
+
+/**
+ * This table holds the list of (VendorID,DeviceID) supported by this driver
+ *
+ */
+static struct pci_device_id aspeed_host_bmc_dev_pci_ids[] = {
+	{ PCI_DEVICE(0x1A03, 0x2402), },
+	{ 0, }
+};
+
+MODULE_DEVICE_TABLE(pci, aspeed_host_bmc_dev_pci_ids);
+
+static struct pci_driver aspeed_host_bmc_dev_driver = {
+	.name		= DRIVER_NAME,
+	.id_table	= aspeed_host_bmc_dev_pci_ids,
+	.probe		= aspeed_pci_host_bmc_device_probe,
+	.remove		= aspeed_pci_host_bmc_device_remove,
+};
+
+static int __init aspeed_host_bmc_device_init(void)
+{
+	int ret;
+
+	/* register pci driver */
+	ret = pci_register_driver(&aspeed_host_bmc_dev_driver);
+	if (ret < 0) {
+		pr_err("pci-driver: can't register pci driver\n");
+		return ret;
+	}
+
+	return 0;
+
+}
+
+static void aspeed_host_bmc_device_exit(void)
+{
+	/* unregister pci driver */
+	pci_unregister_driver(&aspeed_host_bmc_dev_driver);
+}
+
+// late_initcall(aspeed_host_bmc_device_init);
+module_init(aspeed_host_bmc_device_init);
+module_exit(aspeed_host_bmc_device_exit);
+
+MODULE_AUTHOR("Ryan Chen <ryan_chen@aspeedtech.com>");
+MODULE_DESCRIPTION("ASPEED Host BMC DEVICE Driver");
+MODULE_LICENSE("GPL");
diff --git a/drivers/soc/Kconfig b/drivers/soc/Kconfig
index d21e75d69294..6ce6f6300055 100644
--- a/drivers/soc/Kconfig
+++ b/drivers/soc/Kconfig
@@ -31,5 +31,6 @@ source "drivers/soc/ti/Kconfig"
 source "drivers/soc/ux500/Kconfig"
 source "drivers/soc/versatile/Kconfig"
 source "drivers/soc/xilinx/Kconfig"
+source "drivers/soc/thead/Kconfig"
 
 endmenu
diff --git a/drivers/soc/Makefile b/drivers/soc/Makefile
index 0706a27d13be..f19f053b5404 100644
--- a/drivers/soc/Makefile
+++ b/drivers/soc/Makefile
@@ -29,9 +29,11 @@ obj-y				+= renesas/
 obj-y				+= rockchip/
 obj-$(CONFIG_SOC_SAMSUNG)	+= samsung/
 obj-y				+= sifive/
+obj-$(CONFIG_ARCH_SOPHGO)       += sophgo/
 obj-y				+= sunxi/
 obj-$(CONFIG_ARCH_TEGRA)	+= tegra/
 obj-y				+= ti/
 obj-$(CONFIG_ARCH_U8500)	+= ux500/
 obj-$(CONFIG_PLAT_VERSATILE)	+= versatile/
 obj-y				+= xilinx/
+obj-y				+= thead/
diff --git a/drivers/soc/sophgo/Makefile b/drivers/soc/sophgo/Makefile
new file mode 100644
index 000000000000..1e143d85aa17
--- /dev/null
+++ b/drivers/soc/sophgo/Makefile
@@ -0,0 +1,3 @@
+obj-$(CONFIG_ARCH_SOPHGO)		+= top/top_intc.o
+obj-$(CONFIG_ARCH_SOPHGO)		+= umcu/mcu.o
+obj-$(CONFIG_ARCH_SOPHGO)		+= tach/sophgo-tach.o
diff --git a/drivers/soc/sophgo/tach/sophgo-tach.c b/drivers/soc/sophgo/tach/sophgo-tach.c
new file mode 100644
index 000000000000..77884d80eace
--- /dev/null
+++ b/drivers/soc/sophgo/tach/sophgo-tach.c
@@ -0,0 +1,330 @@
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/device.h>
+#include <linux/platform_device.h>
+#include <linux/workqueue.h>
+#include <linux/delay.h>
+#include <linux/of.h>
+#include <linux/netlink.h>
+#include <net/sock.h>
+
+#define DEV_NAME "sophgo-tach"
+#define MHZ 1000000
+#define USER_PORT 100
+#define USER_MSG  30
+
+struct fan_state {
+	unsigned int freq_num;
+	bool enable;
+};
+
+struct sophgo_fan_speed_device {
+	struct device *dev;
+	struct device *parent;
+	struct class *class;
+	dev_t devno;
+	u32 __iomem *regs;
+	struct delayed_work poll_queue;
+	struct fan_state fan_state;
+	struct mutex enable_lock;
+	struct mutex freqnum_lock;
+};
+
+static int fan_index;
+static struct class *sophgo_fan_speed_class;
+static struct sock *nl_fd;
+
+static int send_msg(char *pbuf, uint16_t len)
+{
+	struct sk_buff *nl_skb;
+	struct nlmsghdr *nlh;
+	int ret = 0;
+
+	//alloc a new netlink message
+	nl_skb = nlmsg_new(len, GFP_ATOMIC);
+	if (!nl_skb) {
+		pr_err("sophgo_fan_speed, netlink alloc skb error!\n");
+		return -ENOMEM;
+	}
+
+	//add a new netlink message to skb
+	nlh = nlmsg_put(nl_skb, 0, 0, USER_MSG, len, 0);
+	if (nlh == NULL) {
+		pr_err("sophgo_fan_speed, nlmsg_put error!\n");
+		nlmsg_free(nl_skb);
+		return -EFAULT;
+	}
+
+	memcpy(nlmsg_data(nlh), pbuf, len);
+	ret = netlink_unicast(nl_fd, nl_skb, USER_PORT, MSG_DONTWAIT);
+
+	return ret;
+}
+
+static void recv_cb(struct sk_buff *skb)
+{
+	struct nlmsghdr *nlh = NULL;
+	void *data = NULL;
+
+	if (skb->len >= nlmsg_total_size(0)) {
+		nlh = nlmsg_hdr(skb);
+		data = nlmsg_data(nlh);
+		if (data) {
+			pr_info("sophgo_fan_speed, kernel receive data: %s\n", (int8_t *)data);
+			send_msg(data, nlmsg_len(nlh));
+		}
+	}
+}
+
+struct netlink_kernel_cfg cfg = {
+	.input = recv_cb,
+};
+
+static void fan_speed_check(struct work_struct *work)
+{
+	struct sophgo_fan_speed_device *sophgo_fan = container_of(work,
+				struct sophgo_fan_speed_device, poll_queue.work);
+	int speed, ret = 0;
+	char buf[64];
+
+	speed = readl(sophgo_fan->regs + 1);
+	if (speed == 0) {
+		dev_dbg(sophgo_fan->dev, "fan stop!");
+		ret = snprintf(buf, 32, "%s fan stop!\n", dev_name(sophgo_fan->dev));
+		if (ret <= 0 || ret > 32) {
+			dev_err(sophgo_fan->dev, "%s snprintf failed\n", __func__);
+			return;
+		}
+		ret = send_msg(buf, sizeof(buf));
+		if (ret < 0)
+			dev_dbg(sophgo_fan->dev, "%s send msg failed, ret=%d\n", __func__, ret);
+	}
+	mod_delayed_work(system_freezable_wq, &sophgo_fan->poll_queue,
+				round_jiffies(msecs_to_jiffies(5000)));
+}
+
+static void fan_speed_enable(bool enalbe, struct sophgo_fan_speed_device *sophgo_fan)
+{
+	if (enalbe) {
+		cancel_delayed_work(&sophgo_fan->poll_queue);
+		writel(sophgo_fan->fan_state.freq_num, sophgo_fan->regs);
+		mod_delayed_work(system_freezable_wq, &sophgo_fan->poll_queue,
+					round_jiffies(msecs_to_jiffies(5000)));
+		sophgo_fan->fan_state.enable = true;
+	} else {
+		cancel_delayed_work(&sophgo_fan->poll_queue);
+		writel(0, sophgo_fan->regs);
+		sophgo_fan->fan_state.enable = false;
+	}
+}
+
+static ssize_t freq_num_show(struct device *dev,
+			   struct device_attribute *attr,
+			   char *buf)
+{
+	struct sophgo_fan_speed_device *sophgo_fan;
+
+	sophgo_fan = dev_get_drvdata(dev);
+
+	return sprintf(buf, "%d\n", sophgo_fan->fan_state.freq_num);
+}
+
+static ssize_t freq_num_store(struct device *dev,
+			    struct device_attribute *attr,
+			    const char *buf, size_t size)
+{
+	int val, ret = 0;
+	struct sophgo_fan_speed_device *sophgo_fan;
+
+	sophgo_fan = dev_get_drvdata(dev);
+
+	ret = kstrtoint(buf, 0, &val);
+	if (ret)
+		return ret;
+
+	if (val < (MHZ/10) || val > (1000*MHZ))
+		ret = -EINVAL;
+
+	mutex_lock(&sophgo_fan->freqnum_lock);
+	sophgo_fan->fan_state.freq_num = val;
+	mutex_unlock(&sophgo_fan->freqnum_lock);
+
+	return ret ? : size;
+}
+
+static ssize_t enable_show(struct device *dev,
+			   struct device_attribute *attr,
+			   char *buf)
+{
+	struct sophgo_fan_speed_device *sophgo_fan;
+
+	sophgo_fan = dev_get_drvdata(dev);
+
+	return sprintf(buf, "%d\n", sophgo_fan->fan_state.enable);
+}
+
+static ssize_t enable_store(struct device *dev,
+			    struct device_attribute *attr,
+			    const char *buf, size_t size)
+{
+	int val, ret = 0;
+	struct sophgo_fan_speed_device *sophgo_fan;
+
+	sophgo_fan = dev_get_drvdata(dev);
+
+	ret = kstrtoint(buf, 0, &val);
+	if (ret)
+		return ret;
+
+	mutex_lock(&sophgo_fan->enable_lock);
+	switch (val) {
+	case 0:
+		fan_speed_enable(false, sophgo_fan);
+		break;
+	case 1:
+		fan_speed_enable(true, sophgo_fan);
+		break;
+	default:
+		ret = -EINVAL;
+	}
+	mutex_unlock(&sophgo_fan->enable_lock);
+
+	return ret ? : size;
+}
+
+static ssize_t fan_speed_show(struct device *dev, struct device_attribute *attr, char *buf)
+{
+	int ret = -1;
+	struct sophgo_fan_speed_device *sophgo_fan;
+
+	sophgo_fan = dev_get_drvdata(dev);
+	ret = snprintf(buf, 32, "fan_speed:%d\n", readl(sophgo_fan->regs + 1));
+	if (ret <= 0 || ret > 32) {
+		dev_err(sophgo_fan->dev, "%s snprintf failed %d\n", __func__, ret);
+		return -EFAULT;
+	}
+	dev_dbg(sophgo_fan->dev, "%s\n", buf);
+	return ret;
+}
+
+static DEVICE_ATTR_RW(enable);
+static DEVICE_ATTR_RW(freq_num);
+static DEVICE_ATTR_RO(fan_speed);
+
+static struct attribute *fan_speed_attrs[] = {
+	&dev_attr_enable.attr,
+	&dev_attr_freq_num.attr,
+	&dev_attr_fan_speed.attr,
+	NULL,
+};
+ATTRIBUTE_GROUPS(fan_speed);
+
+static int sophgo_fan_speed_probe(struct platform_device *pdev)
+{
+	struct resource *res;
+	struct sophgo_fan_speed_device *sophgo_fan;
+	char dev_name[32];
+	int ret;
+
+	sophgo_fan = devm_kzalloc(&pdev->dev, sizeof(*sophgo_fan), GFP_KERNEL);
+	if (sophgo_fan == NULL)
+		return -ENOMEM;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	sophgo_fan->regs = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(sophgo_fan->regs))
+		return PTR_ERR(sophgo_fan->regs);
+
+	ret = snprintf(dev_name, 15, "%s-%d", DEV_NAME, fan_index++);
+	if (ret <= 0 || ret > 15) {
+		dev_err(&pdev->dev, "%s snprintf failed\n", __func__);
+		return -EINVAL;
+	}
+	ret = alloc_chrdev_region(&sophgo_fan->devno, 0, 1, dev_name);
+	if (ret < 0) {
+		dev_err(&pdev->dev, "register chrdev error\n");
+		return ret;
+	}
+	sophgo_fan->class = sophgo_fan_speed_class;
+	sophgo_fan->dev = device_create(sophgo_fan->class, sophgo_fan->parent,
+					sophgo_fan->devno, sophgo_fan, dev_name);
+	if (IS_ERR(sophgo_fan->dev)) {
+		ret = PTR_ERR(sophgo_fan->dev);
+		dev_err(&pdev->dev, "create device failed\n");
+		unregister_chrdev_region(sophgo_fan->devno, 1);
+		return ret;
+	}
+
+	//as fan source clk 100M, we advise to set freq num  100M
+	sophgo_fan->fan_state.freq_num = 100*MHZ;
+	mutex_init(&sophgo_fan->freqnum_lock);
+	mutex_init(&sophgo_fan->enable_lock);
+
+	platform_set_drvdata(pdev, sophgo_fan);
+	INIT_DELAYED_WORK(&sophgo_fan->poll_queue, fan_speed_check);
+
+	return 0;
+}
+
+static int sophgo_fan_speed_remove(struct platform_device *pdev)
+{
+	struct sophgo_fan_speed_device *sophgo_fan = platform_get_drvdata(pdev);
+
+	cancel_delayed_work(&sophgo_fan->poll_queue);
+	device_destroy(sophgo_fan->class, sophgo_fan->devno);
+	unregister_chrdev_region(sophgo_fan->devno, 1);
+	kfree(sophgo_fan);
+	sophgo_fan = NULL;
+	return 0;
+}
+
+static const struct of_device_id sophgo_fan_speed_of_match[] = {
+	{
+		.compatible = "sophgo,sophgo-tach",
+	},
+	{}
+};
+
+static struct platform_driver sophgo_fan_speed_driver = {
+	.probe = sophgo_fan_speed_probe,
+	.remove =  sophgo_fan_speed_remove,
+	.driver = {
+		.name = "sophgo,sophgo-tach",
+		.of_match_table = sophgo_fan_speed_of_match,
+	},
+};
+
+static int __init sophgo_fan_speed_init(void)
+{
+	sophgo_fan_speed_class = class_create(DEV_NAME);
+	if (IS_ERR(sophgo_fan_speed_class)) {
+		pr_err("class create failed\n");
+		return PTR_ERR(sophgo_fan_speed_class);
+	}
+	sophgo_fan_speed_class->dev_groups = fan_speed_groups;
+
+	nl_fd = netlink_kernel_create(&init_net, USER_MSG, &cfg);
+	if (!nl_fd) {
+		pr_err("sophgo_fan_speed, cannot create netlink socket!\n");
+		return -1;
+	}
+	fan_index = 0;
+	return platform_driver_register(&sophgo_fan_speed_driver);
+}
+
+static void __exit sophgo_fan_speed_exit(void)
+{
+	class_destroy(sophgo_fan_speed_class);
+	if (nl_fd) {
+		netlink_kernel_release(nl_fd);
+		nl_fd = NULL;
+	}
+}
+
+module_init(sophgo_fan_speed_init);
+module_exit(sophgo_fan_speed_exit);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Xiao Wang");
+MODULE_DESCRIPTION("minimal module");
+MODULE_VERSION("ALPHA");
diff --git a/drivers/soc/sophgo/top/top_intc.c b/drivers/soc/sophgo/top/top_intc.c
new file mode 100644
index 000000000000..2577137fbc4f
--- /dev/null
+++ b/drivers/soc/sophgo/top/top_intc.c
@@ -0,0 +1,412 @@
+#include <linux/module.h>
+#include <linux/kernel.h>
+#include <linux/slab.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/of.h>
+#include <linux/of_platform.h>
+#include <linux/of_pci.h>
+#include <linux/msi.h>
+#include <linux/irq.h>
+#include <linux/irqdomain.h>
+#include <linux/irqchip/chained_irq.h>
+
+#define MAX_IRQ_NUMBER 32
+#define TOP_INTC_NUM 2
+/*
+ * here we assume all plic hwirq and tic hwirq should
+ * be contiguous.
+ * topc_intc hwirq is index of bitmap (both software and
+ * hardware), and starts from 0.
+ * so we use tic hwirq as index to get plic hwirq and its
+ * irq data.
+ * when used as a msi parent, tic hwirq is written to Top
+ * reg for triggering irq by a PCIe device.
+ *
+ * now we pre-requested plic interrupt, but may try request
+ * plic interrupt when needed, like gicp_irq_domain_alloc.
+ */
+struct top_intc_data {
+	struct platform_device *pdev;
+	int irq_num;
+	struct irq_domain *domain;
+	struct irq_chip *chip;
+	int for_msi;
+	int reg_bitwidth;
+
+	DECLARE_BITMAP(irq_bitmap, MAX_IRQ_NUMBER);
+	spinlock_t lock;
+
+	void __iomem *reg_sta;
+	void __iomem *reg_set;
+	void __iomem *reg_clr;
+
+	phys_addr_t reg_set_phys;
+
+	irq_hw_number_t		plic_hwirqs[MAX_IRQ_NUMBER];
+	int			plic_irqs[MAX_IRQ_NUMBER];
+	struct irq_data		*plic_irq_datas[MAX_IRQ_NUMBER];
+	int			tic_to_plic[MAX_IRQ_NUMBER]; // mapping from tic hwirq to plic hwirq
+};
+
+// workaround for using in other modules
+struct top_intc_data *tic_data[TOP_INTC_NUM];
+
+struct irq_domain *cdns_pcie_get_parent_irq_domain(int intc_id)
+{
+	if (intc_id >= TOP_INTC_NUM)
+		return NULL;
+
+	if (tic_data[intc_id])
+		return tic_data[intc_id]->domain;
+	else
+		return NULL;
+}
+
+static int top_intc_domain_translate(struct irq_domain *d,
+				    struct irq_fwspec *fwspec,
+				    unsigned long *hwirq,
+				    unsigned int *type)
+{
+	struct top_intc_data *data = d->host_data;
+
+	if (fwspec->param_count != 2)
+		return -EINVAL;
+	if (fwspec->param[1] >= data->irq_num)
+		return -EINVAL;
+
+	*hwirq = fwspec->param[0];
+	*type = fwspec->param[1] & IRQ_TYPE_SENSE_MASK;
+	pr_debug("%s hwirq %d, flag %d\n", __func__, fwspec->param[0], fwspec->param[1]);
+	return 0;
+}
+
+static int top_intc_domain_alloc(struct irq_domain *domain,
+				unsigned int virq, unsigned int nr_irqs,
+				void *args)
+{
+	unsigned long flags;
+	irq_hw_number_t hwirq;
+	int i, type, ret = -1;
+	struct top_intc_data *data = domain->host_data;
+
+	if (data->for_msi) {
+		// dynamically alloc hwirq
+		spin_lock_irqsave(&data->lock, flags);
+		ret = bitmap_find_free_region(data->irq_bitmap, data->irq_num,
+						order_base_2(nr_irqs));
+		spin_unlock_irqrestore(&data->lock, flags);
+
+		if (ret < 0) {
+			pr_err("%s failed to alloc irq %d, total %d\n", __func__, virq, nr_irqs);
+			return -ENOSPC;
+		}
+
+		hwirq = ret;
+		for (i = 0; i < nr_irqs; i++) {
+			irq_domain_set_info(domain, virq + i, hwirq + i,
+						data->chip,
+						data, handle_edge_irq,
+						NULL, NULL);
+			data->tic_to_plic[hwirq + i] = data->plic_hwirqs[hwirq + i];
+		}
+	} else {
+		// try use hwirq specified in parameter
+		ret = top_intc_domain_translate(domain, args, &hwirq, &type);
+		if (ret) {
+			pr_err("%s failed to translate virq %d, %d\n", __func__, virq, ret);
+			return ret;
+		}
+
+		// try to occupy bitmap for the given hwirq
+		spin_lock_irqsave(&data->lock, flags);
+		ret = bitmap_allocate_region(data->irq_bitmap, hwirq, order_base_2(1));
+		spin_unlock_irqrestore(&data->lock, flags);
+		if (ret < 0) {
+			pr_err("%s virq %d found hwirq %ld occupied\n", __func__, virq, hwirq);
+			return -EBUSY;
+		}
+
+		irq_domain_set_info(domain, virq, hwirq,
+					data->chip,
+					data, handle_edge_irq,
+					NULL, NULL);
+
+		// explicitly set parent
+		data->tic_to_plic[hwirq] = data->plic_hwirqs[hwirq];
+	}
+
+	pr_debug("%s hwirq %ld, irq %d, plic irq %d, total %d\n", __func__,
+		hwirq, virq, data->plic_irqs[hwirq], nr_irqs);
+	return 0;
+}
+
+static void top_intc_domain_free(struct irq_domain *domain,
+				    unsigned int virq, unsigned int nr_irqs)
+{
+	struct irq_data *d = irq_domain_get_irq_data(domain, virq);
+	struct top_intc_data *data = irq_data_get_irq_chip_data(d);
+	unsigned long flags;
+
+	pr_debug("%s hwirq %ld, irq %d, total %d\n", __func__, d->hwirq, virq, nr_irqs);
+
+	spin_lock_irqsave(&data->lock, flags);
+	bitmap_release_region(data->irq_bitmap, d->hwirq,
+				order_base_2(nr_irqs));
+	spin_unlock_irqrestore(&data->lock, flags);
+}
+
+static const struct irq_domain_ops top_intc_domain_ops = {
+	.translate = top_intc_domain_translate,
+	.alloc	= top_intc_domain_alloc,
+	.free	= top_intc_domain_free,
+};
+
+static void top_intc_ack_irq(struct irq_data *d)
+{
+	struct top_intc_data *data  = irq_data_get_irq_chip_data(d);
+	int reg_off, bit_off;
+	struct irq_data *plic_irq_data = data->plic_irq_datas[d->hwirq];
+
+	reg_off = d->hwirq / data->reg_bitwidth;
+	bit_off = d->hwirq - data->reg_bitwidth * reg_off;
+	writel(1 << bit_off, (unsigned int *)data->reg_clr + reg_off);
+
+	pr_debug("%s %ld, parent %s/%ld\n", __func__, d->hwirq,
+		plic_irq_data->domain->name, plic_irq_data->hwirq);
+	if (plic_irq_data->chip->irq_ack)
+		plic_irq_data->chip->irq_ack(plic_irq_data);
+}
+
+static void top_intc_mask_irq(struct irq_data *d)
+{
+	struct top_intc_data *data  = irq_data_get_irq_chip_data(d);
+	struct irq_data *plic_irq_data = data->plic_irq_datas[d->hwirq];
+
+	pr_debug("%s %ld, parent %s/%ld\n", __func__, d->hwirq,
+		plic_irq_data->domain->name, plic_irq_data->hwirq);
+	plic_irq_data->chip->irq_mask(plic_irq_data);
+}
+
+static void top_intc_unmask_irq(struct irq_data *d)
+{
+	struct top_intc_data *data  = irq_data_get_irq_chip_data(d);
+	struct irq_data *plic_irq_data = data->plic_irq_datas[d->hwirq];
+
+	pr_debug("%s %ld, parent %s/%ld\n", __func__, d->hwirq,
+		plic_irq_data->domain->name, plic_irq_data->hwirq);
+	plic_irq_data->chip->irq_unmask(plic_irq_data);
+}
+
+static void top_intc_setup_msi_msg(struct irq_data *d, struct msi_msg *msg)
+{
+	struct top_intc_data *data  = irq_data_get_irq_chip_data(d);
+
+	msg->address_lo = lower_32_bits(data->reg_set_phys);
+	msg->address_hi = upper_32_bits(data->reg_set_phys);
+	msg->data = 1 << d->hwirq;
+
+	pr_debug("%s msi#%d: address_hi %#x, address_lo %#x, data %#x\n", __func__,
+		(int)d->hwirq, msg->address_hi, msg->address_lo, msg->data);
+}
+
+static int top_intc_set_affinity(struct irq_data *d,
+				 const struct cpumask *mask, bool force)
+{
+	struct top_intc_data *data  = irq_data_get_irq_chip_data(d);
+	struct irq_data *plic_irq_data = data->plic_irq_datas[d->hwirq];
+
+	irq_data_update_effective_affinity(d, mask);
+	if (plic_irq_data->chip->irq_set_affinity)
+		return plic_irq_data->chip->irq_set_affinity(plic_irq_data, mask, force);
+	else
+		return -EINVAL;
+}
+
+static int top_intc_set_type(struct irq_data *d, u32 type)
+{
+	/*
+	 * dummy function, so __irq_set_trigger can continue to set
+	 * correct trigger type.
+	 */
+	return 0;
+}
+
+static struct irq_chip top_intc_irq_chip = {
+	.name = "top-intc",
+	.irq_ack = top_intc_ack_irq,
+	.irq_mask = top_intc_mask_irq,
+	.irq_unmask = top_intc_unmask_irq,
+	.irq_compose_msi_msg = top_intc_setup_msi_msg,
+	.irq_set_affinity = top_intc_set_affinity,
+	.irq_set_type = top_intc_set_type,
+};
+
+static void top_intc_irq_handler(struct irq_desc *plic_desc)
+{
+	struct irq_chip *plic_chip = irq_desc_get_chip(plic_desc);
+	struct top_intc_data *data = irq_desc_get_handler_data(plic_desc);
+	irq_hw_number_t plic_hwirq = irq_desc_get_irq_data(plic_desc)->hwirq;
+	irq_hw_number_t top_intc_hwirq;
+	int top_intc_irq, i, ret;
+
+	chained_irq_enter(plic_chip, plic_desc);
+
+	for (i = 0; i < data->irq_num; i++) {
+		if (data->tic_to_plic[i] == plic_hwirq)
+			break;
+	}
+	if (i < data->irq_num) {
+		top_intc_hwirq = i;
+		top_intc_irq = irq_find_mapping(data->domain, top_intc_hwirq);
+		pr_debug("%s plic hwirq %ld, tic hwirq %ld, tic irq %d\n", __func__,
+				plic_hwirq, top_intc_hwirq, top_intc_irq);
+		if (top_intc_irq)
+			ret = generic_handle_irq(top_intc_irq);
+		pr_debug("%s handled tic irq %d, %d\n", __func__, top_intc_irq, ret);
+	} else {
+		pr_debug("%s not found tic hwirq for plic hwirq %ld\n", __func__, plic_hwirq);
+		// workaround, ack unexpected(unregistered) interrupt
+		writel(1 << (plic_hwirq - data->plic_hwirqs[0]), data->reg_clr);
+	}
+
+	chained_irq_exit(plic_chip, plic_desc);
+}
+
+static int top_intc_probe(struct platform_device *pdev)
+{
+	struct top_intc_data *data;
+	struct resource *res;
+	struct fwnode_handle *fwnode = of_node_to_fwnode(pdev->dev.of_node);
+	int ret = 0, i;
+	int intc_id = 0;
+
+	device_property_read_u32(&pdev->dev, "top-intc-id", &intc_id);
+	if (intc_id >= TOP_INTC_NUM)
+		return -EINVAL;
+
+	// alloc private data
+	data = kzalloc(sizeof(struct top_intc_data), GFP_KERNEL);
+	if (!data)
+		return -ENOMEM;
+	platform_set_drvdata(pdev, data);
+	data->pdev = pdev;
+	spin_lock_init(&data->lock);
+
+	if (device_property_read_bool(&pdev->dev, "for-msi")) {
+		dev_info(&pdev->dev, "is a msi parent\n");
+		data->for_msi = 1;
+	}
+	if (device_property_read_u32(&pdev->dev, "reg-bitwidth", &data->reg_bitwidth))
+		data->reg_bitwidth = 32;
+
+	// get register address
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "sta");
+	data->reg_sta = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(data->reg_sta)) {
+		dev_err(&pdev->dev, "failed map status register\n");
+		ret = PTR_ERR(data->reg_sta);
+		goto out;
+	}
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "set");
+	data->reg_set = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(data->reg_set)) {
+		dev_err(&pdev->dev, "failed map set register\n");
+		ret = PTR_ERR(data->reg_set);
+		goto out;
+	}
+	data->reg_set_phys = res->start;
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "clr");
+	data->reg_clr = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(data->reg_clr)) {
+		dev_err(&pdev->dev, "failed map clear register\n");
+		ret = PTR_ERR(data->reg_clr);
+		goto out;
+	}
+
+	// get irq numbers
+	for (i = 0; i < ARRAY_SIZE(data->plic_hwirqs); i++) {
+		char name[8];
+		int irq;
+
+		snprintf(name, ARRAY_SIZE(name), "msi%d", i);
+		irq = platform_get_irq_byname(pdev, name);
+		if (irq < 0)
+			break;
+
+		data->plic_irqs[i] = irq;
+		data->plic_irq_datas[i] = irq_get_irq_data(irq);
+		data->plic_hwirqs[i] = data->plic_irq_datas[i]->hwirq;
+		dev_dbg(&pdev->dev, "%s: plic hwirq %ld, plic irq %d\n", name,
+				data->plic_hwirqs[i], data->plic_irqs[i]);
+	}
+	data->irq_num = i;
+	dev_dbg(&pdev->dev, "got %d plic irqs\n", data->irq_num);
+
+	// create IRQ domain
+	data->domain = irq_domain_create_linear(fwnode, data->irq_num,
+						&top_intc_domain_ops, data);
+	if (!data->domain) {
+		dev_err(&pdev->dev, "create linear irq doamin failed\n");
+		ret = -ENODEV;
+		goto out;
+	}
+	data->chip = &top_intc_irq_chip;
+
+	/*
+	 * workaround to deal with IRQ conflict with TPU driver,
+	 * skip the firt IRQ and mark it as used.
+	 */
+	//bitmap_allocate_region(data->irq_bitmap, 0, order_base_2(1));
+	for (i = 0; i < data->irq_num; i++)
+		irq_set_chained_handler_and_data(data->plic_irqs[i],
+							top_intc_irq_handler, data);
+
+	if (data->for_msi) {
+		irq_domain_update_bus_token(data->domain, DOMAIN_BUS_NEXUS);
+		if (tic_data[intc_id])
+			dev_err(&pdev->dev, "tic_data is not empty, %s\n",
+				dev_name(&tic_data[intc_id]->pdev->dev));
+		tic_data[intc_id] = data;
+	}  else {
+		/*
+		 * populate child nodes. when test device node is a child, it will not be
+		 * automatically enumerated as a platform device.
+		 */
+		of_platform_populate(pdev->dev.of_node, NULL, NULL, NULL);
+	}
+	return ret;
+
+out:
+	if (data->reg_sta)
+		iounmap(data->reg_sta);
+	if (data->reg_set)
+		iounmap(data->reg_set);
+	if (data->reg_clr)
+		iounmap(data->reg_clr);
+	kfree(data);
+	return ret;
+}
+
+static const struct of_device_id top_intc_of_match[] = {
+	{
+		.compatible = "sophgo,top-intc",
+	},
+	{},
+};
+
+static struct platform_driver top_intc_driver = {
+	.driver = {
+		.name = "sophgo,top-intc",
+		.owner = THIS_MODULE,
+		.of_match_table = of_match_ptr(top_intc_of_match),
+	},
+	.probe = top_intc_probe,
+};
+
+static int __init top_intc_init(void)
+{
+	return platform_driver_register(&top_intc_driver);
+}
+
+arch_initcall(top_intc_init);
diff --git a/drivers/soc/sophgo/umcu/mcu.c b/drivers/soc/sophgo/umcu/mcu.c
new file mode 100644
index 000000000000..bf419f1821ef
--- /dev/null
+++ b/drivers/soc/sophgo/umcu/mcu.c
@@ -0,0 +1,1144 @@
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/nvmem-consumer.h>
+#include <linux/i2c.h>
+#include <linux/err.h>
+#include <linux/hwmon.h>
+#include <linux/mutex.h>
+#include <linux/slab.h>
+
+/* fixed MCU registers */
+#define MCU_REG_BOARD_TYPE		0x00
+#define MCU_REG_VERSION			0x01
+#define MCU_REG_SOC_TEMP		0x04
+#define MCU_REG_BOARD_TEMP		0x05
+#define MCU_REG_PWROFF_REASON1		0x06
+#define MCU_REG_PWROFF_REASON2		0x07
+
+#define MCU_REG_CRITICAL_ACTIONS	0x65
+#define MCU_REG_CRITICAL_TEMP		0x66
+#define MCU_REG_REPOWERON_TEMP		0x67
+#define MCU_REG_KEEP_DDR_POWERON	0x68
+
+#define MCU_CRITICAL_ACTION_POWEROFF	0x2
+#define MCU_CRITICAL_ACTION_REBOOT	0X1
+
+#define MANGO_BOARD_TYPE_MASK	1 << 7
+
+#ifndef assert
+#define assert(exp)	WARN_ON(!(exp))
+#endif
+
+struct mcu_features {
+	u8 id;
+	char *proj;
+	char *soc;
+	char *chip;
+
+	int board_type;
+	int mcu_ver;
+	int pcb_ver;
+	int soc_tmp;
+	int board_tmp;
+	int alert_status;
+	int alert_mask;
+	int rst_cnt;
+	int uptime;
+	int lock;
+	int power;
+	int power_tpu;
+	int brd_id;
+	int brd_ip;
+
+	int critical_action;
+	int critical_temp;
+	int repoweron_temp;
+	int keep_ddr_poweron;
+
+	char *alert_table[16];
+};
+
+struct mcu_info {
+	u8 board_type;
+	u8 mcu_ver;
+	u8 pcb_ver;
+	u8 rst_cnt;
+	int updated;
+};
+
+struct mcu_ctx {
+	const struct mcu_features *features;
+	struct i2c_client *i2c;
+	struct mcu_info info;
+	u32 channel_config[4];
+	struct hwmon_channel_info temp_info;
+	const struct hwmon_channel_info *channel_info[3];
+	struct hwmon_chip_info chip;
+	struct mutex update_lock;
+	unsigned int hwmon_update_interval; /* in milliseconds */
+};
+
+const struct mcu_features mcu_list[] = {
+	{
+		0x80, "SG2042 EVB", "SG2042", "GD32",
+		0x00, 0x01, 0x02, 0x04, 0x05, 0x06, 0x08, 0x0a, 0x0b, -1,
+		-1, -1, -1, -1, MCU_REG_CRITICAL_ACTIONS,
+		MCU_REG_CRITICAL_TEMP, MCU_REG_REPOWERON_TEMP,
+		MCU_REG_KEEP_DDR_POWERON,
+		{
+			"SoC overheat",
+			"Power supply overheat",
+			"Board overheat",
+			"Board overheat and shutdown",
+			"SoC overheat and shutdown",
+			"Power supply failure",
+			"12V power supply failure",
+			"SoC required reboot",
+		},
+	},
+
+	{
+		0x83, "SG2042 X4", "SG2042", "GD32",
+		0x00, 0x01, 0x02, 0x04, 0x05, 0x06, 0x08, 0x0a, 0x0b, -1,
+		-1, -1, -1, -1, MCU_REG_CRITICAL_ACTIONS,
+		MCU_REG_CRITICAL_TEMP, MCU_REG_REPOWERON_TEMP,
+		MCU_REG_KEEP_DDR_POWERON,
+		{
+			"SoC overheat",
+			"Power supply overheat",
+			"Board overheat",
+			"Board overheat and shutdown",
+			"SoC overheat and shutdown",
+			"Power supply failure",
+			"12V power supply failure",
+			"SoC required reboot",
+		},
+	},
+
+		{
+		0x90, "MILKV PIONEER", "SG2042", "GD32",
+		0x00, 0x01, 0x02, 0x04, 0x05, 0x06, 0x08, 0x0a, 0x0b, -1,
+		-1, -1, -1, -1, MCU_REG_CRITICAL_ACTIONS,
+		MCU_REG_CRITICAL_TEMP, MCU_REG_REPOWERON_TEMP,
+		MCU_REG_KEEP_DDR_POWERON,
+		{
+			"SoC overheat",
+			"Power supply overheat",
+			"Board overheat",
+			"Board overheat and shutdown",
+			"SoC overheat and shutdown",
+			"Power supply failure",
+			"12V power supply failure",
+			"SoC required reboot",
+		},
+	},
+};
+
+static const char help[] =
+"\n"
+"sys files description\n"
+"======================\n"
+"Bitmain unified mcu device driver\n"
+"You can get/set MCU though read/write operation\n"
+"eg. You can get fixed information though command\n"
+"$cat /sys/bus/i2c/0-0017/information\n"
+"You can set alert mask though command\n"
+"$echo 0xffff /sys/bus/i2c/0-0017/alert\n"
+"\n"
+"information\n"
+"-----------\n"
+"Fixed information during SoC uptime\n"
+"Read this file will return such information\n"
+"Write this file to force SoC re-get such information from MCU\n"
+"No matter what data you write to or just invoke write with a length of 0\n"
+"File pointer will move forward after read,\n"
+"write has no effect on file pointer\n"
+"\n"
+"temperature\n"
+"-----------\n"
+"Temperature value, sensors located on SoC and on board\n"
+"Read this file will return temperature of both in celsius\n"
+"Write is forbidden\n"
+"\n"
+"uptime\n"
+"------\n"
+"Uptime (from SoC poweron) in seconds\n"
+"Read will get this value, write is forbidden\n"
+"\n"
+"alert\n"
+"-----\n"
+"Alert control and status\n"
+"Read will get current alert status\n"
+"Write corresponding bit to 1 will mask this alert\n"
+"You can use 0x/0X for hex, 0 for octal\n"
+"other leading characters will be considered as decimal\n"
+"Values larger than 0xffff is forbidden\n"
+"\n";
+
+enum {
+	MCU_I2C_TYPE_U = 0,
+	MCU_I2C_TYPE_U8,
+	MCU_I2C_TYPE_U16,
+	MCU_I2C_TYPE_U32,
+	MCU_I2C_TYPE_U64,
+	MCU_I2C_TYPE_D,
+	MCU_I2C_TYPE_S8,
+	MCU_I2C_TYPE_S16,
+	MCU_I2C_TYPE_S32,
+	MCU_I2C_TYPE_S64,
+	MCU_I2C_TYPE_MAX,
+};
+
+static const char *mcu_i2c_type_list[MCU_I2C_TYPE_MAX] = {
+	[MCU_I2C_TYPE_U]	=	"u",
+	[MCU_I2C_TYPE_U8]	=	"u8",
+	[MCU_I2C_TYPE_U16]	=	"u16",
+	[MCU_I2C_TYPE_U32]	=	"u32",
+	[MCU_I2C_TYPE_U64]	=	"u64",
+	[MCU_I2C_TYPE_D]	=	"d",
+	[MCU_I2C_TYPE_S8]	=	"s8",
+	[MCU_I2C_TYPE_S16]	=	"s16",
+	[MCU_I2C_TYPE_S32]	=	"s32",
+	[MCU_I2C_TYPE_S64]	=	"s64",
+};
+
+static int check_token(char *token)
+{
+	int i;
+
+	for (i = 0; i < ARRAY_SIZE(mcu_i2c_type_list); ++i) {
+		if (strcmp(token, mcu_i2c_type_list[i]) == 0)
+			return i;
+	}
+	return -EINVAL;
+}
+
+static inline struct device *i2c2dev(struct i2c_client *i2c)
+{
+	return &i2c->dev;
+}
+
+static int mcu_i2c_write_byte(struct i2c_client *i2c, int reg, u8 data)
+{
+	int err;
+
+	if (reg == -1)
+		return 0;
+	err = i2c_smbus_write_byte_data(i2c, reg, data);
+	dev_dbg(i2c2dev(i2c), "%d : %u\n", reg, data);
+	return err;
+}
+
+static int mcu_i2c_read_byte(struct i2c_client *i2c, int reg)
+{
+	int err;
+
+	if (reg == -1)
+		return 0;
+	err = i2c_smbus_read_byte_data(i2c, reg);
+	dev_dbg(i2c2dev(i2c), "%d : %d\n", reg, err);
+	return err;
+}
+
+static int mcu_i2c_write_block(struct i2c_client *i2c, int reg,
+			       int len, void *data)
+{
+	int err, i;
+
+	if (reg == -1)
+		return 0;
+
+	err = i2c_smbus_write_i2c_block_data(i2c, reg, len, data);
+	for (i = 0; i < len; ++i)
+		dev_dbg(i2c2dev(i2c), "%d : %u\n", reg + i, ((u8 *)data)[i]);
+	return err;
+}
+
+static int mcu_i2c_read_block(struct i2c_client *i2c, int reg,
+			      int len, void *data)
+{
+	int err, i;
+
+	if (reg == -1)
+		return 0;
+
+	err = i2c_smbus_read_i2c_block_data(i2c, reg, len, data);
+	for (i = 0; i < len; ++i)
+		dev_dbg(i2c2dev(i2c), "%d : %u\n", reg + i, ((u8 *)data)[i]);
+
+	return err;
+}
+
+static int mcu_i2c_sreadf(struct i2c_client *i2c, const char *fmt, ...)
+{
+	va_list arg;
+	const char *p = fmt;
+	const char *start, *end;
+	char token[16];
+	int tokenlen;
+	int ret = -EINVAL;
+	int idx;
+
+	if (fmt == NULL)
+		return -EINVAL;
+
+	va_start(arg, fmt);
+
+	while (*p) {
+		/* skip all % */
+		while (*p == '%')
+			++p;
+		start = p;
+		while (*p && *p != '%')
+			++p;
+		/* now *p is ether \0 or % */
+		end = p;
+		tokenlen = end - start;
+		if (tokenlen > sizeof(token) - 1) {
+			ret = -EINVAL;
+			goto end;
+		}
+		if (tokenlen == 0)
+			continue;
+		/* get this token */
+		memcpy(token, start, tokenlen);
+		token[tokenlen] = 0; /* terminat this string */
+		idx = check_token(token);
+		if (idx < 0) {
+			ret = idx;
+			goto end;
+		}
+
+		ret = mcu_i2c_read_byte(i2c, va_arg(arg, int));
+		if (ret < 0)
+			goto end;
+
+		switch (idx) {
+		case MCU_I2C_TYPE_U:
+			*va_arg(arg, unsigned int *) = ret;
+			break;
+		case MCU_I2C_TYPE_U8:
+			*va_arg(arg, u8 *) = ret;
+			break;
+		case MCU_I2C_TYPE_U16:
+			*va_arg(arg, u16 *) = ret;
+			break;
+		case MCU_I2C_TYPE_U32:
+			*va_arg(arg, u32 *) = ret;
+			break;
+		case MCU_I2C_TYPE_U64:
+			*va_arg(arg, u64 *) = ret;
+			break;
+		case MCU_I2C_TYPE_D:
+			*va_arg(arg, int *) = ret;
+			break;
+		case MCU_I2C_TYPE_S8:
+			*va_arg(arg, s8 *) = ret;
+			break;
+		case MCU_I2C_TYPE_S16:
+			*va_arg(arg, s16 *) = ret;
+			break;
+		case MCU_I2C_TYPE_S32:
+			*va_arg(arg, s32 *) = ret;
+			break;
+		case MCU_I2C_TYPE_S64:
+			*va_arg(arg, s64 *) = ret;
+			break;
+		default:
+			assert(false);
+			break;
+		}
+	}
+
+	ret = 0;
+end:
+	va_end(arg);
+	return ret;
+}
+
+/* sysfs callbacks */
+
+static inline struct i2c_client *dev2i2c(struct device *dev)
+{
+	return container_of(dev, struct i2c_client, dev);
+}
+
+static const inline struct mcu_features *dev2features(struct device *dev)
+{
+	struct i2c_client *i2c = dev2i2c(dev);
+	struct mcu_ctx *ctx = (struct mcu_ctx *)i2c_get_clientdata(i2c);
+
+	return ctx->features;
+}
+
+static ssize_t help_show(struct device *dev, struct device_attribute *attr,
+		  char *buf)
+{
+	buf[0] = 0;
+	strncpy(buf, help, PAGE_SIZE);
+	return strlen(buf);
+}
+
+static int mcu_msg_append(char *base, unsigned long limit,
+		   const char *fmt, ...)
+{
+	int len = strlen(base);
+	va_list arg;
+
+	va_start(arg, fmt);
+	len += vsnprintf(base + len, limit - len, fmt, arg);
+	va_end(arg);
+	return len;
+}
+
+ssize_t info_show(struct device *dev, struct device_attribute *attr,
+		  char *buf)
+{
+	struct i2c_client *i2c = dev2i2c(dev);
+	struct mcu_ctx *ctx = (struct mcu_ctx *)i2c_get_clientdata(i2c);
+	struct mcu_info *info = &ctx->info;
+	const struct mcu_features *features = ctx->features;
+	int err;
+
+	if (info->updated == 0) {
+		/* get information from mcu through i2c */
+		err = mcu_i2c_sreadf(i2c, "%u8%u8%u8%u8",
+				     features->board_type, &info->board_type,
+				     features->mcu_ver, &info->mcu_ver,
+				     features->pcb_ver, &info->pcb_ver,
+				     features->rst_cnt, &info->rst_cnt);
+		if (err)
+			return err;
+		info->updated = 1;
+	}
+
+	/* convert to json text */
+	mcu_msg_append(buf, PAGE_SIZE, "{\n");
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"model\": \"%s\",\n", features->proj);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"chip\": \"%s\",\n", features->soc);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"mcu\": \"%s\",\n", features->chip);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"board type\": \"0x%02X\",\n", info->board_type);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"mcu version\": \"0x%02X\",\n", info->mcu_ver);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"pcb version\": \"0x%02X\",\n", info->pcb_ver);
+	mcu_msg_append(buf, PAGE_SIZE, "\t\"reset count\": %u\n", info->rst_cnt);
+	err = mcu_msg_append(buf, PAGE_SIZE, "}\n");
+
+	return err;
+}
+
+static ssize_t info_store(struct device *dev, struct device_attribute *attr,
+			  const char *buf, size_t count)
+{
+	struct i2c_client *i2c = dev2i2c(dev);
+	struct mcu_ctx *ctx = (struct mcu_ctx *)i2c_get_clientdata(i2c);
+	struct mcu_info *info = &ctx->info;
+
+	info->updated = 0;
+	return count;
+}
+
+ssize_t brdid_show(struct device *dev, struct device_attribute *attr,
+		    char *buf)
+{
+	int err = 0;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->brd_id == -1)
+		return -ENODEV;
+
+	err = mcu_i2c_read_byte(dev2i2c(dev), features->brd_id);
+	if (err < 0)
+		return err;
+
+	return sprintf(buf, "brdid:%u\n", err);
+}
+
+ssize_t brdip_show(struct device *dev, struct device_attribute *attr,
+		    char *buf)
+{
+	u8 ip[4];
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->brd_ip == -1)
+		return -ENODEV;
+
+	memset(ip, 0, sizeof(ip));
+	err = mcu_i2c_read_block(dev2i2c(dev), features->brd_ip,
+					    sizeof(ip), ip);
+	if (err < 0)
+		return err;
+
+	return mcu_msg_append(buf, PAGE_SIZE, "brdip:%u.%u.%u.%u\n",
+		ip[0], ip[1], ip[2], ip[3]);
+}
+
+static ssize_t brdip_store(struct device *dev, struct device_attribute *attr,
+	const char *ubuf, size_t len)
+{
+	u8 ip[4];
+	char buf[32];
+	char *s, *p, *n;
+	unsigned long res;
+	int i, err;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->brd_ip == -1)
+		return -ENODEV;
+
+	memset(buf, 0, sizeof(buf));
+	len = min(sizeof(buf), len);
+	memcpy(buf, ubuf, len);
+	s = buf;
+	for (i = 0; i < 4; i++) {
+		if (i != 3) {
+			p = strchr(s, '.');
+			n = p+1;
+			*p = '\0';
+		}
+		err = kstrtoul(s, 10, &res);
+		if (err)
+			return err;
+		ip[i] = (u8)res;
+		dev_dbg(dev, "ip[%d] = %d\n", i, ip[i]);
+		s = n;
+	}
+	err = mcu_i2c_write_block(dev2i2c(dev), features->brd_ip,
+					     sizeof(ip), ip);
+	if (err < 0)
+		return err;
+
+	return len;
+}
+ssize_t uptime_show(struct device *dev, struct device_attribute *attr,
+		    char *buf)
+{
+	u8 t[2];
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->uptime,
+					    sizeof(t), t);
+	if (err < 0)
+		return err;
+
+	return mcu_msg_append(buf, PAGE_SIZE,
+			      "%u Seconds\n", t[0] | (t[1] << 8));
+}
+
+ssize_t temp_show(struct device *dev, struct device_attribute *attr,
+		  char *buf)
+{
+	s8 t[2];
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	/* get information from mcu through i2c */
+	err = mcu_i2c_sreadf(dev2i2c(dev), "%s8%s8",
+			     features->soc_tmp, t,
+			     features->board_tmp, t + 1);
+	if (err)
+		return err;
+
+	mcu_msg_append(buf, PAGE_SIZE,
+		       "SoC temperature: %d Cel\n", t[0]);
+	return mcu_msg_append(buf, PAGE_SIZE,
+			      "Board temperature: %d Cel\n", t[1]);
+}
+
+
+static const char *alert_id2name(const struct mcu_features *features, int id)
+{
+	if (features->alert_table[id])
+		return features->alert_table[id];
+	return "Unknown alert";
+}
+
+ssize_t alert_show(struct device *dev, struct device_attribute *attr,
+		   char *buf)
+{
+	int cnt = 0;
+	int i, err;
+	u8 t[4];
+	u16 mask, status;
+	const struct mcu_features *features = dev2features(dev);
+	const char *alt_msg;
+
+	if (features->alert_status == -1)
+		return 0;
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->alert_mask,
+					    sizeof(t), t);
+	/* get information from mcu through i2c */
+	if (err < 0)
+		return err;
+
+	status = t[0] | (t[1] << 8);
+	mask = t[2] | (t[3] << 8);
+	cnt += snprintf(buf + cnt, PAGE_SIZE - cnt,
+			"Mask 0x%02x, Status 0x%02x\n",
+			mask, status);
+
+	if (status == 0) {
+		cnt += snprintf(buf + cnt, PAGE_SIZE - cnt,
+				"Working fine\n");
+	} else {
+		for (i = 0; i < sizeof(status) * 8; ++i) {
+			if ((status >> i) & 1) {
+				alt_msg = alert_id2name(features, i);
+				cnt += snprintf(buf + cnt,
+						PAGE_SIZE - cnt,
+						"%d: %s\n",
+						i, alt_msg);
+			}
+		}
+	}
+	cnt += snprintf(buf + cnt, PAGE_SIZE - cnt,
+			"**************************************************\n");
+
+	for (i = 0; i < 16; ++i) {
+		if (features->alert_table[i] == NULL)
+			continue;
+		cnt += snprintf(buf + cnt, PAGE_SIZE - cnt,
+				"%d: %s\n", i, alert_id2name(features, i));
+	}
+
+	return cnt;
+}
+
+static ssize_t alert_store(struct device *dev, struct device_attribute *attr,
+			  const char *ubuf, size_t len)
+{
+	char buf[32];
+	u8 t[2];
+	unsigned long res;
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->alert_mask == -1)
+		return -ENODEV;
+
+	len = min(sizeof(buf) - 1, len);
+	memcpy(buf, ubuf, len);
+
+	buf[len] = 0; // zero terminated
+	err = kstrtoul(buf, 0, &res);
+	if (err)
+		return err;
+	if (res > 0xffff)
+		return -EINVAL;
+
+	t[0] = res & 0xff;
+	t[1] = (res >> 8) & 0xff;
+	err = mcu_i2c_write_block(dev2i2c(dev), features->alert_mask,
+					     sizeof(t), t);
+	if (err < 0)
+		return err;
+
+	return len;
+}
+
+ssize_t lock_show(struct device *dev, struct device_attribute *attr,
+		   char *buf)
+{
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->lock == -1)
+		return -ENODEV;
+
+	err = mcu_i2c_read_byte(dev2i2c(dev), features->lock);
+
+	if (err < 0)
+		return err;
+
+	return mcu_msg_append(buf, PAGE_SIZE,
+			      "%d", err ? 1 : 0);
+}
+
+static ssize_t lock_store(struct device *dev, struct device_attribute *attr,
+			  const char *buf, size_t len)
+{
+	int err;
+	unsigned long res;
+	const u8 *code[] = { "CK", "LO", };
+	const u8 *p;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->lock == -1)
+		return -ENODEV;
+
+	err = kstrtoul(buf, 0, &res);
+	if (err)
+		return err;
+
+	res = res ? 1 : 0;
+
+	for (p = code[res]; *p; ++p) {
+		err = mcu_i2c_write_byte(dev2i2c(dev), features->lock, *p);
+		if (err < 0)
+			return err;
+	}
+
+	return len;
+}
+
+ssize_t power_show(struct device *dev, struct device_attribute *attr,
+		   char *buf)
+{
+	u8 t[2];
+	int err;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->power < 0)
+		return -EOPNOTSUPP;
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->power, sizeof(t), t);
+	if (err < 0)
+		return err;
+
+	err = sprintf(buf, "%umW\n", ((u16)t[0]) | (t[1] << 8));
+
+	return err;
+}
+
+static ssize_t power_tpu_store(struct device *dev, struct device_attribute *attr,
+			       const char *buf, size_t len)
+{
+	int err;
+	unsigned long res;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->power_tpu < 0)
+		return -EOPNOTSUPP;
+
+	err = kstrtoul(buf, 0, &res);
+	if (err)
+		return err;
+
+	data = res ? 1 : 0;
+
+	err = mcu_i2c_write_block(dev2i2c(dev), features->power_tpu,
+					     sizeof(data), &data);
+	return len;
+}
+
+static ssize_t power_tpu_show(struct device *dev, struct device_attribute *attr,
+			      char *buf)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (features->power_tpu < 0)
+		return -EOPNOTSUPP;
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->power_tpu, sizeof(data), &data);
+	if (err < 0)
+		return err;
+
+	err = sprintf(buf, "%u\n", data);
+
+	return err;
+}
+
+static ssize_t mcu_critical_action_store(struct device *dev,
+					 struct device_attribute *attr,
+					 const char *buf, size_t len)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+
+	if (!strcmp(buf, "reboot\n"))
+		data = MCU_CRITICAL_ACTION_REBOOT;
+	else if (!strcmp(buf, "poweroff\n"))
+		data = MCU_CRITICAL_ACTION_POWEROFF;
+	else
+		data = 0;
+
+	if (data) {
+		err = mcu_i2c_write_block(dev2i2c(dev),
+			features->critical_action, sizeof(data), &data);
+	}
+	return len;
+}
+
+static ssize_t mcu_critical_action_show(struct device *dev,
+					struct device_attribute *attr,
+					char *buf)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->critical_action,
+				 sizeof(data), &data);
+	if (err < 0)
+		return err;
+
+	if (data == MCU_CRITICAL_ACTION_REBOOT)
+		err = sprintf(buf, "reboot\n");
+	else if (data == MCU_CRITICAL_ACTION_POWEROFF)
+		err = sprintf(buf, "poweroff\n");
+	else
+		err = sprintf(buf, "unknown critical action\n");
+
+	return err;
+}
+
+
+static ssize_t mcu_critical_temp_store(struct device *dev,
+				       struct device_attribute *attr,
+				       const char *buf, size_t len)
+{
+	int err;
+	unsigned long res;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = kstrtoul(buf, 0, &res);
+	if (err)
+		return err;
+
+	data = res;
+
+	err = mcu_i2c_write_block(dev2i2c(dev), features->critical_temp,
+					     sizeof(data), &data);
+	return len;
+}
+
+static ssize_t mcu_critical_temp_show(struct device *dev,
+				      struct device_attribute *attr, char *buf)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->critical_temp,
+				 sizeof(data), &data);
+	if (err < 0)
+		return err;
+
+	err = sprintf(buf, "%u Cel\n", data);
+
+	return err;
+}
+
+
+static ssize_t mcu_repoweron_temp_store(struct device *dev,
+					struct device_attribute *attr,
+					const char *buf, size_t len)
+{
+	int err;
+	unsigned long res;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = kstrtoul(buf, 0, &res);
+	if (err)
+		return err;
+
+	data = res;
+
+	err = mcu_i2c_write_block(dev2i2c(dev), features->repoweron_temp,
+					     sizeof(data), &data);
+	return len;
+}
+
+static ssize_t mcu_repoweron_temp_show(struct device *dev,
+				       struct device_attribute *attr, char *buf)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->repoweron_temp,
+				 sizeof(data), &data);
+	if (err < 0)
+		return err;
+
+	err = sprintf(buf, "%u Cel\n", data);
+
+	return err;
+}
+
+
+static ssize_t mcu_keep_ddr_poweron_store(struct device *dev,
+					struct device_attribute *attr,
+					const char *buf, size_t len)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	if (!strcmp(buf, "disable\n"))
+		data = 1;
+	else if (!strcmp(buf, "enable\n"))
+		data = 0;
+	else
+		return 0;
+
+	err = mcu_i2c_write_block(dev2i2c(dev), features->keep_ddr_poweron,
+					     sizeof(data), &data);
+	return len;
+}
+
+static ssize_t mcu_keep_ddr_poweron_show(struct device *dev,
+				       struct device_attribute *attr, char *buf)
+{
+	int err;
+	unsigned char data;
+	const struct mcu_features *features = dev2features(dev);
+
+	err = mcu_i2c_read_block(dev2i2c(dev), features->keep_ddr_poweron,
+				 sizeof(data), &data);
+	if (err < 0)
+		return err;
+
+	if (data == 1)
+		err = sprintf(buf, "disable\n");
+	else if (data == 0)
+		err = sprintf(buf, "enable\n");
+	else
+		err = sprintf(buf, "unknown states\n");
+
+	return err;
+}
+
+/* end of sysfs callbacks */
+
+const struct device_attribute mcu_attrs[] =  {
+	{{"help", 0444}, help_show, NULL},
+	{{"information", 0644}, info_show, info_store},
+	{{"temperature", 0444}, temp_show, NULL},
+	{{"uptime", 0444}, uptime_show, NULL},
+	{{"alert", 0644}, alert_show, alert_store},
+	{{"lock", 0644}, lock_show, lock_store},
+	{{"power-now", 0444}, power_show, NULL},
+	{{"power-tpu", 0644}, power_tpu_show, power_tpu_store},
+	{{"board-id", 0444}, brdid_show, NULL},
+	{{"board-ip", 0644}, brdip_show, brdip_store},
+	{{"critical-action", 0644}, mcu_critical_action_show,
+	  mcu_critical_action_store},
+	{{"critical-temp", 0644}, mcu_critical_temp_show,
+	  mcu_critical_temp_store},
+	{{"repoweron-temp", 0664}, mcu_repoweron_temp_show,
+	  mcu_repoweron_temp_store},
+	{{"keep-ddr-poweron", 0664}, mcu_keep_ddr_poweron_show,
+	  mcu_keep_ddr_poweron_store},
+};
+
+static umode_t mcu_chip_is_visible(const void *data, enum hwmon_sensor_types type,
+								 u32 attr, int channel)
+{
+	switch (type) {
+	case hwmon_chip:
+		return 0444;
+	case hwmon_temp:
+		return 0444;
+	default:
+		return 0;
+	}
+}
+
+static int mcu_hwmon_chip_read(struct device *dev, u32 attr, int channel, long *val)
+{
+	struct mcu_ctx *ctx = dev_get_drvdata(dev);
+
+	switch (attr) {
+	case hwmon_chip_update_interval:
+		*val = ctx->hwmon_update_interval;
+		break;
+	default:
+		return -EOPNOTSUPP;
+	}
+
+	return 0;
+}
+
+static int mcu_hwmon_temp_read(struct device *dev, u32 attr, int channel, long *val)
+{
+	int soc_temp, board_temp;
+
+	struct mcu_ctx *ctx = dev_get_drvdata(dev);
+	struct i2c_client *i2c = ctx->i2c;
+	mutex_lock(&ctx->update_lock);
+	soc_temp = mcu_i2c_read_byte(i2c, MCU_REG_SOC_TEMP);
+	mutex_unlock(&ctx->update_lock);
+
+	mutex_lock(&ctx->update_lock);
+	board_temp = mcu_i2c_read_byte(i2c, MCU_REG_BOARD_TEMP);
+	mutex_unlock(&ctx->update_lock);
+
+	switch (attr) {
+	case hwmon_temp_input:
+		if (channel == 0)
+			*val = soc_temp * 1000;
+		else if (channel == 1)
+			*val = board_temp * 1000;
+		else
+			*val = 0;
+		break;
+	default:
+		return -EOPNOTSUPP;
+	}
+
+	return 0;
+}
+
+
+static int mcu_hwmon_read(struct device *dev, enum hwmon_sensor_types type,
+			u32 attr, int channel, long *val)
+{
+
+	switch (type) {
+	case hwmon_chip:
+		return mcu_hwmon_chip_read(dev, attr, channel, val);
+	case hwmon_temp:
+		return mcu_hwmon_temp_read(dev, attr, channel, val);
+	default:
+		return -EOPNOTSUPP;
+	}
+
+	return 0;
+}
+
+static const struct hwmon_ops mcu_ops = {
+	.is_visible = mcu_chip_is_visible,
+	.read = mcu_hwmon_read,
+	.read_string = NULL,
+	.write = NULL,
+};
+
+static int register_hwmon_temp_sensor(struct i2c_client *i2c,
+			 struct mcu_ctx *ctx)
+{
+	struct device *dev = &i2c->dev;
+	struct hwmon_channel_info *info;
+	struct device *hwmon_dev;
+
+	mutex_init(&ctx->update_lock);
+
+	ctx->i2c = i2c;
+	ctx->hwmon_update_interval = 1000;
+
+	ctx->chip.ops = &mcu_ops;
+	ctx->chip.info = ctx->channel_info;
+	ctx->channel_info[0] = HWMON_CHANNEL_INFO(chip,
+		 HWMON_C_REGISTER_TZ | HWMON_C_UPDATE_INTERVAL);
+	ctx->channel_info[1] = &ctx->temp_info;
+
+	info = &ctx->temp_info;
+	info->type = hwmon_temp;
+	info->config = ctx->channel_config;
+
+	ctx->channel_config[0] = HWMON_T_INPUT;
+	ctx->channel_config[1] = HWMON_T_INPUT;
+	hwmon_dev = devm_hwmon_device_register_with_info(
+						 dev,
+						 dev->driver->name,
+						 ctx,
+						 &ctx->chip,
+						 NULL);
+
+	if (IS_ERR(hwmon_dev))
+		return PTR_ERR(hwmon_dev);
+
+	return 0;
+}
+
+static int sub_probe(struct i2c_client *i2c,
+		     const struct mcu_features *features)
+{
+	struct mcu_ctx *ctx;
+	int i, err;
+
+	ctx = devm_kzalloc(i2c2dev(i2c), sizeof(*ctx), GFP_KERNEL);
+	if (ctx == NULL)
+		return -ENOMEM;
+
+	for (i = 0; i < ARRAY_SIZE(mcu_attrs); ++i) {
+		err = device_create_file(i2c2dev(i2c), mcu_attrs + i);
+		if (err)
+			return err;
+	}
+
+	ctx->features = features;
+
+	assert(features->alert_status + 2 == features->alert_mask);
+
+	if ((features->id & MANGO_BOARD_TYPE_MASK) == 0x80 ) {
+		err = register_hwmon_temp_sensor(i2c, ctx);
+		if (err)
+			dev_warn(i2c2dev(i2c), "mcu board id %u register hwmon failed\n", features->id);
+	}
+
+	i2c_set_clientdata(i2c, ctx);
+	return 0;
+}
+
+static int mcu_i2c_probe(struct i2c_client *i2c)
+{
+	int id;
+	int err;
+	int i;
+	uint8_t regs[3];
+
+	/* get information from mcu through i2c */
+	err = mcu_i2c_sreadf(i2c, "%u8%u8%u8",
+			     MCU_REG_VERSION, regs,
+			     MCU_REG_PWROFF_REASON1, regs + 1,
+			     MCU_REG_PWROFF_REASON2, regs + 2);
+	if (err)
+		return err;
+
+	dev_info(i2c2dev(i2c), "MCU: version 0x%x, reason 0x%x/0x%x\n",
+		regs[0], regs[1], regs[2]);
+
+	id = mcu_i2c_read_byte(i2c, MCU_REG_BOARD_TYPE);
+	if (id < 0)
+		return id;
+
+	for (i = 0; i < ARRAY_SIZE(mcu_list); ++i) {
+		if (mcu_list[i].id == id)
+			return sub_probe(i2c, mcu_list + i);
+	}
+
+	dev_warn(i2c2dev(i2c), "not registered mcu id %u\n", id);
+	return -ENODEV;
+}
+
+static void mcu_i2c_remove(struct i2c_client *i2c)
+{
+	return;
+}
+
+static const struct of_device_id mcu_i2c_dt_table[] = {
+	{ .compatible = "sophgo,sg20xx-mcu" },
+	{},
+};
+
+static const struct i2c_device_id mcu_i2c_id_table[] = {
+	{ "sg20xx-mcu", 0 },
+	{},
+};
+
+static struct i2c_driver mcu_i2c_drv = {
+	.driver = {
+		.name = "sg20xx-mcu",
+		.of_match_table = mcu_i2c_dt_table,
+	},
+	.probe = mcu_i2c_probe,
+	.remove = mcu_i2c_remove,
+	.id_table = mcu_i2c_id_table,
+};
+
+module_i2c_driver(mcu_i2c_drv);
+
+MODULE_DESCRIPTION("MCU I2C driver for bm16xx soc platform");
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Chao.Wei@bitmain.com>");
diff --git a/drivers/soc/thead/Kconfig b/drivers/soc/thead/Kconfig
new file mode 100644
index 000000000000..7948bbb61568
--- /dev/null
+++ b/drivers/soc/thead/Kconfig
@@ -0,0 +1,10 @@
+# SPDX-License-Identifier: GPL-2.0-only
+menu "Thead SoC drivers"
+
+config LIGHT_REBOOTMODE
+	bool "Thead light rebootmode support"
+	default y
+	help
+	 This driver supports check rebootmode feature in Light FM platform
+
+endmenu
diff --git a/drivers/soc/thead/Makefile b/drivers/soc/thead/Makefile
new file mode 100644
index 000000000000..1af5bb20810e
--- /dev/null
+++ b/drivers/soc/thead/Makefile
@@ -0,0 +1,2 @@
+# SPDX-License-Identifier: GPL-2.0-only
+obj-$(CONFIG_LIGHT_REBOOTMODE)	+= light_event.o
diff --git a/drivers/soc/thead/light_event.c b/drivers/soc/thead/light_event.c
new file mode 100644
index 000000000000..f8f6292bac6e
--- /dev/null
+++ b/drivers/soc/thead/light_event.c
@@ -0,0 +1,279 @@
+// SPDX-License-Identifier: GPL-2.0-only
+#include <linux/kernel.h>
+#include <linux/of.h>
+#include <linux/miscdevice.h>
+#include <linux/module.h>
+#include <linux/mfd/syscon.h>
+#include <linux/regmap.h>
+#include <linux/platform_device.h>
+#include <linux/firmware/thead/ipc.h>
+#include <linux/firmware/thead/light_event.h>
+
+/*
+ * AON SRAM total size is 0x10000, reserve 0x100 for event.
+ * Notice: c902 *.ld also need resize.
+ * -------------- 0xff_ffef8000
+ * |		|
+ * |		|
+ * |		|
+ * |    c902	|
+ * |		|
+ * |		|
+ * |		|
+ * -------------- 0xff_fff07f00
+ * |   reserve	|
+ * |		|
+ * --------------
+ */
+#define LIGHT_AON_SRAM_LEN	0x10000
+#define LIGHT_AON_SRAM_RESERV	(LIGHT_AON_SRAM_LEN - 0x100)
+#define LIGHT_EVENT_OFFSET	(LIGHT_AON_SRAM_RESERV + 0x10)
+#define LIGHT_EVENT_CHECK	(LIGHT_EVENT_OFFSET + 0x4)
+
+#define LIGHT_EVENT_MAGIC	0x5A5A5A5A
+
+struct light_aon_msg_event_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 reserve_offset;
+	u32 reserved[5];
+} __packed __aligned(4);
+
+struct light_event {
+	struct device *dev;
+
+	struct light_aon_ipc *ipc_handle;
+	struct light_aon_msg_event_ctrl msg;
+
+	struct regmap *aon_iram;
+	bool init;
+};
+
+struct light_event *light_event;
+
+static void light_event_msg_hdr_fill(struct light_aon_rpc_msg_hdr *hdr, enum light_aon_misc_func func)
+{
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_MISC;
+	hdr->func = (uint8_t)func;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+}
+
+static int light_event_aon_reservemem(struct light_event *event)
+{
+	struct light_aon_ipc *ipc = event->ipc_handle;
+	int ret = 0;
+
+	dev_dbg(event->dev, "aon reservemem...\n");
+
+	light_event_msg_hdr_fill(&event->msg.hdr, LIGHT_AON_MISC_FUNC_AON_RESERVE_MEM);
+	event->msg.reserve_offset = LIGHT_EVENT_OFFSET;
+
+	ret = light_aon_call_rpc(ipc, &event->msg, true);
+	if (ret)
+		dev_err(event->dev, "failed to set aon reservemem\n");
+
+	return ret;
+}
+
+int light_event_set_rebootmode(enum light_rebootmode_index mode)
+{
+	int ret;
+
+	if (!light_event || !light_event->init)
+		return -EINVAL;
+
+	ret = regmap_write(light_event->aon_iram, LIGHT_EVENT_OFFSET, mode);
+	if (ret) {
+		dev_err(light_event->dev, "set rebootmode failed,ret:%d\n", ret);
+		return ret;
+	}
+
+	dev_info(light_event->dev, "set rebootmode:0x%x\n", mode);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(light_event_set_rebootmode);
+
+int light_event_get_rebootmode(enum light_rebootmode_index *mode)
+{
+	int ret;
+
+	if (!light_event || !light_event->init)
+		return -EINVAL;
+
+	ret = regmap_read(light_event->aon_iram, LIGHT_EVENT_OFFSET, mode);
+	if (ret) {
+		dev_err(light_event->dev, "get rebootmode failed,ret:%d\n", ret);
+		return ret;
+	}
+	dev_dbg(light_event->dev, "%s get rebootmode:0x%x\n", __func__, *mode);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(light_event_get_rebootmode);
+
+static int light_event_check_powerup(void)
+{
+	enum light_rebootmode_index mode;
+	unsigned int val;
+	int ret;
+
+	if (!light_event->init)
+		return -EINVAL;
+
+	ret = regmap_read(light_event->aon_iram, LIGHT_EVENT_CHECK, &val);
+	if (ret) {
+		dev_err(light_event->dev, "get magicnum failed,ret:%d\n", ret);
+		return ret;
+	}
+	ret = regmap_read(light_event->aon_iram, LIGHT_EVENT_OFFSET, &mode);
+	if (ret) {
+		dev_err(light_event->dev, "get rebootmode failed,ret:%d\n", ret);
+		return ret;
+	}
+	dev_info(light_event->dev, "magicnum:0x%x mode:0x%x\n", val, mode);
+
+	/* powerup means SRAM data is randam */
+	if (val != LIGHT_EVENT_MAGIC && mode != LIGHT_EVENT_PMIC_ONKEY)
+		light_event_set_rebootmode(LIGHT_EVENT_PMIC_POWERUP);
+
+	ret = regmap_write(light_event->aon_iram, LIGHT_EVENT_CHECK, LIGHT_EVENT_MAGIC);
+	if (ret) {
+		dev_err(light_event->dev, "set magicnum failed,ret:%d\n", ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+static ssize_t rebootmode_store(struct device *dev,
+					struct device_attribute *attr,
+					const char *buf, size_t count)
+{
+	enum light_rebootmode_index mode;
+
+	if (kstrtouint(buf, 0, &mode) < 0)
+		return -EINVAL;
+	light_event_set_rebootmode(mode);
+
+	return count;
+}
+
+static ssize_t
+rebootmode_show(struct device *dev, struct device_attribute *attr, char *buf)
+{
+	enum light_rebootmode_index mode;
+
+	light_event_get_rebootmode(&mode);
+
+	return sprintf(buf, "0x%x\n", mode);
+}
+static DEVICE_ATTR_RW(rebootmode);
+
+static struct attribute *event_attrs[] = {
+	&dev_attr_rebootmode.attr,
+	NULL
+};
+ATTRIBUTE_GROUPS(event);
+
+static int light_event_open(struct inode *inode, struct file *f)
+{
+	return 0;
+}
+
+static int light_event_release(struct inode *inode, struct file *f)
+{
+	return 0;
+}
+
+static long light_event_ioctl(struct file *f, unsigned int ioctl,
+			    unsigned long arg)
+{
+	return 0;
+}
+
+static const struct file_operations light_event_fops = {
+	.owner          = THIS_MODULE,
+	.release        = light_event_release,
+	.open           = light_event_open,
+	.unlocked_ioctl = light_event_ioctl,
+};
+
+static struct miscdevice light_event_misc = {
+	.minor = MISC_DYNAMIC_MINOR,
+	.name = "light-event",
+	.fops = &light_event_fops,
+};
+
+static int light_event_probe(struct platform_device *pdev)
+{
+	struct device		*dev = &pdev->dev;
+	struct device_node	*np = dev->of_node;
+	struct light_event	*thead;
+	int			ret;
+
+	thead = devm_kzalloc(&pdev->dev, sizeof(*thead), GFP_KERNEL);
+	if (!thead)
+		return -ENOMEM;
+
+	ret = light_aon_get_handle(&(thead->ipc_handle));
+	if (ret == -EPROBE_DEFER)
+		return ret;
+
+	platform_set_drvdata(pdev, thead);
+	thead->dev = &pdev->dev;
+
+	thead->aon_iram = syscon_regmap_lookup_by_phandle(np, "aon-iram-regmap");
+	if (IS_ERR(thead->aon_iram))
+		return PTR_ERR(thead->aon_iram);
+
+	ret = misc_register(&light_event_misc);
+	if (ret < 0)
+		return ret;
+
+	ret = light_event_aon_reservemem(thead);
+	if (ret) {
+		dev_err(dev, "set aon reservemem failed!\n");
+		return -EPERM;
+	}
+	thead->init = true;
+	light_event = thead;
+
+	ret = light_event_check_powerup();
+	if (ret) {
+		dev_err(dev, "check powerup failed!\n");
+		light_event = NULL;
+		return -EPERM;
+	}
+	dev_info(dev, "light-event driver init successfully\n");
+
+	return 0;
+}
+
+static int light_event_remove(struct platform_device *pdev)
+{
+	misc_deregister(&light_event_misc);
+
+	return 0;
+}
+
+static const struct of_device_id light_event_of_match[] = {
+	{ .compatible = "thead,light-event" },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, light_event_of_match);
+
+static struct platform_driver light_event_driver = {
+	.probe		= light_event_probe,
+	.remove		= light_event_remove,
+	.driver		= {
+		.name	= "light-event",
+		.dev_groups	= event_groups,
+		.of_match_table	= light_event_of_match,
+	},
+};
+
+module_platform_driver(light_event_driver);
+
+MODULE_DESCRIPTION("light-event driver");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/usb/dwc3/Kconfig b/drivers/usb/dwc3/Kconfig
index 98efcbb76c88..a2183b8e7772 100644
--- a/drivers/usb/dwc3/Kconfig
+++ b/drivers/usb/dwc3/Kconfig
@@ -178,4 +178,24 @@ config USB_DWC3_OCTEON
 	  Only the host mode is currently supported.
 	  Say 'Y' or 'M' here if you have one such device.
 
+config USB_DWC3_RTK
+	tristate "Realtek DWC3 Platform Driver"
+	depends on OF && ARCH_REALTEK
+	default USB_DWC3
+	select USB_ROLE_SWITCH
+	help
+	  RTK DHC RTD SoCs with DesignWare Core USB3 IP inside,
+	  and IP Core configured for USB 2.0 and USB 3.0 in host
+	  or dual-role mode.
+	  Say 'Y' or 'M' if you have such device.
+
+config USB_DWC3_THEAD
+	tristate "T-HEAD Platform"
+	depends on ARCH_THEAD || COMPILE_TEST
+	default USB_DWC3
+	help
+	  Support T-HEAD platform with DesignWare Core USB3 IP.
+	  Only the host mode is currently supported.
+	  Say 'Y' or 'M' here if you have one such device.
+
 endif
diff --git a/drivers/usb/dwc3/Makefile b/drivers/usb/dwc3/Makefile
index fe1493d4bbe5..79afa5c03c10 100644
--- a/drivers/usb/dwc3/Makefile
+++ b/drivers/usb/dwc3/Makefile
@@ -55,3 +55,5 @@ obj-$(CONFIG_USB_DWC3_QCOM)		+= dwc3-qcom.o
 obj-$(CONFIG_USB_DWC3_IMX8MP)		+= dwc3-imx8mp.o
 obj-$(CONFIG_USB_DWC3_XILINX)		+= dwc3-xilinx.o
 obj-$(CONFIG_USB_DWC3_OCTEON)		+= dwc3-octeon.o
+obj-$(CONFIG_USB_DWC3_RTK)		+= dwc3-rtk.o
+obj-$(CONFIG_USB_DWC3_THEAD)		+= dwc3-thead.o
diff --git a/drivers/usb/dwc3/dwc3-thead.c b/drivers/usb/dwc3/dwc3-thead.c
new file mode 100644
index 000000000000..987ac70a5afc
--- /dev/null
+++ b/drivers/usb/dwc3/dwc3-thead.c
@@ -0,0 +1,112 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * dwc3-thead.c - T-HEAD platform specific glue layer
+ *
+ * Inspired by dwc3-of-simple.c
+ *
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ * Copyright (C) 2023 Jisheng Zhang <jszhang@kernel.org>
+ * Copyright (c) 2018, The Linux Foundation. All rights reserved.
+ */
+
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/mfd/syscon.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/of_platform.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+
+#include "core.h"
+
+#define USB_SSP_EN		0x34
+#define  REF_SSP_EN		BIT(0)
+#define USB_SYS			0x3c
+#define  COMMONONN		BIT(0)
+
+#define USB3_DRD_SWRST		0x14
+#define  USB3_DRD_PRST		BIT(0)
+#define  USB3_DRD_PHYRST	BIT(1)
+#define  USB3_DRD_VCCRST	BIT(2)
+#define  USB3_DRD_RSTMASK	(USB3_DRD_PRST | USB3_DRD_PHYRST | USB3_DRD_VCCRST)
+
+struct dwc3_thead {
+	void __iomem		*base;
+	struct regmap		*misc_sysreg;
+	struct regulator	*vbus;
+};
+
+static void dwc3_thead_optimize_power(struct dwc3_thead *thead)
+{
+	u32 val;
+
+	/* config usb top within USB ctrl & PHY reset */
+	regmap_update_bits(thead->misc_sysreg, USB3_DRD_SWRST,
+			   USB3_DRD_RSTMASK, USB3_DRD_PRST);
+
+	/*
+	 * dwc reg also need to be configed to save power
+	 * 1. set USB_SYS[COMMONONN]
+	 * 2. set DWC3_GCTL[SOFITPSYNC](done by core.c)
+	 * 3. set GUSB3PIPECTL[SUSPENDEN] (done by core.c)
+	 */
+	val = readl(thead->base + USB_SYS);
+	val |= COMMONONN;
+	writel(val, thead->base + USB_SYS);
+	val = readl(thead->base + USB_SSP_EN);
+	val |= REF_SSP_EN;
+	writel(val, thead->base + USB_SSP_EN);
+
+	regmap_update_bits(thead->misc_sysreg, USB3_DRD_SWRST,
+			   USB3_DRD_RSTMASK, USB3_DRD_RSTMASK);
+}
+
+static int dwc3_thead_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct dwc3_thead *thead;
+	int ret;
+
+	thead = devm_kzalloc(&pdev->dev, sizeof(*thead), GFP_KERNEL);
+	if (!thead)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, thead);
+
+	ret = devm_regulator_get_enable_optional(dev, "vbus");
+	if (ret < 0 && ret != -ENODEV)
+		return ret;
+
+	thead->misc_sysreg = syscon_regmap_lookup_by_phandle(np, "thead,misc-sysreg");
+	if (IS_ERR(thead->misc_sysreg))
+		return PTR_ERR(thead->misc_sysreg);
+
+	thead->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(thead->base))
+		return PTR_ERR(thead->base);
+
+	dwc3_thead_optimize_power(thead);
+
+	return devm_of_platform_populate(dev);
+}
+
+static const struct of_device_id dwc3_thead_of_match[] = {
+	{ .compatible = "thead,th1520-usb" },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, dwc3_thead_of_match);
+
+static struct platform_driver dwc3_thead_driver = {
+	.probe		= dwc3_thead_probe,
+	.driver		= {
+		.name	= "dwc3-thead",
+		.of_match_table	= dwc3_thead_of_match,
+	},
+};
+module_platform_driver(dwc3_thead_driver);
+
+MODULE_LICENSE("GPL v2");
+MODULE_DESCRIPTION("DesignWare DWC3 T-HEAD Glue Driver");
+MODULE_AUTHOR("Jisheng Zhang <jszhang@kernel.org>");
diff --git a/drivers/watchdog/Kconfig b/drivers/watchdog/Kconfig
index 751458959411..b26aac73333a 100644
--- a/drivers/watchdog/Kconfig
+++ b/drivers/watchdog/Kconfig
@@ -2044,6 +2044,20 @@ config STARFIVE_WATCHDOG
 	  Say Y here to support the watchdog of StarFive JH7100 and JH7110
 	  SoC. This driver can also be built as a module if choose M.
 
+config LIGHT_PMIC_WATCHDOG
+	tristate "THEAD Light pmic watchdog"
+	depends on THEAD_LIGHT_MBOX
+	select WATCHDOG_CORE
+	help
+	  This is the driver for the hardware watchdog on Light Board. This watchdog
+	  simply watches your kernel to make sure it doesn't freeze, and if
+	  it does, it reboots your computer after a certain amount of time.
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called acquirewdt.
+
+	  Most people will say N.
+
 # S390 Architecture
 
 config DIAG288_WATCHDOG
diff --git a/drivers/watchdog/Makefile b/drivers/watchdog/Makefile
index 7eab9de311cb..5c36e33f8b6e 100644
--- a/drivers/watchdog/Makefile
+++ b/drivers/watchdog/Makefile
@@ -196,6 +196,7 @@ obj-$(CONFIG_WATCHDOG_RTAS) += wdrtas.o
 
 # RISC-V Architecture
 obj-$(CONFIG_STARFIVE_WATCHDOG) += starfive-wdt.o
+obj-$(CONFIG_LIGHT_PMIC_WATCHDOG) += light_wdt.o
 
 # S390 Architecture
 obj-$(CONFIG_DIAG288_WATCHDOG) += diag288_wdt.o
diff --git a/drivers/watchdog/light_wdt.c b/drivers/watchdog/light_wdt.c
new file mode 100644
index 000000000000..d5fa5f77cec1
--- /dev/null
+++ b/drivers/watchdog/light_wdt.c
@@ -0,0 +1,376 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/init.h>
+#include <linux/interrupt.h>
+#include <linux/io.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+#include <linux/device.h>
+#include <linux/watchdog.h>
+#include <linux/firmware/thead/ipc.h>
+#include <linux/firmware/thead/light_event.h>
+
+#define DRV_NAME	"light-wdt"
+
+/*
+ *   Watchdog selector to timeout in seconds.
+ *   0: WDT disabled;
+ *   others: timeout = 2048 ms * 2^(TWDSCALE-1).
+ */
+static const unsigned int wdt_timeout[] = {8, 16, 32,128};
+#define LIGHT_TWDSCALE_DISABLE		0
+#define LIGHT_TWDSCALE_MIN		1
+#define LIGHT_TWDSCALE_MAX		(ARRAY_SIZE(wdt_timeout) - 1)
+#define LIGHT_WDT_MIN_TIMEOUT		wdt_timeout[LIGHT_TWDSCALE_MIN]
+#define LIGHT_WDT_MAX_TIMEOUT		wdt_timeout[LIGHT_TWDSCALE_MAX]
+#define LIGHT_WDT_TIMEOUT		wdt_timeout[3]
+#define LIGHT_RESET_PROTECTION_MS	256
+
+struct light_aon_msg_wdg_ctrl {
+	struct light_aon_rpc_msg_hdr hdr;
+	u32 timeout;
+	u32 running_state;
+	u32 reserved[4];
+}_packed __aligned(4);
+
+struct light_wdt_device {
+	struct device *dev;
+	struct light_aon_ipc *ipc_handle;
+	struct light_aon_msg_wdg_ctrl msg;
+	unsigned int    is_aon_wdt_ena;
+};
+
+struct light_wdt_device *light_power_off_wdt;
+
+static unsigned int light_wdt_timeout_to_sel(unsigned secs)
+{
+	unsigned int i;
+
+	for (i = LIGHT_TWDSCALE_MIN; i <= LIGHT_TWDSCALE_MAX; i++) {
+		if (wdt_timeout[i] >= secs)
+			return i;
+	}
+
+	return LIGHT_TWDSCALE_MAX;
+}
+
+static void light_wdt_msg_hdr_fill(struct light_aon_rpc_msg_hdr *hdr, enum light_aon_misc_func func)
+{
+	hdr->ver = LIGHT_AON_RPC_VERSION;
+	hdr->svc = (uint8_t)LIGHT_AON_RPC_SVC_MISC;
+	hdr->func = (uint8_t)func;
+	hdr->size = LIGHT_AON_RPC_MSG_NUM;
+}
+
+static int light_wdt_is_running(struct light_wdt_device *wdt_dev)
+{
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_GET_STATE);
+	wdt_dev->msg.running_state = -1;
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret)
+		return ret;
+
+	pr_debug("ret = %d, timeout = %d, running_state = %d\n", ret, wdt_dev->msg.timeout,
+			wdt_dev->msg.running_state);
+
+	return wdt_dev->msg.running_state;
+}
+
+static int light_wdt_update_timeout(struct light_wdt_device *wdt_dev, unsigned int timeout)
+{
+	/*
+	 * The watchdog triggers a reboot if a timeout value is already
+	 * programmed because the timeout value combines two functions
+	 * in one: indicating the counter limit and starting the watchdog.
+	 * The watchdog must be disabled to be able to change the timeout
+	 * value if the watchdog is already running. Then we can set the
+	 * new timeout value which enables the watchdog again.
+	 */
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_TIMEOUTSET);
+	wdt_dev->msg.timeout = timeout;
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int light_wdt_set_timeout(struct watchdog_device *wdd, unsigned int timeout)
+{
+	struct light_wdt_device *wdt_dev = watchdog_get_drvdata(wdd);
+	int ret = 0;
+
+	/*
+	 * There are two cases when a set_timeout() will be called:
+	 * 1. The watchdog is off and someone wants to set the timeout for the
+	 *    further use.
+	 * 2. The watchdog is already running and a new timeout value should be
+	 *    set.
+	 *
+	 * The watchdog can't store a timeout value not equal zero without
+	 * enabling the watchdog, so the timeout must be buffered by the driver.
+	 */
+	if (watchdog_active(wdd))
+		ret = light_wdt_update_timeout(wdt_dev, timeout);
+	else
+		wdd->timeout = wdt_timeout[light_wdt_timeout_to_sel(timeout)];
+
+	return ret;
+}
+
+static int light_wdt_start(struct watchdog_device *wdd)
+{
+	struct light_wdt_device *wdt_dev = watchdog_get_drvdata(wdd);
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_START);
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int light_wdt_stop(struct watchdog_device *wdd)
+{
+	struct light_wdt_device *wdt_dev = watchdog_get_drvdata(wdd);
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_STOP);
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int light_wdt_ping(struct watchdog_device *wdd)
+{
+	struct light_wdt_device *wdt_dev = watchdog_get_drvdata(wdd);
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_PING);
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+static int light_wdt_restart(struct watchdog_device *wdd, unsigned long action, void *data)
+{
+	struct light_wdt_device *wdt_dev = watchdog_get_drvdata(wdd);
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_RESTART);
+
+	pr_debug("[%s,%d]: Inform aon to restart the whole system....\n", __func__, __LINE__);
+
+	light_event_set_rebootmode(LIGHT_EVENT_SW_REBOOT);
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, false);
+	if (ret)
+		return ret;
+	pr_debug("[%s,%d]: Finish to inform aon to restart the whole system....\n", __func__, __LINE__);
+
+	return 0;
+}
+
+static const struct watchdog_info light_watchdog_info = {
+	.options = WDIOF_SETTIMEOUT | WDIOF_KEEPALIVEPING,
+	.identity = "Light Watchdog",
+};
+
+
+static const struct watchdog_ops light_watchdog_ops = {
+	.owner = THIS_MODULE,
+	.start = light_wdt_start,
+	.stop = light_wdt_stop,
+	.ping = light_wdt_ping,
+	.set_timeout = light_wdt_set_timeout,
+	.restart = light_wdt_restart,
+};
+
+static ssize_t aon_sys_wdt_show(struct device *dev,
+				struct device_attribute *attr, char *buf)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct light_wdt_device *wdt_dev = platform_get_drvdata(pdev);
+	return sprintf(buf,"%u\n",wdt_dev->is_aon_wdt_ena);
+}
+
+static ssize_t aon_sys_wdt_store(struct device *dev,
+				 struct device_attribute *attr,
+				 const char *buf, size_t size)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct light_wdt_device *wdt_dev = platform_get_drvdata(pdev);
+	struct light_aon_ipc *ipc;
+	int ret;
+	char *start = (char *)buf;
+	unsigned long val;
+
+	ipc = wdt_dev->ipc_handle;
+	val = simple_strtoul(start, &start, 0);
+	wdt_dev->is_aon_wdt_ena = val;
+	if (val)
+		light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_AON_WDT_ON);
+	else
+		light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_AON_WDT_OFF);
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+	if (ret){
+		pr_err("%s: err:%d \n",__func__,ret);
+		return -EINVAL;
+	}
+	return size;
+}
+
+void light_pm_power_off(void)
+{
+	struct light_wdt_device *wdt_dev = light_power_off_wdt;
+	struct light_aon_ipc *ipc = wdt_dev->ipc_handle;
+	int ret;
+
+	pr_info("[%s,%d]poweroff system...\n", __func__, __LINE__);
+
+	light_wdt_msg_hdr_fill(&wdt_dev->msg.hdr, LIGHT_AON_MISC_FUNC_WDG_POWER_OFF);
+
+	ret = light_aon_call_rpc(ipc, &wdt_dev->msg, true);
+
+	if (ret)
+		pr_err("failed to power off the system\n");
+}
+
+
+static DEVICE_ATTR(aon_sys_wdt, 0644, aon_sys_wdt_show, aon_sys_wdt_store);
+
+static struct attribute *aon_sys_wdt_sysfs_entries[] = {
+	&dev_attr_aon_sys_wdt.attr,
+	NULL
+};
+static const struct attribute_group dev_attr_aon_sys_wdt_group = {
+	.attrs = aon_sys_wdt_sysfs_entries,
+};
+
+static int light_wdt_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct light_wdt_device *wdt_dev;
+	int ret;
+	struct watchdog_device *wdd;
+
+	wdt_dev = devm_kzalloc(dev, sizeof(*wdt_dev), GFP_KERNEL);
+	if (!wdt_dev)
+		return -ENOMEM;
+	wdt_dev->is_aon_wdt_ena = 0;
+
+	ret = light_aon_get_handle(&(wdt_dev->ipc_handle));
+	if (ret == -EPROBE_DEFER)
+		return ret;
+
+	wdd = devm_kzalloc(dev, sizeof(*wdd), GFP_KERNEL);
+	if (!wdd)
+		return -ENOMEM;
+
+	wdd->info = &light_watchdog_info;
+	wdd->ops = &light_watchdog_ops;
+	wdd->min_timeout = LIGHT_WDT_MIN_TIMEOUT;
+	wdd->max_timeout = LIGHT_WDT_MAX_TIMEOUT;
+	wdd->min_hw_heartbeat_ms = LIGHT_RESET_PROTECTION_MS;
+	wdd->status = WATCHDOG_NOWAYOUT_INIT_STATUS;
+
+	watchdog_set_restart_priority(wdd, 128);
+	watchdog_set_drvdata(wdd, wdt_dev);
+
+	/* Set default timeout, maybe default value if the watchdog is running */
+	wdd->timeout = LIGHT_WDT_TIMEOUT;
+	watchdog_init_timeout(wdd, 0, dev);
+	light_wdt_set_timeout(wdd, wdd->timeout);
+
+	platform_set_drvdata(pdev, wdt_dev);
+	ret = light_wdt_is_running(wdt_dev);
+	if (ret < 0) {
+		pr_err("failed to get pmic wdt running state\n");
+		return ret;
+	}
+
+	if (ret) {
+		light_wdt_update_timeout(wdt_dev, wdd->timeout);
+		set_bit(WDOG_HW_RUNNING, &wdd->status);
+	}
+
+	ret = devm_watchdog_register_device(dev, wdd);
+	if (ret)
+		return ret;
+
+	pr_info("[%s,%d] register power off callback\n", __func__, __LINE__);
+
+	pm_power_off = light_pm_power_off;
+
+	light_power_off_wdt = wdt_dev;
+
+	ret = sysfs_create_group(&pdev->dev.kobj, &dev_attr_aon_sys_wdt_group);
+	if (ret) {
+		dev_err(&pdev->dev, "Failed to create aon_sys_wdt sysfs.\n");
+		return ret;
+	}
+
+	pr_info("succeed to register light pmic watchdog\n");
+
+	return 0;
+}
+
+static struct platform_driver light_wdt_driver = {
+	.driver = {
+		.name = DRV_NAME,
+	},
+	.probe = light_wdt_probe,
+};
+
+static int __init light_wdt_init(void)
+{
+	static struct platform_device *pdev;
+	int ret;
+
+	pdev = platform_device_register_simple(DRV_NAME, -1, NULL, 0);
+	if (IS_ERR(pdev))
+		return PTR_ERR(pdev);
+
+	ret = platform_driver_register(&light_wdt_driver);
+	if (ret) {
+		platform_device_unregister(pdev);
+		return PTR_ERR(pdev);
+	}
+
+	pr_info("Watchdog module: %s loaded\n", DRV_NAME);
+
+	return 0;
+}
+device_initcall(light_wdt_init);
+
+MODULE_AUTHOR("Wei.Liu <lw312886@linux.alibaba.com>");
+MODULE_DESCRIPTION("PMIC Watchdog Driver for Light");
+MODULE_LICENSE("GPL");
diff --git a/include/dt-bindings/clock/light-dspsys.h b/include/dt-bindings/clock/light-dspsys.h
new file mode 100644
index 000000000000..6473e12623c6
--- /dev/null
+++ b/include/dt-bindings/clock/light-dspsys.h
@@ -0,0 +1,25 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef _LIGHT_DSPSYS_H
+#define _LIGHT_DSPSYS_H
+
+#define CLKGEN_DSP0_PCLK			0
+#define CLKGEN_DSP0_CCLK                        1
+#define CLKGEN_DSP1_PCLK                        2
+#define CLKGEN_DSP1_CCLK                        3
+#define CLKGEN_X2X_X4_DSPSLV_DSP0_ACLK_M        4
+#define CLKGEN_X2X_X4_DSPSLV_DSP1_ACLK_M        5
+#define CLKGEN_AXI4_DSPSYS_SLV_ACLK             6
+#define CLKGEN_AXI4_DSPSYS_ACLK                 7
+#define CLKGEN_IOPMP_DSP0_PCLK                  8
+#define CLKGEN_IOPMP_DSP1_PCLK                  9
+#define CLKGEN_AXI4_DSPSYS_SLV_PCLK             10
+#define CLKGEN_AXI4_DSPSYS_PCLK                 11
+#define CLKGEN_X2X_DSP0_ACLK_S			12
+#define CLKGEN_X2X_DSP2_ACLK_S			13
+#define LIGHT_CLKGEN_DSPSYS_CLK_END		14
+
+#endif
diff --git a/include/dt-bindings/clock/light-fm-ap-clock.h b/include/dt-bindings/clock/light-fm-ap-clock.h
new file mode 100644
index 000000000000..8bb23b690f98
--- /dev/null
+++ b/include/dt-bindings/clock/light-fm-ap-clock.h
@@ -0,0 +1,513 @@
+#ifndef _APSYS_CLKGEN_H
+#define _APSYS_CLKGEN_H
+
+#define C910_CCLK_I0                                       0
+#define AXI4_CPUSYS1_ACLK                                  1
+#define CLKGEN_GPIO2_DBCLK                                 2
+#define CLKGEN_MBOX0_PCLK                                  3
+#define CLKGEN_GMAC0_CCLK                                  4
+#define CLKGEN_SPI_PCLK                                    5
+#define CLKGEN_CLK_OUT_1_CLK                               6
+#define PAD_RTC_CLK                                        7
+#define CLKGEN_SPINLOCK_HCLK                               8
+#define CLKGEN_QSPI1_PCLK                                  9
+#define CLKGEN_HDMI_ISCAN_CK_REF_CLK                       10
+#define CLKGEN_IOPMP_AON_PCLK                              11
+#define CLKGEN_ISP_RY_ACLK                                 12
+#define CLKGEN_MIPIDSI0_SCANRXCLKESC                       13
+#define CLKGEN_EIP120SII_HCLK                              14
+#define CLKGEN_MIPI_CSI0_PIXCLK                            15
+#define CLKGEN_SRAM_AXI_ACLK_3                             16
+#define CLKGEN_PERISYS_AHB_HCLK                            17
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK0_CLK                  18
+#define CLKGEN_QSPI0_SSI_CLK                               19
+#define CLKGEN_DW200_ACLK                                  20
+#define CLKGEN_IOPMP_EIP120SIII_PCLK                       21
+#define VISYS_MIPI_CSI2_CFGCLK                             22
+#define CLKGEN_APB3_CPUSYS_HCLK                            23
+#define CLKGEN_PERISYS_APB1_HCLK                           24
+#define CLKGEN_GPU_CORE_CLK                                25
+#define CLKGEN_USB3_DRD_ACLK                               26
+#define CLKGEN_VISYS_ACLK                                  27
+#define CLKGEN_USB3_DRD_CTRL_REF_CLK                       28
+#define CLKGEN_TEE_DMAC_ACLK                               29
+#define CLKGEN_AUDIO_SUBSYS_ACLK_CP2AP                     30
+#define CLKGEN_SRAM_AXI_ACLK_2                             31
+#define CLKGEN_IOPMP_VOSYS_GPU_PCLK                        32
+#define CLKGEN_CFG2TEE_X2H_ACLK                            33
+#define CLKGEN_SRAM_AXI_ACLK_1                             34
+#define MISC_SDIO0_OSC_CLK                                 35
+#define CLKGEN_SDIO0_ACLK                                  36
+#define CLKGEN_MIPI_DSI1_CFGCLK                            37
+#define APB3_CPUSYS_PCLK                                   38
+#define CLKGEN_TEE_DMAC_HCLK                               39
+#define VOSYS_DPU0_PIXELCLK                                40
+#define CLKGEN_CPU2CFG_X2H_MHCLK                           41
+#define CLKGEN_VPSYS_ACLK                                  42
+#define CLKGEN_MIPIDSI1_SCANRXCLKESC                       43
+#define CLKGEN_MISC2VP_X2X_ACLK_S                          44
+#define CLKGEN_MIPI_CSI_SCANBYTECLK                        45
+#define CLKGEN_APB3_TEESYS_HCLK                            46
+#define VENC_CCLK                                          47
+#define VPSYS_VDEC_CCLK                                    48
+#define CLKGEN_MIPI_CSI0_CFG_CLK                           49
+#define CLKGEN_MISCSYS_BUS_CLK                             50
+#define CLKGEN_DPU_HCLK                                    51
+#define CLKGEN_UART1_SCLK                                  52
+#define GMAC_PLL_FOUTPOSTDIV                               53
+#define MISC_BUS_CLK                                       54
+#define CLKGEN_USB3_DRD_SPDCLK                             55
+#define CLKGEN_MIPI_CSI2_CFG_CLK                           56
+#define CLKGEN_TOP_AXI4S_ACLK                              57
+#define CLKGEN_IOPMP_EIP120SII_ACLK                        58
+#define CORE_CLK                                           59
+#define CLKGEN_VPSYS_FCE_ACLK                              60
+#define CLKGEN_I2C3_PCLK                                   61
+#define DPU1_PLL_DIV_CLK                                   62
+#define CLKGEN_USB3_DRD_PHY_REF_CLK                        63
+#define CLKGEN_AON2CPU_A2X_ACLK                            64
+#define CLKGEN_QSPI1_SSI_CLK                               65
+#define CLKGEN_DPU_CCLK                                    66
+#define VISYS_MASTER_BUS_ACLK                              67
+#define CLKGEN_PERI_I2S_SRC_CLK_0                          68
+#define VOSYS_ACLK_M                                       69
+#define TEESYS_I0_HCLK                                     70
+#define CLKGEN_MIPI_DSI1_REFCLK                            71
+#define CLKGEN_MIPI_DSI0_PCLK                              72
+#define CLKGEN_VOSYS_ACLK_S                                73
+#define CLKGEN_CPU2VP_X2P_PCLK                             74
+#define CLKGEN_X2X_CPUSYS_ACLK_S                           75
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK1_CLK                 76
+#define CLKGEN_IOPMP_VOSYS_DPU1_PCLK                       77
+#define CLKGEN_MISC2VP_X2X_ACLK_M                          78
+#define CLKGEN_WDT0_PCLK                                   79
+#define VOSYS_MIPIDSI0_SCANTXCLKESC                        80
+#define VISYS_MIPI_CSI1_CFGCLK                             81
+#define AHB2_CPUSYS_HCLK                                   82
+#define CLKGEN_SDIO1_HCLK                                  83
+#define CLKGEN_SDIO0_HCLK                                  84
+#define CLKGEN_CLK_OUT_3_CLK                               85
+#define CLKGEN_GMAC_AXI_ACLK                               86
+#define GMAC_CCLK                                          87
+#define CLKGEN_VIPRE_PCLK                                  88
+#define CLKGEN_HDMI_ISCAN_TX_CK_OUT2_CLK                   89
+#define CLKGEN_MIPIDSI1_SCANTXCLKESC                       90
+#define CLKGEN_VISYS_SLAVE_HCLK                            91
+#define VOSYS_HDMI_ISCAN_TX_CK_OUT1_CLK                    92
+#define CLKGEN_X2X_CPUSYS_ACLK_M                           93
+#define CLKGEN_CPU2CFG_X2X_ACLK_S                          94
+#define C910_OSC_CLK                                       95
+#define CLKGEN_X2H_DPU1_ACLK                               96
+#define CLKGEN_I2C4_PCLK                                   97
+#define CLKGEN_GMAC0_ACLK                                  98
+#define MISC_USB3_PHY_REF_CLK                              99
+#define VOSYS_MIPIDSI0_CFG_CLK                             100
+#define CLKGEN_VPSYS_VDEC_CCLK                             101
+#define VOSYS_MIPIDSI1_CFG_CLK                             102
+#define CLKGEN_I2S_PCLK                                    103
+#define CLKGEN_DMAC_CPUSYS_ACLK                            104
+#define VISYS_DW200_CLK_DWE                                105
+#define CLKGEN_OCRAM_HCLK                                  106
+#define CLKGEN_EFUSE_PCLK                                  107
+#define CLKGEN_X2H_DPU_ACLK                                108
+#define CLKGEN_IOPMP_SDIO0_ACLK                            109
+#define VOSYS_DPU1_PIXELCLK                                110
+#define CPU_PLL1_FOUT4                                     111
+#define CLKGEN_GPIO2_PCLK                                  112
+#define CLKGEN_GMAC1_CCLK                                  113
+#define CPU_PLL1_FOUTPOSTDIV                               114
+#define VOSYS_HDMI_ISCAN_40M_CLK                           115
+#define CLKGEN_VOSYS_X2X_ACLK_S                            116
+#define CLKGEN_PERISYS_APB2_HCLK                           117
+#define VOSYS_OSC_CLK_MUX_I2S_CLK_OCCBUF                   118
+#define CLKGEN_HDMI_CEC_CLK                                119
+#define CLKGEN_X2P_X4_VOSYS_PCLK                           120
+#define CLKGEN_VOSYS_ACLK_M                                121
+#define CLKGEN_EMMC_SDIO_REF_CLK                           122
+#define CLKGEN_IOPMP_EMMC_ACLK                             123
+#define VIDEO_PLL_FOUTVCO                                  124
+#define CLKGEN_HDMI_ISCAN_CKO_WORD_CLK                     125
+#define CLKGEN_IOPMP_VOSYS_DPU_PCLK                        126
+#define CLKGEN_AXI4_VISYS3_ACLK                            127
+#define CLKGEN_VISYS_SYSREG_PCLK                           128
+#define CLKGEN_MIPIDSI0_SCANTXCLKESC                       129
+#define CLKGEN_HDMI_ISCAN_TX_CK_OUT1_CLK                   130
+#define CLKGEN_IOPMP_EIP120SIII_ACLK                       131
+#define CLKGEN_EIP120SII_ACLK                              132
+#define CLKGEN_MBOX2_PCLK                                  133
+#define CLKGEN_AXI4_VISYS1_ACLK                            134
+#define CLKGEN_UART1_PCLK                                  135
+#define CLK_OUT_3                                          136
+#define CLKGEN_UART5_SCLK                                  137
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK2_CLK                 138
+#define CLKGEN_MBOX3_PCLK                                  139
+#define QSPI1_SSI_CLK                                      140
+#define CLKGEN_I2C1_PCLK                                   141
+#define CLKGEN_HDMI_I2S_CLK                                142
+#define CLKGEN_AXI4_CPUSYS2_PCLK                           143
+#define CLKGEN_CFG2TEE_X2H_MHCLK                           144
+#define CLKGEN_C910_CPU_CLK                                145
+#define VOSYS_HDMI_ISCAN_TX_CK_OUT2_CLK                    146
+#define CLKGEN_HDMI_PCLK                                   147
+#define CLKGEN_IOPMP_EIP120SII_PCLK                        148
+#define CLKGEN_MISCSYS_AXI_PCLK                            149
+#define CLKGEN_EIP120SI_ACLK                               150
+#define TEESYS_I1_HCLK                                     151
+#define PERISYS_APB_PCLK                                   152
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK0_DIV2_CLK             153
+#define CLKGEN_TIMER0_CCLK                                 154
+#define CLKGEN_IOPMP_USB3_ACLK                             155
+#define CLKGEN_UART2_PCLK                                  156
+#define CLK_OUT_4                                          157
+#define AXI4_CPUSYS2_ACLK                                  158
+#define CLKGEN_AUDIO_SUBSYS_ACLK_AP2CP                     159
+#define CLKGEN_I2C3_IC_CLK                                 160
+#define CLKGEN_IOPMP_GPU_ACLK                              161
+#define CLKGEN_TIMER1_CCLK                                 162
+#define VOSYS_I2S_CLK                                      163
+#define CLKGEN_I2C5_IC_CLK                                 164
+#define VOSYS_OSC_CLK_MUX_I2S_CLK                          165
+#define CLKGEN_DDR_SUBSYS_ACLK_0                           166
+#define CLKGEN_TIMER1_PCLK                                 167
+#define CLKGEN_I2C1_IC_CLK                                 168
+#define CLKGEN_I2S_SRC_CLK                                 169
+#define VISYS_DW200_CLK_VSE                                170
+#define CLKGEN_MIPIDSI1_PIXCLK                             171
+#define VOSYS_RTC_CLK                                      172
+#define CLK_OUT_1                                          173
+#define CLKGEN_PERISYS_APB4_HCLK                           174
+#define MISC_USB3_CTRL_REF_CLK                             175
+#define CLKGEN_TEE_SYSREG_PCLK                             176
+#define CLKGEN_MISCSYS_AXI_ACLK                            177
+#define CLKGEN_MIPIDSI1_SCANCLK                            178
+#define CLKGEN_GPIO3_DBCLK                                 179
+#define CLKGEN_HDMI_ISCAN_40M_CLK                          180
+#define CLKGEN_PERI2PERI1_APB_HCLK                         181
+#define CLKGEN_GMAC0_HCLK                                  182
+#define CLKGEN_DDR_SUBSYS_PCLK                             183
+#define VOSYS_PCLK                                         184
+#define CLKGEN_MIPIDSI1_SCANBYTECLK                        185
+#define CLKGEN_VPSYS_G2D_ACLK                              186
+#define CLKGEN_EIP150B_HCLK                                187
+#define CLKGEN_UART4_SCLK                                  188
+#define DPU1_PLL_TEST_CLK                                  189
+#define CLKGEN_VOSYS_X2X_ACLK_M                            190
+#define CLKGEN_IOPMP_EIP120SI_ACLK                         191
+#define CLKGEN_CLK_OUT_4_CLK                               192
+#define CLKGEN_GPIO0_FPCLK                                 193
+#define PAD_OSC_CLK                                        194
+#define CLKGEN_C910_BUS_CLK_NO_ICG                         195
+#define CLKGEN_TIMER0_PCLK                                 196
+#define CLKGEN_AHB2_CPUSYS_HCLK                            197
+#define EMMC_SDIO_REF_CLK                                  198
+#define CLKGEN_IOPMP_CHIP_DBG_PCLK                         199
+#define CLKGEN_BMU_C910_PCLK                               200
+#define CLKGEN_IOPMP_DPU1_ACLK                             201
+#define CLKGEN_PADCTRL0_APSYS_PCLK                         202
+#define MISC_SDIO1_OSC_CLK                                 203
+#define CLKGEN_C910_OSC_CLK                                204
+#define VISYS_ISP_RY_CCLK                                  205
+#define CLKGEN_VPSYS_PCLK                                  206
+#define VISYS_MIPI_CSI0_PIXELCLK                           207
+#define NPU_CCLK                                           208
+#define CLKGEN_AXI4_TEESYS_ACLK                            209
+#define PERI2SYS_APB_PCLK                                  210
+#define CLKGEN_IOPMP_GMAC0_PCLK                            211
+#define CLKGEN_VPSYS_G2D_PCLK                              212
+#define CLKGEN_EMMC_ACLK                                   213
+#define CLKGEN_UART3_SCLK                                  214
+#define AONSYS_BUS_CLK                                     215
+#define DPU0_PLL_FOUT4                                     216
+#define VOSYS_MIPIDSI1_SCANCLK                             217
+#define CLKGEN_UART4_PCLK                                  218
+#define CLKGEN_HDMI_ISCAN_SCL                              219
+#define CLKGEN_MIPI_CSI1_PIXCLK                            220
+#define CLKGEN_APSYS_CLKGEN_PCLK                           221
+#define CLKGEN_GPU_TIMER_REFCLK                            222
+#define GMAC_PLL_FOUT1PH0                                  223
+#define VOSYS_MIPIDSI1_SCANBYTECLK                         224
+#define CLKGEN_GPIO3_FPCLK                                 225
+#define CLKGEN_SDIO1_OSC_CLK                               226
+#define CLKGEN_GPIO3_PCLK                                  227
+#define CLKGEN_VPSYS_AXI_ACLK                              228
+#define CLKGEN_HDMI_ISCAN_TX_CK_20B_CLK                    229
+#define CLKGEN_VOSYSREG_PCLK                               230
+#define VIDEO_PLL_TEST_CLK                                 231
+#define CLKGEN_MBOX1_PCLK                                  232
+#define CLKGEN_I2C2_IC_CLK                                 233
+#define VOSYS_MIPIDSI0_PLL_SCANCLK                         234
+#define VOSYS_MIPIDSI1_SCANTXCLKESC                        235
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK1_DIV2_CLK             236
+#define CLKGEN_UART2_SCLK                                  237
+#define MISC_TEESYS_PCLK                                   238
+#define AUDIO_PLL_TEST_CLK                                 239
+#define CLKGEN_DPU_PIXELCLK1                               240
+#define CLKGEN_IOPMP_TEEDMAC_PCLK                          241
+#define CLKGEN_TOP_APB_SX_PCLK                             242
+#define CLKGEN_I2C4_IC_CLK                                 243
+#define GMAC_PLL_TEST_CLK                                  244
+#define CLKGEN_HDMI_JTAG_TCLK                              245
+#define VISYS_MIPI_CSI0_CFGCLK                             246
+#define CLKGEN_CPU2AON_X2H_ACLK                            247
+#define VOSYS_HDMI_ISCAN_TX_CK_OUT0_CLK                    248
+#define QSPI_SSI_CLK                                       249
+#define VOSYS_DPU_CCLK                                     250
+#define CLKGEN_CPU2VI_X2H_MHCLK                            251
+#define CLKGEN_MIPI_DSI0_REFCLK                            252
+#define CLKGEN_DSPSYS_HCLK                                 253
+#define CLKGEN_IOPMP_AUD_PCLK                              254
+#define CLKGEN_PERI2PERI1_APB_PCLK                         255
+#define CFG_AXI_ACLK                                       256
+#define VPSYS_FCE_CCLK                                     257
+#define CLKGEN_HDMI_ISCAN_CLK                              258
+#define CPU_PLL0_TEST_CLK                                  259
+#define CLKGEN_CPU2PERI_X2H_MHCLK                          260
+#define VISYS_ACLK_M                                       261
+#define VOSYS_HDMI_JTAG_TCLK                               262
+#define CLKGEN_IOPMP_AUD_ACLK                              263
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK1_DIV2_CLK            264
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK1_CLK                  265
+#define VOSYS_MIPIDSI0_REFCLK                              266
+#define CLKGEN_VISYS_ACLK_M                                267
+#define VOSYS_MIPIDSI0_SCANRXCLKESC                        268
+#define CLKGEN_SDIO1_ACLK                                  269
+#define CFG_APB_PCLK                                       270
+#define CLKGEN_PADCTRL1_APSYS_PCLK                         271
+#define VOSYS_MIPIDSI0_SCANCLK                             272
+#define CLKGEN_I2C0_IC_CLK                                 273
+#define CLKGEN_VPSYS_APB_PCLK                              274
+#define CLKGEN_VPSYS_VENC_CCLK                             275
+#define CLKGEN_AXI4_CFG_BUS_ACLK                           276
+#define CLKGEN_MIPIDSI0_SCANBYTECLK                        277
+#define GPIO3_DBCLK                                        278
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK0_CLK                 279
+#define CLKGEN_UART5_PCLK                                  280
+#define DPU0_PLL_FOUTPOSTDIV_ICG                           281
+#define CPU_PLL0_FOUT4                                     282
+#define CLKGEN_GPIO2_FPCLK                                 283
+#define CLKGEN_DPU_ACLK                                    284
+#define CLKGEN_AXI4_CPUSYS2_ACLK                           285
+#define CLKGEN_DSPSYS_PCLK                                 286
+#define TEE_PLL_FOUTPOSTDIV                                287
+#define TIMER_CCLK                                         288
+#define VOSYS_MIPIDSI1_PLL_SCANCLK                         289
+#define CLKGEN_GMAC_AXI_PCLK                               290
+#define CLKGEN_USB3_DRD_PCLK                               291
+#define CLKGEN_AXI4_CPUSYS1_PCLK                           292
+#define VOSYS_ACLK                                         293
+#define CLKGEN_IOPMP_EIP120SI_PCLK                         294
+#define VOSYS_HDMI_ISCAN_TMDSCLKIN_CLK                     295
+#define VOSYS_HDMI_ISCAN_CKO_WORD_CLK                      296
+#define CLKGEN_NPUSYS_AXI_ACLK                             297
+#define CLKGEN_IOPMP_SDIO0_PCLK                            298
+#define CLKGEN_DW200_HCLK                                  299
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK2_CLK                  300
+#define CLKGEN_UART0_PCLK                                  301
+#define CLKGEN_CLK_OUT_2_CLK                               302
+#define CLKGEN_GPIO0_PCLK                                  303
+#define CLKGEN_EMMC_OSC_CLK                                304
+#define VPSYS_APB_PCLK                                     305
+#define CLKGEN_HDMI_PIXCLK                                 306
+#define CLKGEN_IOPMP_TEEDMAC_ACLK                          307
+#define AUDIO_PLL_FOUT4                                    308
+#define CLKGEN_MIPI_CSI2_PCLK                              309
+#define CLKGEN_MIPI_DSI1_PCLK                              310
+#define CLKGEN_MIPI_DSI0_CFGCLK                            311
+#define VISYS_ISP0_CLK                                     312
+#define VISYS_ISP1_CLK                                     313
+#define MISC_EMMC_OSC_CLK                                  314
+#define DPU0_PLL_FOUTPOSTDIV                               315
+#define VISYS_AHB_HCLK                                     316
+#define CLKGEN_IOPMP_SDIO1_ACLK                            317
+#define CLKGEN_EMMC_HCLK                                   318
+#define I2S_CLK                                            319
+#define CLKGEN_CPU2PERI_X2H_ACLK                           320
+#define VPSYS_AXI_ACLK                                     321
+#define CLKGEN_IOPMP_SDIO1_PCLK                            322
+#define CLKGEN_EIP120SIII_HCLK                             323
+#define CLKGEN_BMU_C910_ACLK                               324
+#define CLKGEN_IOPMP_DMAC_CPUSYS_PCLK                      325
+#define GPIO2_DBCLK                                        326
+#define CHIP_DBG_CCLK                                      327
+#define CLKGEN_MISCSYS_TEE_CCLK                            328
+#define CLKGEN_I2C5_PCLK                                   329
+#define CLKGEN_X2H_CPUSYS_MHCLK                            330
+#define CLKGEN_PWM_CCLK                                    331
+#define DPU0_PLL_TEST_CLK                                  332
+#define CLKGEN_VISYS_PCLK                                  333
+#define MISC_TEESYS_HCLK                                   334
+#define SPI_SSI_CLK                                        335
+#define CLKGEN_PWM_PCLK                                    336
+#define VOSYS_MIPIDSI1_SCANRXCLKESC                        337
+#define QSPI0_SSI_CLK                                      338
+#define CLKGEN_HDMI_ISCAN_TMDSCLKIN_CLK                    339
+#define CLKGEN_SPI_SSI_CLK                                 340
+#define VIDEO_PLL_FOUT4                                    341
+#define CLKGEN_IOPMP_GMAC0_ACLK                            342
+#define CLKGEN_VIPRE_ACLK                                  343
+#define MISC_OSC_CLK_DIV24                                 344
+#define CLKGEN_ISP_VENC_SHAKE_PCLK                         345
+#define CLKGEN_HDMI_ISCAN_TX_CK_OUT0_CLK                   346
+#define CLKGEN_VPSYS_G2D_CCLK                              347
+#define CLKGEN_CPU2CFG_X2X_ACLK_M                          348
+#define CLKGEN_GMAC1_PCLK                                  349
+#define CLKGEN_MIPIDSI0_PLL_SCANCLK                        350
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK0_DIV2_CLK            351
+#define TEE_PLL_FOUT4                                      352
+#define PERISYS_AHB_HCLK                                   353
+#define VIDEO_PLL_FOUT1PH0                                 354
+#define CLKGEN_MIPIDSI0_PIXCLK                             355
+#define CLKGEN_PERI_I2S_SRC_CLK_1                          356
+#define CLKGEN_MIPI_CSI0_PCLK                              357
+#define CLKGEN_DDR_SUBSYS_ACLK_1                           358
+#define CLKGEN_GMAC0_PCLK                                  359
+#define CLK_OUT_2                                          360
+#define CLKGEN_EIP120SIII_ACLK                             361
+#define AONSYS_HCLK                                        362
+#define CLKGEN_ISP0_CLK                                    363
+#define CLKGEN_C910_BROM_HCLK                              364
+#define DPU1_PLL_FOUT4                                     365
+#define PERI_I2S_SRC_CLK                                   366
+#define CPU_PLL1_TEST_CLK                                  367
+#define CLKGEN_DDR_SUBSYS_ACLK_2                           368
+#define CLKGEN_MIPIDSI0_SCANCLK                            369
+#define I2C_IC_CLK                                         370
+#define CLKGEN_DPU_PIXELCLK0                               371
+#define CLKGEN_GPIO1_DBCLK                                 372
+#define CLKGEN_C910_TOP_DS_PCLK                            373
+#define CLKGEN_DSPSYS_ACLK_M                               374
+#define CLKGEN_AON2CPU_A2X_HCLK                            375
+#define VOSYS_HDMI_ISCAN_CK_REF_CLK                        376
+#define CLKGEN_IOPMP_EMMC_PCLK                             377
+#define NPU_CORE_CLK                                       378
+#define CLKGEN_IOPMP_USB3_PCLK                             379
+#define VPSYS_PCLK                                         380
+#define VIDEO_PLL_FOUTPOSTDIV                              381
+#define CLKGEN_CPU2VP_X2P_ACLK                             382
+#define CLKGEN_APB_CPU2CFG_HCLK                            383
+#define VOSYS_OSC_CLK_MUX_CEC_CLK_OCCBUF                   384
+#define CLKGEN_GPIO1_PCLK                                  385
+#define CLKGEN_APSYS_SYSREG_PCLK                           386
+#define CLKGEN_VISYS_HCLK                                  387
+#define CLKGEN_MIPI_CSI1_PCLK                              388
+#define CLKGEN_AHB2_TEESYS_HCLK                            389
+#define CLKGEN_DDR_SUBSYS_ACLK_4                           390
+#define SYS_PLL_TEST_CLK                                   391
+#define VISYS_MIPI_CSI_SCANCLK                             392
+#define CPU_PLL0_FOUTPOSTDIV                               393
+#define CLKGEN_UART3_PCLK                                  394
+#define CLKGEN_X2H_CPUSYS_ACLK                             395
+#define CLKGEN_MIPI_CSI1_CFG_CLK                           396
+#define CLKGEN_HDMI_ISCAN_RX_WORD_CLK2_DIV2_CLK            397
+#define CLKGEN_MISCSYS_APB_HCLK                            398
+#define CLKGEN_CPU2CFG_X2H_ACLK                            399
+#define CLKGEN_MIPI_CSI2_FPCLK                             400
+#define CLKGEN_ISP_RY_CCLK                                 401
+#define CLKGEN_X2P_VOSYS_ACLK                              402
+#define CLKGEN_VIPRE_PIXELCLK                              403
+#define VOSYS_GPU_TIMER_REFCLK                             404
+#define VOSYS_OSC_CLK_MUX_CEC_CLK                          405
+#define CLKGEN_APSYS_RSTGEN_PCLK                           406
+#define VOSYS_HDMI_ISCAN_SCL                               407
+#define CLKGEN_ISP_RY_HCLK                                 408
+#define VOSYS_OSC_CLK                                      409
+#define VISYS_PCLK                                         410
+#define CLKGEN_AXI4_VO_ACLK                                411
+#define CLKGEN_MIPIDSI1_PLL_SCANCLK                        412
+#define GPIO1_DBCLK                                        413
+#define CLKGEN_AXI4_VISYS2_ACLK                            414
+#define CLKGEN_EIP120SI_HCLK                               415
+#define CLKGEN_IOPMP_CHIP_DBG_ACLK                         416
+#define VOSYS_HDMI_ISCAN_TX_CK_20B_CLK                     417
+#define VOSYS_MIPIDSI1_REFCLK                              418
+#define CLKGEN_CHIP_DBG_ACLK                               419
+#define VOSYS_CFG_ACLK                                     420
+#define CLKGEN_VOSYS_AXI_ACLK                              421
+#define CPU_BUS_DFTCLK                                     422
+#define VOSYS_HDMI_ISCAN_CLK                               423
+#define VISYS_SLAVE_BUS_HCLK                               424
+#define CLKGEN_VPSYS_VDEC_PCLK                             425
+#define GMAC_PLL_FOUT4                                     426
+#define CLKGEN_QSPI0_PCLK                                  427
+#define CLKGEN_ISP1_CLK                                    428
+#define CLKGEN_MIPI_CSI0_FPCLK                             429
+#define CLKGEN_ISP0_ACLK                                   430
+#define CLKGEN_CPU2VI_X2H_ACLK                             431
+#define C910_CCLK                                          432
+#define CLKGEN_DW200_CLK_VSE                               433
+#define CLKGEN_AXI4_CPUSYS1_ACLK                           434
+#define CLKGEN_GPU_CFG_ACLK                                435
+#define CLKGEN_GPIO1_FPCLK                                 436
+#define CLKGEN_SRAM_AXI_ACLK_0                             437
+#define CLKGEN_I2C2_PCLK                                   438
+#define CLKGEN_IOPMP_GMAC1_PCLK                            439
+#define CLKGEN_ISP0_S_HCLK                                 440
+#define GPIO0_DBCLK                                        441
+#define CLKGEN_AXI4_VO_CFG_ACLK                            442
+#define CLKGEN_NPU_CORE_CLK                                443
+#define DPU0_PLL_DIV_CLK                                   444
+#define VOSYS_MIPIDSI0_SCANBYTECLK                         445
+#define CLKGEN_CHIP_DBG_CCLK                               446
+#define CLKGEN_DMAC_CPUSYS_HCLK                            447
+#define CLKGEN_IOPMP_DPU_ACLK                              448
+#define CLKGEN_DDR_SUBSYS_ACLK_3                           449
+#define CLK_100M                                           450
+#define CLKGEN_DSMART_PCLK                                 451
+#define CLKGEN_DW200_CLK_DWE                               452
+#define VPSYS_G2D_CCLK                                     453
+#define CLKGEN_WDT1_PCLK                                   454
+#define DPU1_PLL_FOUTPOSTDIV                               455
+#define CLKGEN_IOPMP_GMAC1_ACLK                            456
+#define CLKGEN_VPSYS_FCE_PCLK                              457
+#define CLKGEN_MIPI_CSI_SCANCLK                            458
+#define CLKGEN_MIPI_CSI2_PIXCLK                            459
+#define CLKGEN_I2C0_PCLK                                   460
+#define VOSYS_HDMI_ISCAN_RX_WORD_CLK2_DIV2_CLK             461
+#define CLKGEN_HDMI_SFR_CLK                                462
+#define TEE_PLL_TEST_CLK                                   463
+#define CLKGEN_IOPMP_DMAC_CPUSYS_ACLK                      464
+#define CLKGEN_ISP_PIXELCLK                                465
+#define CLKGEN_MIPI_CSI1_FPCLK                             466
+#define SYS_PLL_FOUT4                                      467
+#define CLKGEN_AXI4_VO_PCLK                                468
+#define CLKGEN_UART0_SCLK                                  469
+#define CLKGEN_CPU2AON_X2H_MHCLK                           470
+#define VISYS_MIPI_CSI_SCANBYTECLK                         471
+#define UART_SCLK                                          472
+#define CLKGEN_IOPMP_AON_ACLK                              473
+#define CLKGEN_VPSYS_VDEC_ACLK                             474
+#define CLKGEN_GMAC1_HCLK                                  475
+#define CLKGEN_ISP_VENC_SHAKE_ACLK                         476
+#define TEESYS_HCLK                                        477
+#define PWM_CCLK                                           478
+#define CLKGEN_GPIO0_DBCLK                                 479
+#define CLKGEN_SDIO0_OSC_CLK                               480
+#define CLKGEN_GMAC1_ACLK                                  481
+#define VPSYS_ACLK                                         482
+
+#define AHB2_CPUSYS_HCLK_OUT_DIV			   483
+#define APB3_CPUSYS_PCLK_DIV				   484
+#define CFG_AXI_ACLK_OUT_DIV				   485
+#define PERISYS_AHB_HCLK_OUT_DIV			   486
+#define CLK_OUT_1_OUT_DIV				   487
+#define CLK_OUT_2_OUT_DIV                                  488
+#define CLK_OUT_3_OUT_DIV                                  489
+#define CLK_OUT_4_OUT_DIV                                  490
+#define NPU_CCLK_OUT_DIV				   491
+#define CFG_APB_PCLK_OUT_DIV				   492
+#define CPU_PLL0_BYPASS					   493
+#define CPU_PLL1_BYPASS					   494
+#define GMAC_PLL_BYPASS					   495
+#define VIDEO_PLL_BYPASS				   496
+#define TEE_PLL_BYPASS					   497
+#define DPU0_PLL_BYPASS					   498
+#define DPU1_PLL_BYPASS					   499
+
+#define CLK_DUMMY					   500
+#define OSC_32K						   501
+#define OSC_24M						   502
+#define RC_24M						   503
+
+#define CLK_END						   504
+
+#endif
diff --git a/include/dt-bindings/clock/light-mpw-clock.h b/include/dt-bindings/clock/light-mpw-clock.h
new file mode 100644
index 000000000000..46c2a052a9d2
--- /dev/null
+++ b/include/dt-bindings/clock/light-mpw-clock.h
@@ -0,0 +1,222 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#ifndef __DT_BINDINGS_CLOCK_LIGHT_H
+#define __DT_BINDINGS_CLOCK_LIGHT_H
+
+#define LIGHT_CLK_DUMMY				0
+#define LIGHT_CLK_32K				1
+#define LIGHT_CLK_24M				2
+#define LIGHT_RC_24M				3
+
+#define LIGHT_VIDEO_PLL_FOUTVCO			4
+#define LIGHT_VIDEO_PLL_FOUTPOSTDIV		5
+#define LIGHT_VIDEO_PLL_FOUT4			6
+#define LIGHT_VIDEO_PLL_BYPASS			7
+
+#define LIGHT_GMAC_PLL_FOUTVCO			8
+#define LIGHT_GMAC_PLL_FOUTPOSTDIV		9
+#define LIGHT_GMAC_PLL_FOUT1PH0			10
+#define LIGHT_GMAC_PLL_FOUT4			11
+#define LIGHT_GMAC_PLL_BYPASS			12
+
+#define LIGHT_AUDIO_PLL_FOUTVCO			13
+#define LIGHT_AUDIO_PLL_FOUTPOSTDIV		14
+#define LIGHT_AUDIO_PLL_FOUT3			15
+#define LIGHT_AUDIO_PLL_BYPASS			16
+
+#define LIGHT_SYS_PLL_FOUTVCO			17
+#define LIGHT_SYS_PLL_FOUTPOSTDIV		18
+#define LIGHT_SYS_PLL_FOUT4			19
+#define LIGHT_SYS_PLL_BYPASS			20
+
+#define LIGHT_CPU_PLL0_FOUTVCO			21
+#define LIGHT_CPU_PLL0_FOUTPOSTDIV		22
+#define LIGHT_CPU_PLL0_FOUT4			23
+#define LIGHT_CPU_PLL0_BYPASS			24
+
+#define LIGHT_CPU_PLL1_FOUTVCO			25
+#define LIGHT_CPU_PLL1_FOUTPOSTDIV		26
+#define LIGHT_CPU_PLL1_FOUT4			27
+#define LIGHT_CPU_PLL1_BYPASS			28
+
+#define LIGHT_DDR_PLL_FOUTVCO			29
+#define LIGHT_DDR_PLL_FOUTPOSTDIV		30
+#define LIGHT_DDR_PLL_FOUT4			31
+#define LIGHT_DDR_PLL_BYPASS			32
+
+#define LIGHT_AONSYS_CLK_SWITCH_0		33
+#define LIGHT_AONSYS_CLK_SWITCH_1		34
+#define LIGHT_AONSYS_CLK			35
+#define LIGHT_SHARE_SRAM_CLK			36
+#define LIGHT_CLKGEN_RTC_PCLK			37
+#define LIGHT_CLKGEN_AOGPIO_PCLK		38
+#define LIGHT_CLKGEN_AOI2C_PCLK			39
+#define LIGHT_CLKGEN_PVTC_PCLK			40
+#define LIGHT_CLKGEN_AOAHB_HCLK			41
+#define LIGHT_CLKGEN_AOSRAM_HCLK		42
+#define LIGHT_CLKGEN_AOAPB_HCLK			43
+#define LIGHT_CLKGEN_AOPAD_PCLK			44
+#define LIGHT_CLKGEN_AOTIMER_PCLK		45
+#define LIGHT_CLKGEN_AOTIMER_CCLK		46
+#define LIGHT_CLKGEN_SRAM_AXI_ACLK		47
+#define LIGHT_CLKGEN_CPU2RAM_X2X_ACLK_S		48
+#define LIGHT_CLKGEN_AOGPIO_DBCLK		49
+
+#define LIGHT_GMAC_CORECLK			50
+#define LIGHT_OSC_CLK_DIV24			51
+#define LIGHT_GMAC_PLL_FOUTVCO_DIV5		52
+#define LIGHT_C910_CCLK_I0			53
+#define LIGHT_C910_CCLK				54
+#define LIGHT_CPUSYS_AHB_HCLK			55
+#define LIGHT_CPUSYS_CFG_AXI_ACLK		56
+#define LIGHT_PERISYS_AHB_HCLK			57
+#define LIGHT_CLK_OUT_1				58
+#define LIGHT_CLK_OUT_2				59
+#define LIGHT_CLK_OUT_3				60
+#define LIGHT_CLK_OUT_4				61
+#define LIGHT_CPUSYS_AHB_HCLK_DIV		62
+#define LIGHT_APB3_CPUSYS_PCLK			63
+#define LIGHT_CPUSYS_SUB_AXI_ACLK		64
+#define LIGHT_CPUSYS_CFG_AXI_ACLK_DIV		65
+#define LIGHT_TEESYS_HCLK			66
+#define LIGHT_DMAC_1_CLK			67
+#define LIGHT_DMAC_2_CLK			68
+#define LIGHT_DMAC_3_CLK			69
+#define LIGHT_AXI_PORT4_CLK			70
+#define LIGHT_PERISYS_AHB_HCLK_DIV		71
+#define LIGHT_PERISYS_APB_PCLK			72
+#define LIGHT_CLK_OUT_1_DIV			73
+#define LIGHT_CLK_OUT_2_DIV			74
+#define LIGHT_CLK_OUT_3_DIV			75
+#define LIGHT_CLK_OUT_4_DIV			76
+#define LIGHT_CLKGEN_PERISYS_AXI_ACLK		77
+#define LIGHT_CLKGEN_PERISYS_AHB_HCLK		78
+#define LIGHT_CLKGEN_PERISYS_APB1_HCLK		79
+#define LIGHT_CLKGEN_PERISYS_APB2_HCLK		80
+#define LIGHT_CLKGEN_USB3_DRD_PHY_REF_CLK	81
+#define LIGHT_CLKGEN_USB3_DRD_CTRL_REF_CLK	82
+#define LIGHT_CLKGEN_USB3_DRD_SPDCLK		83
+#define LIGHT_CLKGEN_USB3_DRD_ACLK		84
+#define LIGHT_CLKGEN_EMMC1_X2X_ACLK		85
+#define LIGHT_CLKGEN_EMMC0_X2X_ACLK		86
+#define LIGHT_CLKGEN_EMMC0_HCLK			87
+#define LIGHT_CLKGEN_EMMC1_HCLK			88
+#define LIGHT_CLKGEN_GMAC_ACLK			89
+#define LIGHT_CLKGEN_PWM_PCLK			90
+#define LIGHT_CLKGEN_QSPI0_PCLK			91
+#define LIGHT_CLKGEN_QSPI1_PCLK			92
+#define LIGHT_CLKGEN_SPI_PCLK			93
+#define LIGHT_CLKGEN_UART0_PCLK			94
+#define LIGHT_CLKGEN_UART1_PCLK			95
+#define LIGHT_CLKGEN_UART2_PCLK			96
+#define LIGHT_CLKGEN_UART3_PCLK			97
+#define LIGHT_CLKGEN_UART4_PCLK			98
+#define LIGHT_CLKGEN_UART5_PCLK			99
+#define LIGHT_CLKGEN_GPIO0_PCLK			100
+#define LIGHT_CLKGEN_GPIO1_PCLK			101
+#define LIGHT_CLKGEN_GPIO2_PCLK			102
+#define LIGHT_CLKGEN_I2C0_IC_CLK		103
+#define LIGHT_CLKGEN_I2C1_IC_CLK		104
+#define LIGHT_CLKGEN_I2C2_IC_CLK		105
+#define LIGHT_CLKGEN_I2C3_IC_CLK		106
+#define LIGHT_CLKGEN_I2C4_IC_CLK		107
+#define LIGHT_CLKGEN_I2C5_IC_CLK		108
+#define LIGHT_CLKGEN_PERI2DDR_X2X_ACLK_M	109
+#define LIGHT_CLKGEN_AXI_DUMMY_SLV_4_ACLK	110
+#define LIGHT_CLKGEN_AXI_DUMMY_SLV_3_ACLK	111
+#define LIGHT_CLKGEN_AXI_DUMMY_SLV_2_ACLK	112
+#define LIGHT_CLKGEN_AXI_DUMMY_SLV_1_ACLK	113
+#define LIGHT_CLKGEN_APB_CPU2FG_HCLK		114
+#define LIGHT_CLKGEN_AON2CPU_A2X_ACLK		115
+#define LIGHT_CLKGEN_CPU2CFG_X2X_ACLK_M		116
+#define LIGHT_CLKGEN_CPU2RAM_X2X_ACLK_M		117
+#define LIGHT_CLKGEN_AXI4_CPUSYS2_ACLK		118
+#define LIGHT_CLKGEN_X2X_CPUSYS_ACLK_M		119
+#define LIGHT_CLKGEN_CHIP_DBG_ACLK		120
+#define LIGHT_CLKGEN_AXI4_CFG_BUS_ACLK		121
+#define LIGHT_CLKGEN_X2H_CPUSYS_ACLK		122
+#define LIGHT_CLKGEN_CPU2TEE_X2H_ACLK		123
+#define LIGHT_CLKGEN_CPU2AON_X2H_ACLK		124
+#define LIGHT_CLKGEN_CPU2CFG_X2H_ACLK		125
+#define LIGHT_CLKGEN_CPU2PERI_X2H_MHCLK		126
+#define LIGHT_CLKGEN_AHB2_CPUSYS_HCLK		127
+#define LIGHT_CLKGEN_APB3_CPUSYS_HCLK		128
+#define LIGHT_CLKGEN_C910_BROM_HCLK		129
+#define LIGHT_CLKGEN_DMAC_ACLK			130
+#define LIGHT_CLKGEN_MBOX0_PCLK			131
+#define LIGHT_CLKGEN_MBOX1_PCLK			132
+#define LIGHT_CLKGEN_MBOX2_PCLK			133
+#define LIGHT_CLKGEN_MBOX3_PCLK			134
+#define LIGHT_CLKGEN_WDT0_PCLK			135
+#define LIGHT_CLKGEN_WDT1_PCLK			136
+#define LIGHT_CLKGEN_TIMER0_CCLK		137
+#define LIGHT_CLKGEN_TIMER1_CCLK		138
+#define LIGHT_CLKGEN_TRNG_RB_HCLK		139
+#define LIGHT_CLKGEN_ADC_PCLK			140
+#define LIGHT_CLKGEN_AXI_ACLK_4			141
+#define LIGHT_CLKGEN_AXI_ACLK_3			142
+#define LIGHT_CLKGEN_AXI_ACLK_2			143
+#define LIGHT_CLKGEN_AXI_ACLK_1			145
+#define LIGHT_CLKGEN_AXI_ACLK_0			146
+#define LIGHT_CLKGEN_DMAC_1_ACLK		147
+#define LIGHT_CLKGEN_DMAC_2_ACLK		148
+#define LIGHT_CLKGEN_DMAC_3_ACLK		149
+#define LIGHT_CLKGEN_SRAM_AXI_PCLK		150
+#define LIGHT_CLKGEN_AHB2_TEESYS_HCLK		151
+#define LIGHT_CLKGEN_EFUSE_MPW_PCLK		152
+#define LIGHT_CLKGEN_CLK_OUT_4_CLK		153
+#define LIGHT_CLKGEN_CLK_OUT_3_CLK		154
+#define LIGHT_CLKGEN_CLK_OUT_2_CLK		155
+#define LIGHT_CLKGEN_CLK_OUT_1_CLK		156
+#define LIGHT_CLKGEN_DDR_APB_PCLK		157
+#define LIGHT_CLKGEN_PADCTRL_APSYS_PCLK		158
+#define LIGHT_CLKGEN_CHIP_DBG_CCLK		159
+#define LIGHT_CHIP_DBG_CCLK			160
+#define LIGHT_AXI_ACLK				161
+
+#define LIGHT_CLKGEN_CPU2CFG_X2X_ACLK_S		162
+#define LIGHT_CLKGEN_CPU2CFG_X2H_ACLK_S		163
+#define LIGHT_CLKGEN_AON2CPU_A2X_HCLK		164
+#define LIGHT_CLKGEN_DMAC_HCLK			165
+#define LIGHT_CLKGEN_X2H_CPUSYS_MHCLK		166
+#define LIGHT_CLKGEN_CPU2TEE_X2H_MHCLK		167
+#define LIGHT_CLKGEN_CPU2AON_X2H_MHCLK		168
+#define LIGHT_AXI_HCLK				169
+#define LIGHT_CLKGEN_CPU2CFG_X2H_MHCLK		170
+#define LIGHT_CLKGEN_TIMER0_PCLK		171
+#define LIGHT_CLKGEN_TIMER1_PCLK		172
+#define LIGHT_CLKGEN_PERI2DDR_X2X_ACLK_S	173
+#define LIGHT_CLKGEN_USB3_DRD_PCLK		174
+#define LIGHT_CLKGEN_GMAC_HCLK			175
+#define LIGHT_CLKGEN_GMAC_PCLK			176
+#define LIGHT_CLKGEN_GMAC_CCLK			177
+#define LIGHT_CLKGEN_EMMC0_ACLK			178
+#define LIGHT_CLKGEN_EMMC0_REF_CLK		179
+#define LIGHT_CLKGEN_EMMC0_OSC_CLK		180
+#define LIGHT_CLKGEN_EMMC1_ACLK			181
+#define LIGHT_CLKGEN_EMMC1_REF_CLK		182
+#define LIGHT_CLKGEN_EMMC1_OSC_CLK		183
+#define LIGHT_CLKGEN_PWM_CCLK			184
+#define LIGHT_CLKGEN_QSPI0_SSI_CLK		185
+#define LIGHT_CLKGEN_QSPI1_SSI_CLK		186
+#define LIGHT_CLKGEN_SPI_SSI_CLK		187
+#define LIGHT_CLKGEN_GPIO0_DBCLK		188
+#define LIGHT_CLKGEN_GPIO1_DBCLK		189
+#define LIGHT_CLKGEN_GPIO2_DBCLK		190
+#define LIGHT_CLKGEN_DMAC_1_HCLK		191
+#define LIGHT_CLKGEN_DMAC_2_HCLK		192
+#define LIGHT_CLKGEN_DMAC_3_HCLK		193
+#define LIGHT_EMMC_CLK_DIV			194
+#define LIGHT_EMMC0_OSC_CLK			195
+#define LIGHT_EMMC1_OSC_CLK			196
+#define LIGHT_PWM_CCLK				197
+#define LIGHT_USB3_PHY_REF_CLK			198
+#define LIGHT_SPI_CLK				199
+#define LIGHT_GPIO_DBCLK			200
+#define LIGHT_X2H_HCLK				201
+
+#define LIGHT_CLK_END				202
+#endif
diff --git a/include/dt-bindings/clock/light-visys.h b/include/dt-bindings/clock/light-visys.h
new file mode 100644
index 000000000000..53fed0bfb624
--- /dev/null
+++ b/include/dt-bindings/clock/light-visys.h
@@ -0,0 +1,54 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef _LIGHT_VISYS_H
+#define _LIGHT_VISYS_H
+
+#define LIGHT_CLKGEN_VISYS_ACLK			      0
+#define LIGHT_CLKGEN_DW200_ACLK			      1
+#define LIGHT_CLKGEN_AXI4_VISYS1_ACLK		      2
+#define LIGHT_CLKGEN_AXI4_VISYS2_ACLK                 3
+#define LIGHT_CLKGEN_AXI4_VISYS3_ACLK                 4
+#define LIGHT_CLKGEN_ISP0_ACLK                        5
+#define LIGHT_CLKGEN_ISP_RY_ACLK                      6
+#define LIGHT_CLKGEN_ISP_VENC_SHAKE_ACLK              7
+#define LIGHT_CLKGEN_VIPRE_ACLK                       8
+#define LIGHT_CLKGEN_VISYS_SLAVE_HCLK                 9
+#define LIGHT_CLKGEN_ISP0_S_HCLK                      10
+#define LIGHT_CLKGEN_DW200_HCLK                       11
+#define LIGHT_CLKGEN_ISP_RY_HCLK                      12
+#define LIGHT_CLKGEN_MIPI_CSI0_PCLK                   13
+#define LIGHT_CLKGEN_MIPI_CSI0_FPCLK                  14
+#define LIGHT_CLKGEN_MIPI_CSI1_PCLK                   15
+#define LIGHT_CLKGEN_MIPI_CSI1_FPCLK                  16
+#define LIGHT_CLKGEN_MIPI_CSI2_PCLK                   17
+#define LIGHT_CLKGEN_MIPI_CSI2_FPCLK                  18
+#define LIGHT_CLKGEN_VIPRE_PCLK                       19
+#define LIGHT_CLKGEN_VISYS_PCLK                       20
+#define LIGHT_CLKGEN_VISYS_SYSREG_PCLK                21
+#define LIGHT_CLKGEN_ISP_VENC_SHAKE_PCLK              22
+#define LIGHT_CLKGEN_MIPI_CSI0_PIXCLK                 23
+#define LIGHT_CLKGEN_MIPI_CSI1_PIXCLK                 24
+#define LIGHT_CLKGEN_MIPI_CSI2_PIXCLK                 25
+#define LIGHT_CLKGEN_VIPRE_PIXELCLK                   26
+#define LIGHT_CLKGEN_ISP_PIXELCLK                     27
+#define LIGHT_CLKGEN_MIPI_CSI0_CFG_CLK                28
+#define LIGHT_CLKGEN_MIPI_CSI1_CFG_CLK                29
+#define LIGHT_CLKGEN_MIPI_CSI2_CFG_CLK                30
+#define LIGHT_CLKGEN_DW200_CLK_VSE                    31
+#define LIGHT_CLKGEN_DW200_CLK_DWE                    32
+#define LIGHT_CLKGEN_ISP0_CLK                         33
+#define LIGHT_CLKGEN_ISP1_CLK                         34
+#define LIGHT_CLKGEN_ISP_RY_CCLK                      35
+#define LIGHT_CLKGEN_MIPI_CSI_SCANBYTECLK             36
+#define LIGHT_CLKGEN_MIPI_CSI_SCANCLK                 37
+#define LIGHT_CLKGEN_ISP1_PIXELCLK		      38
+#define LIGHT_CLKGEN_ISP0_PIXELCLK		      39
+#define LIGHT_CLKGEN_ISP1_HCLK			      40
+#define LIGHT_CLKGEN_ISP0_HCLK			      41
+#define LIGHT_CLKGEN_ISP1_ACLK			      42
+#define LIGHT_CLKGEN_VISYS_CLK_END		      43
+
+#endif
diff --git a/include/dt-bindings/clock/light-vosys.h b/include/dt-bindings/clock/light-vosys.h
new file mode 100644
index 000000000000..dbdd7fa7016b
--- /dev/null
+++ b/include/dt-bindings/clock/light-vosys.h
@@ -0,0 +1,41 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef LIGHT_VOSYS_H
+#define LIGHT_VOSYS_H
+
+#define LIGHT_CLKGEN_AXI4_VO_PCLK			0
+#define LIGHT_CLKGEN_IOPMP_VOSYS_DPU_PCLK		1
+#define LIGHT_CLKGEN_IOPMP_VOSYS_DPU1_PCLK		2
+#define LIGHT_CLKGEN_IOPMP_VOSYS_GPU_PCLK		3
+#define LIGHT_CLKGEN_HDMI_PCLK				4
+#define LIGHT_CLKGEN_MIPIDSI0_PCLK			5
+#define LIGHT_CLKGEN_MIPIDSI1_PCLK			6
+#define LIGHT_CLKGEN_AXI4_VO_ACLK			7
+#define LIGHT_CLKGEN_IOPMP_GPU_ACLK			8
+#define LIGHT_CLKGEN_IOPMP_DPU_ACLK			9
+#define LIGHT_CLKGEN_IOPMP_DPU1_ACLK			10
+#define LIGHT_CLKGEN_X2H_DPU_ACLK			11
+#define LIGHT_CLKGEN_X2H_DPU1_ACLK			12
+#define LIGHT_CLKGEN_MIPIDSI0_PIXCLK			13
+#define LIGHT_CLKGEN_HDMI_PIXCLK			14
+#define LIGHT_CLKGEN_MIPIDSI1_PIXCLK			15
+#define LIGHT_CLKGEN_HDMI_SFR_CLK			16
+#define LIGHT_CLKGEN_HDMI_CEC_CLK			17
+#define LIGHT_CLKGEN_HDMI_I2S_CLK			18
+#define LIGHT_CLKGEN_MIPIDSI0_CFG_CLK			19
+#define LIGHT_CLKGEN_MIPIDSI1_CFG_CLK			20
+#define LIGHT_CLKGEN_MIPIDSI0_REFCLK			21
+#define LIGHT_CLKGEN_MIPIDSI1_REFCLK			22
+#define LIGHT_CLKGEN_GPU_CORE_CLK			23
+#define LIGHT_CLKGEN_GPU_CFG_ACLK			24
+#define LIGHT_CLKGEN_DPU_HCLK				25
+#define LIGHT_CLKGEN_DPU_ACLK				26
+#define LIGHT_CLKGEN_DPU_CCLK				27
+#define LIGHT_CLKGEN_DPU_PIXCLK0			28
+#define LIGHT_CLKGEN_DPU_PIXCLK1                        29
+#define LIGHT_CLKGEN_VOSYS_CLK_END			30
+
+#endif
diff --git a/include/dt-bindings/clock/light-vpsys.h b/include/dt-bindings/clock/light-vpsys.h
new file mode 100644
index 000000000000..188aaa6cc435
--- /dev/null
+++ b/include/dt-bindings/clock/light-vpsys.h
@@ -0,0 +1,24 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef _LIGHT_VPSYS_H
+#define _LIGHT_VPSYS_H
+
+#define LIGHT_VPSYS_G2D_PCLK		0
+#define LIGHT_VPSYS_G2D_ACLK		1
+#define LIGHT_VPSYS_G2D_CCLK		2
+#define LIGHT_VPSYS_FCE_PCLK		3
+#define LIGHT_VPSYS_FCE_ACLK		4
+#define LIGHT_VPSYS_VDEC_PCLK		5
+#define LIGHT_VPSYS_VDEC_ACLK		6
+#define LIGHT_VPSYS_VDEC_CCLK		7
+#define LIGHT_VPSYS_AXI_ACLK		8
+#define LIGHT_VPSYS_VENC_CCLK		9
+#define LIGHT_VPSYS_VENC_PCLK		10
+#define LIGHT_VPSYS_VENC_ACLK		11
+#define LIGHT_VPSYS_CLK_END		12
+
+#endif
+
diff --git a/include/dt-bindings/clock/sophgo-mango-clock.h b/include/dt-bindings/clock/sophgo-mango-clock.h
new file mode 100644
index 000000000000..aaed4ad27dc1
--- /dev/null
+++ b/include/dt-bindings/clock/sophgo-mango-clock.h
@@ -0,0 +1,165 @@
+#ifndef __SOPHGO_MANGO_CLOCK__
+#define __SOPHGO_MANGO_CLOCK__
+
+#include <dt-bindings/clock/sophgo.h>
+
+/*div clock*/
+#define DIV_CLK_MPLL_RP_CPU_NORMAL_0 0
+#define DIV_CLK_MPLL_AXI_DDR_0 1
+#define DIV_CLK_FPLL_DDR01_1 2
+#define DIV_CLK_FPLL_DDR23_1 3
+#define DIV_CLK_FPLL_RP_CPU_NORMAL_1 4
+#define DIV_CLK_FPLL_50M_A53 5
+#define DIV_CLK_FPLL_TOP_RP_CMN_DIV2 6
+#define DIV_CLK_FPLL_UART_500M 7
+#define DIV_CLK_FPLL_AHB_LPC 8
+#define DIV_CLK_FPLL_EFUSE 9
+#define DIV_CLK_FPLL_TX_ETH0 10
+#define DIV_CLK_FPLL_PTP_REF_I_ETH0 11
+#define DIV_CLK_FPLL_REF_ETH0 12
+#define DIV_CLK_FPLL_EMMC 13
+#define DIV_CLK_FPLL_SD 14
+#define DIV_CLK_FPLL_TOP_AXI0 15
+#define DIV_CLK_FPLL_TOP_AXI_HSPERI 16
+#define DIV_CLK_FPLL_AXI_DDR_1 17
+#define DIV_CLK_FPLL_DIV_TIMER1 18
+#define DIV_CLK_FPLL_DIV_TIMER2 19
+#define DIV_CLK_FPLL_DIV_TIMER3 20
+#define DIV_CLK_FPLL_DIV_TIMER4 21
+#define DIV_CLK_FPLL_DIV_TIMER5 22
+#define DIV_CLK_FPLL_DIV_TIMER6 23
+#define DIV_CLK_FPLL_DIV_TIMER7 24
+#define DIV_CLK_FPLL_DIV_TIMER8 25
+#define DIV_CLK_FPLL_100K_EMMC 26
+#define DIV_CLK_FPLL_100K_SD 27
+#define DIV_CLK_FPLL_GPIO_DB 28
+#define DIV_CLK_DPLL0_DDR01_0 29
+#define DIV_CLK_DPLL1_DDR23_0 30
+
+/* MPLL */
+#define GATE_CLK_RP_CPU_NORMAL_DIV0 31
+#define GATE_CLK_AXI_DDR_DIV0 32
+
+/* FPLL */
+#define GATE_CLK_RP_CPU_NORMAL_DIV1 33
+#define GATE_CLK_A53_50M 34
+#define GATE_CLK_TOP_RP_CMN_DIV2 35
+#define GATE_CLK_HSDMA 36
+#define GATE_CLK_EMMC_100M 37
+#define GATE_CLK_SD_100M 38
+#define GATE_CLK_TX_ETH0 39
+#define GATE_CLK_PTP_REF_I_ETH0 40
+#define GATE_CLK_REF_ETH0 41
+#define GATE_CLK_UART_500M 42
+#define GATE_CLK_EFUSE 43
+
+#define GATE_CLK_AHB_LPC 44
+#define GATE_CLK_AHB_ROM 45
+#define GATE_CLK_AHB_SF 46
+
+#define GATE_CLK_APB_UART 47
+#define GATE_CLK_APB_TIMER 48
+#define GATE_CLK_APB_EFUSE 49
+#define GATE_CLK_APB_GPIO 50
+#define GATE_CLK_APB_GPIO_INTR 51
+#define GATE_CLK_APB_SPI 52
+#define GATE_CLK_APB_I2C 53
+#define GATE_CLK_APB_WDT 54
+#define GATE_CLK_APB_PWM 55
+#define GATE_CLK_APB_RTC 56
+
+#define GATE_CLK_AXI_PCIE0 57
+#define GATE_CLK_AXI_PCIE1 58
+#define GATE_CLK_SYSDMA_AXI 59
+#define GATE_CLK_AXI_DBG_I2C 60
+#define GATE_CLK_AXI_SRAM 61
+#define GATE_CLK_AXI_ETH0 62
+#define GATE_CLK_AXI_EMMC 63
+#define GATE_CLK_AXI_SD 64
+#define GATE_CLK_TOP_AXI0 65
+#define GATE_CLK_TOP_AXI_HSPERI 66
+
+#define GATE_CLK_TIMER1 67
+#define GATE_CLK_TIMER2 68
+#define GATE_CLK_TIMER3 69
+#define GATE_CLK_TIMER4 70
+#define GATE_CLK_TIMER5 71
+#define GATE_CLK_TIMER6 72
+#define GATE_CLK_TIMER7 73
+#define GATE_CLK_TIMER8 74
+#define GATE_CLK_100K_EMMC 75
+#define GATE_CLK_100K_SD 76
+#define GATE_CLK_GPIO_DB 77
+
+#define GATE_CLK_AXI_DDR_DIV1 78
+#define GATE_CLK_DDR01_DIV1 79
+#define GATE_CLK_DDR23_DIV1 80
+/* DPLL0 */
+#define GATE_CLK_DDR01_DIV0 81
+/* DPLL1 */
+#define GATE_CLK_DDR23_DIV0 82
+
+#define GATE_CLK_DDR01 83
+#define GATE_CLK_DDR23 84
+#define GATE_CLK_RP_CPU_NORMAL 85
+#define GATE_CLK_AXI_DDR 86
+#define GATE_CLK_RXU0 87
+#define GATE_CLK_RXU1 88
+#define GATE_CLK_RXU2 89
+#define GATE_CLK_RXU3 90
+#define GATE_CLK_RXU4 91
+#define GATE_CLK_RXU5 92
+#define GATE_CLK_RXU6 93
+#define GATE_CLK_RXU7 94
+#define GATE_CLK_RXU8 95
+#define GATE_CLK_RXU9 96
+#define GATE_CLK_RXU10 97
+#define GATE_CLK_RXU11 98
+#define GATE_CLK_RXU12 99
+#define GATE_CLK_RXU13 100
+#define GATE_CLK_RXU14 101
+#define GATE_CLK_RXU15 102
+#define GATE_CLK_RXU16 103
+#define GATE_CLK_RXU17 104
+#define GATE_CLK_RXU18 105
+#define GATE_CLK_RXU19 106
+#define GATE_CLK_RXU20 107
+#define GATE_CLK_RXU21 108
+#define GATE_CLK_RXU22 109
+#define GATE_CLK_RXU23 110
+#define GATE_CLK_RXU24 111
+#define GATE_CLK_RXU25 112
+#define GATE_CLK_RXU26 113
+#define GATE_CLK_RXU27 114
+#define GATE_CLK_RXU28 115
+#define GATE_CLK_RXU29 116
+#define GATE_CLK_RXU30 117
+#define GATE_CLK_RXU31 118
+#define GATE_CLK_MP0 119
+#define GATE_CLK_MP1 120
+#define GATE_CLK_MP2 121
+#define GATE_CLK_MP3 122
+#define GATE_CLK_MP4 123
+#define GATE_CLK_MP5 124
+#define GATE_CLK_MP6 125
+#define GATE_CLK_MP7 126
+#define GATE_CLK_MP8 127
+#define GATE_CLK_MP9 128
+#define GATE_CLK_MP10 129
+#define GATE_CLK_MP11 130
+#define GATE_CLK_MP12 131
+#define GATE_CLK_MP13 132
+#define GATE_CLK_MP14 133
+#define GATE_CLK_MP15 134
+
+/* MUX */
+#define MUX_CLK_DDR01 0
+#define MUX_CLK_DDR23 1
+#define MUX_CLK_RP_CPU_NORMAL 2
+#define MUX_CLK_AXI_DDR 3
+
+#define S0_DIV_CLK_TABLE		0
+#define S1_DIV_CLK_TABLE		1
+#define S0_MUX_CLK_TABLE		2
+#define S1_MUX_CLK_TABLE		3
+#endif
diff --git a/include/dt-bindings/clock/sophgo.h b/include/dt-bindings/clock/sophgo.h
new file mode 100644
index 000000000000..5584243f9135
--- /dev/null
+++ b/include/dt-bindings/clock/sophgo.h
@@ -0,0 +1,15 @@
+#ifndef __SOPHGO_CLK__
+#define __SOPHGO_CLK__
+
+//PLL ID
+#define MPLL_CLK	0
+#define FPLL_CLK	3
+#define DPLL0_CLK	4
+#define DPLL1_CLK	5
+
+//clock mode
+#define NORMAL_MODE	0
+#define FAST_MODE	1
+#define SAFE_MODE	2
+#define BYPASS_MODE	3
+#endif
diff --git a/include/dt-bindings/firmware/thead/rsrc.h b/include/dt-bindings/firmware/thead/rsrc.h
new file mode 100644
index 000000000000..8cee0fcaeb74
--- /dev/null
+++ b/include/dt-bindings/firmware/thead/rsrc.h
@@ -0,0 +1,17 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2022 Alibaba Group Holding Limited.
+ */
+
+#ifndef __DT_BINDINGS_RSCRC_LIGHT_H
+#define __DT_BINDINGS_RSCRC_LIGHT_H
+
+#define LIGHT_AON_AUDIO_PD	0
+#define LIGHT_AON_VDEC_PD	1
+#define LIGHT_AON_NPU_PD        2
+#define LIGHT_AON_VENC_PD       3
+#define LIGHT_AON_GPU_PD        4
+#define LIGHT_AON_DSP0_PD       5
+#define LIGHT_AON_DSP1_PD       6
+
+#endif
diff --git a/include/dt-bindings/reset/sophgo-mango-resets.h b/include/dt-bindings/reset/sophgo-mango-resets.h
new file mode 100644
index 000000000000..9ff8ca4c3d67
--- /dev/null
+++ b/include/dt-bindings/reset/sophgo-mango-resets.h
@@ -0,0 +1,96 @@
+/*
+ * Sophgo SoCs Reset definitions
+ *
+ * Copyright (c) 2018 Bitmain Ltd.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#ifndef _DT_BINDINGS_RST_MANGO_H_
+#define _DT_BINDINGS_RST_MANGO_H_
+
+#define RST_MAIN_AP                            0
+#define RST_RISCV_CPU                          1
+#define RST_RISCV_LOW_SPEED_LOGIC              2
+#define RST_RISCV_CMN                          3
+#define RST_HSDMA                              4
+#define RST_SYSDMA                             5
+#define RST_EFUSE0                             6
+#define RST_EFUSE1                             7
+#define RST_RTC                                8
+#define RST_TIMER                              9
+#define RST_WDT                                10
+#define RST_AHB_ROM0                           11
+#define RST_AHB_ROM1                           12
+#define RST_I2C0                               13
+#define RST_I2C1                               14
+#define RST_I2C2                               15
+#define RST_I2C3                               16
+#define RST_GPIO0                              17
+#define RST_GPIO1                              18
+#define RST_GPIO2                              19
+#define RST_PWM                                20
+#define RST_AXI_SRAM0                          21
+#define RST_AXI_SRAM1                          22
+#define RST_SF0                                23
+#define RST_SF1                                24
+#define RST_LPC                                25
+#define RST_ETH0                               26
+#define RST_EMMC                               27
+#define RST_SD                                 28
+#define RST_UART0                              29
+#define RST_UART1                              30
+#define RST_UART2                              31
+
+#define RST_UART3                              32
+#define RST_SPI0                               33
+#define RST_SPI1                               34
+#define RST_DBG_I2C                            35
+#define RST_PCIE0                              36
+#define RST_PCIE1                              37
+#define RST_DDR0                               38
+#define RST_DDR1                               39
+#define RST_DDR2                               40
+#define RST_DDR3                               41
+#define RST_FAU0                               42
+#define RST_FAU1                               43
+#define RST_FAU2                               44
+#define RST_RXU0                               45
+#define RST_RXU1                               46
+#define RST_RXU2                               47
+#define RST_RXU3                               48
+#define RST_RXU4                               49
+#define RST_RXU5                               50
+#define RST_RXU6                               51
+#define RST_RXU7                               52
+#define RST_RXU8                               53
+#define RST_RXU9                               54
+#define RST_RXU10                              55
+#define RST_RXU11                              56
+#define RST_RXU12                              57
+#define RST_RXU13                              58
+#define RST_RXU14                              59
+#define RST_RXU15                              60
+#define RST_RXU16                              61
+#define RST_RXU17                              62
+#define RST_RXU18                              63
+#define RST_RXU19                              64
+#define RST_RXU20                              65
+#define RST_RXU21                              66
+#define RST_RXU22                              67
+#define RST_RXU23                              68
+#define RST_RXU24                              69
+#define RST_RXU25                              70
+#define RST_RXU26                              71
+#define RST_RXU27                              72
+#define RST_RXU28                              73
+#define RST_RXU29                              74
+#define RST_RXU30                              75
+#define RST_RXU31                              76
+
+#define RST_MAX_NUM  (RST_RXU31+1)
+
+#endif
diff --git a/include/dt-bindings/reset/thead,th1520-reset.h b/include/dt-bindings/reset/thead,th1520-reset.h
new file mode 100644
index 000000000000..ec10751814e5
--- /dev/null
+++ b/include/dt-bindings/reset/thead,th1520-reset.h
@@ -0,0 +1,9 @@
+/* SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause) */
+
+#ifndef DT_BINDING_RESET_TH1520_H
+#define DT_BINDING_RESET_TH1520_H
+
+#define TH1520_RESET_WDT0 0
+#define TH1520_RESET_WDT1 1
+
+#endif
diff --git a/include/linux/firmware/thead/ipc.h b/include/linux/firmware/thead/ipc.h
new file mode 100644
index 000000000000..dfda60e76725
--- /dev/null
+++ b/include/linux/firmware/thead/ipc.h
@@ -0,0 +1,74 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Copyright (C) 2021 Alibaba Group Holding Limited.
+ */
+
+#ifndef _SC_IPC_H
+#define _SC_IPC_H
+
+#include <linux/device.h>
+#include <linux/types.h>
+
+#define AON_RPC_MSG_MAGIC       (0xef)
+#define LIGHT_AON_RPC_VERSION	1
+#define LIGHT_AON_RPC_MSG_NUM	7
+
+struct light_aon_ipc;
+
+enum light_aon_rpc_svc {
+	LIGHT_AON_RPC_SVC_UNKNOWN = 0,
+	LIGHT_AON_RPC_SVC_RETURN = 1,
+	LIGHT_AON_RPC_SVC_PM = 2,
+	LIGHT_AON_RPC_SVC_MISC = 3,
+	LIGHT_AON_RPC_SVC_AVFS = 4,
+};
+
+enum light_aon_misc_func {
+	LIGHT_AON_MISC_FUNC_UNKNOWN = 0,
+	LIGHT_AON_MISC_FUNC_SET_CONTROL = 1,
+	LIGHT_AON_MISC_FUNC_GET_CONTROL = 2,
+	LIGHT_AON_MISC_FUNC_WDG_START = 3,
+	LIGHT_AON_MISC_FUNC_WDG_STOP = 4,
+	LIGHT_AON_MISC_FUNC_WDG_PING = 5,
+	LIGHT_AON_MISC_FUNC_WDG_TIMEOUTSET = 6,
+	LIGHT_AON_MISC_FUNC_WDG_RESTART = 7,
+	LIGHT_AON_MISC_FUNC_WDG_GET_STATE = 8,
+	LIGHT_AON_MISC_FUNC_WDG_POWER_OFF = 9,
+	LIGHT_AON_MISC_FUNC_AON_WDT_ON  = 10,
+	LIGHT_AON_MISC_FUNC_AON_WDT_OFF = 11,
+	LIGHT_AON_MISC_FUNC_AON_RESERVE_MEM = 12,
+	LIGHT_AON_MISC_FUNC_REQUIRE_STR = 13,
+	LIGHT_AON_MISC_FUNC_RESUME_STR = 14,
+	LIGHT_AON_MISC_FUNC_REQUIRE_STD = 15,
+	LIGHT_AON_MISC_FUNC_CPUHP = 16,
+};
+
+enum light_aon_pm_func {
+	LIGHT_AON_PM_FUNC_UNKNOWN = 0,
+	LIGHT_AON_PM_FUNC_SET_RESOURCE_REGULATOR = 1,
+	LIGHT_AON_PM_FUNC_GET_RESOURCE_REGULATOR = 2,
+	LIGHT_AON_PM_FUNC_SET_RESOURCE_POWER_MODE = 3,
+	LIGHT_AON_PM_FUNC_PWR_SET  = 4,
+	LIGHT_AON_PM_FUNC_PWR_GET  = 5,
+};
+
+struct light_aon_rpc_msg_hdr {
+	uint8_t ver;                   ///< version of msg hdr
+	uint8_t size;                  ///< msg size ,uinit in bytes,the size includes rpc msg header self.
+	uint8_t svc;                   ///< rpc main service id
+	uint8_t func;                  ///< rpc sub func id of specific service, sent by caller
+} __packed __aligned(4);
+
+/*
+ * Defines for SC PM Power Mode
+ */
+#define LIGHT_AON_PM_PW_MODE_OFF	0	/* Power off */
+#define LIGHT_AON_PM_PW_MODE_STBY	1	/* Power in standby */
+#define LIGHT_AON_PM_PW_MODE_LP		2	/* Power in low-power */
+#define LIGHT_AON_PM_PW_MODE_ON		3	/* Power on */
+
+int light_aon_call_rpc(struct light_aon_ipc *ipc, void *msg, bool have_resp);
+int light_aon_get_handle(struct light_aon_ipc **ipc);
+int light_aon_misc_set_control(struct light_aon_ipc *ipc, u16 resource, u32 ctrl, u32 val);
+int light_aon_misc_get_control(struct light_aon_ipc *ipc, u16 resource, u32 ctrl, u32 *val);
+#endif /* _SC_IPC_H */
diff --git a/include/linux/firmware/thead/light_event.h b/include/linux/firmware/thead/light_event.h
new file mode 100644
index 000000000000..a4f99d41c2d1
--- /dev/null
+++ b/include/linux/firmware/thead/light_event.h
@@ -0,0 +1,35 @@
+/* SPDX-License-Identifier: GPL-2.0 WITH Linux-syscall-note */
+#ifndef _LIGHT_EVENT_H
+#define _LIGHT_EVENT_H
+
+enum light_rebootmode_index {
+	/* C902 event rebootmode */
+        LIGHT_EVENT_PMIC_RESET = 0x0,
+        LIGHT_EVENT_PMIC_ONKEY,
+        LIGHT_EVENT_PMIC_POWERUP,
+
+	/* C910 event rebootmode */
+        LIGHT_EVENT_SW_REBOOT = 0x20,
+        LIGHT_EVENT_SW_WATCHDOG,
+        LIGHT_EVENT_SW_PANIC,
+        LIGHT_EVENT_SW_HANG,
+        LIGHT_EVENT_MAX,
+};
+
+#if IS_ENABLED(CONFIG_LIGHT_REBOOTMODE)
+extern int light_event_set_rebootmode(enum light_rebootmode_index mode);
+extern int light_event_get_rebootmode(enum light_rebootmode_index *mode);
+#else
+static int light_event_set_rebootmode(enum light_rebootmode_index mode)
+{
+	return 0;
+}
+static int light_event_get_rebootmode(enum light_rebootmode_index *mode)
+{
+	*mode = LIGHT_EVENT_MAX;
+
+	return 0;
+}
+#endif
+
+#endif
diff --git a/include/linux/light_rpmsg.h b/include/linux/light_rpmsg.h
new file mode 100644
index 000000000000..8930845604a0
--- /dev/null
+++ b/include/linux/light_rpmsg.h
@@ -0,0 +1,92 @@
+/*
+ * Copyright (C) 2023 Alibaba Group Holding Limited.
+ */
+
+/*
+ * The code contained herein is licensed under the GNU Lesser General
+ * Public License.  You may obtain a copy of the GNU Lesser General
+ * Public License Version 2.1 or later at the following locations:
+ *
+ * http://www.opensource.org/licenses/lgpl-license.html
+ * http://www.gnu.org/copyleft/lgpl.html
+ */
+
+/*
+ * @file linux/light_rpmsg.h
+ *
+ * @brief Global header file for imx RPMSG
+ *
+ * @ingroup RPMSG
+ */
+#ifndef __LINUX_LIGHT_RPMSG_H__
+#define __LINUX_LIGHT_RPMSG_H__
+
+#include <linux/rpmsg.h>
+#include <linux/slab.h>
+#include <linux/virtio.h>
+#include <linux/virtio_config.h>
+#include <linux/virtio_ids.h>
+#include <linux/virtio_ring.h>
+
+/* Category define */
+#define LIGHT_RMPSG_LIFECYCLE	1
+#define LIGHT_RPMSG_PMIC		2
+#define LIGHT_RPMSG_AUDIO		3
+#define LIGHT_RPMSG_KEY		4
+#define LIGHT_RPMSG_GPIO		5
+#define LIGHT_RPMSG_RTC		6
+#define LIGHT_RPMSG_SENSOR	7
+/* rpmsg version */
+#define LIGHT_RMPSG_MAJOR		1
+#define LIGHT_RMPSG_MINOR		0
+
+enum light_rpmsg_variants {
+        LIGHTA,
+        LIGHTB,
+        LIGHT_RPMSG,
+};
+
+struct light_virdev {
+        struct virtio_device vdev;
+        unsigned int vring[2];
+        struct virtqueue *vq[2];
+        int base_vq_id;
+        int num_of_vqs;
+        struct notifier_block nb;
+};
+
+struct light_rpmsg_vproc {
+        char *rproc_name;
+        struct mutex lock;
+        struct clk *mu_clk;
+        enum light_rpmsg_variants variant;
+        int vdev_nums;
+        int first_notify;
+#define MAX_VDEV_NUMS   8
+        struct light_virdev ivdev[MAX_VDEV_NUMS];
+        void __iomem *mu_base;
+        struct delayed_work rpmsg_work;
+        struct blocking_notifier_head notifier;
+#define MAX_NUM 10      /* enlarge it if overflow happen */
+        u32 m4_message[MAX_NUM];
+        u32 in_idx;
+        u32 out_idx;
+        u32 core_id;
+        spinlock_t mu_lock;
+#ifdef CONFIG_PM_SLEEP
+        struct semaphore pm_sem;
+        int sleep_flag;
+#endif
+};
+
+struct light_rpmsg_head {
+	u8 cate;
+	u8 major;
+	u8 minor;
+	u8 type;
+	u8 cmd;
+	u8 reserved[5];
+} __attribute__ ((packed));
+
+#endif /* __LINUX_LIGHT_RPMSG_H__*/
+
diff --git a/kernel/kexec_core.c b/kernel/kexec_core.c
index b7246b7171b7..52de73abd9fc 100644
--- a/kernel/kexec_core.c
+++ b/kernel/kexec_core.c
@@ -51,7 +51,7 @@ atomic_t __kexec_lock = ATOMIC_INIT(0);
 
 /* Flag to indicate we are going to kexec a new kernel */
 bool kexec_in_progress = false;
-
+EXPORT_SYMBOL(kexec_in_progress);
 
 /* Location of the reserved area for the crash kernel */
 struct resource crashk_res = {
diff --git a/kernel/panic.c b/kernel/panic.c
index ef9f9a4e928d..0506d3ceb06c 100644
--- a/kernel/panic.c
+++ b/kernel/panic.c
@@ -37,6 +37,7 @@
 #include <linux/context_tracking.h>
 #include <trace/events/error_report.h>
 #include <asm/sections.h>
+#include <linux/firmware/thead/light_event.h>
 
 #define PANIC_TIMER_STEP 100
 #define PANIC_BLINK_SPD 18
@@ -281,6 +282,11 @@ void panic(const char *fmt, ...)
 	int state = 0;
 	int old_cpu, this_cpu;
 	bool _crash_kexec_post_notifiers = crash_kexec_post_notifiers;
+	enum light_rebootmode_index mode;
+
+	if (!light_event_get_rebootmode(&mode) &&
+		mode != LIGHT_EVENT_SW_WATCHDOG)
+		light_event_set_rebootmode(LIGHT_EVENT_SW_PANIC);
 
 	if (panic_on_warn) {
 		/*
diff --git a/kernel/sched/fair.c b/kernel/sched/fair.c
index 84af50f4285f..e3bbd67beee6 100644
--- a/kernel/sched/fair.c
+++ b/kernel/sched/fair.c
@@ -10496,6 +10496,9 @@ int can_migrate_task(struct task_struct *p, struct lb_env *env)
 	if (kthread_is_per_cpu(p))
 		return 0;
 
+	if (is_migration_disabled(p))
+		return 0;
+
 #ifdef CONFIG_QOS_SCHED_DYNAMIC_AFFINITY
 	set_task_select_cpus(p, NULL, 0);
 	if (!cpumask_test_cpu(env->dst_cpu, p->select_cpus)) {
diff --git a/kernel/time/tick-oneshot.c b/kernel/time/tick-oneshot.c
index 5e2c2c26b3cc..368c8fc21b1f 100644
--- a/kernel/time/tick-oneshot.c
+++ b/kernel/time/tick-oneshot.c
@@ -78,7 +78,7 @@ int tick_switch_to_oneshot(void (*handler)(struct clock_event_device *))
 	if (!dev || !(dev->features & CLOCK_EVT_FEAT_ONESHOT) ||
 		    !tick_device_is_functional(dev)) {
 
-		pr_info("Clockevents: could not switch to one-shot mode:");
+		pr_debug("Clockevents: could not switch to one-shot mode:");
 		if (!dev) {
 			pr_cont(" no tick device\n");
 		} else {
diff --git a/mm/memblock.c b/mm/memblock.c
index b46bcb931a2e..285bc9757ec7 100644
--- a/mm/memblock.c
+++ b/mm/memblock.c
@@ -1780,6 +1780,7 @@ phys_addr_t __init_memblock memblock_end_of_DRAM(void)
 
 static phys_addr_t __init_memblock __find_max_addr(phys_addr_t limit)
 {
+	phys_addr_t phys_ram_base = memblock_start_of_DRAM();
 	phys_addr_t max_addr = PHYS_ADDR_MAX;
 	struct memblock_region *r;
 
@@ -1789,16 +1790,37 @@ static phys_addr_t __init_memblock __find_max_addr(phys_addr_t limit)
 	 * of those regions, max_addr will keep original value PHYS_ADDR_MAX
 	 */
 	for_each_mem_region(r) {
-		if (limit <= r->size) {
-			max_addr = r->base + limit;
+		if ((r->base + r->size) >= (phys_ram_base + limit)) {
+			max_addr = phys_ram_base + limit;
 			break;
 		}
-		limit -= r->size;
 	}
 
 	return max_addr;
 }
 
+#ifdef CONFIG_HIGHMEM
+phys_addr_t __init_memblock find_max_low_addr(phys_addr_t limit)
+{
+	phys_addr_t max_low_addr = PHYS_ADDR_MAX;
+	phys_addr_t max_low_addr_limit;
+	struct memblock_region *r;
+
+	max_low_addr_limit = memblock_start_of_DRAM() + limit;
+
+	for_each_mem_region(r) {
+		if ((r->base+r->size) <= max_low_addr_limit)
+			max_low_addr = r->base + r->size;
+		else if (r->base < max_low_addr_limit)
+			max_low_addr = max_low_addr_limit;
+		else
+			continue;
+	}
+
+	return max_low_addr;
+}
+#endif
+
 void __init memblock_enforce_memory_limit(phys_addr_t limit)
 {
 	phys_addr_t max_addr;
diff --git a/scripts/package/builddeb b/scripts/package/builddeb
index d7dd0d04c70c..259668daea63 100755
--- a/scripts/package/builddeb
+++ b/scripts/package/builddeb
@@ -85,7 +85,7 @@ install_linux_image () {
 	case "${SRCARCH}" in
 	um)
 		installed_image_path="usr/bin/linux-${KERNELRELEASE}";;
-	parisc|mips|powerpc)
+	parisc|mips|powerpc|riscv*)
 		installed_image_path="boot/vmlinux-${KERNELRELEASE}";;
 	*)
 		installed_image_path="boot/vmlinuz-${KERNELRELEASE}";;
diff --git a/sound/pci/hda/hda_intel.c b/sound/pci/hda/hda_intel.c
index ef6d06fe0f5b..a6863ba97d00 100644
--- a/sound/pci/hda/hda_intel.c
+++ b/sound/pci/hda/hda_intel.c
@@ -298,8 +298,7 @@ enum {
 
 /* quirks for ATI/AMD HDMI */
 #define AZX_DCAPS_PRESET_ATI_HDMI \
-	(AZX_DCAPS_NO_TCSEL | AZX_DCAPS_POSFIX_LPIB|\
-	 AZX_DCAPS_NO_MSI64)
+	(AZX_DCAPS_NO_TCSEL | AZX_DCAPS_POSFIX_LPIB)
 
 /* quirks for ATI HDMI with snoop off */
 #define AZX_DCAPS_PRESET_ATI_HDMI_NS \
@@ -313,7 +312,7 @@ enum {
 
 /* quirks for Nvidia */
 #define AZX_DCAPS_PRESET_NVIDIA \
-	(AZX_DCAPS_NO_MSI | AZX_DCAPS_CORBRP_SELF_CLEAR |\
+	(AZX_DCAPS_CORBRP_SELF_CLEAR |\
 	 AZX_DCAPS_SNOOP_TYPE(NVIDIA))
 
 #define AZX_DCAPS_PRESET_CTHDA \
diff --git a/tools/lib/perf/cpumap.c b/tools/lib/perf/cpumap.c
index 2a5a29217374..b53c22b909b8 100644
--- a/tools/lib/perf/cpumap.c
+++ b/tools/lib/perf/cpumap.c
@@ -405,8 +405,8 @@ struct perf_cpu_map *perf_cpu_map__merge(struct perf_cpu_map *orig,
 					 struct perf_cpu_map *other)
 {
 	struct perf_cpu *tmp_cpus;
-	int tmp_len;
-	int i, j, k;
+	unsigned int tmp_len;
+	unsigned int i, j, k;
 	struct perf_cpu_map *merged;
 
 	if (perf_cpu_map__is_subset(orig, other))
@@ -423,7 +423,7 @@ struct perf_cpu_map *perf_cpu_map__merge(struct perf_cpu_map *orig,
 
 	/* Standard merge algorithm from wikipedia */
 	i = j = k = 0;
-	while (i < __perf_cpu_map__nr(orig) && j < __perf_cpu_map__nr(other)) {
+	while (i < (unsigned int)(__perf_cpu_map__nr(orig)) && j < (unsigned int)(__perf_cpu_map__nr(other))) {
 		if (__perf_cpu_map__cpu(orig, i).cpu <= __perf_cpu_map__cpu(other, j).cpu) {
 			if (__perf_cpu_map__cpu(orig, i).cpu == __perf_cpu_map__cpu(other, j).cpu)
 				j++;
@@ -432,10 +432,10 @@ struct perf_cpu_map *perf_cpu_map__merge(struct perf_cpu_map *orig,
 			tmp_cpus[k++] = __perf_cpu_map__cpu(other, j++);
 	}
 
-	while (i < __perf_cpu_map__nr(orig))
+	while (i < (unsigned int)(__perf_cpu_map__nr(orig)))
 		tmp_cpus[k++] = __perf_cpu_map__cpu(orig, i++);
 
-	while (j < __perf_cpu_map__nr(other))
+	while (j < (unsigned int)(__perf_cpu_map__nr(other)))
 		tmp_cpus[k++] = __perf_cpu_map__cpu(other, j++);
 	assert(k <= tmp_len);
 
diff --git a/tools/perf/pmu-events/arch/riscv/mapfile.csv b/tools/perf/pmu-events/arch/riscv/mapfile.csv
index c61b3d6ef616..b42b65d09c36 100644
--- a/tools/perf/pmu-events/arch/riscv/mapfile.csv
+++ b/tools/perf/pmu-events/arch/riscv/mapfile.csv
@@ -15,3 +15,4 @@
 #
 #MVENDORID-MARCHID-MIMPID,Version,Filename,EventType
 0x489-0x8000000000000007-0x[[:xdigit:]]+,v1,sifive/u74,core
+0x5b7-0x0-0x0,v1,thead/c900-legacy,core
diff --git a/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/cache.json b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/cache.json
new file mode 100644
index 000000000000..2b142348d635
--- /dev/null
+++ b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/cache.json
@@ -0,0 +1,67 @@
+[
+  {
+    "EventName": "L1_ICACHE_ACCESS",
+    "EventCode": "0x00000001",
+    "BriefDescription": "L1 instruction cache access"
+  },
+  {
+    "EventName": "L1_ICACHE_MISS",
+    "EventCode": "0x00000002",
+    "BriefDescription": "L1 instruction cache miss"
+  },
+  {
+    "EventName": "ITLB_MISS",
+    "EventCode": "0x00000003",
+    "BriefDescription": "I-UTLB miss"
+  },
+  {
+    "EventName": "DTLB_MISS",
+    "EventCode": "0x00000004",
+    "BriefDescription": "D-UTLB miss"
+  },
+  {
+    "EventName": "JTLB_MISS",
+    "EventCode": "0x00000005",
+    "BriefDescription": "JTLB miss"
+  },
+  {
+    "EventName": "L1_DCACHE_READ_ACCESS",
+    "EventCode": "0x0000000c",
+    "BriefDescription": "L1 data cache read access"
+  },
+  {
+    "EventName": "L1_DCACHE_READ_MISS",
+    "EventCode": "0x0000000d",
+    "BriefDescription": "L1 data cache read miss"
+  },
+  {
+    "EventName": "L1_DCACHE_WRITE_ACCESS",
+    "EventCode": "0x0000000e",
+    "BriefDescription": "L1 data cache write access"
+  },
+  {
+    "EventName": "L1_DCACHE_WRITE_MISS",
+    "EventCode": "0x0000000f",
+    "BriefDescription": "L1 data cache write miss"
+  },
+  {
+    "EventName": "LL_CACHE_READ_ACCESS",
+    "EventCode": "0x00000010",
+    "BriefDescription": "LL Cache read access"
+  },
+  {
+    "EventName": "LL_CACHE_READ_MISS",
+    "EventCode": "0x00000011",
+    "BriefDescription": "LL Cache read miss"
+  },
+  {
+    "EventName": "LL_CACHE_WRITE_ACCESS",
+    "EventCode": "0x00000012",
+    "BriefDescription": "LL Cache write access"
+  },
+  {
+    "EventName": "LL_CACHE_WRITE_MISS",
+    "EventCode": "0x00000013",
+    "BriefDescription": "LL Cache write miss"
+  }
+]
diff --git a/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/firmware.json b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/firmware.json
new file mode 100644
index 000000000000..9b4a032186a7
--- /dev/null
+++ b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/firmware.json
@@ -0,0 +1,68 @@
+[
+  {
+    "ArchStdEvent": "FW_MISALIGNED_LOAD"
+  },
+  {
+    "ArchStdEvent": "FW_MISALIGNED_STORE"
+  },
+  {
+    "ArchStdEvent": "FW_ACCESS_LOAD"
+  },
+  {
+    "ArchStdEvent": "FW_ACCESS_STORE"
+  },
+  {
+    "ArchStdEvent": "FW_ILLEGAL_INSN"
+  },
+  {
+    "ArchStdEvent": "FW_SET_TIMER"
+  },
+  {
+    "ArchStdEvent": "FW_IPI_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_IPI_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_FENCE_I_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_FENCE_I_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_SFENCE_VMA_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_SFENCE_VMA_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_SFENCE_VMA_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_SFENCE_VMA_ASID_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_GVMA_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_GVMA_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_GVMA_VMID_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_GVMA_VMID_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_VVMA_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_VVMA_RECEIVED"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_VVMA_ASID_SENT"
+  },
+  {
+    "ArchStdEvent": "FW_HFENCE_VVMA_ASID_RECEIVED"
+  }
+]
diff --git a/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/instruction.json b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/instruction.json
new file mode 100644
index 000000000000..c822b5373333
--- /dev/null
+++ b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/instruction.json
@@ -0,0 +1,72 @@
+[
+  {
+    "EventName": "INST_BRANCH_MISPREDICT",
+    "EventCode": "0x00000006",
+    "BriefDescription": "Mispredicted branch instructions"
+  },
+  {
+    "EventName": "INST_BRANCH",
+    "EventCode": "0x00000007",
+    "BriefDescription": "Retired branch instructions"
+  },
+  {
+    "EventName": "INST_JMP_MISPREDICT",
+    "EventCode": "0x00000008",
+    "BriefDescription": "Indirect branch mispredict"
+  },
+  {
+    "EventName": "INST_JMP",
+    "EventCode": "0x00000009",
+    "BriefDescription": "Retired jmp instructions"
+  },
+  {
+    "EventName": "INST_STORE",
+    "EventCode": "0x0000000b",
+    "BriefDescription": "Retired store instructions"
+  },
+  {
+    "EventName": "INST_ALU",
+    "EventCode": "0x0000001d",
+    "BriefDescription": "Retired ALU instructions"
+  },
+  {
+    "EventName": "INST_LDST",
+    "EventCode": "0x0000001e",
+    "BriefDescription": "Retired Load/Store instructions"
+  },
+  {
+    "EventName": "INST_VECTOR",
+    "EventCode": "0x0000001f",
+    "BriefDescription": "Retired Vector instructions"
+  },
+  {
+    "EventName": "INST_CSR",
+    "EventCode": "0x00000020",
+    "BriefDescription": "Retired CSR instructions"
+  },
+  {
+    "EventName": "INST_SYNC",
+    "EventCode": "0x00000021",
+    "BriefDescription": "Retired sync instructions (AMO/LR/SC instructions)"
+  },
+  {
+    "EventName": "INST_UNALIGNED_ACCESS",
+    "EventCode": "0x00000022",
+    "BriefDescription": "Retired Store/Load instructions with unaligned memory access"
+  },
+  {
+    "EventName": "INST_ECALL",
+    "EventCode": "0x00000025",
+    "BriefDescription": "Retired ecall instructions"
+  },
+  {
+    "EventName": "INST_LONG_JP",
+    "EventCode": "0x00000026",
+    "BriefDescription": "Retired long jump instructions"
+  },
+  {
+    "EventName": "INST_FP",
+    "EventCode": "0x0000002a",
+    "BriefDescription": "Retired FPU instructions"
+  }
+]
diff --git a/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/microarch.json b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/microarch.json
new file mode 100644
index 000000000000..0ab6f288af91
--- /dev/null
+++ b/tools/perf/pmu-events/arch/riscv/thead/c900-legacy/microarch.json
@@ -0,0 +1,80 @@
+[
+  {
+    "EventName": "LSU_SPEC_FAIL",
+    "EventCode": "0x0000000a",
+    "BriefDescription": "LSU speculation fail"
+  },
+  {
+    "EventName": "IDU_RF_PIPE_FAIL",
+    "EventCode": "0x00000014",
+    "BriefDescription": "Instruction decode unit launch pipeline failed in RF state"
+  },
+  {
+    "EventName": "IDU_RF_REG_FAIL",
+    "EventCode": "0x00000015",
+    "BriefDescription": "Instruction decode unit launch register file fail in RF state"
+  },
+  {
+    "EventName": "IDU_RF_INSTRUCTION",
+    "EventCode": "0x00000016",
+    "BriefDescription": "retired instruction count of Instruction decode unit in RF (Register File) stage"
+  },
+  {
+    "EventName": "LSU_4K_STALL",
+    "EventCode": "0x00000017",
+    "BriefDescription": "LSU stall times for long distance data access (Over 4K)",
+    "PublicDescription": "This stall occurs when translate virtual address with page offset over 4k"
+  },
+  {
+    "EventName": "LSU_OTHER_STALL",
+    "EventCode": "0x00000018",
+    "BriefDescription": "LSU stall times for other reasons (except the 4k stall)"
+  },
+  {
+    "EventName": "LSU_SQ_OTHER_DIS",
+    "EventCode": "0x00000019",
+    "BriefDescription": "LSU store queue discard others"
+  },
+  {
+    "EventName": "LSU_SQ_DATA_DISCARD",
+    "EventCode": "0x0000001a",
+    "BriefDescription": "LSU store queue discard data (uops)"
+  },
+  {
+    "EventName": "BRANCH_DIRECTION_MISPREDICTION",
+    "EventCode": "0x0000001b",
+    "BriefDescription": "Branch misprediction in BTB"
+  },
+  {
+    "EventName": "BRANCH_DIRECTION_PREDICTION",
+    "EventCode": "0x0000001c",
+    "BriefDescription": "All branch prediction in BTB",
+    "PublicDescription": "This event including both successful prediction and failed prediction in BTB"
+  },
+  {
+    "EventName": "INTERRUPT_ACK_COUNT",
+    "EventCode": "0x00000023",
+    "BriefDescription": "acknowledged interrupt count"
+  },
+  {
+    "EventName": "INTERRUPT_OFF_CYCLE",
+    "EventCode": "0x00000024",
+    "BriefDescription": "PLIC arbitration time when the interrupt is not responded",
+    "PublicDescription": "The arbitration time is recorded while meeting any of the following:\n- CPU is M-mode and MIE == 0\n- CPU is S-mode and delegation and SIE == 0\n"
+  },
+  {
+    "EventName": "IFU_STALLED_CYCLE",
+    "EventCode": "0x00000027",
+    "BriefDescription": "Number of stall cycles of the instruction fetch unit (IFU)."
+  },
+  {
+    "EventName": "IDU_STALLED_CYCLE",
+    "EventCode": "0x00000028",
+    "BriefDescription": "hpcp_backend_stall Number of stall cycles of the instruction decoding unit (IDU) and next-level pipeline unit."
+  },
+  {
+    "EventName": "SYNC_STALL",
+    "EventCode": "0x00000029",
+    "BriefDescription": "Sync instruction stall cycle fence/fence.i/sync/sfence"
+  }
+]
-- 
2.34.1

