From 369bfc8ea8c0a9da51b4bd964f0045cb389c3c2f Mon Sep 17 00:00:00 2001
From: ostannard <oliver.stannard@arm.com>
Date: Mon, 26 Feb 2024 12:23:25 +0000
Subject: [PATCH 3/3] [ARM] Update IsRestored for LR based on all returns
 (#82745)

PR #75527 fixed ARMFrameLowering to set the IsRestored flag for LR based
on all of the return instructions in the function, not just one.
However, there is also code in ARMLoadStoreOptimizer which changes
return instructions, but it set IsRestored based on the one instruction
it changed, not the whole function.

The fix is to factor out the code added in #75527, and also call it from
ARMLoadStoreOptimizer if it made a change to return instructions.

Fixes #80287.
---
 llvm/lib/Target/ARM/ARMFrameLowering.cpp      | 11 +++++----
 llvm/lib/Target/ARM/ARMFrameLowering.h        |  4 ++++
 llvm/lib/Target/ARM/ARMLoadStoreOptimizer.cpp | 23 ++++++++-----------
 3 files changed, 21 insertions(+), 17 deletions(-)

diff --git a/llvm/lib/Target/ARM/ARMFrameLowering.cpp b/llvm/lib/Target/ARM/ARMFrameLowering.cpp
index 650f4650eef0..008ba4e5924b 100644
--- a/llvm/lib/Target/ARM/ARMFrameLowering.cpp
+++ b/llvm/lib/Target/ARM/ARMFrameLowering.cpp
@@ -2766,10 +2766,7 @@ void ARMFrameLowering::determineCalleeSaves(MachineFunction &MF,
   AFI->setLRIsSpilled(SavedRegs.test(ARM::LR));
 }
 
-void ARMFrameLowering::processFunctionBeforeFrameFinalized(
-    MachineFunction &MF, RegScavenger *RS) const {
-  TargetFrameLowering::processFunctionBeforeFrameFinalized(MF, RS);
-
+void ARMFrameLowering::updateLRRestored(MachineFunction &MF) {
   MachineFrameInfo &MFI = MF.getFrameInfo();
   if (!MFI.isCalleeSavedInfoValid())
     return;
@@ -2793,6 +2790,12 @@ void ARMFrameLowering::processFunctionBeforeFrameFinalized(
   }
 }
 
+void ARMFrameLowering::processFunctionBeforeFrameFinalized(
+    MachineFunction &MF, RegScavenger *RS) const {
+  TargetFrameLowering::processFunctionBeforeFrameFinalized(MF, RS);
+  updateLRRestored(MF);
+}
+
 void ARMFrameLowering::getCalleeSaves(const MachineFunction &MF,
                                       BitVector &SavedRegs) const {
   TargetFrameLowering::getCalleeSaves(MF, SavedRegs);
diff --git a/llvm/lib/Target/ARM/ARMFrameLowering.h b/llvm/lib/Target/ARM/ARMFrameLowering.h
index 8d2b8beb9a58..3c7358d8cd53 100644
--- a/llvm/lib/Target/ARM/ARMFrameLowering.h
+++ b/llvm/lib/Target/ARM/ARMFrameLowering.h
@@ -59,6 +59,10 @@ public:
   void determineCalleeSaves(MachineFunction &MF, BitVector &SavedRegs,
                             RegScavenger *RS) const override;
 
+  /// Update the IsRestored flag on LR if it is spilled, based on the return
+  /// instructions.
+  static void updateLRRestored(MachineFunction &MF);
+
   void processFunctionBeforeFrameFinalized(
       MachineFunction &MF, RegScavenger *RS = nullptr) const override;
 
diff --git a/llvm/lib/Target/ARM/ARMLoadStoreOptimizer.cpp b/llvm/lib/Target/ARM/ARMLoadStoreOptimizer.cpp
index 93db983b92c0..37d9e1addd1e 100644
--- a/llvm/lib/Target/ARM/ARMLoadStoreOptimizer.cpp
+++ b/llvm/lib/Target/ARM/ARMLoadStoreOptimizer.cpp
@@ -2062,17 +2062,6 @@ bool ARMLoadStoreOpt::MergeReturnIntoLDM(MachineBasicBlock &MBB) {
       MO.setReg(ARM::PC);
       PrevMI.copyImplicitOps(*MBB.getParent(), *MBBI);
       MBB.erase(MBBI);
-      // We now restore LR into PC so it is not live-out of the return block
-      // anymore: Clear the CSI Restored bit.
-      MachineFrameInfo &MFI = MBB.getParent()->getFrameInfo();
-      // CSI should be fixed after PrologEpilog Insertion
-      assert(MFI.isCalleeSavedInfoValid() && "CSI should be valid");
-      for (CalleeSavedInfo &Info : MFI.getCalleeSavedInfo()) {
-        if (Info.getReg() == ARM::LR) {
-          Info.setRestored(false);
-          break;
-        }
-      }
       return true;
     }
   }
@@ -2120,14 +2109,22 @@ bool ARMLoadStoreOpt::runOnMachineFunction(MachineFunction &Fn) {
   isThumb2 = AFI->isThumb2Function();
   isThumb1 = AFI->isThumbFunction() && !isThumb2;
 
-  bool Modified = false;
+  bool Modified = false, ModifiedLDMReturn = false;
   for (MachineBasicBlock &MBB : Fn) {
     Modified |= LoadStoreMultipleOpti(MBB);
     if (STI->hasV5TOps() && !AFI->shouldSignReturnAddress())
-      Modified |= MergeReturnIntoLDM(MBB);
+      ModifiedLDMReturn |= MergeReturnIntoLDM(MBB);
     if (isThumb1)
       Modified |= CombineMovBx(MBB);
   }
+  Modified |= ModifiedLDMReturn;
+
+  // If we merged a BX instruction into an LDM, we need to re-calculate whether
+  // LR is restored. This check needs to consider the whole function, not just
+  // the instruction(s) we changed, because there may be other BX returns which
+  // still need LR to be restored.
+  if (ModifiedLDMReturn)
+    ARMFrameLowering::updateLRRestored(Fn);
 
   Allocator.DestroyAll();
   return Modified;
-- 
2.33.0

