From 3020ae141ef40f06b17eb0f16d2a3c6d5872ff89 Mon Sep 17 00:00:00 2001
From: jiangfangjie <jiangfangjie@huawei.com>
Date: Wed, 29 Jul 2020 08:45:50 +0000
Subject: [PATCH 05/19] delete the in tpm.txt

Signed-off-by: jiangfangjie <jiangfangjie@huawei.com>
---
 docs/specs/tpm.txt | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/docs/specs/tpm.txt b/docs/specs/tpm.txt
index 5d8c26b1..9c8cca04 100644
--- a/docs/specs/tpm.txt
+++ b/docs/specs/tpm.txt
@@ -89,7 +89,7 @@ TPM upon reboot. The PPI specification defines the operation requests and the
 actions the firmware has to take. The system administrator passes the operation
 request number to the firmware through an ACPI interface which writes this
 number to a memory location that the firmware knows. Upon reboot, the firmware
-finds the number and sends commands to the the TPM. The firmware writes the TPM
+finds the number and sends commands to the TPM. The firmware writes the TPM
 result code and the operation request number to a memory location that ACPI can
 read from and pass the result on to the administrator.
 
-- 
2.23.0

