From 42a26d7136b259ee7ff1b39325e19ef5ef9fe0e3 Mon Sep 17 00:00:00 2001
From: "Min Hu (Connor)" <humin29@huawei.com>
Date: Fri, 11 Feb 2022 12:49:22 +0800
Subject: [PATCH 01/13] ethdev: introduce dump API
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Added the ethdev dump API which provides querying private info from device.
There exists many private properties in different PMD drivers, such as
adapter state, Rx/Tx func algorithm in hns3 PMD. The information of these
properties is important for debug. As the information is private, the new
API is introduced.

Signed-off-by: Min Hu (Connor) <humin29@huawei.com>
Acked-by: Morten Brørup <mb@smartsharesystems.com>
Acked-by: Ray Kinsella <mdr@ashroe.eu>
Acked-by: Ajit Khaparde <ajit.khaparde@broadcom.com>
Acked-by: Ferruh Yigit <ferruh.yigit@intel.com>
---
 lib/ethdev/ethdev_driver.h | 23 +++++++++++++++++++++++
 lib/ethdev/rte_ethdev.c    | 17 +++++++++++++++++
 lib/ethdev/rte_ethdev.h    | 21 +++++++++++++++++++++
 3 files changed, 61 insertions(+)

diff --git a/lib/ethdev/ethdev_driver.h b/lib/ethdev/ethdev_driver.h
index d95605a355..e24ff7064c 100644
--- a/lib/ethdev/ethdev_driver.h
+++ b/lib/ethdev/ethdev_driver.h
@@ -990,6 +990,26 @@ typedef int (*eth_representor_info_get_t)(struct rte_eth_dev *dev,
 typedef int (*eth_rx_metadata_negotiate_t)(struct rte_eth_dev *dev,
 				       uint64_t *features);
 
+/**
+
+ * @internal
+ * Dump private info from device to a file.
+ *
+ * @param dev
+ *   Port (ethdev) handle.
+ * @param file
+ *   A pointer to a file for output.
+ *
+ * @return
+ *   Negative value on error, 0 on success.
+ *
+ * @retval 0
+ *   Success
+ * @retval -EINVAL
+ *   Invalid file
+ */
+typedef int (*eth_dev_priv_dump_t)(struct rte_eth_dev *dev, FILE *file);
+
 /**
  * @internal A structure containing the functions exported by an Ethernet driver.
  */
@@ -1186,6 +1206,9 @@ struct eth_dev_ops {
 	 * kinds of metadata to the PMD
 	 */
 	eth_rx_metadata_negotiate_t rx_metadata_negotiate;
+
+	/** Dump private info from device */
+	eth_dev_priv_dump_t eth_dev_priv_dump;
 };
 
 /**
diff --git a/lib/ethdev/rte_ethdev.c b/lib/ethdev/rte_ethdev.c
index a1d475a292..b9a452107f 100644
--- a/lib/ethdev/rte_ethdev.c
+++ b/lib/ethdev/rte_ethdev.c
@@ -6472,6 +6472,23 @@ rte_eth_rx_metadata_negotiate(uint16_t port_id, uint64_t *features)
 		       (*dev->dev_ops->rx_metadata_negotiate)(dev, features));
 }
 
+int
+rte_eth_dev_priv_dump(uint16_t port_id, FILE *file)
+{
+	struct rte_eth_dev *dev;
+
+	RTE_ETH_VALID_PORTID_OR_ERR_RET(port_id, -ENODEV);
+	dev = &rte_eth_devices[port_id];
+
+	if (file == NULL) {
+		RTE_ETHDEV_LOG(ERR, "Invalid file (NULL)\n");
+		return -EINVAL;
+	}
+
+	RTE_FUNC_PTR_OR_ERR_RET(*dev->dev_ops->eth_dev_priv_dump, -ENOTSUP);
+	return eth_err(port_id, (*dev->dev_ops->eth_dev_priv_dump)(dev, file));
+}
+
 RTE_LOG_REGISTER_DEFAULT(rte_eth_dev_logtype, INFO);
 
 RTE_INIT(ethdev_init_telemetry)
diff --git a/lib/ethdev/rte_ethdev.h b/lib/ethdev/rte_ethdev.h
index fa299c8ad7..b8f135ba3f 100644
--- a/lib/ethdev/rte_ethdev.h
+++ b/lib/ethdev/rte_ethdev.h
@@ -5188,6 +5188,27 @@ int rte_eth_representor_info_get(uint16_t port_id,
 __rte_experimental
 int rte_eth_rx_metadata_negotiate(uint16_t port_id, uint64_t *features);
 
+/**
+ * @warning
+ * @b EXPERIMENTAL: this API may change, or be removed, without prior notice
+ *
+ * Dump private info from device to a file. Provided data and the order depends
+ * on the PMD.
+ *
+ * @param port_id
+ *   The port identifier of the Ethernet device.
+ * @param file
+ *   A pointer to a file for output.
+ * @return
+ *   - (0) on success.
+ *   - (-ENODEV) if *port_id* is invalid.
+ *   - (-EINVAL) if null file.
+ *   - (-ENOTSUP) if the device does not support this function.
+ *   - (-EIO) if device is removed.
+ */
+__rte_experimental
+int rte_eth_dev_priv_dump(uint16_t port_id, FILE *file);
+
 #include <rte_ethdev_core.h>
 
 /**
-- 
2.30.0

