From 6e13a3b539105b2773e43055c2d44912cbba7a29 Mon Sep 17 00:00:00 2001
From: lei_ju <lj3074194431@163.com>
Date: Wed, 3 Jun 2020 09:03:49 +0800
Subject: [PATCH] fix unaligned point value with GCC9

---
 firmware/2lib/include/2struct.h | 2 +-
 firmware/include/gpt.h          | 2 +-
 firmware/include/vboot_struct.h | 2 +-
 3 files changed, 3 insertions(+), 3 deletions(-)

diff --git a/firmware/2lib/include/2struct.h b/firmware/2lib/include/2struct.h
index 1d5b353..b045a0b 100644
--- a/firmware/2lib/include/2struct.h
+++ b/firmware/2lib/include/2struct.h
@@ -213,7 +213,7 @@ struct vb2_shared_data {
 	uint32_t gbb_size;
 
 
-} __attribute__((packed));
+} __attribute__((aligned));
 
 /****************************************************************************/
 
diff --git a/firmware/include/gpt.h b/firmware/include/gpt.h
index 4570237..f1da14d 100644
--- a/firmware/include/gpt.h
+++ b/firmware/include/gpt.h
@@ -120,7 +120,7 @@ typedef struct {
 	} attrs;
 	uint16_t name[36];  /* UTF-16 encoded partition name */
 	/* Remainder of entry is reserved and should be 0 */
-} __attribute__((packed)) GptEntry;
+} __attribute__((aligned)) GptEntry;
 
 #define GPTENTRY_EXPECTED_SIZE 128
 
diff --git a/firmware/include/vboot_struct.h b/firmware/include/vboot_struct.h
index fd5777a..a06d038 100644
--- a/firmware/include/vboot_struct.h
+++ b/firmware/include/vboot_struct.h
@@ -478,7 +478,7 @@ typedef struct VbSharedDataHeader {
 	 * all the fields it knows about are present.  Newer firmware needs to
 	 * use reasonable defaults when accessing older structs.
 	 */
-} __attribute__((packed)) VbSharedDataHeader;
+}  __attribute__((aligned)) VbSharedDataHeader;
 
 /*
  * Size of VbSharedDataheader for each version
-- 
2.23.0

